
	[image: ]
	SELECCIÓN ABREVIADA PARA LA ADQUISICIÓN DE BIENES Y SERVICIOS DE CARACTERÍSTICAS TÉCNICAS UNIFORMES POR SUBASTA INVERSA
 No. SUBASTA-005-2023
	Página 1 de 4



ANEXO No. 02 ESPECIFICACIONES TÉCNICAS
	“SUMINISTRO DE CONSUMIBLES PARA EL ÁREA DE AVIACIÓN DE LA DIRECCIÓN DE ANTINARCÓTICOS-POLICIA NACIONAL”.

	

	

	
	[image: ]
	




	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 2 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 3 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 4 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 5 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 6 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 7 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 8 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 9 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 10 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 11 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 12 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 13 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 14 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 15 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 16 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 17 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 18 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 19 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 20 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 21 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 22 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 23 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 24 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 25 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 26 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 27 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 28 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 29 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 30 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 31 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 32 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 33 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 34 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 35 de 39





	
[image: ]
	Proceso:
	Código:
	

	
	GESTIÓN CONTRACTUAL
Formato:
	
	F-2-1-63V4

	
	
	Fecha: (2023-04)

	
	ESPECIFICACIONES TECNICAS
	

	
	
	Página 36 de 39



	
	
2. CONDICIONES TECNICAS ADICIONALES DE OBLIGATORIO CUMPLIMIENTO
	

	
	
	ITEM
	ESPECIFICACIONES DE VERIFICACION TECNICA
	CUMPLE
	NO CUMPLE
	
	

	
	
	El OFERENTE presentará carta en papel membreteada de la Empresa firmada por el representante legal, en la cual MANIFIESTE QUE SE COMPROMETE de forma irrevocable con la Dirección Antinarcóticos Área de Aviación Policial así:
	
	

	
	
	

1
	En el momento de la entrega de los productos, el contratista deberá presentar al personal técnico y almacenista y facilitar el certificado de conformidad o la respectiva información que permita establecer la trazabilidad del producto (certificado de conformidad (COC), certificado de análisis, informe de prueba, FORMA 8130-3, o equivalentes (EASA Form 1, TCCA Form One en caso que aplique), emitido por la casa fabricante respectiva con cada elemento. En dichos documentos deberá figurar el lote, fecha de fabricación y fecha de expiración en los casos aplicables y especialmente para ítems que tengan tiempo de vencimiento. Los elementos consumibles, insumos y químicos
aeronáuticos deberán entregarse en el embalaje propio con el que el fabricante los ofrece en el mercado
	
	
	
	

	
	
	
2
	El contratista presentará mediante carta de compromiso y brindará respaldo postventa y/o garantía de los productos (1 AÑO) en cualquier momento en caso que sea requerido un cambio del material por defectos o inconsistencias documentales. Cuando se requiera hacer efectiva la garantía, el oferente se compromete a cumplirla en un tiempo máximo de 10 días calendario, asumiendo en su totalidad los
gastos que se generen en dicho proceso.
	
	
	
	

	
	
	


3
	ENTREGA DE INSUMOS CONSUMIBLES NO PREVISTOS EN LA LISTA
	
	
	
	

	
	
	
	La Dirección de Antinarcóticos en cabeza del supervisor del Contrato podrá solicitar productos y/o consumibles adicionales o imprevistos a los descritos anteriormente.
	
	
	
	

	
	
	
	Procedimiento para la adquisición:
	
	
	
	

	
	
	
	EL supervisor podrá realizar un estudio de mercado (tres cotizaciones incluida la del contratista, el cual deberá suministrar la cotización con un plazo no superior a 5 días calendario).
	
	
	
	

	
	
	
	El futuro contratista tendrá la obligación de suministrar los consumibles adicionales previo cumplimiento de los siguientes pasos:
	
	
	
	

	
	
	
	1. Aprobación por parte del supervisor.
	
	
	
	

	
	
	
	2. Requerimiento formal de los consumibles al contratista.
	
	
	
	

	
	
	


4
	Análisis de precio del CONSUMIBLE NO PREVISTO
	
	
	
	

	
	
	
	Dentro de las funciones de verificación y control de precios por parte del supervisor del contrato, tratándose de los elementos no matriculados
y que sean solicitados vía cotización;
	
	
	
	

	
	
	
	El funcionario supervisor podrá;
	
	
	
	

	
	
	
	·	solicitar al contratista que presente un mejor valor de venta debido a la tendencia histórica de adquisición del componente o de
cotizaciones en el mercado,
	
	
	
	

	
	
	
	en cuyo caso el contratista deberá verificar esta situación y ajustar su oferta a los precios del mercado si esto resulta viable,
	
	
	
	

	
	
	
	En caso contrario deberá sustentar los motivos por los cuales no puede realizar los ajustes antes mencionados.
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	5
	El contratista se compromete a que en todos los casos los productos y/o consumibles a adquirir deben cumplir con las características técnicas aprobadas por el fabricante debidamente certificado y en condición NUEVO.
	
	
	
	

	
	
	

6
	TIEMPOS DE ENTREGA:
	
	
	
	

	
	
	
	Por tratarse de un contrato de suministro (Tracto sucesivo), los elementos requeridos serán entregados en un plazo máximo de 20 días calendario para la entrega de productos nacionales contados a partir de la solicitud del supervisor del contrato; los elementos que sean
objeto de importación tendrán como máximo un tiempo de entrega de 60 días calendario, de acuerdo a las necesidades de la institución, previa coordinación con el supervisor del contrato.
	
	
	
	

	
	
	
	En el evento que por programación de producción del fabricante de un ítem se exceda los 15 días para su entrega, esta se podrá extender siempre y cuando no supere los términos de ejecución del contrato y previa certificación emitida por la casa fabricante.
	
	
	
	

	
	
	7
	El oferente deberá suministrar la última versión del material producto y/o consumible, y en el evento que un ítem sea objeto de actualización tecnológica por parte del fabricante se deberá coordinar con el supervisor del contrato para su aceptación.
	
	
	
	

	
	
	
8
	Para los productos y/o consumibles que tienen vida útil, no se recibirán elementos consumibles insumos y químicos aeronáuticos que tenga menos del 60% de vida útil (Shelf life), para aquellos elementos consumibles que su vida útil sea inferior a 18 meses, no se recibirán elementos que tengan menos del 90% de la vida útil (shelf life), a menos que exista concepto de validación por parte del Inspector de la
Línea o Taller y en coordinación con el Supervisor del Contrato y se considere necesidad del servicio.
	
	
	
	

	
	
	9
	El contratista se compromete a suministrar junto con los elementos físicos la declaración de importación de dichos bienes debidamente tramitada.
	
	
	
	

	
	
	
10
	El contratista se compromete que durante la ejecución y liquidación del contrato se cumplirá con la normatividad ambiental vigente. Igualmente, el contratista entregará en medio magnético y físico, las hojas de seguridad –MSDS- material safety data sheets-, de los
elementos químicos y las traducciones simples o certificadas al idioma español.
	
	
	
	

	
	
	

11
	Punto de contacto y servicio 24 horas. Para garantizar una fluida ejecución del contrato, el futuro contratista se compromete a colocar a disposición del Supervisor, un representante con teléfono fijo y/o celular que atienda las solicitudes 24 horas al día.
	
	
	
	

	
	
	
	En el momento de la celebración del contrato deberá informarse por escrito especificando la anterior información.
	
	
	
	

	
	
	
	Los tiempos de respuesta para cotización de elementos no deberán exceder 5 días hábiles en un número de hasta 30 ítems. De requerirse un tiempo mayor esto será previamente concertado con el Supervisor del Contrato.
	
	
	
	

	
	
	12
	El embalaje observará las normas internacionales de transporte de mercancía estipuladas por la OACI.
	
	
	
	

	
	
	

13
	PROCEDIMIENTO DE CANCELACIONES Y AMPLIACIONES DE PLAZO DE ENTREGA.
	
	
	
	

	
	
	
	En el caso de darse situaciones referentes a la no consecución de un ítem por razones atribuibles UNICAMENTE a la rigidez de la
programación de su producción en fábrica, o ser considerado un ítem descontinuado, el futuro contratista deberá dentro de los siguientes 10 días calendario a la solicitud informar por escrito así:
	
	
	
	

	
	
	
	Presentar documento emitido por el fabricante o distribuidor autorizado del fabricante referente a las razones por las cuales dicho(s)
elemento(s) no pueden ser suministrados o la necesidad de extender su plazo de entrega.
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	Referente a CANCELACIONES DE ITEMS el supervisor del contrato podrá cancelar uno o varios ítems después de haber radicado la respectiva solicitud del consumible al contratista, siempre que no haya transcurrido 15 días hábiles
	
	
	
	

	
	
	






14
	El oferente que participe en el presente proceso, debe presentar junto con la oferta copia del CERTIFICADO DE CARENCIA DE INFORMES POR TRÁFICO DE ESTUPEFACIENTES PARA EL MANEJO DE SUSTANCIAS Y PRODUCTOS QUÍMICOS CONTROLADOS CON UNA FECHA DE VIGENCIA MÍNIMA A LA FECHA DE EJECUCIÓN DEL FUTURO CONTRATO MAS 3 MESES, expedida por EL MINISTERIO DE JUSTICIA Y DEL DERECHO – SUBDIRECCION DE CONTROL Y FISCALIZACION DE SUSTANCIAS QUIMICAS Y
ESTUPEFACIENTES, A NOMBRE EXCLUSIVAMENTE DEL PROPONENTE (no se acepta la presentación de certificado de terceros), cuya duración debe estar vigente desde la presentación de la oferta, hasta como mínimo el término de ejecución más 3 meses por temas de garantía, permitiéndose como oferente poder garantizar la disponibilidad de las cantidades mínimas para suministrar las sustancias
controladas en los bienes que apliquen en el presente estudio previo, requiriendo cantidades mínimas así:
	
	
	
	

	
	
	
	SUSTANCIA REQUERIDA
	ACTIVIDAD
	CANTIDAD
	UNIDAD
	
	
	
	

	
	
	
	ACETONA
	ABC
	80
	KG
	
	
	
	

	
	
	
	ALCOHOL ISOPROPILICO
	ABC
	800
	KG
	
	
	
	

	
	
	
	METIL ETHIL CETONA MEK
	ABC
	600
	KG
	
	
	
	

	
	
	
	METIL ISOBUTIL CETONA MIBK
	ABC
	250
	KG
	
	
	
	

	
	
	
	THINNER
	ABC
	1200
	GL
	
	
	
	

	
	
	
	TOLUENO
	ABC
	200
	KG
	
	
	
	

	
	
	
	Nota: Las cantidades aquí exigidas son el resultado de proyección del consumo en un año de estas sustancias controladas por las diferentes Compañías Antinarcóticos de Aviación.
	
	
	
	

	
	
	
15
	El contratista deberá dar cumplimiento a lo establecido en el Decreto 1496 del 6 de agosto del 2018, en lo que respecta con la adopción del sistema globalmente armonizado de clasificación y etiquetado de productos químicos- sga de la organización de las naciones unidas, sexta
edición revisada 2015 y de acuerdo a los tiempos establecidos por el ministerio de trabajo, agricultura, y desarrollo rural, transporte y salud y protección social, de acuerdo a las competencias establecidas en el presente decreto.
	
	
	
	

	
	
	
16
	El contratista deberá presentar junto con la oferta certificación suscrita por el representante legal y/o el responsable de seguridad y salud en el trabajo, en la cual se indique el porcentaje de cumplimiento del Sistema de Gestión de Seguridad y Salud en el Trabajo (SG-SST) de
acuerdo a lo establecido en la Resolución No.0312 de 2019.
	
	
	
	

	
	
	17
	El futuro contratista deberá entregar 3 (tres) bombas manuales de extracción de líquidos, y por cada caneca de 50 galones o más deberá entregar kit de reenvase de consumibles compuesto de 5 envases de 5 galones y guantes de seguridad
	
	
	
	

	
	
	

	
Nota1: El componente técnico requerido fue verificado y tramitado por parte del grupo de mantenimiento aeronáutico del Área de Aviación Policía de la Dirección Antinarcóticos de la Policía Nacional ceñido a los manuales vigentes.

Nota2: Con la presentación de la oferta deben entregarse el cuadro de especificaciones técnicas, con la marca ofrecida, referencia de la marca y anexar ficha técnica del bien ofrecido. La no presentación de las marcas ofrecidas con la oferta ó la subsanación en cualquiera de los ítems con una marca o referencia diferente a la ya ofrecida se entenderá como mejoramiento de la oferta y por ende será rechazada.
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Nota3. Los elementos que estén repetidos dentro de las especificaciones técnicas parcial o totalmente que permitan deducir que se trata del mismo producto, deben tener el mismo valor ofertado so pena rechazo de la oferta.

NOTA: el contratista mantendrá los valores ofertados de los bienes objeto del contrato durante la ejecución, teniendo en cuenta la oferta presentada y aprobada por la entidad, además deberá entregar el objeto contractual acorde a las especificaciones técnicas establecidas en los estudios y documentos previos, el pliego de condiciones definitivo, adendas(si las hubiese), además con las especificaciones adicionales ofrecidas con ocasión de la marca o modelos ofertados de los bienes y/o elementos (si aplica), de acuerdo a las características mínimas requeridas en el anexo (ficha técnica del pliego de condiciones, adenda y oferta) , documentos que hacen parte de integral del presente contrato
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33 e FILTRO DE COMBUSTIBLE PRIMARIO|  EA  [FILTRO DE COMBUSTIBLE PRIMARIO 1

M22759/16-2-9 White Tape Coated
3 MS22759/16-2-9 Fiberglass X 100MT RO [White Tape Coated Fiberglass X 100 MT 1
35 994781026 PACKING EA [PACKING 1
POLIURETANO ANTIDESLIZANTE FD- (Coating Compound, Nonslip, designed to meet A-A-59166, Type Il Volume Solids: 49.91 =
b 37030 M7 |Lo, Viscosit 80-90 K, WeightSolds: 71.32 = 1.0
TIRE 17.00-16 PLY RATING 12.Rated Speed (MPH) 160, Maximum Braking Load (Lbs)

ik frooxie i EA 123900, Rated infiation Ps1) 60 !
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46 99-4346-152 PACKING EA_|PACKING
Producto Mulfusos lubrica piezas movles como bisagras, raedas, odilos, cadenas y
lengrancies. Protege conta el ¢ido y a corosicn en elementos como herramientas y
a Wp-40 Lubricante Mulfusos 362 i1 )
e S lequipos, PUNTO DE EBULLICION: 150°C (300° F), PUNTO DE INFLAMABILIDAD59°C
(138°F) (7CC)
[adhesite, slient fee, Hxolropicsiicone pasteused as  costing sealart or fileting
Primerless Silcone Firewall Sealant -6 material nthe construcion, epair and mainenance ofallypes of aircrat Excellet fre
4| AMSIITADType 1 )
e a2 Cartidge resistance o 3500°F (1927°C) Serice temperature of -85°F to 400°F (-54°C 10 204°C)
Qualifid to BMIS 5.63, AMS3374, BAMS 552-004, and GMINPO0S
Blush etaring tinner used in rinming cellose ntate dopes and lacquers, Specific
9 MIL-T-5085 THINNER EXTRAFINODE52GL | DRUM
araiy. 0843.0.859, Non-iolatle content (max) 10 mg/100 mi
£ V2538811057 PACKING EA_[PACKING
[Acetone technical Mests ASTNFD-328, Flash point 1°F, CAS 67-64-1, Specifc Graiy
51 ASTMD-320 ACETONAXSGL PAL
07918, Puriy. 29.8% by Weight.
2 DATEOT FILTRODE ARE EA_|FILTRODEARE
S e e BIS &3 Sl 1201 bpically used for neror cabi stuctures incuding sets, uggage bins
5 BMS 83120 sEaddes M RO [bukheads,lavetores, wallpanels and in honeycomb srucures, Weave Stle 4 Hamess
Satin,Bresking Strength Warp 160 bfin
o — prny o [P X8 8R16 PLY RATING 12Rated Speed (MPH) 190, Masimur Brakig Load (1)

16500, Rated Inflation (PSI) 140
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|Advance multipurpose grease, itis inhibited against corrosion and has excellent resistance:

55 MILPRF-238278 AEROSHELL GREASE 7 6.6 1b G TRR 1
. to water, useful operating temperature range is -73 °Cto +120 °C mees MILPRF-23827
Coating with excelent chemical resistance, outstanding toughness, fleibilty, abrasion
S AT resistance, and excellent uside durabilty. Conforms to MIL-PRF-85285E Type |- IV, Mix

56 i POLIURETANO BLANCOBRILLANTE |  KIT ~ |Ratio: 3: 1 by Volume, Application Thickness: 18- 2.3 mils, Theoretical Coverage: 800- | 1
190012 @ 1 mil, Impact Flexbilt: 40% Elongation @ RT, Low-Temp Flexibilty: 1* mandrel
bend @ 65°F

i s D £y |Lmpiavios S30Cird, €5 un agene mpaidrios e secado apido- apcacin drecta- |
Producto Biodegradable-que no contiene amoniaco-y no irita i causa dafio a quien lo usa

5% 6895177 ELEMENT FILTERFUELPUMP | EA |ELEMENT FILTER FUEL PUMP. 1

59 o FILTRO DE COMBUSTIBLEPRIMARIO|  EA  |FILTRO DE COMBUSTIBLE PRIMARIO 1
Cables designed primarily for use i aircraft and ground support equipment their high
performance and versatlty makes them ideal in a wide variety of general-purpose electrical

60 | M27500-22TG3TH4 CABLEX 1000FT RO 1
and electronic applications. White Jacket 22 ANG 3 Conductor Shielded White Jacket 22
|AWG 3 Conductor Shielded

61 MS29561-247 PACKING EA_|PACKING 1

62 MS25237-327 LAVP EA_|LAWP 1

63 259881916 PACKING EA_|PACKING 1

64 DWDCO5/16 DRILLS 516 EA |BROCA COBALTO DWDCO SERIES 5/16 1
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EZ TURN LUBRICANT FUEL LUBE

Sealant and lubricant for oil and fuel line valves. Resistant to high temperatures, Worked

& MILG 8032 e Penetration 220 ASTM D-1403, Color Cream, Low Temperature Torque at0° F - Statng
Torque 55,250 g-cm ASTMD-1478
% CH8T101 OILFILTER B [oLFLTER 1
G BT237 FILTRO DE ACEITE EA_|FILTRODEACEITE 1
El V2598811022 PACKING FUEL A |PACKING FUEL 1
5 HL20PBE5-68 HILOKPINCOLLARPACKX100_| EA_[HILOKPINCOLLAR PACK X 100 1
70 DWDCOT8 DRILLS 18 EA_|BROCACOBALTO DWDCO SEREES 18 1
7 VIS24694553 SCREW MACHINE EA_| SCREWMACHINE 1
Two-component ixolopic paste epoxy ystem designed or bonding mefals and
72 | Magnobond 6308451 | TTXOtOpicPaste i‘:‘m i composite structures, Cure Schedule, 7 days @ 77°F or 1 hour @ 150°-250°F, Specific
G Graity, Part 4 13 PartB: 10Mix: 125
The JPS Kerlar® Dry Fabric 353 s an aramid ber reinforcement for use n aerospace
7 HCS2411035 FIBRAKEVLAR 353.50 X 50 VARDAS appiications wherehigh srength, low weight and impactresistance are essentil, Sl
353, Weate: 4 Hamess Satin Dy Fabric Nominal Thickness- 8 4mil (24mm)
7] ANS-QQA2505 SHEET METAL 0,020 EA_|Lamina de aluminio AMS-QQ-A-2505 0,020
75 DAST0 FILTRO DE ARE EA_|FILTRODEARE
7 53085014 ORING EA_|ORNG
= e R Ml EvyiKeone Proxide,CAS Nr. 1336.234, Viscosy t20°C. 6rmPa, Dersiya

20°C. 1,128 giml
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EZ TURN LUBRICANT FUEL LUBE

Sealant and lubricant for oil and fuel line valves. Resistant to high temperatures, Worked
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7 HCS2411035 FIBRAKEVLAR 353.50 X 50 VARDAS appiications wherehigh srength, low weight and impactresistance are essentil, Sl
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78 | ABRASIVE 240 GRIT Abrasive Cloth or Paper, XPLEGO | EA _|Abrasive Cloth or Paper, X PLIEGO
Coating with excelent chemical resistance, outstanding toughness, fleibilty, abrasion
resistance, and excellent uside durabilty. Conforms to MIL-PRF-85285E Type |-V, Mix

79 | MILPRF-85285E Type |-V POUURET;SJOE;%T(ZTL??N POMCE | |Ratio 31 by Volume, Appication Thickness: 1823 ik, Theoreical Coerage: 800-
19002 @ 1 mil, Impact Flexbilt: 40% Elongation @ RT, Low-Temp Flexibiy: 1" mandrel
bend @ 65°F

80 WF336680 FILTER ELEMENT OIL EA_|FILTER ELEMENT OIL

81 MS29513-124 PACKING EA_|PACKING
POLYURETHANE THINNER This product conforms to MIL-T-81772, Type |, MIN. FLASH

82| MLT817728TPOI THINNER TIPO X5 GL PAL  [POINT F ('C) 22°F (-5°C) is infended for use with:MIL-PRF-83231, 83286, 85285, 85322 (2
Part Alihatic Polyurethane Coatings) MIL-DTL46168 (2 Part GARC Polyurethane Goating)

83 4415122 FILTRO SEPARADOR DE AGUA EA_|FILTRO SEPARADOR DEAGUA
Nombre Comercial Tolueno, Fommula Quimica G7HS, CAS 188-88-3, DENSIDAD 087 glcc,

84 g i PALIPUNTO DE INFLAMACION 4 5°C , INDICE DE REFRACCION. 14967

8 DEWEZS19 SCREW EXTRACTORS X SET EA_|SCREW EXTRACTORS SET SIZE-RANGE 1-6 DEWEZST-9

" I GREASE ARCRAFT Mobi grease 28, | _, | General pupose arcrfl Grease Supreme perormance, high femperatre, aniwear rease

134 0ztube meets the qualty leve! of U.S. Miltary Specification MIL-G-81322€, NLGI Grade 1.5

&7 DWDC05/32 DRILLS 532 EA__|BROCA COBALTO DWDCO SERIES 5/32

8 60002 TEMP-PLATE EA_|TEMP-PLATE

89 MS24665-377 PINCOTTER EA |PNCOTTER
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Bateria 24M-XHD Amperios de arranque en frio (CCA) 800, Amperios de arranque

| 2amxe sooccatooomca BATERIA B4} (c4)1000,Resena de Capacidad (RC) 135 minutos 1
91 INTK8S SCRAPER PLASTIC EA_|SCRAPER PLASTIC 1
; Hexcel's HexForce® Fiberglass Dry Fabric 1681, Fir resistance, Thermal and electical
92 HCS2410-020 FmE:zt’tiﬂ?m?i:& \VSSL’AN "\ RO [nsting propertie,Fabri Thickness: 8 5mil (22mim), Weate Sl & Harness Sat, 1
[Weave Stle 8 Hamess Satin, Breaking Strengih Warp 450 Iofin, Fillng 380 bfin
o |PR-1428 GLASS B s atwo-par manganese doxide cured, pofsfide compound.thas a
93 PR14288 112 ADHESIVE SEALANT 7 |Feice temperatue range fom 85°F (54°C) 0 250°F (121°C) Tested n accordance it | 1
MILS-8784 CLASS B
94_[AMS-QQ-A-250-2024-T3.0.04 SHEET METAL EA_|Lamina de aluminio 2024-T3 de 0,040 de 48 X 144" (4 X 1211) 1
& o GINTAANTIFRIGGIONMODEL'S- | _ " [3V15423 UHMIN Film Tape 2" 18 yis Reducesficton,nofse and vbraton on materal |
18660 handing equipment Handles temperatures from ~30°F to 225°F
% VAC1SET STEP DRILLSXSET EA_|STEP DRILLVAC SERIES 5Piece Set#1,2,3,4, 6 VACI6SET 1
o7 281881-001 BATERIAS 12V. DELCO EA_|281881-001 DEKABATTERY 12VOLT-HOBART GROUND SYSTEM 1
% | 299 LIJA Siikit De 3m 2599 P80 RO _|LWA SiikitDe 3m 2599 P80 1
% TELADE GARZA TELADE GARZAX 100MT RO | TELADE GARZAX100MT 1
0 - FILW, RELEASE NON-PERFORATED 1| _ | HCS2108-VP i an FEP resin base elease fim exb high eongalon and excellent ;
ROLL =48" WIDTHX 200YDS release characteristics, maximum use temperature 500 °F (260°C) Elongation MD: 160 %,
101 CINTAENWASCARAR 255+ DEABMM | 2y | CINTA ENMASCARAR 233+ DE 4GMM X S5MT = 1

TAPE MASKING 2in

X55MT =2
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Bateria 24M-XHD Amperios de arranque en frio (CCA) 800, Amperios de arranque
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102 MS24665-306 PINCOTTER EA |PINCOTTER 1

Costing withexcellent chemical resistance, outstanding oughness, flexibilty, abrasion
' resistance, and excellent utside durablt. Conforms fo MIL-PRF-85285E Type -V, Mix

103 M‘L'PRW;Z':? eV | oL URETAN GRIS MATE KIT  [Ratio: 3 1byVolume, Applicaton Thickness: 18-23mils, Theoretcal Corerage: 800- | 1
50012 @ 1 mil,Impact Flexibilty: 0% Elongation @ RT, Low-Temp Fleibilty: * mandrel
bend @ -65°F

0 2921 OILFILTER EA_|OLFILTER 1

105 | CEPILLO CERDAMETALICA | CEPILLODE CERDADEBRONCE | EA |CEPILLO DE GERDADE BRONCE 1

106 TSD275T BROCANO 27 TALADRODE0 | EA |BROCANo 27 TALADRODE 80 1

07 ANG25-10R6 SCREW MACHINE EA_| SCREWMACHINE 1

CINTAENMASCARAR 233 DE 18MM !

| ppetieiicn g RO [CINTAENMASCARAR 233+ DE 18MIM X 55MT= 34 1

109 RG-400 RGA[sgg;: Ccffx)‘(as‘uc;?f PHE | RO |cable coaxial de RF flexble estandar RG 400 DXE RG400-CTL X500 FT 1

10| 304018 AW 3840188 ARFILTER EA_|ARFILTER 1

i DWDCO27 DRILLS No 27 A |BROCACOBALTO DWDCO SERES No27 1

2 TSDER2ST BROCANO 532 TAADRODE S0 | EA _|THREADED SHANK DRILLS Stubby Series SIZE 552 1

13|  PINCEL No8PLAND PINCEL N'o 8 PLAND A |PINCELN08PLANO T
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Extremely strong, medium-cure, water-resistant clear adhesive that will sef-level after

14 14310 Devcon® 14310 2-Ton-25 ml Tube | TB application, Color (Mixed) Clear Senice Temperature Dry, 40°F to 200°F, Impact 1
Resistance 6.5 fL-b.in.(2), 14310 25 mi Dev-Tube
CINTAENMASCARAR 233+ DE 6MM X
e ey RO |CINTAENMASCARAR 233+ DE 6MM X 55MT: 1
116 TSD40ST BROCA No 40 TALADRO DE 90 EA_| THREADED SHANK DRILLS Stubby Series SIZE 40 1
117 691035 FUELFILTER EA_|FUELFILTER 1
118 05113107515 Scotch Bie Roloc Blue 2° EA_|Scotch-Brite Roloc Blue 2 1
119 DWDCO7132 DRILLS 7132 EA__|BROCA COBALTO DWDCO SERIES 7/32 1
120 HCS2108-P5 . RELEASEZZE:EOWED“ 1 R0 |HCS2108.P5 FILM, RELEASE PERFORATED, 48° X200YD 1
121 MS9388-009 PACKING EA_|PACKING 1
122 SKF 17699 RADIAL SHAFT SEAL EA_|RADIAL SHAFT SEAL 1
e P REMOVEDOR DEPINTURAX 5 GL | patL_|I9"-Perorming paint tipper forremovingurehanes, epares, pimers and enamels i
Conforms To MILR81294
[EPOXY THINNER This product conforms fo MIL-T-81772, Type Il MIN. FLASH POINT *F
(C) 32°F (0°C) Eposy Thinner s infended for use with:MIL-DTL-24441 Paint & Primer ll
24| MLTBIT72BTPON THINNER TIPO I X5 GL PAIL | Types MIL-PRF-22750 Epoxy Polyamide Coatings, MIL-PRF-23236 Epoxy Primers & 1

(Coatings, MIL-PRF-23377 Epoxy Polyamide Primer Goatings MIL-DTL-53022 Epoxy
Primer MIL-PRF 4556 Epoxy Primer & Topcoat





image23.jpeg
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14 14310 Devcon® 14310 2-Ton-25 ml Tube | TB application, Color (Mixed) Clear Senice Temperature Dry, 40°F to 200°F, Impact 1
Resistance 6.5 fL-b.in.(2), 14310 25 mi Dev-Tube
CINTAENMASCARAR 233+ DE 6MM X
e ey RO |CINTAENMASCARAR 233+ DE 6MM X 55MT: 1
116 TSD40ST BROCA No 40 TALADRO DE 90 EA_| THREADED SHANK DRILLS Stubby Series SIZE 40 1
117 691035 FUELFILTER EA_|FUELFILTER 1
118 05113107515 Scotch Bie Roloc Blue 2° EA_|Scotch-Brite Roloc Blue 2 1
119 DWDCO7132 DRILLS 7132 EA__|BROCA COBALTO DWDCO SERIES 7/32 1
120 HCS2108-P5 . RELEASEZZE:EOWED“ 1 R0 |HCS2108.P5 FILM, RELEASE PERFORATED, 48° X200YD 1
121 MS9388-009 PACKING EA_|PACKING 1
122 SKF 17699 RADIAL SHAFT SEAL EA_|RADIAL SHAFT SEAL 1
e P REMOVEDOR DEPINTURAX 5 GL | patL_|I9"-Perorming paint tipper forremovingurehanes, epares, pimers and enamels i
Conforms To MILR81294
[EPOXY THINNER This product conforms fo MIL-T-81772, Type Il MIN. FLASH POINT *F
(C) 32°F (0°C) Eposy Thinner s infended for use with:MIL-DTL-24441 Paint & Primer ll
24| MLTBIT72BTPON THINNER TIPO I X5 GL PAIL | Types MIL-PRF-22750 Epoxy Polyamide Coatings, MIL-PRF-23236 Epoxy Primers & 1

(Coatings, MIL-PRF-23377 Epoxy Polyamide Primer Goatings MIL-DTL-53022 Epoxy
Primer MIL-PRF 4556 Epoxy Primer & Topcoat
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125 WK1030 MANFILTER EA |MANFILTER 1

26| M2T0022TGaT A CABLEX1000FT RO _[White Jacket 22 ANG 2 ConduclorShielded Cable, MaterialTn Pated CopperETFE 1
Class | Salent cuback corrosion preventive compound, FLASH PMCC Minimum 106°F,

127 cpe CPCGRADO2 o 1
Specifc Graty @S0°F (156 °C) 0.88, CURE TIME 24 HOURS

28 BROCHAT" BROCHAPELO DE MARTA EA_| BROCHAPELO DEMARTA 1

129 | UmPUDOR DETAPICERM | WMPADOR DEAL’;:‘CER‘A ESPUMA | &4 |LIMPIDOR DE TAPICERIAESPUMA 400mI 1

30 TSDDST BROCALETRAD TAADRODE 90 | EA | THREADED SHANK DRILLS Stubby Series SIZED 1

31| 30547-3078G1 16 HP VANGUARD ENGINE EA_[4790Vanguard Series Engine With 1 In Tapped 38 - 24 Keyway Crankshaf (CARE) 1
LOCTITE EA S320NA AERO i a two-component paste adhesive with good peel srength as

182|  HYSOLEAS320NA AEROEPOXY ADHESIVE 1 QTKIT | QT /KIT |well as elevatedtemperalure resistance. The femperature of the separale componens prir | 1
o mixing isnotcical but should b close o toom temperature (77°F/25°C)

3 ANGBOIDTOL WASHER B [WaSHER 1

134 V250881152 PACKING EA_[PACKING 1

% 512480 GUANTES DENITRILO BOX_|GUANTESDENITRILO 1

136 HUT12260 DRILL GAUGES EA_|DRILL GAUGES Wire Gauge Sizes #1060 HUT12260 1
RTVI06 sealant s paste-consistency sealantsandard svength ightermperature

Momente Sealant Red, 10.1
137 RTVI08 fomenthe SealantRed. 10162 | 15 |scalant Application Rate,(gmin) 400, TackFree Time, min 20 1
cartidge
38 831 BATERIAS FS-16NP 350 AMP A |BATERIA DE 350 AMP F5.16NP T
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139 214-040-812-003 SEAL, GREASE EA |SEAL GREASE 1

140 DWDN&/16 DRILLS 8/16 EA_|BROCAH.SS DWDN SERIES 9/16 1

141 151394 VELCROBLACKLOOP 50 MM X 25M | RO _|VELCRO BLACKLOOP 50 MM X 25M 1

142 453209162 PACKING PREFORMED EA__|PACKING PREFORMED 1

143 DWDCO25/64 DRILLS 25/64 EA_|BROCA COBALTO DWDCO SERIES 25/64 1

LIMPIADOR DE TAPIZADO

4 SIMONIZ Hson gy EA  [LIMPIADOR DE TAPIZADO ESPUMAX 400mi 1

145 DWDCO3/16 DRILLS 3/16 EA__|BROCA COBALTO DWDCO SERIES 316 1
Producto multuso de mantenimiento en spray. Acaba con el xidoy la corrosion, desplaza

146 CRC556 Lubricante 5-66 penetrante 400cc |  EA  |el aguay elimina el Gxido y la suciedad. 400 m, Peso especifico (@ 20°C): 0.82, Purtode | 1
inflamacion (vaso cerrado) : 78°C, Viscosidad (@ 40°C) : 26 mPas

7 AN381-2-16 PINCOTTER 1/16 EA_|PNCOTTER 1/16 1
Coating with excelent chemical resistance, outstanding toughness, flebilty, abrasion

» resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type I-IV, Mix
14g | MILPRFES2E Tipe V| oo e TaNO GRISBRILLANTE | KIT |Rator 31 by Volume, Application Tickness- 1823 mil, Theoreical Corerage: 800- | 1

16251

19002 @ 1 mil, Impact Flexibilt: 40% Elongation @ RT, Low-Temp Flexibity: 1* mandrel

bend @ -65°F
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149 AS5685, 0,041 LOCK WIRE LB |Steel, Corrosion Resistant, Safety Wire AS5685, 0,041" Diameter
e oo e o |TIRE 9006PLY RATING 10 Rated Speed (WPH) 120, Maimum Braking Load (L] 6520
Reted infation (PSI) 58
75| WYPALLX80REGULAR WYPALL X80 REGULAR RO _[WYPALL X-80 REGULAR
152 400642003 VOLTIVETRO 26VDC EA_|VOLTIVIETER DC 400642-003 HOBART
(General purpose, sahentbased adhesire/coatings with good adhesion tosymhefic
3™ Soofch-Weld™ Fuel Resistant
163 EC776 colchield " FEIRESISENt | QT |rubber, metal, glass and many plastics, Flash Point (Closed Cup)S5°F (13°C)Viscosity 1500
Coating EC-776 Quart
- 500 cps, Color Transparent Amber
£ VACS STEPDRLLS EA_|STEP DRILLS 12 STEPS, RANGE 1 4—1-38%8hsVACS
155 BROCHATIN BROCHAT'IN EA_|BROCHATIN
; PINT-_[PR-1440 CLASS A an arcaf integral uelank sealant Cured speciic raviy 157/ Non
i i bl KIT_|iolte content %88, Tested in accordance wih AVS-5-8802
LPS 04016 (07416) no-flammable eleciro contact leaner i deal forremoving dr,
LPS 04015 NoF lash Electro Contact
157 04016 et e o 4| A |maisure, dust. flxand oxides. Baing Pont/ Range 116°F (47.78°C),VOC Corlent695%
: Water Solubity <014 g1L @ 68°F
758 DWDN37/64 DRILLS 37164 EA_|BROCAH 5 S DWDN SEREES 37164
HCS 2125 5  hgh temperature sealanttape for autoclare applicatons up 10 450 °F (232
i HeS20S SEALANT TAPE Black Roll -HCS2125| RO oc, g 1003, non flammable, standar size 0,125 0.5 321
760 DWDCOT364 DRILLS 1364 EA_|BROCACOBALTO DWDCO SEREES 1364
161 MS2461733 SCREW EA|SCREW
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|Acidic liquid cleaner developed for removal of hard water scale and accumulated waste

162 Honey Bee 60T SERVICE WASTE DISPOSAL EA  [materias from vacuum and re-circulating toletsystems in aircref Blue liquid, Surfactants | 1
biodegradable

163 400641012 AMPERIMETRO EA_|Ammeter, DC, 02000 Amps, 50 mVDC 1

164 AS3085-126 PACKING PREFORMED EA_|PACKING PREFORMED 1

165 |AMS-QQ-A-250-2024-T3-0.05 SHEET METAL EA_|Lamina de aluminio 2024-T3 de 0,050 de 48 X 144" (4 X 1211) 1

166 AA2T1 BAGSPLOTH EA_|BAGSPLOTHAA27H4 1

167 PERMALON 327 Lubricant, Dry Film 14 OZ CAN Aerosol | _EA | Lubricant, Dry Film 14 OZ CAN Aerosol PERMALON 327 1

168 AN960416 WASHER EA_|WASHER 1

169 MS287784 ORNG EA_|ORING 1

170 ST3002.05 PACKING EA_|PACKING 1

; PINT-|PR-1428 CLASS A's alow adhesion sealant Cured specific graity 149 / Non volatle

m FR1ZEAR ADHESVE SEALANT KIT _|content % 92 Tested in accordance with MIL-S-8784 CLASS A !
Fast Dry, Two Component Aeroprime Primer per MIL-PRF-23377K. Type |, Class C2,

- — EPOXY PRIVERMLPRF-23377K TY1| .~ |ADS31&-FD Aeroprime Primer - Component A Weigh per Galln: 12.11bs. +-02.Curng |

cLc2 |Agent - Component B, Weight per Gallon: 7.1 Ibs. +0.2, Catalyzation Raio: 3:1 by volume,

Viscosity: 21 - 25° #2 Zahn

73 3029566 GASKET, FUEL NOZZLE EA |GASKET, FUELNOZZLE 1
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High Build, Fast Drying, Urethane Primer Surfacer, used to eliminate mild imperfections in

174 53039WPX PRIMER PARA COMPUESTOS KT |composite substrates, It meets and exceeds the performance requirements of MEP 10-070,
Catalyzaton Ratio: 31 by volume , Weight Solids:69.1% = 1.0, Viscosity: 28 = 5'#4 Ford
175 6873905 RINGRETANING EA_|RINGRETANNG
176 403809002 SWITCHPRESION DE ACEITE EA_|SWITCH PRESION DE ACEITE
- < Pliobond 20 s a general thermosetting adhesive that can be used fo bond virtually all porous
i PLIOBOND 20 s EN;ﬁgzaéDHES‘\ £ PT  [and nonporous substrates, Base synthetic Rubber, specific graviy 0.868, lash poitn 20°F,
application temperature 40-100°F
[Acnjic, plastc and glass cleaner. TESTED AGAINST FEDERAL TEST STANDARD
178 PGC13 PRISTACRYLIGPLASTIC GLASS. |, 14100 N, 406 AND MIL-P-008184D worksinside an outsice th aicraf, and on metal
CLEANER 13 az Aerosol Can
and vyl without harming painted surfaces. 13 oz Aerosol Can
General purpose silicone adhesivelsealant Stable and flexible from -60°C 10 +180°C (76°F
179 RTV732 DOWSIL732-90mL (30z) Tube | B |lo+356°F), with short peaks up to +205°C (401°F) Complies with MIL-A-46106, Specific
Jgravty 1.04
3V13743 Carton Sealing Tape - Clear,
180 510169 355 yds MODEL RO [3m 3743 Cinta Transparente Para Cajas - Largo x AnchoS0 m x 76 mm -X ROLLO
NO.S-10169
[Approved MIL-PRF-680 Type | cleaner sultable for the replacement of
181 AXAREL 1000 CLEANING SOLVENT X5 GL PAIL |isopropl alcohol (PA), acetone, methyl ety ketone (MEK), Low Toxicity, Non-Corrosive,

Flash Point 127 °F (53 °C), Viscosity (25 °C) 136 cps
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182 DWDCO10 DRILLS No 10 EA |BROCA COBALTO DWDCO SERIES No 10 1
i - ACF-50 Lubricant 10013 Pupl, 130z | _, ™ [Anicorosionlubricant compound, hat has been speciicall designed orhe Aerospace |
aerosol can Industy, qualified to Mil-C-81309E, Type I class |
184 DWDACX51/16 DRILLS 6 116 EA_|BROCAHSS DWDAC SERES 6 1/16 1
185 LIMPADORDEPANTALLASLEDXS0 | ¢4 | pupOR DE PANTALLAS LOD x50 ml 1
BINNER ml
& selfetching primer thatis chromate-free and chemically bonds with aluminum and steel o
185 ATO1 PRIMER Zin Phosphate Yellow (12az)|  EA  fform a corrosion resistant base coat. Tack free - 10 minutes, Fullydry ~48 hours, Meets | 1
performance standards outined in Federal Specification TTP17578
187 MS3367-2.9 STRAP TIEDOWN, PACKX100PCS | EA |STRAP TIEDOWN, PACKX 100 PCS 1
188 MS25488 PLUG CONTACTOR SALIDA EA_|PLUG CONTACTOR SALIDA 1
189 DWDCO15/64 DRILLS 16164 EA_|BROCA COBALTO DWDCO SERIES 16164 1
190 TSD20ST BROCA No 20 TALADRO DE 90 EA_| THREADED SHANK DRILLS Stubby Series SIZE 20 1
Extra high performance, synihefic aircraftype gas urbine lubricant engineered
to meet the performance requirements fo gas turbine engines used in commercial and
191) MOBILOL JET 254 R ity aicrf The ffectve operating range ofthe lubricant s between 40°C (40°F)and | '
1232°C (450°F). Specific Grasity 1.0044
PR-1440 Class B is an aircraft infegral fuel tank sealan. has a senice lemperature range
192 PR-A440B-112. ADHESIVE SEALANT QT/KIT [from -65°F (-54°C)to 250°F (121°C) Tack free time (hours)<4, Cure ime to 35 A Durometer| 1

(hours) 12
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Red-dyed, mineral oil based hydraulic fluid developed for the severe duty demands

193 MILH-5606 HIDRAULICO 756 QT |ofaerospace and industial senice, Wide operating temperature range, Low temperature:
idity meets MIL-SPEC: MIL-PRF-5606H, Flash Point, COC, °F 231, API Grauiy 308
REMOVAL AND INSERT PLASTICO ; ;
194 —— prssiy EA|REMOVAL AND INSERT PLASTICOVERDE
195 MS20995C25 LOCKWIRE LB | MS20995C25 Stainless Steel 0.025" Diameler Saety Wire -1 Ib Rol
TIRE 22X6.75-10 PLY RATING 10 Rated Speed (MPH) 190, Maximum Braking Load (Lbs)
% mRgn TRE E4 losso, Rated nfton (Ps1) 125
S Talcum Pouter, Technical rade, | g |29 200y welht magnesium oxide and 400 b weigh magresum oxide and 350 by
[weight siicon dioside and 65.0 by weight ilicon dioxide
198 ANG235-3A GREEN FILTER ELEMENT EA_|GREEN FILTER ELEMENT
199 287562 SOLENOIDE ACELERACION JET X4D | EA _|SOLENOIDE ACELERACION JET X4D
200 6870032 FILTER ELEMENT LUBR EA_|FILTERELEMENT
For melalmetal combinations with slow to medium fast movements and high loads. Sutable
- i MOLYKOTE Ani-Friction Goatng Spra,| -, o the permanentluibication ofighlysiressed lding gides withlow iding speeds,
8 312gm Viscosity at 23°C (#3 cup) seconds 23, Density at 20°C gii 1.07 Seniice temperature range:
°C-18010450
TIRE 19.5%6.75-8 PLY RATING 10,Rated Speed (MPH) 225, Maximum Braking Load (Lbs)
i ki i EA Jo400, Reted ntton Ps1) 110
- — R —— Ca | Graphie Fim Spra i for pre-assemblyan asenbly ubricaion,heatolerant o 3000

°F, Dry in 2-3 min, excellent conductor for electrical applications.
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S Talcum Pouter, Technical rade, | g |29 200y welht magnesium oxide and 400 b weigh magresum oxide and 350 by
[weight siicon dioside and 65.0 by weight ilicon dioxide
198 ANG235-3A GREEN FILTER ELEMENT EA_|GREEN FILTER ELEMENT
199 287562 SOLENOIDE ACELERACION JET X4D | EA _|SOLENOIDE ACELERACION JET X4D
200 6870032 FILTER ELEMENT LUBR EA_|FILTERELEMENT
For melalmetal combinations with slow to medium fast movements and high loads. Sutable
- i MOLYKOTE Ani-Friction Goatng Spra,| -, o the permanentluibication ofighlysiressed lding gides withlow iding speeds,
8 312gm Viscosity at 23°C (#3 cup) seconds 23, Density at 20°C gii 1.07 Seniice temperature range:
°C-18010450
TIRE 19.5%6.75-8 PLY RATING 10,Rated Speed (MPH) 225, Maximum Braking Load (Lbs)
i ki i EA Jo400, Reted ntton Ps1) 110
- — R —— Ca | Graphie Fim Spra i for pre-assemblyan asenbly ubricaion,heatolerant o 3000

°F, Dry in 2-3 min, excellent conductor for electrical applications.
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204|  206-010-147-001 PLUGPROTECTVE EA  |PLUGPROTECTNVE 1
205 TSOFST BROCALETRAF TALADRODE S0 | EA | THREADED SHANK DRILLS Subby Series SIZEF 1
LOCTITE EAS34NA AERO is a two-component fiolropic paste adhesive, which cures at
toom temperature and possesses superior strength fo 300°F/149°C and higher, MMI-A-
206 HYSOL934 Aero Epoxy Paste Adh kit |QT/KIT 1
RSN ESIS 8 132 Qualified The temperature ofthe separate componernts priorto mixing is not citcal, but
shouldbe close o room temperature (T7°F/25°C)
207 VILWA8723 ARCRAFT SOLVENT TYPEWAX | GL | Wax hat cleans and polishes aircraf fuselages ref mirw-18723 1
28 DWDCOS DRILLSNoS EA_|BROCACOBALTO DWDCO SERES No§ 1
[sceite de excelente rendmiento para cojinetesy engrancies, disefiados para proporcionar
un seniio destacado en feminos de proteccion de evipos,ida del acetey operacion sin
20 SHC 626 OIL TRANSMISION X5 GL PAL 1
problemas, it ndice de viscosidad y ausencia d ceras, Grado de viscosidad IS0 68,
purto de congelamiento 48°C, purto de nflamacién 236°C
Elecho contact cleaner ASTM 518, Type 1C, Boiing Port/ Range 1409°F (605°C),
CFCFREE ELECTRO CONTACT
210 03116 i EA|Flash Point Aetosol: < 14°F (<-17.0°C) TCC, Safe on Plasic, Fast Evaporating; Leates No| 1
Residue
E5 un ubricantey poteclr de accion rapiday penelracion profunda, poporciona un
recubrimiento aceitoso ligero, Resisencia deléctica 33 K Punto de infamacion 175°F
21 00216 LUBRICANTE LPS N2 ) 1
(76°C) TCC-dispensediquid, Gravedad especiica 082 - 086 @ 20°C, Rango de
femperatura, 32° (0°C ) to 325°F (163°C)
Plasic leaner removes grease, sains and i, ceaning most lastics wihoutscratcing,
212 80183 PLASTIC CLEANER, 1602 T8 1
: Physical Form Liquid, Pimary Contaner Type Can, NSN 7630014420667
73 02758 BRUSH EA_|BRUSH 1
214  DWD2SIDBSET QUALTECHDRILLBLANKS XSET | EA |DRILLSET Qualtech Dril Blanks DWD26J-DB-SET 1
215 204040760108 FILTER ELEMENT FLUD EA_|FILTER ELEVEENT FLUD 1
216 BROCHAZ' IN BROCHAZ'IN EA |BROCHAZ IN T
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204|  206-010-147-001 PLUGPROTECTVE EA  |PLUGPROTECTNVE 1
205 TSOFST BROCALETRAF TALADRODE S0 | EA | THREADED SHANK DRILLS Subby Series SIZEF 1
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purto de congelamiento 48°C, purto de nflamacién 236°C
Elecho contact cleaner ASTM 518, Type 1C, Boiing Port/ Range 1409°F (605°C),
CFCFREE ELECTRO CONTACT
210 03116 i EA|Flash Point Aetosol: < 14°F (<-17.0°C) TCC, Safe on Plasic, Fast Evaporating; Leates No| 1
Residue
E5 un ubricantey poteclr de accion rapiday penelracion profunda, poporciona un
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(76°C) TCC-dispensediquid, Gravedad especiica 082 - 086 @ 20°C, Rango de
femperatura, 32° (0°C ) to 325°F (163°C)
Plasic leaner removes grease, sains and i, ceaning most lastics wihoutscratcing,
212 80183 PLASTIC CLEANER, 1602 T8 1
: Physical Form Liquid, Pimary Contaner Type Can, NSN 7630014420667
73 02758 BRUSH EA_|BRUSH 1
214  DWD2SIDBSET QUALTECHDRILLBLANKS XSET | EA |DRILLSET Qualtech Dril Blanks DWD26J-DB-SET 1
215 204040760108 FILTER ELEMENT FLUD EA_|FILTER ELEVEENT FLUD 1
216 BROCHAZ' IN BROCHAZ'IN EA |BROCHAZ IN T
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MIL-PRF-85285E Type |-V

Coating with excellent chemical resistance, outstanding toughness, flexibilty, abrasion
resistance, and excellent uside durabilty. Conforms to MIL-PRF-85285E Type |-V, Mix

o 17886 POLIURETANOBEIGE BRILLANTE | KIT  |Ratio: 31 byVolume, Application Thickness: 18-2:3 mils, Theoretcal Corerage: 800-
190012 @ 1 mil, Impact Fleibilty: 40% Elongation @ RT, Low-Temp Flexibilty 1 mandrel
bend @ -65°F

218 |AMS-QQ-A250-2024-T3.0.02 SHEET METAL EA_|Lamina de aluminio 2024-T3 de 0,020 de 48" X 144"~ (4X 121)

PR-1428 CLASS B s  wo-part manganese dioxide cured, polysulfide compound.thas @
219|  PR1426,CLASSB2 ADHESIVE SEALANT Q/KIT |senice temperature range from -85°F (-64°C) to 250°F (121°C) Tested in accordance with
MIL-S-6784 CLASS B Cured specific araiy 1,50/ Non olatile content % 67
2 INS27021 INSERT BITS EA_|INSERT BITS W/ 14 SHANK PHILLIPS SIZE P2
Dow Coring® 736 Nonslumping sealant designed fr sealng and bonding
' appiications exposed foemperatures as high a5 316°C (B00°F)for Aerospace
21 RTV736 Do X‘a"“t' RTV736 90mL | 5 |qaskeing Sealing and encapsulaling heating elements in appliancs, Tack Free Time
Z minutes 17, Cure Time (3.mm [18-inch] thickness) 24 hours

» ANG25 8327 SCREW EA_[scREW
Solucion efectva que eliming los melos olores dejando Una sensacion de Impiezay

2 BRIZZE 300ML AMBIENTADOR AEROSOL 300ML | A [fescura en el ambiente. Elimina el 9% de las bacterias, Rango de femperatura
Joptimo 15-35°C, incoloro,Densidad 0.85 0,05 g

24 DWDCOD DRILLS LETRAD A |BROCA COBALTO DWDCO SERIES SIZED
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MIL-PRF-85285E Type |-V

Coating with excellent chemical resistance, outstanding toughness, flexibilty, abrasion
resistance, and excellent uside durabilty. Conforms to MIL-PRF-85285E Type |-V, Mix
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2 INS27021 INSERT BITS EA_|INSERT BITS W/ 14 SHANK PHILLIPS SIZE P2
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21 RTV736 Do X‘a"“t' RTV736 90mL | 5 |qaskeing Sealing and encapsulaling heating elements in appliancs, Tack Free Time
Z minutes 17, Cure Time (3.mm [18-inch] thickness) 24 hours

» ANG25 8327 SCREW EA_[scREW
Solucion efectva que eliming los melos olores dejando Una sensacion de Impiezay

2 BRIZZE 300ML AMBIENTADOR AEROSOL 300ML | A [fescura en el ambiente. Elimina el 9% de las bacterias, Rango de femperatura
Joptimo 15-35°C, incoloro,Densidad 0.85 0,05 g

24 DWDCOD DRILLS LETRAD A |BROCA COBALTO DWDCO SERIES SIZED
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|AeroShell Oil W10 is an ashiless dispersant oil, promotes engine cleaniiness, help reduce:
oil comsumption AeroShell W100 provides compatiilty with other approved aircraft piston

= Mi-L-22851D ACEITEAEROSHELL W100 AT Jengine s, AeroShell 01100 s produced o meet ful the SAE specication 1559
(Grades SAE 30, 40, 50 and 60 respeciively) SAE viscosit grade 50.

226 CR324344 RVET BLIND EA_|RVETBLIND

RESISTOR 10 OHM 100 WATT

27 S s EA |100W Fixed Resistor

228 204040760109 FILTER ASSY EA_|FILTERASSY

229 ST3001-214 PACKING EA_|PACKING
Coating with excelent chemical resistance, outstanding toughness, flebilty, abrasion
resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type |-V, Mix

230 | MILPRF-85285E Type |-V CLEAR URETHANE KIT  [Ratio: 3:1 by Volume, Application Thickness: 1.8- 2.3 s, Theoretical Coverage: 800-
19002 @ 1 mil, Impact Flexibilt: 40% Elongation @ RT, Low-Temp Flexibity: 1* mandrel
bend @ 65°F

%1 DWDCO1A4 DRILLS 1/4 EA__|BROCA COBALTO DWDCO SERIES 1/4

’ Exira fast seting, wo—component room temperalure curing epoxy adhesive. The

232 4001 DOUB;?S:S:S:?%DEXEWV EA  [system willcure at as low as ~18 °C (0 °F). Viscosity @ 25 °C.cps, part 455,000, Flash
Point, PMCC, °C PartA: 167

233 204-040-760-105 FILTERASSY EA |FILTERASSY
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|AeroShell Oil W10 is an ashiless dispersant oil, promotes engine cleaniiness, help reduce:
oil comsumption AeroShell W100 provides compatiilty with other approved aircraft piston

= Mi-L-22851D ACEITEAEROSHELL W100 AT Jengine s, AeroShell 01100 s produced o meet ful the SAE specication 1559
(Grades SAE 30, 40, 50 and 60 respeciively) SAE viscosit grade 50.

226 CR324344 RVET BLIND EA_|RVETBLIND

RESISTOR 10 OHM 100 WATT

27 S s EA |100W Fixed Resistor

228 204040760109 FILTER ASSY EA_|FILTERASSY

229 ST3001-214 PACKING EA_|PACKING
Coating with excelent chemical resistance, outstanding toughness, flebilty, abrasion
resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type |-V, Mix

230 | MILPRF-85285E Type |-V CLEAR URETHANE KIT  [Ratio: 3:1 by Volume, Application Thickness: 1.8- 2.3 s, Theoretical Coverage: 800-
19002 @ 1 mil, Impact Flexibilt: 40% Elongation @ RT, Low-Temp Flexibity: 1* mandrel
bend @ 65°F

%1 DWDCO1A4 DRILLS 1/4 EA__|BROCA COBALTO DWDCO SERIES 1/4

’ Exira fast seting, wo—component room temperalure curing epoxy adhesive. The

232 4001 DOUB;?S:S:S:?%DEXEWV EA  [system willcure at as low as ~18 °C (0 °F). Viscosity @ 25 °C.cps, part 455,000, Flash
Point, PMCC, °C PartA: 167

233 204-040-760-105 FILTERASSY EA |FILTERASSY
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|Water-dilutable general-purpose cleaner for aircraft exterior surfaces, Conforms To MIL-

2 CEE BEEA882 SHAUPOO AERONAUTICOXSS 6L | DRUM |oo e o bl solaton
25 MB3461/1-212 PACKING EA_|PACKING
236 WF336-680 FILTER ASSY EA_|FILTERASSY
237 DWDAICX63/32 DRILLS 6 332 EA_|BROCA HSS DWDAC SERES 6 3532
|AeroShell Oil W 15 W 50 is apremium semi-syrihetic muligrade ashless dispersant oi
- I Aeroshell Synthetic Engine qr |speciicall dercoped or aviton piion engines MILL-G0B2E replace by These new SAE
g OiLW15W50 Standard J-1899 Lubricating Oil, Arcrat Piston Engine (Ashless Dispersant) SAE viscosity
lgrade: Muligrade, flash point 220 min, total acidity mgKOHIg 1,0 max
15WA0 4T Lubricante de molor 4 iempos de ala calidad Excelentes propiedades ant-
¥ ldesgaste que protegen los componentes del motory el embrague, conllevando a reducir de
b o SR CL s costosde mantenimierto\iscosidad @ 100°C, oSt 142, ndie de Viscosidad 137,
Purto de infamacion, °C 232
QUALTECH HSS LEFT HAND
20 T s EA |DRILLSET Qualtech HSS LeftHand Jobber
CINTAENMASCARAR 233+ DE 36MM .
L ——— T . RO |CINTAENMASCARAR 233+ DE 36MM X 55MT =1 1/2 PULGADA
242 TSD3165T BROCAN03/16 TALADRODE90 | EA | THREADED SHANK DRILLS Stubby Series SIZE 3/16





image45.jpeg
|Water-dilutable general-purpose cleaner for aircraft exterior surfaces, Conforms To MIL-

2 CEE BEEA882 SHAUPOO AERONAUTICOXSS 6L | DRUM |oo e o bl solaton
25 MB3461/1-212 PACKING EA_|PACKING
236 WF336-680 FILTER ASSY EA_|FILTERASSY
237 DWDAICX63/32 DRILLS 6 332 EA_|BROCA HSS DWDAC SERES 6 3532
|AeroShell Oil W 15 W 50 is apremium semi-syrihetic muligrade ashless dispersant oi
- I Aeroshell Synthetic Engine qr |speciicall dercoped or aviton piion engines MILL-G0B2E replace by These new SAE
g OiLW15W50 Standard J-1899 Lubricating Oil, Arcrat Piston Engine (Ashless Dispersant) SAE viscosity
lgrade: Muligrade, flash point 220 min, total acidity mgKOHIg 1,0 max
15WA0 4T Lubricante de molor 4 iempos de ala calidad Excelentes propiedades ant-
¥ ldesgaste que protegen los componentes del motory el embrague, conllevando a reducir de
b o SR CL s costosde mantenimierto\iscosidad @ 100°C, oSt 142, ndie de Viscosidad 137,
Purto de infamacion, °C 232
QUALTECH HSS LEFT HAND
20 T s EA |DRILLSET Qualtech HSS LeftHand Jobber
CINTAENMASCARAR 233+ DE 36MM .
L ——— T . RO |CINTAENMASCARAR 233+ DE 36MM X 55MT =1 1/2 PULGADA
242 TSD3165T BROCAN03/16 TALADRODE90 | EA | THREADED SHANK DRILLS Stubby Series SIZE 3/16
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PR-1440 Class Bis an aircraft integral fuel tank sealant It has a senice temperature range

23 PR-1440B-2 ADHESIVE SEALANT QT/KIT [from -65°F (-54°C)to 250°F (121°C) Tackfree time (hours)<8, Cure fime to 35 A Durometer
(hours) 16
244 DWDCO17i64 DRILLS 1764 EA_|BROCA COBALTO DWDCO SERIES 17164
High temperature grease composed of a mineral oi thickened with Microgel, Meets MIL G-
i i Hmna e E4 |sst5c, The usefloperatingemperature range s 23°C 10+177°C.
246 DWDCO12 DRILLS 112 EA_|BROCA COBALTO DWDCO SERIES 112
HIGH VISCOSITY-GRAVITY CONSTANT (VGC) PROCESS OIL, Viscosity @ 40 °C (cSY)
7 MILPRE 12070 FOGOILCALSOLBIOMILPRF- |, |206, 4P| Graviy @80 °F 24.1,Specifc Grav @ 60 °F 0.9091,Vicosiy-Graiy Constant
120708 10.871, Molecular Weight 305, Pour Point (°F) -58, Maximum Oil Loading (PHR) for Various
INeoprenes: (GNA 20) (WHY 22)
248 SP-1AFR100 SPIROBAND MT_|Spiral band spial cable wrap SP-UAFR100
249 TSDGST BROCALETRAG TALADRODES0 | EA |THREADED SHANK DRILLS Stubby Series SIZE G
250 AA59298 Tape, Adhesive, Pressure Sensifie | RO | Tape, Adhesive, Pressure Sensilive A-4-59298
LOCTITE EA 960F AERO (fast) is  fairing and smoothing compound for exteror arcraft
251 | ADHESNEHYSOLEASSD | Hysol EAGGOF Epom AdresveKi |/ |"V7202S: His atwocomponentsysem, which ure apicya ror emperature Visoosty,

@ 77°F PART AG500 Poise PART B 600 Poise, Pot Life (100 gram mass) 30 minutes @
77°F125°C Method - ASTM D 2471
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ANEXO ESPECIFICACIONES TECNICAS

UNIDAD

ITEM|  NUMERO DE PARTE DESCRIPCION DE ESPECIFICACION TECNICA ary| MARCA | ererencia| CUNPLENO
OFRECIDA CUMPLE
MEDIDA|
T_|AMS-QQA250-2024-T3:0.032 SHEET METAL EA_|Lamina de aluminio 2024-T3 de 0,032 de 48 X 144"- (4 X 1211) 1
2 10605000 Tape, Adhesive, Reflectorized Sheeling | RO | Tape, Adhesive, Reflectorized Sheefing 1
3 - L CA;??/:“R’DSSLE BHE0X | R0 |FIBRADE CARBON  STYLE 264-50 X50 YARDAS, presertacion oo 1
4 HCX46 FRANING FILTRO DE ACEITE EA_|FILTRODEACEITE 1
Coating with excelent chemical resistance, outstanding toughness, flexibilty, abrasion
, resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type |- IV, Mix
5 M‘L'PRF'HfégjsE L POLIURETANO AZUL KIT  [Ratio: 3:1 by Volume, Application Thickness: 1.8-23 mils, Theoretical Coverage: 800- | 1
190012 @ 1 mil, Impact Flexibilt: 40% Elongation @ RT, Low-Temp Flexibilty: 1* mandrel
bend @ -65°F
6 AMS-QQ-A250/6 SHEET METAL 0025 EA_|Lamina de aluminio AMS-QQ-A-250/6,0,025 1
7 DWDCO DRILLS 27164 EA__|BROCA COBALTO DWDCO SERIES 27164 1
8 DWDCO40 DRILLS No 40 EA_|BROCA COBALTO DWDCO SERIES No 40 1
9 205076034007 FILTER EA |FILTER 1





image47.jpeg
PR-1440 Class Bis an aircraft integral fuel tank sealant It has a senice temperature range

23 PR-1440B-2 ADHESIVE SEALANT QT/KIT [from -65°F (-54°C)to 250°F (121°C) Tackfree time (hours)<8, Cure fime to 35 A Durometer
(hours) 16
244 DWDCO17i64 DRILLS 1764 EA_|BROCA COBALTO DWDCO SERIES 17164
High temperature grease composed of a mineral oi thickened with Microgel, Meets MIL G-
i i Hmna e E4 |sst5c, The usefloperatingemperature range s 23°C 10+177°C.
246 DWDCO12 DRILLS 112 EA_|BROCA COBALTO DWDCO SERIES 112
HIGH VISCOSITY-GRAVITY CONSTANT (VGC) PROCESS OIL, Viscosity @ 40 °C (cSY)
7 MILPRE 12070 FOGOILCALSOLBIOMILPRF- |, |206, 4P| Graviy @80 °F 24.1,Specifc Grav @ 60 °F 0.9091,Vicosiy-Graiy Constant
120708 10.871, Molecular Weight 305, Pour Point (°F) -58, Maximum Oil Loading (PHR) for Various
INeoprenes: (GNA 20) (WHY 22)
248 SP-1AFR100 SPIROBAND MT_|Spiral band spial cable wrap SP-UAFR100
249 TSDGST BROCALETRAG TALADRODES0 | EA |THREADED SHANK DRILLS Stubby Series SIZE G
250 AA59298 Tape, Adhesive, Pressure Sensifie | RO | Tape, Adhesive, Pressure Sensilive A-4-59298
LOCTITE EA 960F AERO (fast) is  fairing and smoothing compound for exteror arcraft
251 | ADHESNEHYSOLEASSD | Hysol EAGGOF Epom AdresveKi |/ |"V7202S: His atwocomponentsysem, which ure apicya ror emperature Visoosty,

@ 77°F PART AG500 Poise PART B 600 Poise, Pot Life (100 gram mass) 30 minutes @
77°F125°C Method - ASTM D 2471





image48.jpeg
Clear Acnylic Sheets offer excellent clarity, impact strength and economical performance in

252 48X96X5mm PLEXI GLASS 48" x 96 SHEET EA [alightweight plastic material. Plexigless sheet is a common reference term for acric
sheets, PLEXI GLASS 48" x 96" SHEET
[Aceite mineral, Proporciona una muy buena proteccion al molory ayuda a fomentar lalarga

253 SAE20W50 ACEITEMOTOR GL  ida il del mismo, Grado SAE20W50, Indice de viscosidad, ASTM D 2270 (141), Punto de
fidez, °C, ASTM D §7 (-30), Punto de inflamacion, °C, ASTM D 92 (230)

254 038088.08 FILTER EA_|FILTER

255 BROCHAZ" BROCHA PELO DE MARTA EA_|BROCHAPELO DE MARTA

256 SPIFR SPIROBAND MT_[Spiral band spiral cable wrap SP-1 FR
Solvent culback, fim fim, black asphaltc corrosion prevenfive compound, approved under

v g Witary Specifications MIL-PRF-16173E, Grade 1,for Class ./ Flash, PMCC, Minimum

7| MILPREIGISCRIIGL | - CPOANTICORROSNO GRADOT | G \y06er. ) specifc Graity @ 60F (156.C) 0.8 Approximate Diyto Touch Time @77 F (25
) 2hours

i —_— RTV133Black Sicone Electical | .~ [RTV133 black, one-componen, read-o-ise Operaling mperature range of-60-205°C (-

Sealant-10.1 oz Cartridge 70-400°F), Application Rete, gmimin. 650, Tensile Sirength, ky/cm2(1bin2) 46 (650)

Designed for edge sealing offim edges in heavl used areas, clear liquid, material

29 3950 EDGE SEALER 8 0Z CAN EA  [AcylicNinyl solution in Xylene, clear, Minimurn viscosity 300 Centipoise, Senice
ftemperature -51°C to +65°C

260 DWDCO27/64 DRILLS 27/64 EA|BROCA COBALTO DWDCO SERIES 27/64
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Clear Acnylic Sheets offer excellent clarity, impact strength and economical performance in

252 48X96X5mm PLEXI GLASS 48" x 96 SHEET EA [alightweight plastic material. Plexigless sheet is a common reference term for acric
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Sealant-10.1 oz Cartridge 70-400°F), Application Rete, gmimin. 650, Tensile Sirength, ky/cm2(1bin2) 46 (650)

Designed for edge sealing offim edges in heavl used areas, clear liquid, material

29 3950 EDGE SEALER 8 0Z CAN EA  [AcylicNinyl solution in Xylene, clear, Minimurn viscosity 300 Centipoise, Senice
ftemperature -51°C to +65°C

260 DWDCO27/64 DRILLS 27/64 EA|BROCA COBALTO DWDCO SERIES 27/64
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Used for general coating and bonding applications when extended working and cure time:

21 10512068 WEST SYSTEMEPOXYRESINKIT | KIT  |are needed orto proide adequate working fme athigher temperatures, Acceptable raio
range by weight 484 1106.19 1, Mixviscosity (st 72°F) ASTM D-2383 (125 cps, Specific
%2 53208257 PACKING PREFORMED EA_|PACKING PREFORMED
i drying, MoS2 based said i ubricant wit an epory binder system, Densiy” 3= 05
LUBRHBOND® 220 12 0Z AEROSOL
%3 LUBRIBOND g EA|lbigal (995 = 60 gramsiiter), Flash Paint 45°F (7°C) Good corosion esisance, Fair
chemical resistance, Suiablefor feld applcations
%4 DWDACYG18 DRILLS 618 EA_|BROCAHSS DWDAC SERES 6" 18
%5 DWDN3E DRILLS 38 A |BROCAH 55 DWDN SERES 38
%5 VINPEL VINPEL 45 Cm X 400 Mt RO _|VINPEL45Cm X400 Mt
RTVI02, sealants are standard srengh paste consisency products which can be applied
. — Momertve SealantRTV1028.cz e, | fovrical andoveheadsuacs where pourblelseleelng sealansar ot pracica
28cztube Specifc Gravty 1.05 Tack Free Time, minutes 20, Tear Srength,
kg/em (i) 8 (45)
5 p— oy o |TIRE 1846 6 PLY RATING 10Rafed Speed (MPH) 210, Maximum Braing Load (L) 600
Rated Infiaion (PSI) 140
269 | SUPERKOTE 2000 REFRIGERANTE MOTOR GL_|Anticongelante/ Refrgerante, Liquido verde fuorescerte
VETIL ETIL CETONA MEK, GAS 76-63-3, Formula molecular CAHBO, Punto de Fusion -
0 MEK METHLETHILCETONAXSGL | PAIL : g g
87 (-125°F), Masa molar 72,11 gimol, Presion de Vapor: 71 2 20 C
PIG Absoroent Mat Pad: 28 czVolume Absorbed Per Pad, 22.gal (100
a7 H 15" x 20100 padsperbag | EA
MAT403 leanyweight1s™x pads perbag Pads) MaterialPolypropylene Perforated Size10in x 15 in
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Used for general coating and bonding applications when extended working and cure time:

21 10512068 WEST SYSTEMEPOXYRESINKIT | KIT  |are needed orto proide adequate working fme athigher temperatures, Acceptable raio
range by weight 484 1106.19 1, Mixviscosity (st 72°F) ASTM D-2383 (125 cps, Specific
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212 Dwpco? DRILLS No7 EA |BROCA COBALTO DWDCO SERIESNo 7

3 T—— QUALTECT{;BSESE;? o EA | DRILLSET Qualtech HSS TIN Coated Jobbers

274 DPAS30W TAPAOIDOS BOX_|TAPAOIDOS

CINTAENMASCARAR 233+ DE 12MM

L — o RO |CINTAENMASCARAR 233+ DE 12MM X 55MT =

276 KDB51511 FILTERKIT EA_|FILTERKIT
Coating with excelent chemical resistance, outstanding toughness, fleibilty, abrasion
resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type |- IV, Mix

277 | MILPRF-85285E Type |-V | POLIURETANO VERDE METALIZADO |  KIT  |Ratio: 31 by Volume, Application Thickness: 1.8 - 23 mils, Theoretical Coverage: 800-
190012 @ 1 mil, Impact Flexibilt: 40% Elongation @ RT, Low-Temp Flexibilty: 1* mandrel
bend @ 65°F

278 MS20995CY1548 LOCKWIRE COPPER LB _|COOPER SAFETY WIRE MS209850Y15-48

279 PWC06-002 PETROLATUMW-P-236- 11bCan_| LB | Pelrolatum white PWC06-002 WW-P-235 coloriess, white grease-like technical grade

280 TSDIBST BROCA No 1/8 TALADRO DE 90 EA_| THREADED SHANK DRILLS Stubby Series SIZE 1/8
LOCTITE 404 esta disefiado para a union de componentes plasticos y elastomeros,

281 AA309T ADHESVE LOCTITE 404, 4z EA |donde sea necesaria unafjacion muy répida. Cianoacilato de Eflo, Peso especifico @ 25

°C 1,09, Temperatura de Transicién Vitrea, ASTM E 228, °C 120
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212 Dwpco? DRILLS No7 EA |BROCA COBALTO DWDCO SERIESNo 7
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°C 1,09, Temperatura de Transicién Vitrea, ASTM E 228, °C 120
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Loctite EA 9392 AERO Epoxy Adhesive

LOCTITE EA 9392 AERO is a two-component paste adhesive, which cures at room
{temperature and possesses excellent shear sirength at high temperatures Viscosity @ 77°F

" B fieen Gray 1 qtkit AT TKITIoART A4 200 Poise, PART B 6600 oise Pot Lie (100 mass) 75 minutes @ 77°FI25°C
Method - ASTM D247 1 in weter bath
Lubricante que proporciona una capa delgada y seca que penetra en las grietes resistente
23 00116 LUBRICANT,SOLID FILMLPS1 EA  [alaceite, polvo y acumulacion de suciedad, punto de inflamacion 175 °F, gravedad
lespecifica 840 aprox, Temperatura de descongelacion -35°F
PR-1782 Class B is alow densiy arcraft fueltank and general purpose sealant fthas a
24 PRI7828-112 ADHESIVE SEALANT SEMKIT |senice temperature range flom -54°C o 121°C (-65°F to 250°F) Tack free time (Hours)<5,
Cure time to 35 Shore A" Durometer (hours) 7
285 TSDI0ST BROCA No 10 TALADRO DE 90 EA_| THREADED SHANK DRILLS Stubby Series SIZE 10
o, |1 resistantsealat oruse o nfegral ue ks and presured cabins s well 25 ofter
266 | CS3204A112 Flamemaster SEALING COMPOUND 7 |(reas subectio conactwith aicrffuels,ubricants, s, waler andor wealhering meets
|AMS-5-8802E Type 2, Mixing Retio by weight) 100:10, Non Volaie Content 86%
287 486719055 FUEL SENDER EA_|FUEL SENDER 486719.055
288 AN525-832R8 SCREWMACHINE EA | SCREWMACHINE
289 DWDCO16 DRILLSNo 16 EA|BROCA COBALTO DWDCO SERIES No 16
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Loctite EA 9392 AERO Epoxy Adhesive

LOCTITE EA 9392 AERO is a two-component paste adhesive, which cures at room
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289 DWDCO16 DRILLSNo 16 EA|BROCA COBALTO DWDCO SERIES No 16
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290 BROCHA3 BROCHAPELO DE MARTA EA |BROCHAPELO DE MARTA

291 ST3001-145 PACKING EA_|PACKING
Coating with excelent chemical resistance, outstanding toughness, fleibilty, abrasion

| resistance, and excellent uside durabilty. Conforms to MIL-PRF-85285E Type |- IV, Mix

22 M‘L'PRF'S?ﬁ:E Lo POLIURETANO AMARILLO KIT  [Ratio: 3:1 by Volume, Application Thickness: 1.8- 2.3 mils, Theoretical Coverage: 800-
190012 @ 1 mil, Impact Flexbilt: 40% Elongation @ RT, Low-Temp Flexibilty: 1* mandrel
bend @ 65°F

293 DWDAICX85/32 DRILLS 6 532 EA_|BROCA HSS DWDAIC SERES 6 5132

24 CR324342 RVET BLIND EA_|RVETBLIND

SCOTCH-BRITE REF 7447 XROLLO

25 -~ PSS RO [SCOTCH-BRITE REF 7447 X ROLLO DE 6 PULGADAS X 30PIES

29 MS246945-60 SCREW EA | SCREW

27 DWDCOG DRILLSLETRAG EA__|BROCA COBALTO DWDCO SERIES SIZE G

28 02591 SMILLASTIK GRANO 220 ROLLORON | 2y oy 11 §TIk GRAND 220 ROLLO ol 234" x 45 yd

2.3 x45yd
299 MS29561-237 PACKING EA_|PACKING
KIT FUEL MINIFOLD PACKING Y
300 o~ oo KIT  |KIT FUEL MINIFOLD PACKING Y GASKET
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290 BROCHA3 BROCHAPELO DE MARTA EA |BROCHAPELO DE MARTA
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SCOTCH GRIP RUBBER ADHESIVE

3M™ Neoprene High Performance Rubber & Gasket Adhesives 1300 and 1300L are
the most versatile of our rubber and gasket adhesives. Mees specification requirements of

" . 1300L AT MM A-121 Temperature peromance range s 30°F (34°C)1o 300°F (149°C) Bonding
Range: up to 8 minutes.

302|  DWDT5-DBSET QUALTECH DRILL BLANKS EA_| Qualtech Drll Blanks DWD115JDB-SET

CINTAENMASCARAR 233+ DE 24MM <

M| i o i RO |CINTAENMASCARAR 233+ DE 24MM X 55MT = 1

304 DWDN1/16 DRILLS 1/16 EA_|BROCAH.SS DWDN SERIES 1/16

305 SP-12FR25 SPIROBAND MT_|Spiral band spiral cable wrap SP-1/2 FR25

P B T L |EROSHELL 17 AW AEROSHELL 64 6,6 b can Exreme pressure Arfame Grease, meefs
MILG-21164

307|  NASI329H4K200L RIVNUT BLIND EA_|RIVNUTBLIND
Forms atransparent, sof, waxyfim for profection and lubricalion Penetrates to displace

308 00316 LUBRICANTE LPS N°3, 11 0Z EA  |moisture, Conformsto: MilPRF-16173E Grade 2, Flash Point: (TCC)
100°F (40°C) minimum Pour Point: 0°F (- 18°C) Propellant Carbon Dioxide

309 DWDACX63/16 DRILLS 6 3116 EA_|BROCA HSS DWDAC SEREES 6" 3/16

310 103760 CEPILLO DE COBRE EA_ |Cepillo de cerdas de cobre multiusos de plastico color negro
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SCOTCH GRIP RUBBER ADHESIVE

3M™ Neoprene High Performance Rubber & Gasket Adhesives 1300 and 1300L are
the most versatile of our rubber and gasket adhesives. Mees specification requirements of

" . 1300L AT MM A-121 Temperature peromance range s 30°F (34°C)1o 300°F (149°C) Bonding
Range: up to 8 minutes.
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31 Ms9386-126 ORING EA_|ORING
0 P HOS21UNP ~6~NonPorous Ful | . |Reease Fabri Tefon s anon porous elase o costed Toerlas designed o elease
Roll(38inx 100yds) and resin esticton. Thickness 3 mils (007in, (0.8mm), mavimur use temp 550 °F (268
3 DWDCOH DRILLSLETRAH EA_|BROCACOBALTO DWDCO SERES SIZEH
B TSDSST BROCANo 5 TALADRO DE 80 EA_|THREADED SHANK DRILLS Stubby Seres SZE 5
Industiel ade siicone forms a lear, tin,nor-stcky, water repellent ubricaing im. Use
SILICONE SPRAY 8034, 105 0
315 | SILICONE SPRAY 8034 e EA|attemperatures between 40°F and 110°F (5°C and 43°C), Color:Coloress, ransparen,
Specifc graity @70°F 070
Lociled Hysol 5340 s a generalpurpose achesie wih exceplonal
Locite Hysol 340 Epory Adhesiie -5 b igh temperature performance. Pot Life @ 77°F, 100 grams mins mixed 90, Cure Schedule
36| HYSOLEASHO KT
it 3 Days @ 77°F Test Temp °F 40, Typical Value 2100, Hardness, Shore D >80
37| 206076034003 ELEVENT FILTER EA_|ELEMENT FILTER
Super-Penetrating, Water Displacing, Corosion Infibiing Compound, hycrocarbon wit
CORROSION PREVENTNE ARCRAFT
38 w8 e PAL [05% aromatics max,fiash point 104°F (40°C) vscosity 71 sec. Meels MIL-C-16173D,
GRADE 4
SOLID CARBIDE BUR SETS (SA42, SA43, SCA42, SD42, SE4T, SF42, SG41, SG43, SHAT,
319 DULSSET SOLID CARBIDE BUR SETS By B
RTVI08 sealants are standard srengh paste consisency products which can be applied )
Momente Sealant RTV108
320 RTVI08 e B |vertcal and overhead surfaces where pourableiselfleveling sealants are not practical. Tack

Translucent, 2.8 oz tube

Free- Time 20 min, Elongation % 400, Hardness Shore A 30
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ALCOHOL ISOPROPILICO

ALCOHOL ISOPROPILICO TT-735

Mests Grade A estandar for TT-1-735, Purity >99 8% Acidity (% of acetic acid) <0.001,

21 DRUM
CANECA CANECAX S56L Density @ 20 °C 0.785—0.786 gimL., Specifc araty @20 °C/ 20 °C 0.785—0787 g
Heavy duty waterdisplacing, corosion nhibiing compound, Flash Pornt 38 °C 100 °F
CORROSION PREVENTNVE ARCRAFT
2 w100 bt PAL [minimum , Density at 23 °C (73 °F) 890 kgjm®, Applcaton Temperature 151030 °C /6010
85 °F . Colour Transparent beige ,Film Appearance Firm wayy im
[viton Grease uses an advanced hickening agent and superio addifve fechology which
extibis a high rsistance fo water washout, and s idealfor reventing corosion on
seril Th 2 Grease 3810:0
32 NLGI GRADE 2 o :gi’:a:; ":;:e T8 |components which can resultin longer ife and increased productivy, 3810-0 (425 tube
gl 460) Meets or Exceeds the folloning: BELL Consumable Materal Ref C-551, Densiy @
120°C (gimL) 105, Pour Pint (°C) 15 5 °F)
Hylomar PL32M (Vedum) Aerograde Highly engineered, polester-urelnane based nion-
2 PIC0S-005 SILICONE GREASE EA[seting and nonhardening gasketng compound, oruse n the aeronautcalindusty for
seaiing joirs in et urbine engines NSN 8030.99-220-2370
P/5 890 Class B s an aitcra negralfueltank sealant. It has a serie emperature range
from -65°F (-54°C) 0 250°F (121°C), with intemtent 0275°F (136°C) with
325 | AMS-5-8802 (PS890B 112) ADHESIVE SEALANT T o S LB C)250E (121°C) N imemikient exciriots up 1 275 F{1357C). o

|AMS-5-8802 Class B specification, Tack free fime (hours) <4, Cure ime to 35 A Durometer
(hours) 30, Cured specific gravity 1.55
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326 | OVEROLES TYVEKDUPONT | OVEROLES TYVEK DUPONT EA |OVEROLES TYVEK DUPONT 1
27 VIS35768-26 GASKET A [GasKkeT 1
28 3070542:01 FILTER FUEL PUVP EA_|FILTERFUELPUMP 1
32 3010880 GASKET A [GasKeT 1
3% 8349948 CLEANEAR SAVPLINGKIT, OL_|KIT_|CLEANEAR SAMPLINGKIT, OIL 1
ubricante para oscas a base Ge aceft &5 para Uso &n acero moxdable y aleaciones de
] PIC0S-023 ANTISEIZEXLB 18 |altatemperatura, Puede funcionar a temperaturas de hasta 1500 °F (815 °C) Pratt& 1
Writney Canad Especifcacion: PWC06-023
Costing withexcellent chemical resistance, outstanding oughness, flexibilty, abrasion
y resistance, and excellent utside durablt. Conforms fo MIL-PRF-85285E Type -V, Mix
32 M‘L'PRF'H;Z;;% b POLIURETANO ROJO KIT  [Ratio: 3 1byVolume, Applicaton Thickness: 18-23mils Theoretcal Coverage: 800- | 1
190012.@ 1 mil, Impact Fleibilt: 40% Elongation @ R, Low-Temp Flexibily 1 mandrel
bend @ -65°F
(General purpose airame grease fo use n antificton bearings, gearbores and plain
|| Wmoaaieiie | AOSTOEAE eI | T8 | vps whiime e range o020 512170 e MLGITIIA !
" i CREASEUTILTY 1602 TUBE | 15 |Grease designed o those aplicatons where a greas e ubcant possessing exterrely |

lgood water repellency and superiorlubrication characterstcs are desired. NLGINo. 1,
Mineral Oil Viscosity: cSt @ 40°C (135)
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y resistance, and excellent utside durablt. Conforms fo MIL-PRF-85285E Type -V, Mix
32 M‘L'PRF'H;Z;;% b POLIURETANO ROJO KIT  [Ratio: 3 1byVolume, Applicaton Thickness: 18-23mils Theoretcal Coverage: 800- | 1
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bend @ -65°F
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TT-N-95B, TYPE II: For cleaning acrylic plastics, VOLATILE ORGANIC COMPOUNDS.

- bbb Ansaces CL 706766 ramsifer, SPECIFIC GRAVITY 708 768, DENSITY 589639 bsiga

3% 5320818 ORING EA_|ORING

337 453209-235 PACKING PREFORMED EA__|PACKING PREFORMED

338 800L5 GUANTES DENITRLLO BOX_|GUANTES DENITRILO
The BreatherBleeder Cloth HCS2102-10 QMF17 is a needlepunch polyester breather

- o Heatcon HCS2102-10 Breather R0 |s1tem commoniyused as avacuum tansier medium i the vacuum bagging process 100z

Ful Roll(80in x 50yds) Weight,Used atpressures up to 200 psi (138 bars) Max. recommended use temp: 400°F

(204°C).

340 MS20995C32 LOCKWIRE LB | MS20995C32 Stainless Steel 0.032" Diameler Satety Wire -1 Ib Rol

B DWDACX614 DRILLS6 14 EA_|BROCAHSS DWDAC SEREES 6 1/4

32| MILC5040, Typell Cord, Fibrous, Nylon, X 100 FT RO _|Milftary Specification MIL-C-5040 Type Il Black Paracord X 100 FT

PAPEL KRAFT ROLLO DE 160 CMX

u3 PAPEL KRAFT A RO | PAPEL KRAFT ROLLO DE 160 CM X 200 METROS

4 DWDCO57 DRILLS No57 EA_|BROCA COBALTO DWDCO SERIES No 57

| ieenyi PR o |Buperor calcium stearate base grease compound for general use n indusy, Part No. 10-
1206 21, 0z Tube

346 TSD30ST BROCA No 30 TALADRO DE 90 EA | THREADED SHANK DRILLS Stubby Series SIZE 30
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FILM, BAGGING NYLONX 1000F T

High temperature Nylon Film which can be used for cures up to 401 °F (205 °C), Tensile

b rESama (APPROX 333YDS) RO |tengh 80MPa, Elongation MD: 300%, TD: 300% Wicth 301n (open 60ir)
M 53208144 PACKING OIL ESCAVATION EA_|PACKING OLL ESCAVATION
2 VIS20095620 LOCKWRE LB | MS20985020 Stanless Steel 0.020" Diameter Safey Wre 1 b Roll
13 VS28775-015 ORING EA_|ORNG
TIRE 11.00-12 PLY RATING 10 Rated Speed (MPH) 160, Maximum Braking Load (Lbs)
* e b EA 1180, Rated inaton s 60
5 PAS2A FILTRODE ARE EA_|FILTRODEARE
ROYCO 782 s synhetc hydraulic fuid developed o meet e severe duty
16 MIL-+83282 HIDRAULICO 782 QT |demands oftoday's miltary and industial equipment, suable foruse i applicatons
loperating atemperatures from -40°C to 205°C, qualfiedto MIL-SPEC: MIL-PRF-£32820
; [ctvador para adhesivos y selladores anaerdbicos de Locife peso especifico @ 25 °C 079,
% LOCTITESF7640 | Actvadorabase dedisolvente/450Z | BA \\io 124 @ 20 °C, mPas (cP) 2, Tiempo de Secado a 20 °C, segundos 30y 70
Coating with excellent chemical resistance, outstanding oughness, flxibilty, abrasion
' resistance, and excellent utside durablty. Conforms fo MIL-PRF-85285E Type -V, Mix
18 M‘L'PRF'HZ%;E P2V ROUURETANONEGROMATE | KIT  |Ratio 31 by Volume, Appication Thickness: 1823 i, Theoreical Coerage: 800-
190012 @ 1 mil, Impact Fleibilt: 40% Elongation @ RT, Low-Temp Flexibilty 1 mandrel
bend @ -65°F
19 14806960 HOUSING FLUORESCENT LIGHTS | EA |HOUSING FLUORESCENT LIGHTS
20 CR355358 REMACHE PACK X 100 A |REMACHE PACK X 100
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SIZE 22X6 510 PLY RATING 6 Rated Speed (MPH) 190, Maximurn Braking Load (Lbs)

e Bep b FA L4200, Reted ntaton (st 68
Methylisobut ketone (IBK) is a clear, coloress organic iquid compound. MIBK s used
8 MIEK METHILISOBUTILCETONAX5 GL | PAIL |as a chemical ntermediate, a solvent for manufacturing pairts, Molecular Weight 100.2
lgimol, Freezing Point 84.7°C (-120°F), Boiling Point @ 760mmHg 115°C (239°F)
349 M25988/1-916 PACKING FUEL EA_|PACKING FUEL
350 HUT80 INDEXES & DISPENSERS EA_[80PC Wire Gauge Sizes # 10 #80
351 DWDN17/32 DRILLS 17132 A |BROCAH.SS DWDN SERIES 17132
SIZE 319.75-14 PLY RATING 12 Rated Speed (MPH) 190, Maximum Braking Load (Lbs)
e i b FA 16650, Rated inton P 115
5 — DOWSIL 730 Whie Slvet Sealant-%0] | One-component fuarsiicone adhesielsealat, Stabl and flebe fom -65°C
ml Tube (85°F) o 260°C (S00°F), Aceloxy cure systen.
354 VELCRO B NEG:?;:AATC:OVHEMBRA RO |VELCRONEGRO MACHO Y HEMBRAX 25 MTS
35 MS24693-529 SCREW EA_|SCREW
Hysol EA 956 is a two-component adhesive, which has excellent elevated tempereture:
35 HYSOL EA956NA LOCTITE ADHESNE QT/KIT [strengih. Viscosity, 77°F PART A 350 Poise, PART B 20 Poise, MIXED 162 Poise, Viscosity,

125°C PART A 35 Pa-S, PART B 2Pa'S.
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Turbine oil qualified and approved for MIL-PRF-23699 Viscosity, Kinematic @ 100°C 4.97

357 MILPRF-23699 OILMOTOR 2380 Ll
358 MS287784 PACKING EA_|PACKING
Coating with excelent chemical resistance, outstanding toughness, flebilty, abrasion
resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type |-V, Mix
359 | MILPRF-85285E Type IV | POLIURETANO GRISMETALIZADO | KIT  [Ratio: 3:1byVolume, Application Thickness: 18- 2.3 mils, Theoretical Coverage: 800-
900 12 @ 1 mil,Impact Flexibity: 40% Elongation @ R, Low-Temp Flexibilty: 1° mandrel
bend @ 65°F
360 TSDM4ST BROCA No /4 TALADRO DE 90 EA_| THREADED SHANK DRILLS Stubby Series SIZE 1/4
LOCTITE EA9309.3NAAERO is atoughened two-part paste adhesive.t contains 5 mill).13
361|  HYSOLEA309.3NA LOCT‘I;EJE?&QS‘:::E: AERO. ) T 11T i glass beadsfor bordiine hickress corirol PotL e (450 gram mass) 36 minutes @
77°F125°C Method - ASTM D2471 in water bath. Density (gim) PART A1.15, PART B1.0
362 MS20995CY20 LOCKWIRE COPPER LB | MS20995CY20 Copper 0.020 Diameter Breakaway Wire -1 Ib Rol
Designed for the bonding od cylinrical fiting pars, tested for Mil-R 460828, Specific gravty
363 609 LOCTITE 609, 50 ML B | o0t )0 et
Aircraftype gas turbine lubricantApproved against U S. Miltary Specification Mi-
34 JET OIL 254 MILPRF-23699 QT [PRF 2369F High Thermal Stabilly (HTS) Flash Point, °C (F), ASTM D 92 254 (489), Fire
Point “C (F) 288 (550)
365 174104001 FACEFILTER O EA_|FACEFILTEROL
45| CADMUMLHES070 | PLATING SOLUTION BOTTLEX5LT | _, ™ |Cadmium GODE 5070, Purityofdeposi 39%,ph 7.7 pe: erous non erous,
ISPS50705LT OR5BOTTLESXLT Specification AMS 2451 /4B, UN2922, Corrosive Liquid, Toxic.
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FILM, BAGGING NYLONX 1000F T
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loperating atemperatures from -40°C to 205°C, qualfiedto MIL-SPEC: MIL-PRF-£32820
; [ctvador para adhesivos y selladores anaerdbicos de Locife peso especifico @ 25 °C 079,
% LOCTITESF7640 | Actvadorabase dedisolvente/450Z | BA \\io 124 @ 20 °C, mPas (cP) 2, Tiempo de Secado a 20 °C, segundos 30y 70
Coating with excellent chemical resistance, outstanding oughness, flxibilty, abrasion
' resistance, and excellent utside durablty. Conforms fo MIL-PRF-85285E Type -V, Mix
18 M‘L'PRF'HZ%;E P2V ROUURETANONEGROMATE | KIT  |Ratio 31 by Volume, Appication Thickness: 1823 i, Theoreical Coerage: 800-
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21 AS568-110 ORING EA_|ORING 1

Coating with excelent chemical resistance, outstanding toughness, flexibilty, abrasion
MILPRF-85285E Type IV resistance, and excellent ouside durabilty. Conforms to MIL-PRF-85285E Type I-IV, Mix

2 17038 POLIURETANO NEGROBRILLANTE |  KIT  |Ratio: 3: 1 by Volume, Application Thickness: 1.8 -23 mils, Theoretical Coverage: 800- | 1
900 12 @ 1 mil,Impact Flexibity: 40% Elongation @ R, Low-Temp Flexibilty: 1* mandrel
bend @ -65°F

23 BT-339 FILTRO DE ACEITE EA_|FILTRODEACEITE 1

% AMS-QQ-A-2506. SHEET METAL 0032 EA_|Lamina de aluminio AMS-QQ-A-250/6 0,032 1

% DWDC03532 DRILLS 3532 EA__|BROCA COBALTO DWDCO SERIES 332 1

% DWDN35/64 DRILLS 36/64 EA_|BROCAH.S'S DWDN SERIES 36/64 1
SIZE 450X190-5 PLY RATING 10 Rated Speed (MPH) 190, Maximum Braking Load (Lbs)

7 4os0e2 TRE E4 |s400, Reted ntton (Ps1) 75 !
Supreme perormance, high temperature, anfiwear grease Oil Separation, 30 hr. at 177°C,

3 MOBIL28 GREASEREDMOBIL 28/44Ibcan | TRR [ASTMD6184,v0l% 25, Evaporation Loss, ASTM D 2595, 22 rs @ 177°C, wl% 52, | 1
COLORRED

2% CR35535-10 REMACHE PACK X 100 EA_|REMACHE PACKX 100 1

£l DWDACX51/16 DRILLS 1/16 EA_|BROCAHSS DWDAC SEREES 6 1/16 1

“ p— s Tape (el de composte) | R0 |POYeST @b backed il afly pressre sicone advesve, Masimum cure eperatire |

1400 °F (204 °C), Standard size 1" x 72 YD





