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1 Structure Data
This chapter provides model geometry information, including items such as story levels, point coordinates, and element connectivity.
1.1 Story Data
Table 1.1 - Story Definitions
	Tower
	Name
	Height
m
	Master Story
	Similar To
	Splice Story
	Splice Height
m
	Color

	T1
	Story2
	2
	No
	None
	No
	
	Blue

	T1
	Story1
	1.65
	No
	None
	No
	
	Blue

	T1
	cubierta
	4
	No
	None
	No
	
	Blue



1.2 Grid Data
Table 1.2 - Grid Definitions - General
	Tower
	Name
	Type
	Ux
m
	Uy
m
	Rz
deg
	Story Range
	User Top Story
	User Bottom Story
	Bubble Size
mm
	Color

	T1
	G1
	Cartesian
	0
	0
	0
	Default
	
	
	700
	Gray6



Table 1.3 - Grid Definitions - Grid Lines
	Name
	Grid Line Type
	Ordinate
m
	Angle
m
	X1
m
	Y1
m
	X2
m
	Y2
m
	Bubble Location
	Visible

	G1
	General (Cartesian)
	
	
	60.9328
	-0.0001
	0
	0
	End
	Yes

	G1
	General (Cartesian)
	
	
	60.9328
	15.4265
	0
	15.4357
	End
	Yes



1.3 Point Coordinates
Table 1.4 - Point Bays
	Label
	Is Auto Point
	X
m
	Y
m
	DZBelow
m

	1
	No
	0
	0
	0

	2
	No
	20.4112
	41.9143
	0

	3
	No
	5.1771
	15.4355
	0

	4
	No
	12.1686
	15.4355
	0

	5
	No
	5.169
	0.0003
	0

	6
	No
	-2.9167
	16.803
	0

	7
	No
	-2.9155
	-1.1653
	0

	8
	No
	8.6963
	-5.1801
	0

	9
	No
	20.1523
	-1.2087
	0

	10
	No
	20.1509
	16.8642
	0

	11
	No
	8.6962
	20.8244
	0

	12
	No
	63.8441
	16.803
	0

	13
	No
	12.1682
	0.0003
	0

	14
	No
	63.8429
	-1.1653
	0

	15
	No
	52.2311
	-5.1801
	0

	16
	No
	23.5379
	-3.2965
	0

	17
	No
	40.7751
	-1.2087
	0

	18
	No
	40.7765
	16.8642
	0

	19
	No
	30.3729
	-3.306
	0

	20
	No
	52.2312
	20.8244
	0

	21
	No
	37.2643
	-3.3043
	0

	22
	No
	20.2689
	2.948E-05
	0

	23
	No
	20.1522
	-3.4267
	0

	24
	No
	40.775
	-3.4267
	0

	25
	No
	40.6608
	0.0003
	0

	26
	No
	27.5699
	41.9728
	0

	27
	No
	22.9806
	-3.894E-05
	0

	28
	No
	20.1522
	-0.1397
	0

	29
	No
	30.4083
	-0.0001
	0

	30
	No
	20.151
	15.637
	0

	31
	No
	37.8123
	-0.0001
	0

	32
	No
	33.2913
	41.9728
	0

	33
	No
	20.2689
	15.4327
	0

	34
	No
	40.7765
	15.637
	0

	35
	No
	40.7765
	41.9728
	0

	36
	No
	30.3995
	15.4311
	0

	37
	No
	40.6584
	15.4358
	0

	38
	No
	15.2291
	15.576
	0

	39
	No
	20.259
	15.2952
	0

	40
	No
	20.2689
	15.5761
	0

	41
	No
	40.6584
	15.5751
	0

	42
	No
	20.151
	41.9728
	0

	43
	No
	40.8727
	30.8772
	0

	44
	No
	40.6584
	15.2958
	0

	45
	No
	59.9828
	-0.0001
	0

	46
	No
	40.677
	26.4057
	0

	47
	No
	33.2913
	15.296
	0

	48
	No
	27.5699
	15.5761
	0

	49
	No
	60.9328
	0.9999
	0

	50
	No
	23.1782
	15.2952
	0

	51
	No
	40.7966
	22.0257
	0

	52
	No
	60.9328
	14.3265
	0

	53
	No
	59.9328
	15.4265
	0

	54
	No
	20.1533
	22.3954
	0

	55
	No
	0.025
	15.45
	0

	56
	No
	1.025
	15.45
	0

	57
	No
	0
	14.3607
	0

	58
	No
	0
	1
	0

	59
	No
	1.025
	0
	0

	60
	No
	20.3065
	26.6396
	0

	61
	No
	20.1968
	31.3766
	0

	62
	No
	20.151
	35.0948
	0

	65
	No
	49.4143
	15.5267
	0

	66
	No
	47.6387
	0.1029
	0

	67
	No
	55.3898
	-0.0001
	0

	68
	No
	54.9
	15.5
	0

	75
	No
	57.9578
	-0.0001
	0

	78
	No
	23.1409
	37.3713
	0

	79
	No
	27.5699
	37.3722
	0

	80
	No
	33.2913
	37.3693
	0

	81
	No
	37.7224
	37.3722
	0

	82
	No
	37.7224
	33.0022
	0

	83
	No
	37.722
	28.6325
	0

	84
	No
	37.7224
	24.2593
	0

	85
	No
	37.7224
	19.8894
	0

	86
	No
	33.2913
	19.8883
	0

	87
	No
	27.5699
	19.8894
	0

	88
	No
	23.1409
	19.8885
	0

	89
	No
	23.1409
	24.2613
	0

	90
	No
	23.1405
	28.6316
	0

	91
	No
	23.1409
	33.0013
	0

	92
	No
	27.5699
	33.0022
	0

	93
	No
	33.2913
	33.0011
	0

	94
	No
	23.1405
	28.6287
	0

	95
	No
	27.5696
	28.6325
	0

	96
	No
	33.291
	28.6296
	0

	97
	No
	23.1502
	24.2624
	0

	98
	No
	27.5699
	24.2622
	0

	99
	No
	33.2913
	24.2611
	0

	100
	No
	37.7224
	24.2622
	0

	101
	No
	27.5736
	28.6325
	0

	102
	No
	33.2913
	37.3711
	0

	103
	No
	33.2988
	28.6314
	0

	104
	No
	60.9328
	15.4265
	0

	105
	No
	0
	15.4357
	0

	106
	No
	15.2291
	15.616
	0

	107
	No
	15.229
	15.2952
	0

	108
	No
	15.294
	15.576
	0

	109
	No
	26.0974
	15.5762
	0

	110
	No
	26.0974
	15.2952
	0

	111
	No
	20.2689
	15.6358
	0

	112
	No
	20.2689
	15.2358
	0

	113
	No
	60.9328
	-0.0001
	0

	114
	No
	58.8224
	0.1397
	0

	115
	No
	60.7915
	0.1397
	0

	116
	No
	60.7915
	2.3793
	0

	117
	No
	58.8224
	-0.1403
	0

	118
	No
	61.0805
	-0.1403
	0

	119
	No
	61.0805
	2.3793
	0

	120
	No
	58.8259
	15.5761
	0

	121
	No
	61.0719
	15.5761
	0

	122
	No
	61.0719
	13.0617
	0

	123
	No
	58.8259
	15.296
	0

	124
	No
	60.7915
	15.296
	0

	125
	No
	60.7915
	13.0617
	0

	126
	No
	30.3995
	15.5347
	0

	127
	No
	30.3995
	15.2364
	0

	128
	No
	34.6962
	15.5751
	0

	129
	No
	45.6859
	15.5751
	0

	130
	No
	45.6859
	15.2958
	0

	131
	No
	34.6962
	15.2958
	0

	132
	No
	40.6584
	15.6358
	0

	133
	No
	40.6584
	15.2358
	0

	134
	No
	37.8111
	15.5148
	0

	135
	No
	37.8128
	15.2358
	0

	136
	No
	41.8597
	15.4294
	0

	137
	No
	44.7699
	15.429
	0

	140
	No
	43.6278
	0.1406
	0

	141
	No
	45.69
	0.1489
	0

	142
	No
	43.6278
	-0.14
	0

	143
	No
	45.69
	-0.14
	0

	144
	No
	20.2665
	0.31
	0

	145
	No
	20.2713
	-0.31
	0

	156
	No
	40.6608
	0.31
	0

	157
	No
	40.6608
	-0.3094
	0

	160
	No
	5.1771
	15.5355
	0

	161
	No
	5.1771
	15.3355
	0

	162
	No
	12.169
	15.5355
	0

	163
	No
	12.1682
	15.3355
	0

	164
	No
	5.169
	0.1003
	0

	165
	No
	5.169
	-0.0997
	0

	166
	No
	12.1682
	0.1003
	0

	167
	No
	12.1682
	-0.0997
	0

	168
	No
	2.1004
	15.5758
	0

	169
	No
	-0.1452
	15.5758
	0

	170
	No
	-0.1452
	13.063
	0

	171
	No
	2.1004
	15.296
	0

	172
	No
	0.1394
	15.296
	0

	173
	No
	0.1394
	13.063
	0

	174
	No
	2.1004
	-0.1401
	0

	175
	No
	-0.1452
	-0.1401
	0

	176
	No
	-0.1452
	2.3728
	0

	177
	No
	2.1004
	0.1397
	0

	178
	No
	0.1394
	0.1397
	0

	179
	No
	0.1394
	2.3728
	0

	180
	No
	15.2228
	-0.14
	0

	181
	No
	15.2228
	0.1403
	0

	182
	No
	17.3138
	-0.14
	0

	183
	No
	17.3138
	0.1403
	0

	208
	No
	54.3762
	-0.0001
	0

	228
	No
	56.4034
	-0.0001
	0

	230
	No
	57.417
	-0.0001
	0

	231
	No
	58.4306
	-0.0001
	0

	234
	No
	52.349
	-0.0001
	0

	245
	No
	0.5125
	-8.685E-07
	0



1.4 Line Connectivity
Table 1.5 - Column Bays
	Label
	PointBayI
	PointBayJ
	IEndStory

	C1
	81
	81
	Below

	C3
	80
	80
	Below

	C4
	79
	79
	Below

	C5
	78
	78
	Below

	C6
	91
	91
	Below

	C7
	92
	92
	Below

	C8
	90
	90
	Below

	C9
	95
	95
	Below

	C10
	93
	93
	Below

	C11
	96
	96
	Below

	C12
	83
	83
	Below

	C13
	82
	82
	Below

	C14
	84
	84
	Below

	C15
	99
	99
	Below

	C16
	98
	98
	Below

	C17
	89
	89
	Below

	C18
	88
	88
	Below

	C19
	87
	87
	Below

	C20
	86
	86
	Below

	C21
	85
	85
	Below

	C22
	3
	3
	Below

	C23
	4
	4
	Below

	C24
	5
	5
	Below

	C25
	13
	13
	Below

	C26
	16
	16
	Below

	C27
	19
	19
	Below

	C28
	21
	21
	Below

	C29
	22
	22
	Below

	C30
	25
	25
	Below

	C31
	27
	27
	Below

	C32
	29
	29
	Below

	C33
	31
	31
	Below

	C35
	33
	33
	Below

	C36
	36
	36
	Below

	C37
	37
	37
	Below



Table 1.6 - Beam Bays
	Label
	PointBayI
	PointBayJ

	B1
	7
	6

	B2
	7
	8

	B3
	1
	59

	B4
	8
	9

	B5
	9
	10

	B6
	11
	10

	B7
	6
	11

	B8
	14
	12

	B9
	15
	14

	B10
	17
	15

	B11
	59
	5

	B12
	17
	18

	B13
	18
	20

	B14
	20
	12

	B15
	23
	24

	B16
	24
	17

	B17
	2
	78

	B18
	5
	13

	B19
	13
	22

	B20
	23
	28

	B21
	22
	27

	B22
	81
	35

	B23
	34
	35

	B24
	42
	35

	B25
	27
	29

	B26
	29
	31

	B27
	31
	25

	B28
	30
	42

	B29
	79
	26

	B30
	80
	32

	B31
	82
	43

	B32
	83
	43

	B33
	83
	46

	B34
	45
	113

	B35
	84
	46

	B36
	78
	79

	B37
	85
	134

	B38
	47
	86

	B39
	48
	87

	B40
	79
	80

	B41
	50
	88

	B42
	84
	51

	B43
	85
	51

	B44
	80
	81

	B45
	54
	88

	B46
	82
	81

	B47
	83
	82

	B48
	54
	89

	B49
	60
	89

	B50
	60
	90

	B51
	61
	90

	B52
	61
	91

	B53
	62
	91

	B54
	62
	78

	B55
	160
	11

	B66
	25
	234

	B67
	84
	83

	B68
	234
	208

	B69
	208
	228

	B70
	85
	84

	B71
	86
	85

	B72
	87
	86

	B73
	88
	87

	B74
	88
	89

	B75
	89
	90

	B76
	90
	91

	B77
	91
	78

	B78
	91
	92

	B79
	92
	93

	B80
	93
	82

	B81
	94
	95

	B82
	95
	96

	B83
	96
	83

	B84
	97
	98

	B85
	98
	99

	B86
	99
	100

	B87
	92
	79

	B88
	101
	92

	B89
	98
	101

	B90
	87
	98

	B91
	93
	102

	B92
	103
	93

	B93
	99
	103

	B94
	86
	99

	B95
	105
	104

	B96
	107
	106

	B97
	108
	109

	B98
	110
	109

	B99
	107
	110

	B100
	112
	111

	B101
	1
	105

	B102
	11
	162

	B103
	113
	104

	B104
	114
	115

	B105
	115
	116

	B106
	117
	114

	B107
	117
	118

	B108
	118
	119

	B109
	116
	119

	B110
	120
	121

	B111
	122
	121

	B112
	123
	120

	B113
	123
	124

	B114
	125
	124

	B115
	125
	122

	B116
	127
	126

	B117
	128
	129

	B118
	130
	129

	B119
	131
	130

	B120
	131
	128

	B121
	133
	132

	B122
	135
	134

	B123
	136
	137

	B124
	164
	8

	B125
	140
	141

	B126
	142
	143

	B127
	143
	141

	B128
	142
	140

	B129
	145
	144

	B130
	8
	166

	B131
	65
	20

	B133
	66
	15

	B134
	15
	67

	B135
	157
	156

	B136
	20
	68

	B137
	161
	160

	B138
	163
	162

	B139
	165
	164

	B140
	167
	166

	B141
	169
	168

	B142
	170
	169

	B143
	171
	168

	B144
	172
	171

	B145
	173
	172

	B146
	170
	173

	B147
	175
	174

	B148
	175
	176

	B149
	174
	177

	B150
	178
	177

	B151
	178
	179

	B152
	176
	179

	B153
	180
	181

	B154
	182
	183

	B155
	181
	183

	B156
	180
	182

	B157
	228
	230

	B158
	230
	75

	B159
	75
	231

	B160
	231
	45

	B172
	245
	25



1.5 Area Connectivity
Table 1.7 - Floor Bays
	Label
	NumPoints
	PointNumber
	PointBay

	F1
	16
	1
	6

	F1
	
	2
	11

	F1
	
	3
	10

	F1
	
	4
	42

	F1
	
	5
	35

	F1
	
	6
	18

	F1
	
	7
	20

	F1
	
	8
	12

	F1
	
	9
	14

	F1
	
	10
	15

	F1
	
	11
	17

	F1
	
	12
	24

	F1
	
	13
	23

	F1
	
	14
	9

	F1
	
	15
	8

	F1
	
	16
	7



Table 1.8 - Wall Bays
	Label
	NumPoints
	PointNumber
	PointBay
	PointStory

	W1
	4
	1
	120
	Below

	W1
	
	2
	121
	Below

	W1
	
	3
	121
	Same

	W1
	
	4
	120
	Same

	W2
	4
	1
	121
	Below

	W2
	
	2
	122
	Below

	W2
	
	3
	122
	Same

	W2
	
	4
	121
	Same

	W3
	4
	1
	122
	Below

	W3
	
	2
	125
	Below

	W3
	
	3
	125
	Same

	W3
	
	4
	122
	Same

	W4
	4
	1
	125
	Below

	W4
	
	2
	124
	Below

	W4
	
	3
	124
	Same

	W4
	
	4
	125
	Same

	W5
	4
	1
	124
	Below

	W5
	
	2
	123
	Below

	W5
	
	3
	123
	Same

	W5
	
	4
	124
	Same

	W6
	4
	1
	123
	Below

	W6
	
	2
	120
	Below

	W6
	
	3
	120
	Same

	W6
	
	4
	123
	Same

	W7
	4
	1
	119
	Below

	W7
	
	2
	118
	Below

	W7
	
	3
	118
	Same

	W7
	
	4
	119
	Same

	W8
	4
	1
	118
	Below

	W8
	
	2
	117
	Below

	W8
	
	3
	117
	Same

	W8
	
	4
	118
	Same

	W9
	4
	1
	117
	Below

	W9
	
	2
	114
	Below

	W9
	
	3
	114
	Same

	W9
	
	4
	117
	Same

	W10
	4
	1
	114
	Below

	W10
	
	2
	115
	Below

	W10
	
	3
	115
	Same

	W10
	
	4
	114
	Same

	W11
	4
	1
	115
	Below

	W11
	
	2
	116
	Below

	W11
	
	3
	116
	Same

	W11
	
	4
	115
	Same

	W12
	4
	1
	116
	Below

	W12
	
	2
	119
	Below

	W12
	
	3
	119
	Same

	W12
	
	4
	116
	Same

	W13
	4
	1
	176
	Below

	W13
	
	2
	175
	Below

	W13
	
	3
	175
	Same

	W13
	
	4
	176
	Same

	W14
	4
	1
	175
	Below

	W14
	
	2
	174
	Below

	W14
	
	3
	174
	Same

	W14
	
	4
	175
	Same

	W15
	4
	1
	174
	Below

	W15
	
	2
	177
	Below

	W15
	
	3
	177
	Same

	W15
	
	4
	174
	Same

	W16
	4
	1
	177
	Below

	W16
	
	2
	178
	Below

	W16
	
	3
	178
	Same

	W16
	
	4
	177
	Same

	W17
	4
	1
	178
	Below

	W17
	
	2
	179
	Below

	W17
	
	3
	179
	Same

	W17
	
	4
	178
	Same

	W18
	4
	1
	179
	Below

	W18
	
	2
	176
	Below

	W18
	
	3
	176
	Same

	W18
	
	4
	179
	Same

	W19
	4
	1
	181
	Below

	W19
	
	2
	180
	Below

	W19
	
	3
	180
	Same

	W19
	
	4
	181
	Same

	W20
	4
	1
	180
	Below

	W20
	
	2
	182
	Below

	W20
	
	3
	182
	Same

	W20
	
	4
	180
	Same

	W21
	4
	1
	182
	Below

	W21
	
	2
	183
	Below

	W21
	
	3
	183
	Same

	W21
	
	4
	182
	Same

	W22
	4
	1
	183
	Below

	W22
	
	2
	181
	Below

	W22
	
	3
	181
	Same

	W22
	
	4
	183
	Same

	W23
	4
	1
	108
	Below

	W23
	
	2
	38
	Below

	W23
	
	3
	38
	Same

	W23
	
	4
	108
	Same

	W24
	4
	1
	38
	Below

	W24
	
	2
	107
	Below

	W24
	
	3
	107
	Same

	W24
	
	4
	38
	Same

	W25
	4
	1
	107
	Below

	W25
	
	2
	39
	Below

	W25
	
	3
	39
	Same

	W25
	
	4
	107
	Same

	W26
	4
	1
	39
	Below

	W26
	
	2
	110
	Below

	W26
	
	3
	110
	Same

	W26
	
	4
	39
	Same

	W27
	4
	1
	110
	Below

	W27
	
	2
	109
	Below

	W27
	
	3
	109
	Same

	W27
	
	4
	110
	Same

	W28
	4
	1
	109
	Below

	W28
	
	2
	40
	Below

	W28
	
	3
	40
	Same

	W28
	
	4
	109
	Same

	W29
	4
	1
	40
	Below

	W29
	
	2
	106
	Below

	W29
	
	3
	106
	Same

	W29
	
	4
	40
	Same

	W30
	4
	1
	128
	Below

	W30
	
	2
	41
	Below

	W30
	
	3
	41
	Same

	W30
	
	4
	128
	Same

	W31
	4
	1
	41
	Below

	W31
	
	2
	129
	Below

	W31
	
	3
	129
	Same

	W31
	
	4
	41
	Same

	W32
	4
	1
	129
	Below

	W32
	
	2
	130
	Below

	W32
	
	3
	130
	Same

	W32
	
	4
	129
	Same

	W33
	4
	1
	130
	Below

	W33
	
	2
	44
	Below

	W33
	
	3
	44
	Same

	W33
	
	4
	130
	Same

	W34
	4
	1
	44
	Below

	W34
	
	2
	131
	Below

	W34
	
	3
	131
	Same

	W34
	
	4
	44
	Same

	W35
	4
	1
	131
	Below

	W35
	
	2
	128
	Below

	W35
	
	3
	128
	Same

	W35
	
	4
	131
	Same

	W36
	4
	1
	169
	Below

	W36
	
	2
	170
	Below

	W36
	
	3
	170
	Same

	W36
	
	4
	169
	Same

	W37
	4
	1
	170
	Below

	W37
	
	2
	173
	Below

	W37
	
	3
	173
	Same

	W37
	
	4
	170
	Same

	W38
	4
	1
	173
	Below

	W38
	
	2
	172
	Below

	W38
	
	3
	172
	Same

	W38
	
	4
	173
	Same

	W39
	4
	1
	172
	Below

	W39
	
	2
	171
	Below

	W39
	
	3
	171
	Same

	W39
	
	4
	172
	Same

	W40
	4
	1
	171
	Below

	W40
	
	2
	168
	Below

	W40
	
	3
	168
	Same

	W40
	
	4
	171
	Same

	W41
	4
	1
	168
	Below

	W41
	
	2
	169
	Below

	W41
	
	3
	169
	Same

	W41
	
	4
	168
	Same

	W42
	4
	1
	140
	Below

	W42
	
	2
	141
	Below

	W42
	
	3
	141
	Same

	W42
	
	4
	140
	Same

	W43
	4
	1
	141
	Below

	W43
	
	2
	143
	Below

	W43
	
	3
	143
	Same

	W43
	
	4
	141
	Same

	W44
	4
	1
	143
	Below

	W44
	
	2
	142
	Below

	W44
	
	3
	142
	Same

	W44
	
	4
	143
	Same

	W45
	4
	1
	142
	Below

	W45
	
	2
	140
	Below

	W45
	
	3
	140
	Same

	W45
	
	4
	142
	Same

	W46
	4
	1
	113
	Below

	W46
	
	2
	45
	Below

	W46
	
	3
	45
	Same

	W46
	
	4
	113
	Same

	W47
	4
	1
	113
	Below

	W47
	
	2
	49
	Below

	W47
	
	3
	49
	Same

	W47
	
	4
	113
	Same

	W49
	4
	1
	104
	Below

	W49
	
	2
	52
	Below

	W49
	
	3
	52
	Same

	W49
	
	4
	104
	Same

	W50
	4
	1
	104
	Below

	W50
	
	2
	53
	Below

	W50
	
	3
	53
	Same

	W50
	
	4
	104
	Same

	W52
	4
	1
	55
	Below

	W52
	
	2
	56
	Below

	W52
	
	3
	56
	Same

	W52
	
	4
	55
	Same

	W53
	4
	1
	105
	Below

	W53
	
	2
	57
	Below

	W53
	
	3
	57
	Same

	W53
	
	4
	105
	Same

	W54
	4
	1
	1
	Below

	W54
	
	2
	58
	Below

	W54
	
	3
	58
	Same

	W54
	
	4
	1
	Same

	W55
	4
	1
	1
	Below

	W55
	
	2
	59
	Below

	W55
	
	3
	59
	Same

	W55
	
	4
	1
	Same



1.6 Mass
Table 1.9 - Mass Source Definition
	Name
	Is Default
	Include Lateral Mass?
	Include Vertical Mass?
	Lump Mass?
	Source Self Mass?
	Source Added Mass?
	Source Load Patterns?
	Move Mass Centroid?
	Move Ratio X
	Move Ratio Y
	Load Pattern
	Multiplier

	MsSrc1
	Yes
	Yes
	No
	Yes
	No
	Yes
	Yes
	No
	
	
	Dead
	1



Table 1.10 - Mass Summary by Story
	Story
	UX
kg
	UY
kg
	UZ
kg

	Story2
	0
	0
	0

	Story1
	0
	0
	0

	cubierta
	98347.96
	98347.96
	0

	Base
	65832.81
	65832.81
	0



Table 1.11 - Mass Summary by Group
	Group
	Self Mass
kg
	Self Weight
kN
	Mass X
kg
	Mass Y
kg
	Mass Z
kg

	All
	0
	1610.0634
	164180.77
	164180.77
	0



1.7 Groups
Table 1.12 - Group Definitions
	Name
	Color
	Steel Design?
	Concrete Design?
	Composite Design?

	All
	Yellow
	No
	No
	No



Structure Data		4/12/2020

	Page 1 of 1	
2 Properties
This chapter provides property information for materials, frame sections, shell sections, and links.
2.1 Materials
Table 2.1 - Material Properties - General
	Material
	Type
	SymType
	Grade
	Color
	Notes

	3000Psi
	Concrete
	Isotropic
	Unknown
	Gray8Dark
	

	4000Psi
	Concrete
	Isotropic
	Unknown
	Blue
	

	A416Gr270
	Tendon
	Uniaxial
	Unknown
	Magenta
	

	A500Gr c
	Steel
	Isotropic
	Grade B, Fy 46 (HSS Rect.)
	Red
	

	A572Gr50
	Steel
	Isotropic
	Grade 50
	Cyan
	

	A615Gr60
	Rebar
	Uniaxial
	Unknown
	Cyan
	

	A992Fy50
	Steel
	Isotropic
	Unknown
	Yellow
	

	MAT
	Other
	Isotropic
	Unknown
	Green
	



2.2 Frame Sections
Table 2.2 - Frame Section Property Definitions - Summary (Part 1 of 3)
	Name
	Material
	Shape
	Color
	Area
cm2
	J
cm4
	I33
cm4
	I22
cm4
	I23
cm4
	IMajor
cm4
	IMinor
cm4
	MajorAngle
deg

	C0.40
	3000Psi
	Concrete Circle
	12615935
	1256.6
	251327.4
	125663.7
	125663.7
	
	
	
	

	C0.60
	3000Psi
	Concrete Circle
	Magenta
	2827.4
	1272345
	636172.5
	636172.5
	
	
	
	

	c200x200x5
	A500Gr c
	Steel Tube
	Blue
	39
	3707.4
	2473.3
	2473.3
	
	
	
	

	C3050
	4000Psi
	Concrete Rectangular
	Gray8Dark
	1500
	281737.1
	112500
	312500
	
	
	
	

	C4040
	4000Psi
	Concrete Rectangular
	Red
	1600
	360533.3
	213333.3
	213333.3
	
	
	
	

	C40X40
	3000Psi
	Concrete Rectangular
	Cyan
	1600
	360533.3
	213333.3
	213333.3
	
	
	
	

	CC6X4
	A500Gr c
	Steel Pipe
	Magenta
	18.3
	978.4
	489.2
	489.2
	
	
	
	

	v100x100x3
	A500Gr c
	Steel Tube
	4194432
	11.6
	273.8
	182.7
	182.7
	
	
	
	

	v150x150x4
	A500Gr c
	Steel Tube
	Yellow
	23.4
	1244.9
	830.5
	830.5
	
	
	
	

	V1540
	4000Psi
	Concrete Rectangular
	Cyan
	600
	34386.3
	80000
	11250
	
	
	
	

	V2040
	4000Psi
	Concrete Rectangular
	Green
	800
	73241.7
	106666.7
	26666.7
	
	
	
	

	V3040
	4000Psi
	Concrete Rectangular
	Blue
	1200
	194385.1
	160000
	90000
	
	
	
	

	V35X50
	4000Psi
	Concrete Rectangular
	Yellow
	1750
	405757.3
	364583.3
	178645.8
	
	
	
	

	V40x50
	4000Psi
	Concrete Rectangular
	Magenta
	2000
	547416.7
	416666.7
	266666.7
	
	
	
	

	W12X22
	A992Fy50
	Steel I/Wide Flange
	Magenta
	41.8
	12.2
	6493.2
	194
	
	
	
	



Table 2.2 - Frame Section Property Definitions - Summary (Part 2 of 3)
	As2
cm2
	As3
cm2
	S33Pos
cm3
	S33Neg
cm3
	S22Pos
cm3
	S22Neg
cm3
	Z33
cm3
	Z22
cm3
	R33
mm
	R22
mm
	Cw
cm6
	Fillet Radius
mm
	CG Offset 3
mm

	1131
	1131
	6283.2
	6283.2
	6283.2
	6283.2
	10666.7
	10666.7
	100
	100
	
	
	0

	2544.7
	2544.7
	21205.8
	21205.8
	21205.8
	21205.8
	36000
	36000
	150
	150
	
	
	0

	19.8
	19.8
	247.3
	247.3
	247.3
	247.3
	285.3
	285.3
	79.6
	79.6
	
	
	0

	1250
	1250
	7500
	7500
	12500
	12500
	11250
	18750
	86.6
	144.3
	
	
	0

	1333.3
	1333.3
	10666.7
	10666.7
	10666.7
	10666.7
	16000
	16000
	115.5
	115.5
	
	
	0

	1333.3
	1333.3
	10666.7
	10666.7
	10666.7
	10666.7
	16000
	16000
	115.5
	115.5
	
	
	0

	9.2
	9.2
	65.2
	65.2
	65.2
	65.2
	85.3
	85.3
	51.6
	51.6
	
	
	0

	5.9
	5.9
	36.5
	36.5
	36.5
	36.5
	42.4
	42.4
	39.6
	39.6
	
	
	0

	11.9
	11.9
	110.7
	110.7
	110.7
	110.7
	127.9
	127.9
	59.6
	59.6
	
	
	0

	500
	500
	4000
	4000
	1500
	1500
	6000
	2250
	115.5
	43.3
	
	
	0

	666.7
	666.7
	5333.3
	5333.3
	2666.7
	2666.7
	8000
	4000
	115.5
	57.7
	
	
	0

	1000
	1000
	8000
	8000
	6000
	6000
	12000
	9000
	115.5
	86.6
	
	
	0

	1458.3
	1458.3
	14583.3
	14583.3
	10208.3
	10208.3
	21875
	15312.5
	144.3
	101
	
	
	0

	1666.7
	1666.7
	16666.7
	16666.7
	13333.3
	13333.3
	25000
	20000
	144.3
	115.5
	
	
	0

	20.6
	18.4
	415.7
	415.7
	37.9
	37.9
	480.1
	60
	124.6
	21.5
	43889.7
	7.6
	0



Table 2.2 - Frame Section Property Definitions - Summary (Part 3 of 3)
	CG Offset 2
mm
	PNA Offset 3
mm
	PNA Offset 2
mm
	SC Offset 3
mm
	SC Offset 2
mm
	Area Modifier
	As2 Modifier
	As3 Modifier
	J Modifier
	I33 Modifier
	I22 Modifier
	Mass Modifier
	Weight Modifier

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1

	0
	0
	0
	
	
	1
	1
	1
	1
	1
	1
	1
	1



2.3 Shell Sections
Table 2.3 - Area Section Property Definitions - Summary
	Name
	Type
	Element Type
	Material
	Total Thickness
mm
	Deck Material
	Deck Depth
mm

	CUB
	Slab
	Membrane
	MAT
	60
	
	

	Deck1
	Deck
	Membrane
	4000Psi
	162.5
	A992Fy50
	75

	MURO MAMP
	Wall
	Shell-Thick
	3000Psi
	120
	
	

	MUROCONC12
	Wall
	Shell-Thin
	3000Psi
	120
	
	

	PLACA
	Slab
	Membrane
	4000Psi
	800
	
	

	Plank1
	Slab
	Membrane
	4000Psi
	200
	
	



2.4 Reinforcement Sizes
Table 2.4 - Reinforcing Bar Sizes
	Name
	Diameter
mm
	Area
cm2

	6
	6
	0.3

	8
	8
	0.5

	10
	10
	0.8

	12
	12
	1.1

	14
	14
	1.5

	16
	16
	2

	18
	18
	2.5

	20
	20
	3.1

	22
	22
	3.8

	25
	25
	4.9

	26
	26
	5.3

	28
	28
	6.2

	32
	32
	8

	36
	36
	10.2

	40
	40
	12.6

	50
	50
	19.6

	#2
	6.4
	0.3

	#3
	9.5
	0.7

	#4
	12.7
	1.3

	#5
	15.9
	2

	#6
	19.1
	2.8

	#7
	22.2
	3.9

	#8
	25.4
	5.1

	#9
	28.7
	6.5

	#10
	32.3
	8.2

	#11
	35.8
	10.1

	#14
	43
	14.5

	#18
	57.3
	25.8



2.5 Links
Table 2.5 - Link Property Definitions - Summary
	Name
	Type
	Degrees of Freedom
	Mass
kg
	Weight
kN
	Defined Length
m
	Defined Area
m2

	Link1
	Linear
	U1
	0
	0
	1
	1



2.6 Tendon Sections
Table 2.6 - Tendon Section Properties
	Name
	Material
	StrandArea
cm2
	Color
	Notes

	Tendon1
	A416Gr270
	1
	Magenta
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3 Assignments
This chapter provides a listing of the assignments applied to the model.
3.1 Joint Assignments
Table 3.1 - Joint Assignments - Summary
	Story
	Label
	UniqueName
	Diaphragm
	Restraints
	Spring
	Added Mass
	Panel Zone
	Include in Mesh

	cubierta
	1
	196
	From Area
	
	
	
	
	

	cubierta
	6
	135
	From Area
	
	
	
	
	

	cubierta
	7
	136
	From Area
	
	
	
	
	

	cubierta
	8
	137
	From Area
	
	
	
	
	

	cubierta
	9
	138
	From Area
	
	
	
	
	

	cubierta
	10
	139
	From Area
	
	
	
	
	

	cubierta
	11
	140
	From Area
	
	
	
	
	

	cubierta
	12
	141
	From Area
	
	
	
	
	

	cubierta
	14
	142
	From Area
	
	
	
	
	

	cubierta
	15
	143
	From Area
	
	
	
	
	

	cubierta
	17
	144
	From Area
	
	
	
	
	

	cubierta
	18
	145
	From Area
	
	
	
	
	

	cubierta
	20
	146
	From Area
	
	
	
	
	

	cubierta
	23
	147
	From Area
	
	
	
	
	

	cubierta
	24
	148
	From Area
	
	
	
	
	

	cubierta
	28
	150
	From Area
	
	
	
	
	

	cubierta
	30
	151
	From Area
	
	
	
	
	

	cubierta
	34
	152
	From Area
	
	
	
	
	

	cubierta
	35
	153
	From Area
	
	
	
	
	

	cubierta
	42
	154
	From Area
	
	
	
	
	

	cubierta
	78
	161
	From Area
	
	
	
	
	

	cubierta
	79
	162
	From Area
	
	
	
	
	

	cubierta
	80
	163
	From Area
	
	
	
	
	

	cubierta
	81
	164
	From Area
	
	
	
	
	

	cubierta
	82
	165
	From Area
	
	
	
	
	

	cubierta
	83
	166
	From Area
	
	
	
	
	

	cubierta
	84
	167
	From Area
	
	
	
	
	

	cubierta
	85
	168
	From Area
	
	
	
	
	

	cubierta
	86
	169
	From Area
	
	
	
	
	

	cubierta
	87
	170
	From Area
	
	
	
	
	

	cubierta
	88
	171
	From Area
	
	
	
	
	

	cubierta
	89
	172
	From Area
	
	
	
	
	

	cubierta
	90
	173
	From Area
	
	
	
	
	

	cubierta
	91
	174
	From Area
	
	
	
	
	

	cubierta
	92
	175
	From Area
	
	
	
	
	

	cubierta
	93
	176
	From Area
	
	
	
	
	

	cubierta
	94
	177
	From Area
	
	
	
	
	

	cubierta
	95
	178
	From Area
	
	
	
	
	

	cubierta
	96
	179
	From Area
	
	
	
	
	

	cubierta
	97
	180
	From Area
	
	
	
	
	

	cubierta
	98
	181
	From Area
	
	
	
	
	

	cubierta
	99
	182
	From Area
	
	
	
	
	

	cubierta
	100
	183
	From Area
	
	
	
	
	

	cubierta
	101
	184
	From Area
	
	
	
	
	

	cubierta
	102
	185
	From Area
	
	
	
	
	

	cubierta
	103
	186
	From Area
	
	
	
	
	

	cubierta
	104
	187
	From Area
	
	
	
	
	

	cubierta
	105
	188
	From Area
	
	
	
	
	

	cubierta
	106
	189
	From Area
	
	
	
	
	

	cubierta
	107
	190
	From Area
	
	
	
	
	

	cubierta
	108
	191
	From Area
	
	
	
	
	

	cubierta
	109
	192
	From Area
	
	
	
	
	

	cubierta
	110
	193
	From Area
	
	
	
	
	

	cubierta
	111
	194
	From Area
	
	
	
	
	

	cubierta
	112
	195
	From Area
	
	
	
	
	

	cubierta
	113
	197
	From Area
	
	
	
	
	

	cubierta
	114
	198
	From Area
	
	
	
	
	

	cubierta
	115
	199
	From Area
	
	
	
	
	

	cubierta
	116
	200
	From Area
	
	
	
	
	

	cubierta
	117
	201
	From Area
	
	
	
	
	

	cubierta
	118
	202
	From Area
	
	
	
	
	

	cubierta
	119
	203
	From Area
	
	
	
	
	

	cubierta
	120
	204
	From Area
	
	
	
	
	

	cubierta
	121
	205
	From Area
	
	
	
	
	

	cubierta
	122
	206
	From Area
	
	
	
	
	

	cubierta
	123
	207
	From Area
	
	
	
	
	

	cubierta
	124
	208
	From Area
	
	
	
	
	

	cubierta
	125
	209
	From Area
	
	
	
	
	

	cubierta
	126
	210
	From Area
	
	
	
	
	

	cubierta
	127
	211
	From Area
	
	
	
	
	

	cubierta
	128
	212
	From Area
	
	
	
	
	

	cubierta
	129
	213
	From Area
	
	
	
	
	

	cubierta
	130
	214
	From Area
	
	
	
	
	

	cubierta
	131
	215
	From Area
	
	
	
	
	

	cubierta
	132
	216
	From Area
	
	
	
	
	

	cubierta
	133
	217
	From Area
	
	
	
	
	

	cubierta
	134
	218
	From Area
	
	
	
	
	

	cubierta
	135
	219
	From Area
	
	
	
	
	

	cubierta
	136
	220
	From Area
	
	
	
	
	

	cubierta
	137
	221
	From Area
	
	
	
	
	

	cubierta
	140
	224
	From Area
	
	
	
	
	

	cubierta
	141
	225
	From Area
	
	
	
	
	

	cubierta
	142
	226
	From Area
	
	
	
	
	

	cubierta
	143
	227
	From Area
	
	
	
	
	

	cubierta
	144
	228
	From Area
	
	
	
	
	

	cubierta
	145
	229
	From Area
	
	
	
	
	

	cubierta
	156
	240
	From Area
	
	
	
	
	

	cubierta
	157
	241
	From Area
	
	
	
	
	

	cubierta
	160
	244
	From Area
	
	
	
	
	

	cubierta
	161
	245
	From Area
	
	
	
	
	

	cubierta
	162
	246
	From Area
	
	
	
	
	

	cubierta
	163
	247
	From Area
	
	
	
	
	

	cubierta
	164
	248
	From Area
	
	
	
	
	

	cubierta
	165
	249
	From Area
	
	
	
	
	

	cubierta
	166
	250
	From Area
	
	
	
	
	

	cubierta
	167
	251
	From Area
	
	
	
	
	

	cubierta
	168
	252
	From Area
	
	
	
	
	

	cubierta
	169
	253
	From Area
	
	
	
	
	

	cubierta
	170
	254
	From Area
	
	
	
	
	

	cubierta
	171
	255
	From Area
	
	
	
	
	

	cubierta
	172
	256
	From Area
	
	
	
	
	

	cubierta
	173
	257
	From Area
	
	
	
	
	

	cubierta
	174
	258
	From Area
	
	
	
	
	

	cubierta
	175
	259
	From Area
	
	
	
	
	

	cubierta
	176
	260
	From Area
	
	
	
	
	

	cubierta
	177
	261
	From Area
	
	
	
	
	

	cubierta
	178
	262
	From Area
	
	
	
	
	

	cubierta
	179
	263
	From Area
	
	
	
	
	

	cubierta
	180
	264
	From Area
	
	
	
	
	

	cubierta
	181
	265
	From Area
	
	
	
	
	

	cubierta
	182
	266
	From Area
	
	
	
	
	

	cubierta
	183
	267
	From Area
	
	
	
	
	

	cubierta
	3
	25
	From Area
	
	
	
	
	

	cubierta
	4
	27
	From Area
	
	
	
	
	

	cubierta
	5
	29
	From Area
	
	
	
	
	

	cubierta
	13
	31
	From Area
	
	
	
	
	

	cubierta
	16
	33
	From Area
	
	
	
	
	

	cubierta
	19
	35
	From Area
	
	
	
	
	

	cubierta
	21
	37
	From Area
	
	
	
	
	

	cubierta
	22
	39
	From Area
	
	
	
	
	

	cubierta
	25
	41
	From Area
	
	
	
	
	

	cubierta
	27
	43
	From Area
	
	
	
	
	

	cubierta
	29
	45
	From Area
	
	
	
	
	

	cubierta
	31
	47
	From Area
	
	
	
	
	

	cubierta
	33
	51
	From Area
	
	
	
	
	

	cubierta
	36
	53
	From Area
	
	
	
	
	

	cubierta
	37
	55
	From Area
	
	
	
	
	

	cubierta
	38
	80
	From Area
	
	
	
	
	

	cubierta
	39
	83
	From Area
	
	
	
	
	

	cubierta
	40
	87
	From Area
	
	
	
	
	

	cubierta
	41
	91
	From Area
	
	
	
	
	

	cubierta
	44
	95
	From Area
	
	
	
	
	

	cubierta
	45
	109
	From Area
	
	
	
	
	

	cubierta
	49
	111
	From Area
	
	
	
	
	

	cubierta
	52
	118
	From Area
	
	
	
	
	

	cubierta
	53
	120
	From Area
	
	
	
	
	

	cubierta
	55
	127
	From Area
	
	
	
	
	

	cubierta
	56
	126
	From Area
	
	
	
	
	

	cubierta
	57
	130
	From Area
	
	
	
	
	

	cubierta
	58
	133
	From Area
	
	
	
	
	

	cubierta
	59
	149
	From Area
	
	
	
	
	

	cubierta
	75
	800
	From Area
	
	
	
	
	

	cubierta
	208
	855
	From Area
	
	
	
	
	

	cubierta
	228
	848
	From Area
	
	
	
	
	

	cubierta
	230
	850
	From Area
	
	
	
	
	

	cubierta
	231
	851
	From Area
	
	
	
	
	

	cubierta
	234
	854
	From Area
	
	
	
	
	

	cubierta
	245
	867
	From Area
	
	
	
	
	

	cubierta
	2
	1
	From Area
	
	
	
	
	

	cubierta
	26
	2
	From Area
	
	
	
	
	

	cubierta
	32
	3
	From Area
	
	
	
	
	

	cubierta
	43
	48
	From Area
	
	
	
	
	

	cubierta
	46
	49
	From Area
	
	
	
	
	

	cubierta
	47
	112
	From Area
	
	
	
	
	

	cubierta
	48
	113
	From Area
	
	
	
	
	

	cubierta
	50
	114
	From Area
	
	
	
	
	

	cubierta
	51
	115
	From Area
	
	
	
	
	

	cubierta
	54
	121
	From Area
	
	
	
	
	

	cubierta
	60
	122
	From Area
	
	
	
	
	

	cubierta
	61
	123
	From Area
	
	
	
	
	

	cubierta
	62
	155
	From Area
	
	
	
	
	

	cubierta
	65
	156
	From Area
	
	
	
	
	

	cubierta
	66
	157
	From Area
	
	
	
	
	

	cubierta
	67
	158
	From Area
	
	
	
	
	

	cubierta
	68
	159
	From Area
	
	
	
	
	

	Base
	1
	131
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	78
	7
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	79
	6
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	80
	5
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	81
	4
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	82
	15
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	83
	14
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	84
	16
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	85
	23
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	86
	22
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	87
	21
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	88
	20
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	89
	19
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	90
	10
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	91
	8
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	92
	9
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	93
	12
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	95
	11
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	96
	13
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	98
	18
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	99
	17
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	104
	116
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	105
	128
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	106
	88
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	107
	81
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	108
	78
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	109
	85
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	110
	84
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	113
	107
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	114
	65
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	115
	66
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	116
	67
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	117
	64
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	118
	63
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	119
	62
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	120
	56
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	121
	57
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	122
	58
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	123
	61
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	124
	60
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	125
	59
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	128
	89
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	129
	92
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	130
	93
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	131
	96
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	140
	103
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	141
	104
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	142
	106
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	143
	105
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	168
	102
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	169
	97
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	170
	98
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	171
	101
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	172
	100
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	173
	99
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	174
	70
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	175
	69
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	176
	68
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	177
	71
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	178
	72
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	179
	73
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	180
	75
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	181
	74
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	182
	76
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	183
	77
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	3
	24
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	4
	26
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	5
	28
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	13
	30
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	16
	32
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	19
	34
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	21
	36
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	22
	38
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	25
	40
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	27
	42
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	29
	44
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	31
	46
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	33
	50
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	36
	52
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	37
	54
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	38
	79
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	39
	82
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	40
	86
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	41
	90
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	44
	94
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	45
	108
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	49
	110
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	52
	117
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	53
	119
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	55
	124
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	56
	125
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	57
	129
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	58
	132
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	

	Base
	59
	134
	From Area
	UX; UY; UZ; RX; RY; RZ
	
	
	
	



3.2 Frame Assignments
Table 3.2 - Frame Assignments - Summary (Part 1 of 2)
	Story
	Label
	UniqueName
	Design Type
	Length
m
	Auto Select
	Analysis Section
	Design Section
	Axis Angle
deg
	Max Station Spacing
m
	Min Number Stations
	Releases
	User Offsets

	cubierta
	B1
	273E
	Beam
	17.9684
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B2
	273F
	Beam
	12.2862
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B4
	2740
	Beam
	12.1249
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B5
	2741
	Beam
	18.0729
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B6
	2742
	Beam
	12.1199
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B7
	2743
	Beam
	12.2895
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B8
	2744
	Beam
	17.9684
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B9
	2745
	Beam
	12.2862
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B10
	2746
	Beam
	12.1249
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B12
	2747
	Beam
	18.0729
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B13
	2748
	Beam
	12.1199
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B14
	2749
	Beam
	12.2895
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B15
	274A
	Beam
	20.6228
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B16
	274B
	Beam
	2.2179
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B20
	274D
	Beam
	3.2869
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B23
	301D
	Beam
	26.3359
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B24
	301E
	Beam
	20.6256
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B28
	301F
	Beam
	26.3359
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B36
	3E4E
	Beam
	4.4291
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B40
	3E4F
	Beam
	5.7214
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B44
	3E50
	Beam
	4.431
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B46
	3E51
	Beam
	4.37
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B47
	3E52
	Beam
	4.3697
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B67
	3E53
	Beam
	4.3732
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B70
	3E54
	Beam
	4.3699
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B71
	3E55
	Beam
	4.431
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B72
	3E56
	Beam
	5.7214
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B73
	3E57
	Beam
	4.4291
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B74
	3E58
	Beam
	4.3728
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B75
	3E59
	Beam
	4.3703
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B76
	3E5A
	Beam
	4.3697
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B77
	3E5B
	Beam
	4.37
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B78
	3E5C
	Beam
	4.4291
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B79
	3E5D
	Beam
	5.7214
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B80
	3E5E
	Beam
	4.431
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B81
	3E5F
	Beam
	4.4291
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B82
	3E60
	Beam
	5.7214
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B83
	3E61
	Beam
	4.431
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B84
	3E62
	Beam
	4.4197
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B85
	3E63
	Beam
	5.7214
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B86
	3E64
	Beam
	4.431
	
	v100x100x3
	N/A
	
	0.5
	
	
	

	cubierta
	B87
	3E65
	Beam
	4.37
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B88
	3E66
	Beam
	4.3697
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B89
	3E67
	Beam
	4.3703
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B90
	3E68
	Beam
	4.3728
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B91
	3E69
	Beam
	4.37
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B92
	3E6A
	Beam
	4.3697
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B93
	3E6B
	Beam
	4.3703
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B94
	3E6C
	Beam
	4.3728
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B95
	3E6D
	Beam
	60.9328
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B96
	3E6E
	Beam
	0.3208
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B97
	3E6F
	Beam
	10.8034
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B98
	3E70
	Beam
	0.2811
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B99
	3E71
	Beam
	10.8684
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B100
	3E72
	Beam
	0.4
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B101
	3E73
	Beam
	15.4357
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B103
	3E75
	Beam
	15.4266
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B104
	3E76
	Beam
	1.9691
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B105
	3E77
	Beam
	2.2395
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B106
	3E78
	Beam
	0.2801
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B107
	3E79
	Beam
	2.258
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B108
	3E7A
	Beam
	2.5196
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B109
	3E7B
	Beam
	0.2889
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B110
	3E7C
	Beam
	2.246
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B111
	3E7D
	Beam
	2.5144
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B112
	3E7E
	Beam
	0.2801
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B113
	3E7F
	Beam
	1.9656
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B114
	3E80
	Beam
	2.2343
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B115
	3E81
	Beam
	0.2804
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B116
	3E82
	Beam
	0.2983
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B117
	3E83
	Beam
	10.9897
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B118
	3E84
	Beam
	0.2793
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B119
	3E85
	Beam
	10.9897
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B120
	3E86
	Beam
	0.2793
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B121
	3E87
	Beam
	0.4
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B122
	3E88
	Beam
	0.279
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B123
	3E89
	Beam
	2.9102
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B125
	3E8B
	Beam
	2.0621
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B126
	3E8C
	Beam
	2.0621
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B127
	3E8D
	Beam
	0.2889
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B128
	3E8E
	Beam
	0.2805
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B129
	3E8F
	Beam
	0.62
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B135
	3E95
	Beam
	0.6194
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B137
	3E97
	Beam
	0.2
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B138
	3E98
	Beam
	0.2
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B139
	3E99
	Beam
	0.2
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B140
	3E9A
	Beam
	0.2
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B141
	3E9B
	Beam
	2.2457
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B142
	3E9C
	Beam
	2.5129
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B143
	3E9D
	Beam
	0.2798
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B144
	3E9E
	Beam
	1.961
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B145
	3E9F
	Beam
	2.2331
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B146
	3EA0
	Beam
	0.2847
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B147
	3EA1
	Beam
	2.2457
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B148
	3EA2
	Beam
	2.5129
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B149
	3EA3
	Beam
	0.2798
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B150
	3EA4
	Beam
	1.961
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B151
	3EA5
	Beam
	2.2331
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B152
	3EA6
	Beam
	0.2847
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B153
	3EA7
	Beam
	0.2802
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B154
	3EA8
	Beam
	0.2802
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B155
	3EA9
	Beam
	2.091
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B156
	3EAA
	Beam
	2.091
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B3
	40
	Beam
	1.025
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B11
	41
	Beam
	4.144
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B18
	42
	Beam
	6.9992
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B19
	43
	Beam
	8.1007
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B21
	44
	Beam
	2.7117
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B25
	45
	Beam
	7.4276
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B26
	46
	Beam
	7.404
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B27
	47
	Beam
	2.8486
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B34
	51
	Beam
	0.95
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B66
	428
	Beam
	11.6882
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B68
	429
	Beam
	2.0272
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B69
	430
	Beam
	2.0272
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B157
	431
	Beam
	1.0136
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B158
	432
	Beam
	0.5408
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B159
	433
	Beam
	0.4728
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B160
	434
	Beam
	1.5522
	
	V1540
	V1540
	
	0.5
	
	
	

	cubierta
	B172
	472
	Beam
	40.1483
	
	W12X22
	N/A
	
	0.5
	
	
	

	cubierta
	B17
	1
	Beam
	5.3
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B22
	2
	Beam
	5.5221
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B29
	35
	Beam
	4.6007
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B30
	39
	Beam
	4.6035
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B31
	48
	Beam
	3.8
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B32
	49
	Beam
	3.8686
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B33
	50
	Beam
	3.7
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B35
	52
	Beam
	3.652
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B37
	53
	Beam
	4.3755
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B38
	54
	Beam
	4.5923
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B39
	55
	Beam
	4.3133
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B41
	56
	Beam
	4.5935
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B42
	57
	Beam
	3.8
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B43
	58
	Beam
	3.7437
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B45
	59
	Beam
	3.9
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B48
	60
	Beam
	3.5224
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B49
	61
	Beam
	3.7
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B50
	62
	Beam
	3.4641
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B51
	63
	Beam
	4.025
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B52
	64
	Beam
	3.3626
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B53
	65
	Beam
	3.65
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B54
	66
	Beam
	3.7579
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B55
	67
	Beam
	6.3527
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B102
	68
	Beam
	6.3271
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B124
	69
	Beam
	6.3501
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B130
	70
	Beam
	6.3195
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B131
	71
	Beam
	6
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B133
	73
	Beam
	7
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B134
	74
	Beam
	6.0671
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	B136
	72
	Beam
	5.9558
	
	v150x150x4
	N/A
	
	0.5
	
	
	

	cubierta
	C1
	3
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C3
	4
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C4
	5
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C5
	6
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C6
	7
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C7
	8
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C8
	9
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C9
	10
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C10
	11
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C11
	12
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C12
	13
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C13
	14
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C14
	15
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C15
	16
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C16
	17
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C17
	18
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C18
	19
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C19
	20
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C20
	21
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C21
	22
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C22
	23
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C23
	24
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C24
	25
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C25
	26
	Column
	4
	
	c200x200x5
	N/A
	
	
	3
	
	

	cubierta
	C26
	27
	Column
	4
	
	v100x100x3
	N/A
	
	
	3
	
	

	cubierta
	C27
	28
	Column
	4
	
	v100x100x3
	N/A
	
	
	3
	
	

	cubierta
	C28
	29
	Column
	4
	
	v100x100x3
	N/A
	
	
	3
	
	

	cubierta
	C29
	30
	Column
	4
	
	C0.60
	C0.60
	
	
	3
	
	

	cubierta
	C30
	31
	Column
	4
	
	C0.60
	C0.60
	
	
	3
	
	

	cubierta
	C31
	32
	Column
	4
	
	C0.40
	C0.40
	
	
	3
	
	

	cubierta
	C32
	33
	Column
	4
	
	C0.40
	C0.40
	
	
	3
	
	

	cubierta
	C33
	34
	Column
	4
	
	W12X22
	N/A
	
	
	3
	
	

	cubierta
	C35
	36
	Column
	4
	
	C4040
	C4040
	
	
	3
	
	

	cubierta
	C36
	37
	Column
	4
	
	C4040
	C4040
	
	
	3
	
	

	cubierta
	C37
	38
	Column
	4
	
	C4040
	C4040
	
	
	3
	
	



Table 3.2 - Frame Assignments - Summary (Part 2 of 2)
	Added Mass
kg/m
	Pier
	Spandrel
	Spring
	Modifiers
	T/C Limits
	Moment Beam Type

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	



3.3 Shell Assignments
Table 3.3 - Area Assignments - Summary
	Story
	Label
	UniqueName
	Section Property
	Property Type
	Diaphragm
	Axis Angle
deg
	Added Mass
kg/m2
	Pier
	Spandrel
	Spandrel Story
	Spring
	Modifiers

	cubierta
	F1
	48
	CUB
	Slab
	
	
	
	
	
	
	
	

	cubierta
	W1
	1
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W2
	2
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W3
	3
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W4
	4
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W5
	5
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W6
	6
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W7
	7
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W8
	8
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W9
	9
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W10
	10
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W11
	11
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W12
	12
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W13
	13
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W14
	14
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W15
	15
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W16
	16
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W17
	17
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W18
	18
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W19
	19
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W20
	20
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W21
	21
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W22
	22
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W23
	23
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W24
	24
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W25
	25
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W26
	26
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W27
	27
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W28
	28
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W29
	29
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W30
	30
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W31
	31
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W32
	32
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W33
	33
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W34
	34
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W35
	35
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W36
	36
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W37
	37
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W38
	38
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W39
	39
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W40
	40
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W41
	41
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W42
	42
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W43
	43
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W44
	44
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W45
	45
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W46
	46
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W47
	47
	MURO MAMP
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W49
	49
	MUROCONC12
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W50
	50
	MUROCONC12
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W52
	52
	MUROCONC12
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W53
	53
	MUROCONC12
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W54
	54
	MUROCONC12
	Wall
	
	
	
	
	
	
	
	

	cubierta
	W55
	55
	MUROCONC12
	Wall
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4 Loads
This chapter provides loading information as applied to the model.
4.1 Load Patterns
Table 4.1 - Load Pattern Definitions
	Name
	Is Auto Load
	Type
	Self Weight Multiplier
	Auto Load

	~LLRF
	Yes
	Other
	0
	

	Dead
	No
	Dead
	1
	

	FHEx
	No
	Seismic
	0
	User Coefficient

	FHEy
	No
	Seismic
	0
	User Coefficient

	Live
	No
	Live
	0
	



4.2 Auto Seismic Loading
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User Coefficient Auto Seismic Load Calculation
This calculation presents the automatically generated lateral seismic loads for load pattern FHEx using the user input coefficients, as calculated by ETABS.
Direction and Eccentricity
Direction = X + Eccentricity Y
Eccentricity Ratio = 5% for all diaphragms
Factors and Coefficients
Equivalent Lateral Forces
	Base Shear Coefficient, C
	
	

	Base Shear, V
	
	



Calculated Base Shear
	Direction
	Period Used

 (sec)
	C
	W

 (kN)
	V

 (kN)

	X + Ecc. Y
	0
	0
	964.464
	954.8194




Applied Story Forces
	[image: ]
	

		Story
	Elevation
	X-Dir
	Y-Dir

	
	m
	kN
	kN

	Story2
	7.65
	0
	0

	Story1
	5.65
	0
	0

	cubierta
	4
	954.8194
	0

	Base
	0
	0
	0
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User Coefficient Auto Seismic Load Calculation
This calculation presents the automatically generated lateral seismic loads for load pattern FHEy using the user input coefficients, as calculated by ETABS.
Direction and Eccentricity
Direction = Y + Eccentricity X
Eccentricity Ratio = 5% for all diaphragms
Factors and Coefficients
Equivalent Lateral Forces
	Base Shear Coefficient, C
	
	

	Base Shear, V
	
	



Calculated Base Shear
	Direction
	Period Used

 (sec)
	C
	W

 (kN)
	V

 (kN)

	Y + Ecc. X
	0
	0
	964.464
	954.8194




Applied Story Forces
	[image: ]

		Story
	Elevation
	X-Dir
	Y-Dir

	
	m
	kN
	kN

	Story2
	7.65
	0
	0

	Story1
	5.65
	0
	0

	cubierta
	4
	0
	954.8194

	Base
	0
	0
	0
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4.3 Functions
4.3.1 Response Spectrum Functions
Table 4.4 - Functions - Response Spectrum - Columbia NSR-10
	Name
	Period
sec
	Value
	Aa
	Av
	Ae
	Ad
	Group of Use
	Fa
	Fv
	Damping Ratio

	NSR-PER
	0
	0.99
	0.25
	0.25
	0.2
	0.1
	2
	1.44
	2.4
	0.05

	NSR-PER
	0.1
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.2
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.3
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.4
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.5
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.6
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.7
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.8
	0.99
	
	
	
	
	
	
	
	

	NSR-PER
	0.9
	0.88
	
	
	
	
	
	
	
	

	NSR-PER
	1
	0.792
	
	
	
	
	
	
	
	

	NSR-PER
	1.2
	0.66
	
	
	
	
	
	
	
	

	NSR-PER
	1.5
	0.528
	
	
	
	
	
	
	
	

	NSR-PER
	1.7
	0.465882
	
	
	
	
	
	
	
	

	NSR-PER
	2
	0.396
	
	
	
	
	
	
	
	

	NSR-PER
	2.5
	0.3168
	
	
	
	
	
	
	
	

	NSR-PER
	3
	0.264
	
	
	
	
	
	
	
	

	NSR-PER
	3.5
	0.226286
	
	
	
	
	
	
	
	

	NSR-PER
	4
	0.198
	
	
	
	
	
	
	
	

	NSR-PER
	5
	0.1584
	
	
	
	
	
	
	
	

	NSR-PER
	8
	0.07128
	
	
	
	
	
	
	
	

	NSR-PER
	11
	0.037702
	
	
	
	
	
	
	
	

	NSR-PER
	15
	0.020275
	
	
	
	
	
	
	
	



4.3.2 Time History Functions
Table 4.5 - Functions - Time History - User Defined
	Name
	Time
sec
	Value

	RampTH
	0
	0

	RampTH
	1
	1

	RampTH
	4
	1

	UnifTH
	0
	1

	UnifTH
	1
	1



4.4 Load Cases
Table 4.6 - Load Case Definitions - Summary
	Name
	Type
	Notes

	Modal
	Modal - Eigen
	

	Dead
	Linear Static
	

	Live
	Linear Static
	

	FHEx
	Linear Static
	

	FHEy
	Linear Static
	

	Sx
	Response Spectrum
	

	Sy
	Response Spectrum
	



4.5 Load Combinations
Table 4.7 - Load Combination Definitions
	Name
	Type
	Is Auto
	Load Name
	Mode
	SF
	Notes

	Comb1
	Linear Add
	No
	Dead
	
	1.4
	

	Comb2
	Linear Add
	No
	Dead
	
	1.2
	

	Comb2
	
	
	Live
	
	1.6
	

	Comb3
	Linear Add
	No
	Dead
	
	1.2
	

	Comb3
	
	
	Live
	
	1
	

	Comb4
	Linear Add
	No
	Dead
	
	1.2
	

	Comb4
	
	
	Live
	
	1
	

	Comb4
	
	
	Sx
	
	0.142857
	

	Comb5
	Linear Add
	No
	Dead
	
	1.2
	

	Comb5
	
	
	Live
	
	1
	

	Comb5
	
	
	Sy
	
	0.1429
	

	Comb6
	Linear Add
	No
	Dead
	
	0.9
	

	Comb7
	Linear Add
	No
	Dead
	
	0.9
	

	Comb7
	
	
	Sx
	
	0.142857
	

	Comb8
	Linear Add
	No
	Dead
	
	0.9
	

	Comb8
	
	
	Sy
	
	0.1429
	

	ENVDIS
	Envelope
	No
	Comb1
	
	1
	

	ENVDIS
	
	
	Comb2
	
	1
	

	ENVDIS
	
	
	Comb3
	
	1
	

	ENVDIS
	
	
	Comb4
	
	1
	

	ENVDIS
	
	
	Comb5
	
	1
	

	ENVDIS
	
	
	Comb6
	
	1
	

	ENVDIS
	
	
	Comb7
	
	1
	

	ENVDIS
	
	
	Comb8
	
	1
	

	ENVSERV
	Envelope
	No
	Serv1
	
	1
	

	ENVSERV
	
	
	Serv2
	
	1
	

	ENVSERV
	
	
	Serv3
	
	1
	

	ENVSERV
	
	
	Serv4
	
	1
	

	ENVSERV
	
	
	Serv5
	
	1
	

	ENVSERV
	
	
	Serv6
	
	1
	

	ENVSERV
	
	
	Serv7
	
	1
	

	ENVSERV
	
	
	Serv8
	
	1
	

	ENVSERV
	
	
	Serv9
	
	1
	

	ENVSERV
	
	
	Serv10
	
	1
	

	Serv1
	Linear Add
	No
	Dead
	
	1
	

	Serv2
	Linear Add
	No
	Dead
	
	1
	

	Serv2
	
	
	Live
	
	1
	

	Serv3
	Linear Add
	No
	Dead
	
	1
	

	Serv3
	
	
	Live
	
	0.75
	

	Serv4
	Linear Add
	No
	Dead
	
	1
	

	Serv4
	
	
	Sx
	
	0.1
	

	Serv5
	Linear Add
	No
	Dead
	
	1
	

	Serv5
	
	
	Sy
	
	0.1
	

	Serv6
	Linear Add
	No
	Dead
	
	1
	

	Serv6
	
	
	Live
	
	0.75
	

	Serv6
	
	
	Sx
	
	0.075
	

	Serv7
	Linear Add
	No
	Dead
	
	1
	

	Serv7
	
	
	Live
	
	0.75
	

	Serv7
	
	
	Sy
	
	0.075
	

	Serv8
	Linear Add
	No
	Dead
	
	0.6
	

	Serv9
	Linear Add
	No
	Dead
	
	0.6
	

	Serv9
	
	
	Sx
	
	0.1
	

	Serv10
	Linear Add
	No
	Dead
	
	0.6
	

	Serv10
	
	
	Sy
	
	0.1
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5 Analysis Results
This chapter provides analysis results.
5.1 Structure Results
Table 5.1 - Base Reactions
	Output Case
	Case Type
	Step Type
	Step Number
	Step Label
	FX
kN
	FY
kN
	FZ
kN
	MX
kN-m
	MY
kN-m
	MZ
kN-m
	X
m
	Y
m
	Z
m

	Dead
	LinStatic
	
	
	
	0
	2.074E-06
	1610.0697
	17902.3104
	-48728.4038
	0.0001
	0
	0
	0

	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0
	0
	0
	0

	FHEx
	LinStatic
	
	
	
	-954.8177
	-1.679E-06
	0
	6.005E-06
	-3819.2709
	11134.2843
	0
	0
	0

	FHEy
	LinStatic
	
	
	
	-0.0006
	-954.8194
	0
	3819.2774
	-0.0025
	-28870.5278
	0
	0
	0

	Sx
	LinRespSpec
	Max
	
	
	503.6574
	42.0208
	0
	168.0832
	2014.6295
	4797.2071
	0
	0
	0

	Sy
	LinRespSpec
	Max
	
	
	42.0209
	698.2403
	0
	2792.9611
	168.0834
	21464.4118
	0
	0
	0

	Comb1
	Combination
	
	
	
	0
	2.903E-06
	2254.0975
	25063.2346
	-68219.7653
	0.0001
	0
	0
	0

	Comb2
	Combination
	
	
	
	0
	2.488E-06
	1932.0836
	21482.7725
	-58474.0845
	0.0001
	0
	0
	0

	Comb3
	Combination
	
	
	
	0
	2.488E-06
	1932.0836
	21482.7725
	-58474.0845
	0.0001
	0
	0
	0

	Comb4
	Combination
	Max
	
	
	71.951
	6.003
	1932.0836
	21506.7844
	-58186.2804
	685.3152
	0
	0
	0

	Comb4
	Combination
	Min
	
	
	-71.951
	-6.003
	1932.0836
	21458.7606
	-58761.8886
	-685.315
	0
	0
	0

	Comb5
	Combination
	Max
	
	
	6.0048
	99.7785
	1932.0836
	21881.8866
	-58450.0654
	3067.2646
	0
	0
	0

	Comb5
	Combination
	Min
	
	
	-6.0048
	-99.7785
	1932.0836
	21083.6583
	-58498.1036
	-3067.2643
	0
	0
	0

	Comb6
	Combination
	
	
	
	0
	1.866E-06
	1449.0627
	16112.0794
	-43855.5634
	0.0001
	0
	0
	0

	Comb7
	Combination
	Max
	
	
	71.951
	6.003
	1449.0627
	16136.0912
	-43567.7593
	685.3152
	0
	0
	0

	Comb7
	Combination
	Min
	
	
	-71.951
	-6.003
	1449.0627
	16088.0675
	-44143.3675
	-685.315
	0
	0
	0

	Comb8
	Combination
	Max
	
	
	6.0048
	99.7785
	1449.0627
	16511.1935
	-43831.5443
	3067.2645
	0
	0
	0

	Comb8
	Combination
	Min
	
	
	-6.0048
	-99.7785
	1449.0627
	15712.9652
	-43879.5825
	-3067.2644
	0
	0
	0

	ENVDIS
	Combination
	Max
	
	
	71.951
	99.7785
	2254.0975
	25063.2346
	-43567.7593
	3067.2646
	0
	0
	0

	ENVDIS
	Combination
	Min
	
	
	-71.951
	-99.7785
	1449.0627
	15712.9652
	-68219.7653
	-3067.2644
	0
	0
	0

	Serv1
	Combination
	
	
	
	0
	2.074E-06
	1610.0697
	17902.3104
	-48728.4038
	0.0001
	0
	0
	0

	Serv2
	Combination
	
	
	
	0
	2.074E-06
	1610.0697
	17902.3104
	-48728.4038
	0.0001
	0
	0
	0

	Serv3
	Combination
	
	
	
	0
	2.074E-06
	1610.0697
	17902.3104
	-48728.4038
	0.0001
	0
	0
	0

	Serv4
	Combination
	Max
	
	
	50.3657
	4.2021
	1610.0697
	17919.1187
	-48526.9408
	479.7208
	0
	0
	0

	Serv4
	Combination
	Min
	
	
	-50.3657
	-4.2021
	1610.0697
	17885.5021
	-48929.8667
	-479.7206
	0
	0
	0

	Serv5
	Combination
	Max
	
	
	4.2021
	69.824
	1610.0697
	18181.6065
	-48711.5954
	2146.4413
	0
	0
	0

	Serv5
	Combination
	Min
	
	
	-4.2021
	-69.824
	1610.0697
	17623.0143
	-48745.2121
	-2146.4411
	0
	0
	0

	Serv6
	Combination
	Max
	
	
	37.7743
	3.1516
	1610.0697
	17914.9166
	-48577.3066
	359.7906
	0
	0
	0

	Serv6
	Combination
	Min
	
	
	-37.7743
	-3.1516
	1610.0697
	17889.7042
	-48879.501
	-359.7904
	0
	0
	0

	Serv7
	Combination
	Max
	
	
	3.1516
	52.368
	1610.0697
	18111.7825
	-48715.7975
	1609.831
	0
	0
	0

	Serv7
	Combination
	Min
	
	
	-3.1516
	-52.368
	1610.0697
	17692.8383
	-48741.01
	-1609.8308
	0
	0
	0

	Serv8
	Combination
	
	
	
	0
	1.244E-06
	966.0418
	10741.3862
	-29237.0423
	0.0001
	0
	0
	0

	Serv9
	Combination
	Max
	
	
	50.3657
	4.2021
	966.0418
	10758.1946
	-29035.5793
	479.7208
	0
	0
	0

	Serv9
	Combination
	Min
	
	
	-50.3657
	-4.2021
	966.0418
	10724.5779
	-29438.5052
	-479.7206
	0
	0
	0

	Serv10
	Combination
	Max
	
	
	4.2021
	69.824
	966.0418
	11020.6824
	-29220.2339
	2146.4412
	0
	0
	0

	Serv10
	Combination
	Min
	
	
	-4.2021
	-69.824
	966.0418
	10462.0901
	-29253.8506
	-2146.4411
	0
	0
	0

	ENVSERV
	Combination
	Max
	
	
	50.3657
	69.824
	1610.0697
	18181.6065
	-29035.5793
	2146.4413
	0
	0
	0

	ENVSERV
	Combination
	Min
	
	
	-50.3657
	-69.824
	966.0418
	10462.0901
	-48929.8667
	-2146.4411
	0
	0
	0



5.2 Story Results
Table 5.2 - Story Drifts
	Story
	Output Case
	Case Type
	Step Type
	Step Number
	Step Label
	Direction
	Drift
	Drift/
	Label
	X
m
	Y
m
	Z
m

	cubierta
	Dead
	LinStatic
	
	
	
	X
	1.5E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Dead
	LinStatic
	
	
	
	Y
	4.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	FHEx
	LinStatic
	
	
	
	X
	0.000271
	
	78
	23.1409
	37.3713
	4

	cubierta
	FHEy
	LinStatic
	
	
	
	Y
	0.001984
	
	19
	30.3729
	-3.306
	4

	cubierta
	Sx
	LinRespSpec
	Max
	
	
	X
	0.000249
	
	78
	23.1409
	37.3713
	4

	cubierta
	Sx
	LinRespSpec
	Max
	
	
	Y
	9.2E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Sy
	LinRespSpec
	Max
	
	
	Y
	0.002012
	
	19
	30.3729
	-3.306
	4

	cubierta
	Comb1
	Combination
	
	
	
	X
	2.1E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Comb1
	Combination
	
	
	
	Y
	6.4E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb2
	Combination
	
	
	
	X
	1.8E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Comb2
	Combination
	
	
	
	Y
	5.4E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb3
	Combination
	
	
	
	X
	1.8E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Comb3
	Combination
	
	
	
	Y
	5.4E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb4
	Combination
	Max
	
	
	X
	2.2E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb4
	Combination
	Max
	
	
	Y
	6.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb4
	Combination
	Min
	
	
	X
	5.3E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Comb4
	Combination
	Min
	
	
	Y
	4.9E-05
	
	80
	33.2913
	37.3693
	4

	cubierta
	Comb5
	Combination
	Max
	
	
	Y
	0.000294
	
	19
	30.3729
	-3.306
	4

	cubierta
	Comb5
	Combination
	Min
	
	
	Y
	0.000281
	
	19
	30.3729
	-3.306
	4

	cubierta
	Comb6
	Combination
	
	
	
	X
	1.3E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Comb6
	Combination
	
	
	
	Y
	4.1E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb7
	Combination
	Max
	
	
	X
	2.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb7
	Combination
	Max
	
	
	Y
	5.2E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Comb7
	Combination
	Min
	
	
	X
	4.9E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Comb7
	Combination
	Min
	
	
	Y
	3.6E-05
	
	80
	33.2913
	37.3693
	4

	cubierta
	Comb8
	Combination
	Max
	
	
	Y
	0.000292
	
	19
	30.3729
	-3.306
	4

	cubierta
	Comb8
	Combination
	Min
	
	
	Y
	0.000283
	
	19
	30.3729
	-3.306
	4

	cubierta
	ENVDIS
	Combination
	Max
	
	
	Y
	0.000294
	
	19
	30.3729
	-3.306
	4

	cubierta
	ENVDIS
	Combination
	Min
	
	
	X
	5.3E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	ENVDIS
	Combination
	Min
	
	
	Y
	0.000283
	
	19
	30.3729
	-3.306
	4

	cubierta
	Serv1
	Combination
	
	
	
	X
	1.5E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv1
	Combination
	
	
	
	Y
	4.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv2
	Combination
	
	
	
	X
	1.5E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv2
	Combination
	
	
	
	Y
	4.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv3
	Combination
	
	
	
	X
	1.5E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv3
	Combination
	
	
	
	Y
	4.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv4
	Combination
	Max
	
	
	X
	1.4E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv4
	Combination
	Max
	
	
	Y
	5.3E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv4
	Combination
	Min
	
	
	X
	4E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv4
	Combination
	Min
	
	
	Y
	4.1E-05
	
	80
	33.2913
	37.3693
	4

	cubierta
	Serv5
	Combination
	Max
	
	
	Y
	0.000207
	
	19
	30.3729
	-3.306
	4

	cubierta
	Serv5
	Combination
	Min
	
	
	Y
	0.000196
	
	19
	30.3729
	-3.306
	4

	cubierta
	Serv6
	Combination
	Max
	
	
	X
	1.1E-05
	
	58
	0
	1
	4

	cubierta
	Serv6
	Combination
	Max
	
	
	Y
	5.1E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv6
	Combination
	Min
	
	
	X
	3.3E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv6
	Combination
	Min
	
	
	Y
	4.2E-05
	
	80
	33.2913
	37.3693
	4

	cubierta
	Serv7
	Combination
	Max
	
	
	Y
	0.000156
	
	19
	30.3729
	-3.306
	4

	cubierta
	Serv7
	Combination
	Min
	
	
	X
	1.9E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv7
	Combination
	Min
	
	
	Y
	0.000146
	
	19
	30.3729
	-3.306
	4

	cubierta
	Serv8
	Combination
	
	
	
	X
	9E-06
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv8
	Combination
	
	
	
	Y
	2.7E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv9
	Combination
	Max
	
	
	X
	1.8E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv9
	Combination
	Max
	
	
	Y
	3.5E-05
	
	81
	37.7224
	37.3722
	4

	cubierta
	Serv9
	Combination
	Min
	
	
	X
	3.4E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	Serv9
	Combination
	Min
	
	
	Y
	2.4E-05
	
	80
	33.2913
	37.3693
	4

	cubierta
	Serv10
	Combination
	Max
	
	
	Y
	0.000204
	
	19
	30.3729
	-3.306
	4

	cubierta
	Serv10
	Combination
	Min
	
	
	Y
	0.000198
	
	19
	30.3729
	-3.306
	4

	cubierta
	ENVSERV
	Combination
	Max
	
	
	Y
	0.000207
	
	19
	30.3729
	-3.306
	4

	cubierta
	ENVSERV
	Combination
	Min
	
	
	X
	4E-05
	
	78
	23.1409
	37.3713
	4

	cubierta
	ENVSERV
	Combination
	Min
	
	
	Y
	0.000198
	
	19
	30.3729
	-3.306
	4



Table 5.3 - Story Forces
	Story
	Output Case
	Case Type
	Step Type
	Step Number
	Step Label
	Location
	P
kN
	VX
kN
	VY
kN
	T
kN-m
	MX
kN-m
	MY
kN-m

	cubierta
	Dead
	LinStatic
	
	
	
	Top
	318.871
	0
	2.074E-06
	0.0001
	4591.7265
	-9592.2931

	cubierta
	Dead
	LinStatic
	
	
	
	Bottom
	1610.0697
	0
	2.074E-06
	0.0001
	17902.3104
	-48728.4038

	cubierta
	Live
	LinStatic
	
	
	
	Top
	0
	0
	0
	0
	0
	0

	cubierta
	Live
	LinStatic
	
	
	
	Bottom
	0
	0
	0
	0
	0
	0

	cubierta
	FHEx
	LinStatic
	
	
	
	Top
	0
	-954.8177
	-1.679E-06
	11134.2843
	-7.134E-07
	0

	cubierta
	FHEx
	LinStatic
	
	
	
	Bottom
	0
	-954.8177
	-1.679E-06
	11134.2843
	6.005E-06
	-3819.2709

	cubierta
	FHEy
	LinStatic
	
	
	
	Top
	0
	-0.0006
	-954.8194
	-28870.5278
	0
	-2.215E-06

	cubierta
	FHEy
	LinStatic
	
	
	
	Bottom
	0
	-0.0006
	-954.8194
	-28870.5278
	3819.2774
	-0.0025

	cubierta
	Sx
	LinRespSpec
	Max
	
	
	Top
	0
	503.6574
	42.0208
	4797.2071
	0
	8.339E-07

	cubierta
	Sx
	LinRespSpec
	Max
	
	
	Bottom
	0
	503.6574
	42.0208
	4797.2071
	168.0832
	2014.6295

	cubierta
	Sy
	LinRespSpec
	Max
	
	
	Top
	0
	42.0209
	698.2403
	21464.4118
	8.229E-07
	2.113E-06

	cubierta
	Sy
	LinRespSpec
	Max
	
	
	Bottom
	0
	42.0209
	698.2403
	21464.4118
	2792.9611
	168.0834

	cubierta
	Comb1
	Combination
	
	
	
	Top
	446.4194
	0
	2.903E-06
	0.0001
	6428.4172
	-13429.2103

	cubierta
	Comb1
	Combination
	
	
	
	Bottom
	2254.0975
	0
	2.903E-06
	0.0001
	25063.2346
	-68219.7653

	cubierta
	Comb2
	Combination
	
	
	
	Top
	382.6452
	0
	2.488E-06
	0.0001
	5510.0718
	-11510.7517

	cubierta
	Comb2
	Combination
	
	
	
	Bottom
	1932.0836
	0
	2.488E-06
	0.0001
	21482.7725
	-58474.0845

	cubierta
	Comb3
	Combination
	
	
	
	Top
	382.6452
	0
	2.488E-06
	0.0001
	5510.0718
	-11510.7517

	cubierta
	Comb3
	Combination
	
	
	
	Bottom
	1932.0836
	0
	2.488E-06
	0.0001
	21482.7725
	-58474.0845

	cubierta
	Comb4
	Combination
	Max
	
	
	Top
	382.6452
	71.951
	6.003
	685.3152
	5510.0718
	-11510.7517

	cubierta
	Comb4
	Combination
	Max
	
	
	Bottom
	1932.0836
	71.951
	6.003
	685.3152
	21506.7844
	-58186.2804

	cubierta
	Comb4
	Combination
	Min
	
	
	Top
	382.6452
	-71.951
	-6.003
	-685.315
	5510.0718
	-11510.7517

	cubierta
	Comb4
	Combination
	Min
	
	
	Bottom
	1932.0836
	-71.951
	-6.003
	-685.315
	21458.7606
	-58761.8886

	cubierta
	Comb5
	Combination
	Max
	
	
	Top
	382.6452
	6.0048
	99.7785
	3067.2646
	5510.0718
	-11510.7517

	cubierta
	Comb5
	Combination
	Max
	
	
	Bottom
	1932.0836
	6.0048
	99.7785
	3067.2646
	21881.8866
	-58450.0654

	cubierta
	Comb5
	Combination
	Min
	
	
	Top
	382.6452
	-6.0048
	-99.7785
	-3067.2643
	5510.0718
	-11510.7517

	cubierta
	Comb5
	Combination
	Min
	
	
	Bottom
	1932.0836
	-6.0048
	-99.7785
	-3067.2643
	21083.6583
	-58498.1036

	cubierta
	Comb6
	Combination
	
	
	
	Top
	286.9839
	0
	1.866E-06
	0.0001
	4132.5539
	-8633.0638

	cubierta
	Comb6
	Combination
	
	
	
	Bottom
	1449.0627
	0
	1.866E-06
	0.0001
	16112.0794
	-43855.5634

	cubierta
	Comb7
	Combination
	Max
	
	
	Top
	286.9839
	71.951
	6.003
	685.3152
	4132.5539
	-8633.0638

	cubierta
	Comb7
	Combination
	Max
	
	
	Bottom
	1449.0627
	71.951
	6.003
	685.3152
	16136.0912
	-43567.7593

	cubierta
	Comb7
	Combination
	Min
	
	
	Top
	286.9839
	-71.951
	-6.003
	-685.315
	4132.5539
	-8633.0638

	cubierta
	Comb7
	Combination
	Min
	
	
	Bottom
	1449.0627
	-71.951
	-6.003
	-685.315
	16088.0675
	-44143.3675

	cubierta
	Comb8
	Combination
	Max
	
	
	Top
	286.9839
	6.0048
	99.7785
	3067.2645
	4132.5539
	-8633.0638

	cubierta
	Comb8
	Combination
	Max
	
	
	Bottom
	1449.0627
	6.0048
	99.7785
	3067.2645
	16511.1935
	-43831.5443

	cubierta
	Comb8
	Combination
	Min
	
	
	Top
	286.9839
	-6.0048
	-99.7785
	-3067.2644
	4132.5539
	-8633.0638

	cubierta
	Comb8
	Combination
	Min
	
	
	Bottom
	1449.0627
	-6.0048
	-99.7785
	-3067.2644
	15712.9652
	-43879.5825

	cubierta
	ENVDIS
	Combination
	Max
	
	
	Top
	446.4194
	71.951
	99.7785
	3067.2646
	6428.4172
	-8633.0638

	cubierta
	ENVDIS
	Combination
	Max
	
	
	Bottom
	2254.0975
	71.951
	99.7785
	3067.2646
	25063.2346
	-43567.7593

	cubierta
	ENVDIS
	Combination
	Min
	
	
	Top
	286.9839
	-71.951
	-99.7785
	-3067.2644
	4132.5539
	-13429.2103

	cubierta
	ENVDIS
	Combination
	Min
	
	
	Bottom
	1449.0627
	-71.951
	-99.7785
	-3067.2644
	15712.9652
	-68219.7653

	cubierta
	Serv1
	Combination
	
	
	
	Top
	318.871
	0
	2.074E-06
	0.0001
	4591.7265
	-9592.2931

	cubierta
	Serv1
	Combination
	
	
	
	Bottom
	1610.0697
	0
	2.074E-06
	0.0001
	17902.3104
	-48728.4038

	cubierta
	Serv2
	Combination
	
	
	
	Top
	318.871
	0
	2.074E-06
	0.0001
	4591.7265
	-9592.2931

	cubierta
	Serv2
	Combination
	
	
	
	Bottom
	1610.0697
	0
	2.074E-06
	0.0001
	17902.3104
	-48728.4038

	cubierta
	Serv3
	Combination
	
	
	
	Top
	318.871
	0
	2.074E-06
	0.0001
	4591.7265
	-9592.2931

	cubierta
	Serv3
	Combination
	
	
	
	Bottom
	1610.0697
	0
	2.074E-06
	0.0001
	17902.3104
	-48728.4038

	cubierta
	Serv4
	Combination
	Max
	
	
	Top
	318.871
	50.3657
	4.2021
	479.7208
	4591.7265
	-9592.2931

	cubierta
	Serv4
	Combination
	Max
	
	
	Bottom
	1610.0697
	50.3657
	4.2021
	479.7208
	17919.1187
	-48526.9408

	cubierta
	Serv4
	Combination
	Min
	
	
	Top
	318.871
	-50.3657
	-4.2021
	-479.7206
	4591.7265
	-9592.2931

	cubierta
	Serv4
	Combination
	Min
	
	
	Bottom
	1610.0697
	-50.3657
	-4.2021
	-479.7206
	17885.5021
	-48929.8667

	cubierta
	Serv5
	Combination
	Max
	
	
	Top
	318.871
	4.2021
	69.824
	2146.4413
	4591.7265
	-9592.2931

	cubierta
	Serv5
	Combination
	Max
	
	
	Bottom
	1610.0697
	4.2021
	69.824
	2146.4413
	18181.6065
	-48711.5954

	cubierta
	Serv5
	Combination
	Min
	
	
	Top
	318.871
	-4.2021
	-69.824
	-2146.4411
	4591.7265
	-9592.2931

	cubierta
	Serv5
	Combination
	Min
	
	
	Bottom
	1610.0697
	-4.2021
	-69.824
	-2146.4411
	17623.0143
	-48745.2121

	cubierta
	Serv6
	Combination
	Max
	
	
	Top
	318.871
	37.7743
	3.1516
	359.7906
	4591.7265
	-9592.2931

	cubierta
	Serv6
	Combination
	Max
	
	
	Bottom
	1610.0697
	37.7743
	3.1516
	359.7906
	17914.9166
	-48577.3066

	cubierta
	Serv6
	Combination
	Min
	
	
	Top
	318.871
	-37.7743
	-3.1516
	-359.7904
	4591.7265
	-9592.2931

	cubierta
	Serv6
	Combination
	Min
	
	
	Bottom
	1610.0697
	-37.7743
	-3.1516
	-359.7904
	17889.7042
	-48879.501

	cubierta
	Serv7
	Combination
	Max
	
	
	Top
	318.871
	3.1516
	52.368
	1609.831
	4591.7265
	-9592.2931

	cubierta
	Serv7
	Combination
	Max
	
	
	Bottom
	1610.0697
	3.1516
	52.368
	1609.831
	18111.7825
	-48715.7975

	cubierta
	Serv7
	Combination
	Min
	
	
	Top
	318.871
	-3.1516
	-52.368
	-1609.8308
	4591.7265
	-9592.2931

	cubierta
	Serv7
	Combination
	Min
	
	
	Bottom
	1610.0697
	-3.1516
	-52.368
	-1609.8308
	17692.8383
	-48741.01

	cubierta
	Serv8
	Combination
	
	
	
	Top
	191.3226
	0
	1.244E-06
	0.0001
	2755.0359
	-5755.3758

	cubierta
	Serv8
	Combination
	
	
	
	Bottom
	966.0418
	0
	1.244E-06
	0.0001
	10741.3862
	-29237.0423

	cubierta
	Serv9
	Combination
	Max
	
	
	Top
	191.3226
	50.3657
	4.2021
	479.7208
	2755.0359
	-5755.3758

	cubierta
	Serv9
	Combination
	Max
	
	
	Bottom
	966.0418
	50.3657
	4.2021
	479.7208
	10758.1946
	-29035.5793

	cubierta
	Serv9
	Combination
	Min
	
	
	Top
	191.3226
	-50.3657
	-4.2021
	-479.7206
	2755.0359
	-5755.3758

	cubierta
	Serv9
	Combination
	Min
	
	
	Bottom
	966.0418
	-50.3657
	-4.2021
	-479.7206
	10724.5779
	-29438.5052

	cubierta
	Serv10
	Combination
	Max
	
	
	Top
	191.3226
	4.2021
	69.824
	2146.4412
	2755.0359
	-5755.3758

	cubierta
	Serv10
	Combination
	Max
	
	
	Bottom
	966.0418
	4.2021
	69.824
	2146.4412
	11020.6824
	-29220.2339

	cubierta
	Serv10
	Combination
	Min
	
	
	Top
	191.3226
	-4.2021
	-69.824
	-2146.4411
	2755.0359
	-5755.3758

	cubierta
	Serv10
	Combination
	Min
	
	
	Bottom
	966.0418
	-4.2021
	-69.824
	-2146.4411
	10462.0901
	-29253.8506

	cubierta
	ENVSERV
	Combination
	Max
	
	
	Top
	318.871
	50.3657
	69.824
	2146.4413
	4591.7265
	-5755.3758

	cubierta
	ENVSERV
	Combination
	Max
	
	
	Bottom
	1610.0697
	50.3657
	69.824
	2146.4413
	18181.6065
	-29035.5793

	cubierta
	ENVSERV
	Combination
	Min
	
	
	Top
	191.3226
	-50.3657
	-69.824
	-2146.4411
	2755.0359
	-9592.2931

	cubierta
	ENVSERV
	Combination
	Min
	
	
	Bottom
	966.0418
	-50.3657
	-69.824
	-2146.4411
	10462.0901
	-48929.8667



5.3 Point Results
Table 5.4 - Joint Reactions
	Story
	Label
	Unique Name
	Output Case
	Case Type
	Step Type
	Step Number
	Step Label
	FX
kN
	FY
kN
	FZ
kN
	MX
kN-m
	MY
kN-m
	MZ
kN-m

	Base
	1
	131
	Dead
	LinStatic
	
	
	
	1.5875
	1.3377
	10.9673
	0.0663
	-0.0835
	0.0055

	Base
	1
	131
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	1
	131
	FHEx
	LinStatic
	
	
	
	-4.0392
	-1.9613
	-20.7898
	-0.3213
	-1.9467
	0.5658

	Base
	1
	131
	FHEy
	LinStatic
	
	
	
	-8.6041
	-5.2979
	-55.17
	2.1468
	-2.1168
	-0.3039

	Base
	1
	131
	Sx
	LinRespSpec
	Max
	
	
	4.7438
	1.8444
	22.0568
	0.4457
	1.9092
	1.1356

	Base
	1
	131
	Sy
	LinRespSpec
	Max
	
	
	8.8051
	5.078
	47.6803
	1.2844
	2.5273
	0.6346

	Base
	1
	131
	Comb1
	Combination
	
	
	
	2.2225
	1.8727
	15.3542
	0.0928
	-0.1169
	0.0078

	Base
	1
	131
	Comb2
	Combination
	
	
	
	1.905
	1.6052
	13.1607
	0.0795
	-0.1002
	0.0067

	Base
	1
	131
	Comb3
	Combination
	
	
	
	1.905
	1.6052
	13.1607
	0.0795
	-0.1002
	0.0067

	Base
	1
	131
	Comb4
	Combination
	Max
	
	
	2.5827
	1.8687
	16.3117
	0.1432
	0.1725
	0.1689

	Base
	1
	131
	Comb4
	Combination
	Min
	
	
	1.2273
	1.3417
	10.0098
	0.0158
	-0.373
	-0.1556

	Base
	1
	131
	Comb5
	Combination
	Max
	
	
	3.1633
	2.3309
	19.9742
	0.263
	0.2609
	0.0973

	Base
	1
	131
	Comb5
	Combination
	Min
	
	
	0.6468
	0.8796
	6.3472
	-0.104
	-0.4614
	-0.084

	Base
	1
	131
	Comb6
	Combination
	
	
	
	1.4288
	1.2039
	9.8705
	0.0596
	-0.0752
	0.005

	Base
	1
	131
	Comb7
	Combination
	Max
	
	
	2.1064
	1.4674
	13.0215
	0.1233
	0.1976
	0.1672

	Base
	1
	131
	Comb7
	Combination
	Min
	
	
	0.7511
	0.9404
	6.7196
	-0.004
	-0.3479
	-0.1572

	Base
	1
	131
	Comb8
	Combination
	Max
	
	
	2.687
	1.9295
	16.6841
	0.2432
	0.286
	0.0957

	Base
	1
	131
	Comb8
	Combination
	Min
	
	
	0.1705
	0.4783
	3.057
	-0.1239
	-0.4363
	-0.0857

	Base
	1
	131
	ENVDIS
	Combination
	Max
	
	
	3.1633
	2.3309
	19.9742
	0.263
	0.286
	0.1689

	Base
	1
	131
	ENVDIS
	Combination
	Min
	
	
	0.1705
	0.4783
	3.057
	-0.1239
	-0.4614
	-0.1572

	Base
	1
	131
	Serv1
	Combination
	
	
	
	1.5875
	1.3377
	10.9673
	0.0663
	-0.0835
	0.0055

	Base
	1
	131
	Serv2
	Combination
	
	
	
	1.5875
	1.3377
	10.9673
	0.0663
	-0.0835
	0.0055

	Base
	1
	131
	Serv3
	Combination
	
	
	
	1.5875
	1.3377
	10.9673
	0.0663
	-0.0835
	0.0055

	Base
	1
	131
	Serv4
	Combination
	Max
	
	
	2.0619
	1.5221
	13.1729
	0.1108
	0.1074
	0.1191

	Base
	1
	131
	Serv4
	Combination
	Min
	
	
	1.1131
	1.1532
	8.7616
	0.0217
	-0.2745
	-0.108

	Base
	1
	131
	Serv5
	Combination
	Max
	
	
	2.468
	1.8455
	15.7353
	0.1947
	0.1692
	0.069

	Base
	1
	131
	Serv5
	Combination
	Min
	
	
	0.707
	0.8299
	6.1992
	-0.0622
	-0.3363
	-0.0579

	Base
	1
	131
	Serv6
	Combination
	Max
	
	
	1.9433
	1.476
	12.6215
	0.0997
	0.0597
	0.0907

	Base
	1
	131
	Serv6
	Combination
	Min
	
	
	1.2317
	1.1993
	9.313
	0.0328
	-0.2267
	-0.0796

	Base
	1
	131
	Serv7
	Combination
	Max
	
	
	2.2479
	1.7185
	14.5433
	0.1626
	0.106
	0.0531

	Base
	1
	131
	Serv7
	Combination
	Min
	
	
	0.9271
	0.9568
	7.3912
	-0.0301
	-0.2731
	-0.0421

	Base
	1
	131
	Serv8
	Combination
	
	
	
	0.9525
	0.8026
	6.5804
	0.0398
	-0.0501
	0.0033

	Base
	1
	131
	Serv9
	Combination
	Max
	
	
	1.4269
	0.987
	8.786
	0.0843
	0.1408
	0.1169

	Base
	1
	131
	Serv9
	Combination
	Min
	
	
	0.4781
	0.6182
	4.3747
	-0.0048
	-0.241
	-0.1102

	Base
	1
	131
	Serv10
	Combination
	Max
	
	
	1.833
	1.3104
	11.3484
	0.1682
	0.2026
	0.0668

	Base
	1
	131
	Serv10
	Combination
	Min
	
	
	0.072
	0.2948
	1.8123
	-0.0887
	-0.3029
	-0.0601

	Base
	1
	131
	ENVSERV
	Combination
	Max
	
	
	2.468
	1.8455
	15.7353
	0.1947
	0.2026
	0.1191

	Base
	1
	131
	ENVSERV
	Combination
	Min
	
	
	0.072
	0.2948
	1.8123
	-0.0887
	-0.3363
	-0.1102

	Base
	78
	7
	Dead
	LinStatic
	
	
	
	-6.3813
	3.9709
	12.5588
	-5.1429
	-8.3684
	-0.0029

	Base
	78
	7
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	78
	7
	FHEx
	LinStatic
	
	
	
	-0.3526
	-0.1674
	0.0229
	0.4244
	-1.1354
	0.0361

	Base
	78
	7
	FHEy
	LinStatic
	
	
	
	-0.0853
	-0.9124
	0.5528
	2.3802
	-0.1086
	0.002

	Base
	78
	7
	Sx
	LinRespSpec
	Max
	
	
	0.327
	0.1851
	0.0413
	0.4706
	1.0453
	0.037

	Base
	78
	7
	Sy
	LinRespSpec
	Max
	
	
	0.0994
	0.9273
	0.5639
	2.4193
	0.2222
	0.0077

	Base
	78
	7
	Comb1
	Combination
	
	
	
	-8.9338
	5.5593
	17.5823
	-7.2001
	-11.7157
	-0.0041

	Base
	78
	7
	Comb2
	Combination
	
	
	
	-7.6575
	4.7651
	15.0706
	-6.1715
	-10.042
	-0.0035

	Base
	78
	7
	Comb3
	Combination
	
	
	
	-7.6575
	4.7651
	15.0706
	-6.1715
	-10.042
	-0.0035

	Base
	78
	7
	Comb4
	Combination
	Max
	
	
	-7.6108
	4.7915
	15.0765
	-6.1043
	-9.8927
	0.0018

	Base
	78
	7
	Comb4
	Combination
	Min
	
	
	-7.7042
	4.7386
	15.0647
	-6.2387
	-10.1914
	-0.0088

	Base
	78
	7
	Comb5
	Combination
	Max
	
	
	-7.6433
	4.8976
	15.1512
	-5.8258
	-10.0103
	-0.0024

	Base
	78
	7
	Comb5
	Combination
	Min
	
	
	-7.6717
	4.6326
	14.99
	-6.5172
	-10.0738
	-0.0046

	Base
	78
	7
	Comb6
	Combination
	
	
	
	-5.7431
	3.5738
	11.3029
	-4.6286
	-7.5315
	-0.0026

	Base
	78
	7
	Comb7
	Combination
	Max
	
	
	-5.6964
	3.6002
	11.3088
	-4.5614
	-7.3822
	0.0027

	Base
	78
	7
	Comb7
	Combination
	Min
	
	
	-5.7899
	3.5474
	11.297
	-4.6959
	-7.6809
	-0.0079

	Base
	78
	7
	Comb8
	Combination
	Max
	
	
	-5.7289
	3.7063
	11.3835
	-4.2829
	-7.4998
	-0.0015

	Base
	78
	7
	Comb8
	Combination
	Min
	
	
	-5.7574
	3.4413
	11.2224
	-4.9744
	-7.5633
	-0.0037

	Base
	78
	7
	ENVDIS
	Combination
	Max
	
	
	-5.6964
	5.5593
	17.5823
	-4.2829
	-7.3822
	0.0027

	Base
	78
	7
	ENVDIS
	Combination
	Min
	
	
	-8.9338
	3.4413
	11.2224
	-7.2001
	-11.7157
	-0.0088

	Base
	78
	7
	Serv1
	Combination
	
	
	
	-6.3813
	3.9709
	12.5588
	-5.1429
	-8.3684
	-0.0029

	Base
	78
	7
	Serv2
	Combination
	
	
	
	-6.3813
	3.9709
	12.5588
	-5.1429
	-8.3684
	-0.0029

	Base
	78
	7
	Serv3
	Combination
	
	
	
	-6.3813
	3.9709
	12.5588
	-5.1429
	-8.3684
	-0.0029

	Base
	78
	7
	Serv4
	Combination
	Max
	
	
	-6.3486
	3.9894
	12.5629
	-5.0959
	-8.2638
	0.0008

	Base
	78
	7
	Serv4
	Combination
	Min
	
	
	-6.414
	3.9524
	12.5547
	-5.19
	-8.4729
	-0.0066

	Base
	78
	7
	Serv5
	Combination
	Max
	
	
	-6.3713
	4.0636
	12.6152
	-4.901
	-8.3461
	-0.0021

	Base
	78
	7
	Serv5
	Combination
	Min
	
	
	-6.3912
	3.8782
	12.5024
	-5.3849
	-8.3906
	-0.0037

	Base
	78
	7
	Serv6
	Combination
	Max
	
	
	-6.3567
	3.9848
	12.5619
	-5.1076
	-8.29
	-0.0001

	Base
	78
	7
	Serv6
	Combination
	Min
	
	
	-6.4058
	3.957
	12.5557
	-5.1782
	-8.4468
	-0.0057

	Base
	78
	7
	Serv7
	Combination
	Max
	
	
	-6.3738
	4.0404
	12.6011
	-4.9615
	-8.3517
	-0.0023

	Base
	78
	7
	Serv7
	Combination
	Min
	
	
	-6.3887
	3.9013
	12.5165
	-5.3244
	-8.385
	-0.0035

	Base
	78
	7
	Serv8
	Combination
	
	
	
	-3.8288
	2.3825
	7.5353
	-3.0858
	-5.021
	-0.0017

	Base
	78
	7
	Serv9
	Combination
	Max
	
	
	-3.7961
	2.401
	7.5394
	-3.0387
	-4.9165
	0.002

	Base
	78
	7
	Serv9
	Combination
	Min
	
	
	-3.8615
	2.364
	7.5312
	-3.1328
	-5.1255
	-0.0054

	Base
	78
	7
	Serv10
	Combination
	Max
	
	
	-3.8188
	2.4753
	7.5917
	-2.8438
	-4.9988
	-0.001

	Base
	78
	7
	Serv10
	Combination
	Min
	
	
	-3.8387
	2.2898
	7.4789
	-3.3277
	-5.0432
	-0.0025

	Base
	78
	7
	ENVSERV
	Combination
	Max
	
	
	-3.7961
	4.0636
	12.6152
	-2.8438
	-4.9165
	0.002

	Base
	78
	7
	ENVSERV
	Combination
	Min
	
	
	-6.414
	2.2898
	7.4789
	-5.3849
	-8.4729
	-0.0066

	Base
	79
	6
	Dead
	LinStatic
	
	
	
	0.0714
	12.0592
	15.8444
	-15.7836
	0.1268
	-0.0023

	Base
	79
	6
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	79
	6
	FHEx
	LinStatic
	
	
	
	-0.3831
	-0.0874
	0.0185
	0.1982
	-1.1735
	0.0329

	Base
	79
	6
	FHEy
	LinStatic
	
	
	
	0.0056
	-0.8294
	0.4125
	2.2584
	0.0102
	0.0014

	Base
	79
	6
	Sx
	LinRespSpec
	Max
	
	
	0.3518
	0.0966
	0.0247
	0.2264
	1.0769
	0.035

	Base
	79
	6
	Sy
	LinRespSpec
	Max
	
	
	0.0736
	0.8429
	0.42
	2.2966
	0.2235
	0.0072

	Base
	79
	6
	Comb1
	Combination
	
	
	
	0.1
	16.8829
	22.1822
	-22.097
	0.1775
	-0.0032

	Base
	79
	6
	Comb2
	Combination
	
	
	
	0.0857
	14.4711
	19.0133
	-18.9403
	0.1522
	-0.0028

	Base
	79
	6
	Comb3
	Combination
	
	
	
	0.0857
	14.4711
	19.0133
	-18.9403
	0.1522
	-0.0028

	Base
	79
	6
	Comb4
	Combination
	Max
	
	
	0.136
	14.4849
	19.0168
	-18.9079
	0.306
	0.0022

	Base
	79
	6
	Comb4
	Combination
	Min
	
	
	0.0354
	14.4573
	19.0098
	-18.9726
	-0.0017
	-0.0078

	Base
	79
	6
	Comb5
	Combination
	Max
	
	
	0.0962
	14.5915
	19.0733
	-18.6121
	0.1841
	-0.0017

	Base
	79
	6
	Comb5
	Combination
	Min
	
	
	0.0752
	14.3506
	18.9533
	-19.2685
	0.1202
	-0.0038

	Base
	79
	6
	Comb6
	Combination
	
	
	
	0.0643
	10.8533
	14.26
	-14.2052
	0.1141
	-0.0021

	Base
	79
	6
	Comb7
	Combination
	Max
	
	
	0.1145
	10.8671
	14.2635
	-14.1729
	0.268
	0.0029

	Base
	79
	6
	Comb7
	Combination
	Min
	
	
	0.014
	10.8395
	14.2564
	-14.2376
	-0.0397
	-0.0071

	Base
	79
	6
	Comb8
	Combination
	Max
	
	
	0.0748
	10.9738
	14.32
	-13.877
	0.1461
	-0.001

	Base
	79
	6
	Comb8
	Combination
	Min
	
	
	0.0538
	10.7328
	14.1999
	-14.5334
	0.0822
	-0.0031

	Base
	79
	6
	ENVDIS
	Combination
	Max
	
	
	0.136
	16.8829
	22.1822
	-13.877
	0.306
	0.0029

	Base
	79
	6
	ENVDIS
	Combination
	Min
	
	
	0.014
	10.7328
	14.1999
	-22.097
	-0.0397
	-0.0078

	Base
	79
	6
	Serv1
	Combination
	
	
	
	0.0714
	12.0592
	15.8444
	-15.7836
	0.1268
	-0.0023

	Base
	79
	6
	Serv2
	Combination
	
	
	
	0.0714
	12.0592
	15.8444
	-15.7836
	0.1268
	-0.0023

	Base
	79
	6
	Serv3
	Combination
	
	
	
	0.0714
	12.0592
	15.8444
	-15.7836
	0.1268
	-0.0023

	Base
	79
	6
	Serv4
	Combination
	Max
	
	
	0.1066
	12.0689
	15.8469
	-15.7609
	0.2345
	0.0012

	Base
	79
	6
	Serv4
	Combination
	Min
	
	
	0.0362
	12.0496
	15.8419
	-15.8062
	0.0191
	-0.0058

	Base
	79
	6
	Serv5
	Combination
	Max
	
	
	0.0788
	12.1435
	15.8864
	-15.5539
	0.1491
	-0.0016

	Base
	79
	6
	Serv5
	Combination
	Min
	
	
	0.0641
	11.9749
	15.8024
	-16.0132
	0.1044
	-0.003

	Base
	79
	6
	Serv6
	Combination
	Max
	
	
	0.0978
	12.0665
	15.8463
	-15.7666
	0.2076
	0.0003

	Base
	79
	6
	Serv6
	Combination
	Min
	
	
	0.045
	12.052
	15.8425
	-15.8006
	0.046
	-0.0049

	Base
	79
	6
	Serv7
	Combination
	Max
	
	
	0.0769
	12.1224
	15.8759
	-15.6113
	0.1436
	-0.0018

	Base
	79
	6
	Serv7
	Combination
	Min
	
	
	0.0659
	11.996
	15.8129
	-15.9558
	0.11
	-0.0028

	Base
	79
	6
	Serv8
	Combination
	
	
	
	0.0429
	7.2355
	9.5066
	-9.4701
	0.0761
	-0.0014

	Base
	79
	6
	Serv9
	Combination
	Max
	
	
	0.078
	7.2452
	9.5091
	-9.4475
	0.1838
	0.0021

	Base
	79
	6
	Serv9
	Combination
	Min
	
	
	0.0077
	7.2259
	9.5042
	-9.4928
	-0.0316
	-0.0049

	Base
	79
	6
	Serv10
	Combination
	Max
	
	
	0.0502
	7.3198
	9.5486
	-9.2405
	0.0984
	-0.0007

	Base
	79
	6
	Serv10
	Combination
	Min
	
	
	0.0355
	7.1512
	9.4646
	-9.6998
	0.0537
	-0.0021

	Base
	79
	6
	ENVSERV
	Combination
	Max
	
	
	0.1066
	12.1435
	15.8864
	-9.2405
	0.2345
	0.0021

	Base
	79
	6
	ENVSERV
	Combination
	Min
	
	
	0.0077
	7.1512
	9.4646
	-16.0132
	-0.0316
	-0.0058

	Base
	80
	5
	Dead
	LinStatic
	
	
	
	-0.2243
	11.2101
	14.6007
	-14.6568
	-0.2651
	-0.0017

	Base
	80
	5
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	80
	5
	FHEx
	LinStatic
	
	
	
	-0.3834
	0.0629
	-0.0278
	-0.1466
	-1.1733
	0.0328

	Base
	80
	5
	FHEy
	LinStatic
	
	
	
	0.0005
	-0.8207
	0.4299
	2.2463
	0.0008
	-0.0006

	Base
	80
	5
	Sx
	LinRespSpec
	Max
	
	
	0.3523
	0.0608
	0.0267
	0.1434
	1.077
	0.0339

	Base
	80
	5
	Sy
	LinRespSpec
	Max
	
	
	0.0724
	0.8395
	0.4396
	2.2969
	0.2213
	0.0071

	Base
	80
	5
	Comb1
	Combination
	
	
	
	-0.3141
	15.6941
	20.441
	-20.5195
	-0.3711
	-0.0024

	Base
	80
	5
	Comb2
	Combination
	
	
	
	-0.2692
	13.4521
	17.5208
	-17.5881
	-0.3181
	-0.002

	Base
	80
	5
	Comb3
	Combination
	
	
	
	-0.2692
	13.4521
	17.5208
	-17.5881
	-0.3181
	-0.002

	Base
	80
	5
	Comb4
	Combination
	Max
	
	
	-0.2189
	13.4608
	17.5247
	-17.5677
	-0.1643
	0.0028

	Base
	80
	5
	Comb4
	Combination
	Min
	
	
	-0.3195
	13.4434
	17.517
	-17.6086
	-0.472
	-0.0069

	Base
	80
	5
	Comb5
	Combination
	Max
	
	
	-0.2589
	13.5721
	17.5837
	-17.2599
	-0.2865
	-0.001

	Base
	80
	5
	Comb5
	Combination
	Min
	
	
	-0.2796
	13.3322
	17.458
	-17.9164
	-0.3497
	-0.003

	Base
	80
	5
	Comb6
	Combination
	
	
	
	-0.2019
	10.0891
	13.1406
	-13.1911
	-0.2386
	-0.0015

	Base
	80
	5
	Comb7
	Combination
	Max
	
	
	-0.1516
	10.0978
	13.1444
	-13.1706
	-0.0847
	0.0033

	Base
	80
	5
	Comb7
	Combination
	Min
	
	
	-0.2522
	10.0804
	13.1368
	-13.2116
	-0.3924
	-0.0064

	Base
	80
	5
	Comb8
	Combination
	Max
	
	
	-0.1916
	10.2091
	13.2034
	-12.8629
	-0.207
	-0.0005

	Base
	80
	5
	Comb8
	Combination
	Min
	
	
	-0.2123
	9.9691
	13.0778
	-13.5193
	-0.2702
	-0.0025

	Base
	80
	5
	ENVDIS
	Combination
	Max
	
	
	-0.1516
	15.6941
	20.441
	-12.8629
	-0.0847
	0.0033

	Base
	80
	5
	ENVDIS
	Combination
	Min
	
	
	-0.3195
	9.9691
	13.0778
	-20.5195
	-0.472
	-0.0069

	Base
	80
	5
	Serv1
	Combination
	
	
	
	-0.2243
	11.2101
	14.6007
	-14.6568
	-0.2651
	-0.0017

	Base
	80
	5
	Serv2
	Combination
	
	
	
	-0.2243
	11.2101
	14.6007
	-14.6568
	-0.2651
	-0.0017

	Base
	80
	5
	Serv3
	Combination
	
	
	
	-0.2243
	11.2101
	14.6007
	-14.6568
	-0.2651
	-0.0017

	Base
	80
	5
	Serv4
	Combination
	Max
	
	
	-0.1891
	11.2162
	14.6034
	-14.6424
	-0.1574
	0.0017

	Base
	80
	5
	Serv4
	Combination
	Min
	
	
	-0.2596
	11.204
	14.598
	-14.6711
	-0.3728
	-0.0051

	Base
	80
	5
	Serv5
	Combination
	Max
	
	
	-0.2171
	11.294
	14.6447
	-14.4271
	-0.243
	-0.001

	Base
	80
	5
	Serv5
	Combination
	Min
	
	
	-0.2316
	11.1262
	14.5567
	-14.8865
	-0.2872
	-0.0024

	Base
	80
	5
	Serv6
	Combination
	Max
	
	
	-0.1979
	11.2147
	14.6027
	-14.646
	-0.1843
	0.0008

	Base
	80
	5
	Serv6
	Combination
	Min
	
	
	-0.2508
	11.2055
	14.5987
	-14.6675
	-0.3459
	-0.0042

	Base
	80
	5
	Serv7
	Combination
	Max
	
	
	-0.2189
	11.2731
	14.6337
	-14.4845
	-0.2485
	-0.0012

	Base
	80
	5
	Serv7
	Combination
	Min
	
	
	-0.2298
	11.1471
	14.5677
	-14.8291
	-0.2817
	-0.0022

	Base
	80
	5
	Serv8
	Combination
	
	
	
	-0.1346
	6.7261
	8.7604
	-8.7941
	-0.1591
	-0.001

	Base
	80
	5
	Serv9
	Combination
	Max
	
	
	-0.0994
	6.7321
	8.7631
	-8.7797
	-0.0514
	0.0024

	Base
	80
	5
	Serv9
	Combination
	Min
	
	
	-0.1698
	6.72
	8.7577
	-8.8084
	-0.2667
	-0.0044

	Base
	80
	5
	Serv10
	Combination
	Max
	
	
	-0.1274
	6.81
	8.8044
	-8.5644
	-0.1369
	-0.0003

	Base
	80
	5
	Serv10
	Combination
	Min
	
	
	-0.1419
	6.6421
	8.7165
	-9.0238
	-0.1812
	-0.0017

	Base
	80
	5
	ENVSERV
	Combination
	Max
	
	
	-0.0994
	11.294
	14.6447
	-8.5644
	-0.0514
	0.0024

	Base
	80
	5
	ENVSERV
	Combination
	Min
	
	
	-0.2596
	6.6421
	8.7165
	-14.8865
	-0.3728
	-0.0051

	Base
	81
	4
	Dead
	LinStatic
	
	
	
	4.7723
	8.1609
	12.6157
	-10.6365
	6.3132
	-0.0009

	Base
	81
	4
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	81
	4
	FHEx
	LinStatic
	
	
	
	-0.3323
	0.1379
	0.0264
	-0.3664
	-1.1062
	0.0363

	Base
	81
	4
	FHEy
	LinStatic
	
	
	
	0.0039
	-0.8161
	0.4353
	2.2509
	0.0041
	-0.0028

	Base
	81
	4
	Sx
	LinRespSpec
	Max
	
	
	0.305
	0.1404
	0.0201
	0.3738
	1.0144
	0.0379

	Base
	81
	4
	Sy
	LinRespSpec
	Max
	
	
	0.0635
	0.8396
	0.4438
	2.315
	0.209
	0.0091

	Base
	81
	4
	Comb1
	Combination
	
	
	
	6.6812
	11.4252
	17.6619
	-14.8911
	8.8384
	-0.0012

	Base
	81
	4
	Comb2
	Combination
	
	
	
	5.7268
	9.793
	15.1388
	-12.7638
	7.5758
	-0.0011

	Base
	81
	4
	Comb3
	Combination
	
	
	
	5.7268
	9.793
	15.1388
	-12.7638
	7.5758
	-0.0011

	Base
	81
	4
	Comb4
	Combination
	Max
	
	
	5.7703
	9.8131
	15.1417
	-12.7104
	7.7207
	0.0044

	Base
	81
	4
	Comb4
	Combination
	Min
	
	
	5.6832
	9.773
	15.1359
	-12.8172
	7.4309
	-0.0065

	Base
	81
	4
	Comb5
	Combination
	Max
	
	
	5.7358
	9.913
	15.2022
	-12.433
	7.6057
	0.0002

	Base
	81
	4
	Comb5
	Combination
	Min
	
	
	5.7177
	9.673
	15.0754
	-13.0946
	7.5459
	-0.0024

	Base
	81
	4
	Comb6
	Combination
	
	
	
	4.2951
	7.3448
	11.3541
	-9.5729
	5.6818
	-0.0008

	Base
	81
	4
	Comb7
	Combination
	Max
	
	
	4.3387
	7.3648
	11.357
	-9.5195
	5.8267
	0.0046

	Base
	81
	4
	Comb7
	Combination
	Min
	
	
	4.2515
	7.3247
	11.3512
	-9.6263
	5.5369
	-0.0062

	Base
	81
	4
	Comb8
	Combination
	Max
	
	
	4.3041
	7.4647
	11.4175
	-9.242
	5.7117
	0.0005

	Base
	81
	4
	Comb8
	Combination
	Min
	
	
	4.286
	7.2248
	11.2907
	-9.9037
	5.652
	-0.0021

	Base
	81
	4
	ENVDIS
	Combination
	Max
	
	
	6.6812
	11.4252
	17.6619
	-9.242
	8.8384
	0.0046

	Base
	81
	4
	ENVDIS
	Combination
	Min
	
	
	4.2515
	7.2248
	11.2907
	-14.8911
	5.5369
	-0.0065

	Base
	81
	4
	Serv1
	Combination
	
	
	
	4.7723
	8.1609
	12.6157
	-10.6365
	6.3132
	-0.0009

	Base
	81
	4
	Serv2
	Combination
	
	
	
	4.7723
	8.1609
	12.6157
	-10.6365
	6.3132
	-0.0009

	Base
	81
	4
	Serv3
	Combination
	
	
	
	4.7723
	8.1609
	12.6157
	-10.6365
	6.3132
	-0.0009

	Base
	81
	4
	Serv4
	Combination
	Max
	
	
	4.8028
	8.1749
	12.6177
	-10.5991
	6.4146
	0.0029

	Base
	81
	4
	Serv4
	Combination
	Min
	
	
	4.7418
	8.1468
	12.6137
	-10.6739
	6.2117
	-0.0047

	Base
	81
	4
	Serv5
	Combination
	Max
	
	
	4.7787
	8.2448
	12.66
	-10.405
	6.3341
	2.972E-05

	Base
	81
	4
	Serv5
	Combination
	Min
	
	
	4.766
	8.0769
	12.5713
	-10.868
	6.2922
	-0.0018

	Base
	81
	4
	Serv6
	Combination
	Max
	
	
	4.7952
	8.1714
	12.6172
	-10.6085
	6.3892
	0.002

	Base
	81
	4
	Serv6
	Combination
	Min
	
	
	4.7494
	8.1503
	12.6142
	-10.6646
	6.2371
	-0.0037

	Base
	81
	4
	Serv7
	Combination
	Max
	
	
	4.7771
	8.2238
	12.649
	-10.4629
	6.3288
	-0.0002

	Base
	81
	4
	Serv7
	Combination
	Min
	
	
	4.7675
	8.0979
	12.5824
	-10.8101
	6.2975
	-0.0016

	Base
	81
	4
	Serv8
	Combination
	
	
	
	2.8634
	4.8965
	7.5694
	-6.3819
	3.7879
	-0.0005

	Base
	81
	4
	Serv9
	Combination
	Max
	
	
	2.8939
	4.9106
	7.5714
	-6.3445
	3.8893
	0.0033

	Base
	81
	4
	Serv9
	Combination
	Min
	
	
	2.8329
	4.8825
	7.5674
	-6.4193
	3.6865
	-0.0043

	Base
	81
	4
	Serv10
	Combination
	Max
	
	
	2.8697
	4.9805
	7.6138
	-6.1504
	3.8088
	0.0004

	Base
	81
	4
	Serv10
	Combination
	Min
	
	
	2.857
	4.8125
	7.525
	-6.6134
	3.767
	-0.0014

	Base
	81
	4
	ENVSERV
	Combination
	Max
	
	
	4.8028
	8.2448
	12.66
	-6.1504
	6.4146
	0.0033

	Base
	81
	4
	ENVSERV
	Combination
	Min
	
	
	2.8329
	4.8125
	7.525
	-10.868
	3.6865
	-0.0047

	Base
	82
	15
	Dead
	LinStatic
	
	
	
	1.1496
	-1.1669
	1.2607
	1.6418
	1.5379
	-0.0013

	Base
	82
	15
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	82
	15
	FHEx
	LinStatic
	
	
	
	-0.2748
	0.174
	0.0489
	-0.4068
	-0.8894
	0.0339

	Base
	82
	15
	FHEy
	LinStatic
	
	
	
	0.0661
	-1.1145
	0.0184
	2.6363
	0.0869
	9.64E-06

	Base
	82
	15
	Sx
	LinRespSpec
	Max
	
	
	0.2472
	0.1761
	0.0434
	0.412
	0.7963
	0.034

	Base
	82
	15
	Sy
	LinRespSpec
	Max
	
	
	0.092
	1.1447
	0.0187
	2.7074
	0.2007
	0.007

	Base
	82
	15
	Comb1
	Combination
	
	
	
	1.6094
	-1.6337
	1.765
	2.2986
	2.1531
	-0.0019

	Base
	82
	15
	Comb2
	Combination
	
	
	
	1.3795
	-1.4003
	1.5128
	1.9702
	1.8455
	-0.0016

	Base
	82
	15
	Comb3
	Combination
	
	
	
	1.3795
	-1.4003
	1.5128
	1.9702
	1.8455
	-0.0016

	Base
	82
	15
	Comb4
	Combination
	Max
	
	
	1.4148
	-1.3752
	1.519
	2.0291
	1.9593
	0.0033

	Base
	82
	15
	Comb4
	Combination
	Min
	
	
	1.3442
	-1.4255
	1.5066
	1.9114
	1.7318
	-0.0065

	Base
	82
	15
	Comb5
	Combination
	Max
	
	
	1.3926
	-1.2367
	1.5155
	2.3571
	1.8742
	-0.0006

	Base
	82
	15
	Comb5
	Combination
	Min
	
	
	1.3664
	-1.5639
	1.5102
	1.5833
	1.8168
	-0.0026

	Base
	82
	15
	Comb6
	Combination
	
	
	
	1.0346
	-1.0502
	1.1346
	1.4777
	1.3841
	-0.0012

	Base
	82
	15
	Comb7
	Combination
	Max
	
	
	1.0699
	-1.0251
	1.1408
	1.5365
	1.4979
	0.0037

	Base
	82
	15
	Comb7
	Combination
	Min
	
	
	0.9993
	-1.0754
	1.1284
	1.4188
	1.2704
	-0.0061

	Base
	82
	15
	Comb8
	Combination
	Max
	
	
	1.0478
	-0.8867
	1.1373
	1.8645
	1.4128
	-0.0002

	Base
	82
	15
	Comb8
	Combination
	Min
	
	
	1.0215
	-1.2138
	1.1319
	1.0908
	1.3555
	-0.0022

	Base
	82
	15
	ENVDIS
	Combination
	Max
	
	
	1.6094
	-0.8867
	1.765
	2.3571
	2.1531
	0.0037

	Base
	82
	15
	ENVDIS
	Combination
	Min
	
	
	0.9993
	-1.6337
	1.1284
	1.0908
	1.2704
	-0.0065

	Base
	82
	15
	Serv1
	Combination
	
	
	
	1.1496
	-1.1669
	1.2607
	1.6418
	1.5379
	-0.0013

	Base
	82
	15
	Serv2
	Combination
	
	
	
	1.1496
	-1.1669
	1.2607
	1.6418
	1.5379
	-0.0013

	Base
	82
	15
	Serv3
	Combination
	
	
	
	1.1496
	-1.1669
	1.2607
	1.6418
	1.5379
	-0.0013

	Base
	82
	15
	Serv4
	Combination
	Max
	
	
	1.1743
	-1.1493
	1.265
	1.683
	1.6176
	0.0021

	Base
	82
	15
	Serv4
	Combination
	Min
	
	
	1.1249
	-1.1845
	1.2564
	1.6006
	1.4583
	-0.0047

	Base
	82
	15
	Serv5
	Combination
	Max
	
	
	1.1588
	-1.0525
	1.2626
	1.9126
	1.558
	-0.0006

	Base
	82
	15
	Serv5
	Combination
	Min
	
	
	1.1404
	-1.2814
	1.2588
	1.3711
	1.5179
	-0.002

	Base
	82
	15
	Serv6
	Combination
	Max
	
	
	1.1681
	-1.1537
	1.2639
	1.6727
	1.5977
	0.0012

	Base
	82
	15
	Serv6
	Combination
	Min
	
	
	1.131
	-1.1801
	1.2574
	1.6109
	1.4782
	-0.0039

	Base
	82
	15
	Serv7
	Combination
	Max
	
	
	1.1565
	-1.0811
	1.2621
	1.8449
	1.553
	-0.0008

	Base
	82
	15
	Serv7
	Combination
	Min
	
	
	1.1427
	-1.2528
	1.2593
	1.4388
	1.5229
	-0.0019

	Base
	82
	15
	Serv8
	Combination
	
	
	
	0.6897
	-0.7002
	0.7564
	0.9851
	0.9228
	-0.0008

	Base
	82
	15
	Serv9
	Combination
	Max
	
	
	0.7145
	-0.6825
	0.7607
	1.0263
	1.0024
	0.0026

	Base
	82
	15
	Serv9
	Combination
	Min
	
	
	0.665
	-0.7178
	0.7521
	0.9439
	0.8431
	-0.0042

	Base
	82
	15
	Serv10
	Combination
	Max
	
	
	0.6989
	-0.5857
	0.7583
	1.2558
	0.9428
	-0.0001

	Base
	82
	15
	Serv10
	Combination
	Min
	
	
	0.6805
	-0.8146
	0.7545
	0.7144
	0.9027
	-0.0015

	Base
	82
	15
	ENVSERV
	Combination
	Max
	
	
	1.1743
	-0.5857
	1.265
	1.9126
	1.6176
	0.0026

	Base
	82
	15
	ENVSERV
	Combination
	Min
	
	
	0.665
	-1.2814
	0.7521
	0.7144
	0.8431
	-0.0047

	Base
	83
	14
	Dead
	LinStatic
	
	
	
	1.2717
	0.1741
	4.273
	-0.1306
	1.6917
	-0.0014

	Base
	83
	14
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	83
	14
	FHEx
	LinStatic
	
	
	
	-0.1908
	0.1646
	0.0529
	-0.3793
	-0.6416
	0.0326

	Base
	83
	14
	FHEy
	LinStatic
	
	
	
	0.0091
	-1.1331
	-0.0185
	2.6523
	0.0125
	-0.0007

	Base
	83
	14
	Sx
	LinRespSpec
	Max
	
	
	0.1644
	0.166
	0.0468
	0.3826
	0.5526
	0.0326

	Base
	83
	14
	Sy
	LinRespSpec
	Max
	
	
	0.037
	1.1618
	0.0234
	2.7193
	0.1173
	0.0069

	Base
	83
	14
	Comb1
	Combination
	
	
	
	1.7804
	0.2438
	5.9822
	-0.1828
	2.3684
	-0.002

	Base
	83
	14
	Comb2
	Combination
	
	
	
	1.526
	0.209
	5.1276
	-0.1567
	2.03
	-0.0017

	Base
	83
	14
	Comb3
	Combination
	
	
	
	1.526
	0.209
	5.1276
	-0.1567
	2.03
	-0.0017

	Base
	83
	14
	Comb4
	Combination
	Max
	
	
	1.5495
	0.2327
	5.1343
	-0.102
	2.109
	0.0029

	Base
	83
	14
	Comb4
	Combination
	Min
	
	
	1.5025
	0.1852
	5.1209
	-0.2114
	1.9511
	-0.0064

	Base
	83
	14
	Comb5
	Combination
	Max
	
	
	1.5313
	0.375
	5.1309
	0.2319
	2.0468
	-0.0007

	Base
	83
	14
	Comb5
	Combination
	Min
	
	
	1.5207
	0.0429
	5.1242
	-0.5453
	2.0133
	-0.0027

	Base
	83
	14
	Comb6
	Combination
	
	
	
	1.1445
	0.1567
	3.8457
	-0.1175
	1.5225
	-0.0013

	Base
	83
	14
	Comb7
	Combination
	Max
	
	
	1.168
	0.1804
	3.8524
	-0.0629
	1.6015
	0.0034

	Base
	83
	14
	Comb7
	Combination
	Min
	
	
	1.121
	0.133
	3.839
	-0.1722
	1.4436
	-0.006

	Base
	83
	14
	Comb8
	Combination
	Max
	
	
	1.1498
	0.3227
	3.849
	0.2711
	1.5393
	-0.0003

	Base
	83
	14
	Comb8
	Combination
	Min
	
	
	1.1392
	-0.0093
	3.8423
	-0.5061
	1.5058
	-0.0023

	Base
	83
	14
	ENVDIS
	Combination
	Max
	
	
	1.7804
	0.375
	5.9822
	0.2711
	2.3684
	0.0034

	Base
	83
	14
	ENVDIS
	Combination
	Min
	
	
	1.121
	-0.0093
	3.839
	-0.5453
	1.4436
	-0.0064

	Base
	83
	14
	Serv1
	Combination
	
	
	
	1.2717
	0.1741
	4.273
	-0.1306
	1.6917
	-0.0014

	Base
	83
	14
	Serv2
	Combination
	
	
	
	1.2717
	0.1741
	4.273
	-0.1306
	1.6917
	-0.0014

	Base
	83
	14
	Serv3
	Combination
	
	
	
	1.2717
	0.1741
	4.273
	-0.1306
	1.6917
	-0.0014

	Base
	83
	14
	Serv4
	Combination
	Max
	
	
	1.2881
	0.1907
	4.2777
	-0.0923
	1.747
	0.0018

	Base
	83
	14
	Serv4
	Combination
	Min
	
	
	1.2552
	0.1575
	4.2683
	-0.1689
	1.6364
	-0.0047

	Base
	83
	14
	Serv5
	Combination
	Max
	
	
	1.2754
	0.2903
	4.2753
	0.1413
	1.7034
	-0.0008

	Base
	83
	14
	Serv5
	Combination
	Min
	
	
	1.268
	0.0579
	4.2706
	-0.4025
	1.68
	-0.0021

	Base
	83
	14
	Serv6
	Combination
	Max
	
	
	1.284
	0.1866
	4.2765
	-0.1019
	1.7331
	0.001

	Base
	83
	14
	Serv6
	Combination
	Min
	
	
	1.2593
	0.1617
	4.2695
	-0.1593
	1.6502
	-0.0039

	Base
	83
	14
	Serv7
	Combination
	Max
	
	
	1.2745
	0.2613
	4.2747
	0.0734
	1.7005
	-0.0009

	Base
	83
	14
	Serv7
	Combination
	Min
	
	
	1.2689
	0.087
	4.2712
	-0.3345
	1.6829
	-0.002

	Base
	83
	14
	Serv8
	Combination
	
	
	
	0.763
	0.1045
	2.5638
	-0.0784
	1.015
	-0.0009

	Base
	83
	14
	Serv9
	Combination
	Max
	
	
	0.7794
	0.1211
	2.5685
	-0.0401
	1.0703
	0.0024

	Base
	83
	14
	Serv9
	Combination
	Min
	
	
	0.7466
	0.0879
	2.5591
	-0.1166
	0.9597
	-0.0041

	Base
	83
	14
	Serv10
	Combination
	Max
	
	
	0.7667
	0.2207
	2.5661
	0.1936
	1.0267
	-0.0002

	Base
	83
	14
	Serv10
	Combination
	Min
	
	
	0.7593
	-0.0117
	2.5615
	-0.3503
	1.0033
	-0.0016

	Base
	83
	14
	ENVSERV
	Combination
	Max
	
	
	1.2881
	0.2903
	4.2777
	0.1936
	1.747
	0.0024

	Base
	83
	14
	ENVSERV
	Combination
	Min
	
	
	0.7466
	-0.0117
	2.5591
	-0.4025
	0.9597
	-0.0047

	Base
	84
	16
	Dead
	LinStatic
	
	
	
	1.5326
	-0.2761
	3.9203
	0.4555
	2.0282
	-0.0019

	Base
	84
	16
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	84
	16
	FHEx
	LinStatic
	
	
	
	-0.1272
	0.1482
	0.0374
	-0.3351
	-0.4259
	0.0309

	Base
	84
	16
	FHEy
	LinStatic
	
	
	
	0.0503
	-1.1465
	0.0349
	2.6605
	0.0652
	0.0007

	Base
	84
	16
	Sx
	LinRespSpec
	Max
	
	
	0.1044
	0.1507
	0.0305
	0.3415
	0.3482
	0.0295

	Base
	84
	16
	Sy
	LinRespSpec
	Max
	
	
	0.0597
	1.1732
	0.0341
	2.7222
	0.1082
	0.006

	Base
	84
	16
	Comb1
	Combination
	
	
	
	2.1457
	-0.3865
	5.4884
	0.6377
	2.8395
	-0.0026

	Base
	84
	16
	Comb2
	Combination
	
	
	
	1.8392
	-0.3313
	4.7043
	0.5466
	2.4338
	-0.0023

	Base
	84
	16
	Comb3
	Combination
	
	
	
	1.8392
	-0.3313
	4.7043
	0.5466
	2.4338
	-0.0023

	Base
	84
	16
	Comb4
	Combination
	Max
	
	
	1.8541
	-0.3098
	4.7087
	0.5954
	2.4836
	0.002

	Base
	84
	16
	Comb4
	Combination
	Min
	
	
	1.8243
	-0.3528
	4.7
	0.4978
	2.3841
	-0.0065

	Base
	84
	16
	Comb5
	Combination
	Max
	
	
	1.8477
	-0.1637
	4.7092
	0.9356
	2.4493
	-0.0014

	Base
	84
	16
	Comb5
	Combination
	Min
	
	
	1.8306
	-0.499
	4.6994
	0.1576
	2.4184
	-0.0031

	Base
	84
	16
	Comb6
	Combination
	
	
	
	1.3794
	-0.2485
	3.5282
	0.4099
	1.8254
	-0.0017

	Base
	84
	16
	Comb7
	Combination
	Max
	
	
	1.3943
	-0.227
	3.5326
	0.4587
	1.8751
	0.0025

	Base
	84
	16
	Comb7
	Combination
	Min
	
	
	1.3645
	-0.27
	3.5239
	0.3611
	1.7756
	-0.0059

	Base
	84
	16
	Comb8
	Combination
	Max
	
	
	1.3879
	-0.0808
	3.5331
	0.7989
	1.8408
	-0.0008

	Base
	84
	16
	Comb8
	Combination
	Min
	
	
	1.3709
	-0.4161
	3.5234
	0.0209
	1.8099
	-0.0026

	Base
	84
	16
	ENVDIS
	Combination
	Max
	
	
	2.1457
	-0.0808
	5.4884
	0.9356
	2.8395
	0.0025

	Base
	84
	16
	ENVDIS
	Combination
	Min
	
	
	1.3645
	-0.499
	3.5234
	0.0209
	1.7756
	-0.0065

	Base
	84
	16
	Serv1
	Combination
	
	
	
	1.5326
	-0.2761
	3.9203
	0.4555
	2.0282
	-0.0019

	Base
	84
	16
	Serv2
	Combination
	
	
	
	1.5326
	-0.2761
	3.9203
	0.4555
	2.0282
	-0.0019

	Base
	84
	16
	Serv3
	Combination
	
	
	
	1.5326
	-0.2761
	3.9203
	0.4555
	2.0282
	-0.0019

	Base
	84
	16
	Serv4
	Combination
	Max
	
	
	1.5431
	-0.261
	3.9233
	0.4896
	2.063
	0.0011

	Base
	84
	16
	Serv4
	Combination
	Min
	
	
	1.5222
	-0.2912
	3.9172
	0.4213
	1.9934
	-0.0048

	Base
	84
	16
	Serv5
	Combination
	Max
	
	
	1.5386
	-0.1588
	3.9237
	0.7277
	2.039
	-0.0013

	Base
	84
	16
	Serv5
	Combination
	Min
	
	
	1.5267
	-0.3934
	3.9169
	0.1833
	2.0174
	-0.0025

	Base
	84
	16
	Serv6
	Combination
	Max
	
	
	1.5405
	-0.2648
	3.9226
	0.4811
	2.0543
	0.0003

	Base
	84
	16
	Serv6
	Combination
	Min
	
	
	1.5248
	-0.2874
	3.918
	0.4299
	2.0021
	-0.0041

	Base
	84
	16
	Serv7
	Combination
	Max
	
	
	1.5371
	-0.1881
	3.9228
	0.6596
	2.0363
	-0.0014

	Base
	84
	16
	Serv7
	Combination
	Min
	
	
	1.5282
	-0.3641
	3.9177
	0.2513
	2.0201
	-0.0023

	Base
	84
	16
	Serv8
	Combination
	
	
	
	0.9196
	-0.1657
	2.3522
	0.2733
	1.2169
	-0.0011

	Base
	84
	16
	Serv9
	Combination
	Max
	
	
	0.93
	-0.1506
	2.3552
	0.3074
	1.2517
	0.0018

	Base
	84
	16
	Serv9
	Combination
	Min
	
	
	0.9092
	-0.1807
	2.3491
	0.2391
	1.1821
	-0.0041

	Base
	84
	16
	Serv10
	Combination
	Max
	
	
	0.9256
	-0.0483
	2.3556
	0.5455
	1.2277
	-0.0005

	Base
	84
	16
	Serv10
	Combination
	Min
	
	
	0.9136
	-0.283
	2.3488
	0.0011
	1.2061
	-0.0017

	Base
	84
	16
	ENVSERV
	Combination
	Max
	
	
	1.5431
	-0.0483
	3.9237
	0.7277
	2.063
	0.0018

	Base
	84
	16
	ENVSERV
	Combination
	Min
	
	
	0.9092
	-0.3934
	2.3488
	0.0011
	1.1821
	-0.0048

	Base
	85
	23
	Dead
	LinStatic
	
	
	
	0.9361
	0.1658
	2.5039
	-0.1336
	1.2364
	-0.0002

	Base
	85
	23
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	85
	23
	FHEx
	LinStatic
	
	
	
	-0.0692
	0.1054
	-0.0033
	-0.2482
	-0.2269
	0.0235

	Base
	85
	23
	FHEy
	LinStatic
	
	
	
	0.0351
	-1.0988
	0.2461
	2.586
	0.0385
	-0.0044

	Base
	85
	23
	Sx
	LinRespSpec
	Max
	
	
	0.0505
	0.1125
	0.0127
	0.2655
	0.1649
	0.0235

	Base
	85
	23
	Sy
	LinRespSpec
	Max
	
	
	0.0389
	1.1215
	0.2499
	2.6393
	0.0565
	0.0085

	Base
	85
	23
	Comb1
	Combination
	
	
	
	1.3105
	0.2322
	3.5055
	-0.1871
	1.731
	-0.0003

	Base
	85
	23
	Comb2
	Combination
	
	
	
	1.1233
	0.199
	3.0047
	-0.1603
	1.4837
	-0.0002

	Base
	85
	23
	Comb3
	Combination
	
	
	
	1.1233
	0.199
	3.0047
	-0.1603
	1.4837
	-0.0002

	Base
	85
	23
	Comb4
	Combination
	Max
	
	
	1.1305
	0.2151
	3.0065
	-0.1224
	1.5073
	0.0031

	Base
	85
	23
	Comb4
	Combination
	Min
	
	
	1.1161
	0.1829
	3.0029
	-0.1983
	1.4602
	-0.0036

	Base
	85
	23
	Comb5
	Combination
	Max
	
	
	1.1288
	0.3593
	3.0404
	0.2168
	1.4918
	0.001

	Base
	85
	23
	Comb5
	Combination
	Min
	
	
	1.1177
	0.0387
	2.969
	-0.5375
	1.4756
	-0.0014

	Base
	85
	23
	Comb6
	Combination
	
	
	
	0.8425
	0.1492
	2.2536
	-0.1203
	1.1128
	-0.0002

	Base
	85
	23
	Comb7
	Combination
	Max
	
	
	0.8497
	0.1653
	2.2554
	-0.0823
	1.1363
	0.0032

	Base
	85
	23
	Comb7
	Combination
	Min
	
	
	0.8352
	0.1332
	2.2517
	-0.1582
	1.0892
	-0.0035

	Base
	85
	23
	Comb8
	Combination
	Max
	
	
	0.848
	0.3095
	2.2893
	0.2569
	1.1209
	0.001

	Base
	85
	23
	Comb8
	Combination
	Min
	
	
	0.8369
	-0.011
	2.2178
	-0.4974
	1.1047
	-0.0014

	Base
	85
	23
	ENVDIS
	Combination
	Max
	
	
	1.3105
	0.3593
	3.5055
	0.2569
	1.731
	0.0032

	Base
	85
	23
	ENVDIS
	Combination
	Min
	
	
	0.8352
	-0.011
	2.2178
	-0.5375
	1.0892
	-0.0036

	Base
	85
	23
	Serv1
	Combination
	
	
	
	0.9361
	0.1658
	2.5039
	-0.1336
	1.2364
	-0.0002

	Base
	85
	23
	Serv2
	Combination
	
	
	
	0.9361
	0.1658
	2.5039
	-0.1336
	1.2364
	-0.0002

	Base
	85
	23
	Serv3
	Combination
	
	
	
	0.9361
	0.1658
	2.5039
	-0.1336
	1.2364
	-0.0002

	Base
	85
	23
	Serv4
	Combination
	Max
	
	
	0.9411
	0.1771
	2.5052
	-0.1071
	1.2529
	0.0021

	Base
	85
	23
	Serv4
	Combination
	Min
	
	
	0.931
	0.1546
	2.5027
	-0.1602
	1.2199
	-0.0025

	Base
	85
	23
	Serv5
	Combination
	Max
	
	
	0.94
	0.278
	2.5289
	0.1303
	1.2421
	0.0006

	Base
	85
	23
	Serv5
	Combination
	Min
	
	
	0.9322
	0.0537
	2.479
	-0.3975
	1.2308
	-0.001

	Base
	85
	23
	Serv6
	Combination
	Max
	
	
	0.9399
	0.1743
	2.5049
	-0.1137
	1.2488
	0.0016

	Base
	85
	23
	Serv6
	Combination
	Min
	
	
	0.9323
	0.1574
	2.503
	-0.1535
	1.2241
	-0.002

	Base
	85
	23
	Serv7
	Combination
	Max
	
	
	0.939
	0.2499
	2.5227
	0.0643
	1.2407
	0.0004

	Base
	85
	23
	Serv7
	Combination
	Min
	
	
	0.9332
	0.0817
	2.4852
	-0.3316
	1.2322
	-0.0008

	Base
	85
	23
	Serv8
	Combination
	
	
	
	0.5616
	0.0995
	1.5024
	-0.0802
	0.7419
	-0.0001

	Base
	85
	23
	Serv9
	Combination
	Max
	
	
	0.5667
	0.1108
	1.5036
	-0.0536
	0.7583
	0.0022

	Base
	85
	23
	Serv9
	Combination
	Min
	
	
	0.5566
	0.0882
	1.5011
	-0.1067
	0.7254
	-0.0025

	Base
	85
	23
	Serv10
	Combination
	Max
	
	
	0.5655
	0.2116
	1.5274
	0.1838
	0.7475
	0.0007

	Base
	85
	23
	Serv10
	Combination
	Min
	
	
	0.5578
	-0.0127
	1.4774
	-0.3441
	0.7362
	-0.001

	Base
	85
	23
	ENVSERV
	Combination
	Max
	
	
	0.9411
	0.278
	2.5289
	0.1838
	1.2529
	0.0022

	Base
	85
	23
	ENVSERV
	Combination
	Min
	
	
	0.5566
	-0.0127
	1.4774
	-0.3975
	0.7254
	-0.0025

	Base
	86
	22
	Dead
	LinStatic
	
	
	
	-0.0591
	-0.1066
	2.4281
	0.223
	-0.0736
	-0.0025

	Base
	86
	22
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	86
	22
	FHEx
	LinStatic
	
	
	
	-0.0756
	0.0331
	0.0038
	-0.0824
	-0.2372
	0.0256

	Base
	86
	22
	FHEy
	LinStatic
	
	
	
	-0.0023
	-0.9315
	-0.2924
	2.3741
	-0.0051
	0.0045

	Base
	86
	22
	Sx
	LinRespSpec
	Max
	
	
	0.0538
	0.0351
	0.0076
	0.0887
	0.1707
	0.0247

	Base
	86
	22
	Sy
	LinRespSpec
	Max
	
	
	0.0109
	0.9488
	0.2979
	2.4181
	0.0347
	0.0074

	Base
	86
	22
	Comb1
	Combination
	
	
	
	-0.0827
	-0.1492
	3.3994
	0.3122
	-0.103
	-0.0035

	Base
	86
	22
	Comb2
	Combination
	
	
	
	-0.0709
	-0.1279
	2.9138
	0.2676
	-0.0883
	-0.003

	Base
	86
	22
	Comb3
	Combination
	
	
	
	-0.0709
	-0.1279
	2.9138
	0.2676
	-0.0883
	-0.003

	Base
	86
	22
	Comb4
	Combination
	Max
	
	
	-0.0632
	-0.1229
	2.9148
	0.2803
	-0.0639
	0.0005

	Base
	86
	22
	Comb4
	Combination
	Min
	
	
	-0.0786
	-0.1329
	2.9127
	0.2549
	-0.1127
	-0.0065

	Base
	86
	22
	Comb5
	Combination
	Max
	
	
	-0.0693
	0.0077
	2.9563
	0.6132
	-0.0833
	-0.002

	Base
	86
	22
	Comb5
	Combination
	Min
	
	
	-0.0725
	-0.2634
	2.8712
	-0.0779
	-0.0932
	-0.0041

	Base
	86
	22
	Comb6
	Combination
	
	
	
	-0.0532
	-0.0959
	2.1853
	0.2007
	-0.0662
	-0.0023

	Base
	86
	22
	Comb7
	Combination
	Max
	
	
	-0.0455
	-0.0909
	2.1864
	0.2134
	-0.0418
	0.0013

	Base
	86
	22
	Comb7
	Combination
	Min
	
	
	-0.0609
	-0.1009
	2.1842
	0.188
	-0.0906
	-0.0058

	Base
	86
	22
	Comb8
	Combination
	Max
	
	
	-0.0516
	0.0397
	2.2279
	0.5462
	-0.0612
	-0.0012

	Base
	86
	22
	Comb8
	Combination
	Min
	
	
	-0.0547
	-0.2315
	2.1427
	-0.1448
	-0.0712
	-0.0033

	Base
	86
	22
	ENVDIS
	Combination
	Max
	
	
	-0.0455
	0.0397
	3.3994
	0.6132
	-0.0418
	0.0013

	Base
	86
	22
	ENVDIS
	Combination
	Min
	
	
	-0.0827
	-0.2634
	2.1427
	-0.1448
	-0.1127
	-0.0065

	Base
	86
	22
	Serv1
	Combination
	
	
	
	-0.0591
	-0.1066
	2.4281
	0.223
	-0.0736
	-0.0025

	Base
	86
	22
	Serv2
	Combination
	
	
	
	-0.0591
	-0.1066
	2.4281
	0.223
	-0.0736
	-0.0025

	Base
	86
	22
	Serv3
	Combination
	
	
	
	-0.0591
	-0.1066
	2.4281
	0.223
	-0.0736
	-0.0025

	Base
	86
	22
	Serv4
	Combination
	Max
	
	
	-0.0537
	-0.103
	2.4289
	0.2319
	-0.0565
	-4.712E-05

	Base
	86
	22
	Serv4
	Combination
	Min
	
	
	-0.0645
	-0.1101
	2.4274
	0.2141
	-0.0906
	-0.005

	Base
	86
	22
	Serv5
	Combination
	Max
	
	
	-0.058
	-0.0117
	2.4579
	0.4648
	-0.0701
	-0.0018

	Base
	86
	22
	Serv5
	Combination
	Min
	
	
	-0.0602
	-0.2014
	2.3983
	-0.0188
	-0.077
	-0.0032

	Base
	86
	22
	Serv6
	Combination
	Max
	
	
	-0.0551
	-0.1039
	2.4287
	0.2297
	-0.0608
	-0.0007

	Base
	86
	22
	Serv6
	Combination
	Min
	
	
	-0.0631
	-0.1092
	2.4276
	0.2164
	-0.0864
	-0.0044

	Base
	86
	22
	Serv7
	Combination
	Max
	
	
	-0.0583
	-0.0354
	2.4505
	0.4044
	-0.071
	-0.002

	Base
	86
	22
	Serv7
	Combination
	Min
	
	
	-0.0599
	-0.1777
	2.4058
	0.0416
	-0.0762
	-0.0031

	Base
	86
	22
	Serv8
	Combination
	
	
	
	-0.0355
	-0.0639
	1.4569
	0.1338
	-0.0441
	-0.0015

	Base
	86
	22
	Serv9
	Combination
	Max
	
	
	-0.0301
	-0.0604
	1.4576
	0.1427
	-0.0271
	0.001

	Base
	86
	22
	Serv9
	Combination
	Min
	
	
	-0.0408
	-0.0674
	1.4561
	0.1249
	-0.0612
	-0.004

	Base
	86
	22
	Serv10
	Combination
	Max
	
	
	-0.0344
	0.0309
	1.4867
	0.3756
	-0.0407
	-0.0008

	Base
	86
	22
	Serv10
	Combination
	Min
	
	
	-0.0365
	-0.1588
	1.4271
	-0.108
	-0.0476
	-0.0022

	Base
	86
	22
	ENVSERV
	Combination
	Max
	
	
	-0.0301
	0.0309
	2.4579
	0.4648
	-0.0271
	0.001

	Base
	86
	22
	ENVSERV
	Combination
	Min
	
	
	-0.0645
	-0.2014
	1.4271
	-0.108
	-0.0906
	-0.005

	Base
	87
	21
	Dead
	LinStatic
	
	
	
	0.0545
	-0.4321
	2.7976
	0.6472
	0.077
	0.0003

	Base
	87
	21
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	87
	21
	FHEx
	LinStatic
	
	
	
	-0.0704
	-0.0415
	-0.0157
	0.113
	-0.2308
	0.0223

	Base
	87
	21
	FHEy
	LinStatic
	
	
	
	0.0034
	-0.8071
	-0.4247
	2.2119
	0.0105
	0.0024

	Base
	87
	21
	Sx
	LinRespSpec
	Max
	
	
	0.0505
	0.053
	0.0239
	0.1446
	0.167
	0.0238

	Base
	87
	21
	Sy
	LinRespSpec
	Max
	
	
	0.0123
	0.8191
	0.4314
	2.2448
	0.0401
	0.0055

	Base
	87
	21
	Comb1
	Combination
	
	
	
	0.0763
	-0.605
	3.9166
	0.9061
	0.1078
	0.0004

	Base
	87
	21
	Comb2
	Combination
	
	
	
	0.0654
	-0.5186
	3.3571
	0.7766
	0.0924
	0.0003

	Base
	87
	21
	Comb3
	Combination
	
	
	
	0.0654
	-0.5186
	3.3571
	0.7766
	0.0924
	0.0003

	Base
	87
	21
	Comb4
	Combination
	Max
	
	
	0.0726
	-0.511
	3.3605
	0.7973
	0.1162
	0.0037

	Base
	87
	21
	Comb4
	Combination
	Min
	
	
	0.0582
	-0.5261
	3.3537
	0.756
	0.0685
	-0.0031

	Base
	87
	21
	Comb5
	Combination
	Max
	
	
	0.0672
	-0.4015
	3.4188
	1.0974
	0.0981
	0.0011

	Base
	87
	21
	Comb5
	Combination
	Min
	
	
	0.0636
	-0.6356
	3.2955
	0.4558
	0.0867
	-0.0004

	Base
	87
	21
	Comb6
	Combination
	
	
	
	0.0491
	-0.3889
	2.5178
	0.5825
	0.0693
	0.0003

	Base
	87
	21
	Comb7
	Combination
	Max
	
	
	0.0563
	-0.3814
	2.5212
	0.6031
	0.0931
	0.0037

	Base
	87
	21
	Comb7
	Combination
	Min
	
	
	0.0418
	-0.3965
	2.5144
	0.5618
	0.0454
	-0.0031

	Base
	87
	21
	Comb8
	Combination
	Max
	
	
	0.0508
	-0.2719
	2.5795
	0.9033
	0.075
	0.001

	Base
	87
	21
	Comb8
	Combination
	Min
	
	
	0.0473
	-0.506
	2.4562
	0.2617
	0.0636
	-0.0005

	Base
	87
	21
	ENVDIS
	Combination
	Max
	
	
	0.0763
	-0.2719
	3.9166
	1.0974
	0.1162
	0.0037

	Base
	87
	21
	ENVDIS
	Combination
	Min
	
	
	0.0418
	-0.6356
	2.4562
	0.2617
	0.0454
	-0.0031

	Base
	87
	21
	Serv1
	Combination
	
	
	
	0.0545
	-0.4321
	2.7976
	0.6472
	0.077
	0.0003

	Base
	87
	21
	Serv2
	Combination
	
	
	
	0.0545
	-0.4321
	2.7976
	0.6472
	0.077
	0.0003

	Base
	87
	21
	Serv3
	Combination
	
	
	
	0.0545
	-0.4321
	2.7976
	0.6472
	0.077
	0.0003

	Base
	87
	21
	Serv4
	Combination
	Max
	
	
	0.0595
	-0.4268
	2.8
	0.6616
	0.0937
	0.0027

	Base
	87
	21
	Serv4
	Combination
	Min
	
	
	0.0495
	-0.4374
	2.7952
	0.6327
	0.0603
	-0.0021

	Base
	87
	21
	Serv5
	Combination
	Max
	
	
	0.0557
	-0.3502
	2.8407
	0.8717
	0.081
	0.0008

	Base
	87
	21
	Serv5
	Combination
	Min
	
	
	0.0533
	-0.5141
	2.7544
	0.4227
	0.073
	-0.0003

	Base
	87
	21
	Serv6
	Combination
	Max
	
	
	0.0583
	-0.4282
	2.7994
	0.658
	0.0895
	0.0021

	Base
	87
	21
	Serv6
	Combination
	Min
	
	
	0.0507
	-0.4361
	2.7958
	0.6363
	0.0645
	-0.0015

	Base
	87
	21
	Serv7
	Combination
	Max
	
	
	0.0554
	-0.3707
	2.8299
	0.8155
	0.08
	0.0007

	Base
	87
	21
	Serv7
	Combination
	Min
	
	
	0.0536
	-0.4936
	2.7652
	0.4788
	0.074
	-0.0001

	Base
	87
	21
	Serv8
	Combination
	
	
	
	0.0327
	-0.2593
	1.6786
	0.3883
	0.0462
	0.0002

	Base
	87
	21
	Serv9
	Combination
	Max
	
	
	0.0377
	-0.254
	1.6809
	0.4028
	0.0629
	0.0025

	Base
	87
	21
	Serv9
	Combination
	Min
	
	
	0.0277
	-0.2646
	1.6762
	0.3739
	0.0295
	-0.0022

	Base
	87
	21
	Serv10
	Combination
	Max
	
	
	0.0339
	-0.1774
	1.7217
	0.6128
	0.0502
	0.0007

	Base
	87
	21
	Serv10
	Combination
	Min
	
	
	0.0315
	-0.3412
	1.6354
	0.1638
	0.0422
	-0.0004

	Base
	87
	21
	ENVSERV
	Combination
	Max
	
	
	0.0595
	-0.1774
	2.8407
	0.8717
	0.0937
	0.0027

	Base
	87
	21
	ENVSERV
	Combination
	Min
	
	
	0.0277
	-0.5141
	1.6354
	0.1638
	0.0295
	-0.0022

	Base
	88
	20
	Dead
	LinStatic
	
	
	
	-0.5669
	0.19
	2.8539
	-0.1794
	-0.74
	-0.0026

	Base
	88
	20
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	88
	20
	FHEx
	LinStatic
	
	
	
	-0.0614
	-0.1236
	-0.0003
	0.2896
	-0.2118
	0.0236

	Base
	88
	20
	FHEy
	LinStatic
	
	
	
	0.0041
	-1.1053
	0.2075
	2.5934
	0.0209
	-0.0056

	Base
	88
	20
	Sx
	LinRespSpec
	Max
	
	
	0.0435
	0.1452
	0.0095
	0.341
	0.1517
	0.0221

	Base
	88
	20
	Sy
	LinRespSpec
	Max
	
	
	0.0145
	1.116
	0.2084
	2.6176
	0.0505
	0.01

	Base
	88
	20
	Comb1
	Combination
	
	
	
	-0.7936
	0.2659
	3.9954
	-0.2512
	-1.036
	-0.0036

	Base
	88
	20
	Comb2
	Combination
	
	
	
	-0.6803
	0.2279
	3.4246
	-0.2153
	-0.888
	-0.0031

	Base
	88
	20
	Comb3
	Combination
	
	
	
	-0.6803
	0.2279
	3.4246
	-0.2153
	-0.888
	-0.0031

	Base
	88
	20
	Comb4
	Combination
	Max
	
	
	-0.674
	0.2487
	3.426
	-0.1666
	-0.8664
	0.0001

	Base
	88
	20
	Comb4
	Combination
	Min
	
	
	-0.6865
	0.2072
	3.4233
	-0.264
	-0.9097
	-0.0063

	Base
	88
	20
	Comb5
	Combination
	Max
	
	
	-0.6782
	0.3874
	3.4544
	0.1588
	-0.8808
	-0.0017

	Base
	88
	20
	Comb5
	Combination
	Min
	
	
	-0.6823
	0.0685
	3.3949
	-0.5893
	-0.8952
	-0.0045

	Base
	88
	20
	Comb6
	Combination
	
	
	
	-0.5102
	0.171
	2.5685
	-0.1615
	-0.666
	-0.0023

	Base
	88
	20
	Comb7
	Combination
	Max
	
	
	-0.504
	0.1917
	2.5698
	-0.1127
	-0.6443
	0.0008

	Base
	88
	20
	Comb7
	Combination
	Min
	
	
	-0.5164
	0.1502
	2.5671
	-0.2102
	-0.6877
	-0.0055

	Base
	88
	20
	Comb8
	Combination
	Max
	
	
	-0.5081
	0.3304
	2.5983
	0.2126
	-0.6588
	-0.0009

	Base
	88
	20
	Comb8
	Combination
	Min
	
	
	-0.5123
	0.0115
	2.5387
	-0.5355
	-0.6732
	-0.0038

	Base
	88
	20
	ENVDIS
	Combination
	Max
	
	
	-0.504
	0.3874
	3.9954
	0.2126
	-0.6443
	0.0008

	Base
	88
	20
	ENVDIS
	Combination
	Min
	
	
	-0.7936
	0.0115
	2.5387
	-0.5893
	-1.036
	-0.0063

	Base
	88
	20
	Serv1
	Combination
	
	
	
	-0.5669
	0.19
	2.8539
	-0.1794
	-0.74
	-0.0026

	Base
	88
	20
	Serv2
	Combination
	
	
	
	-0.5669
	0.19
	2.8539
	-0.1794
	-0.74
	-0.0026

	Base
	88
	20
	Serv3
	Combination
	
	
	
	-0.5669
	0.19
	2.8539
	-0.1794
	-0.74
	-0.0026

	Base
	88
	20
	Serv4
	Combination
	Max
	
	
	-0.5625
	0.2045
	2.8548
	-0.1453
	-0.7249
	-0.0004

	Base
	88
	20
	Serv4
	Combination
	Min
	
	
	-0.5712
	0.1754
	2.8529
	-0.2135
	-0.7552
	-0.0048

	Base
	88
	20
	Serv5
	Combination
	Max
	
	
	-0.5654
	0.3016
	2.8747
	0.0824
	-0.735
	-0.0016

	Base
	88
	20
	Serv5
	Combination
	Min
	
	
	-0.5683
	0.0784
	2.833
	-0.4412
	-0.7451
	-0.0036

	Base
	88
	20
	Serv6
	Combination
	Max
	
	
	-0.5636
	0.2008
	2.8546
	-0.1538
	-0.7286
	-0.0009

	Base
	88
	20
	Serv6
	Combination
	Min
	
	
	-0.5701
	0.1791
	2.8532
	-0.205
	-0.7514
	-0.0042

	Base
	88
	20
	Serv7
	Combination
	Max
	
	
	-0.5658
	0.2737
	2.8695
	0.0169
	-0.7362
	-0.0018

	Base
	88
	20
	Serv7
	Combination
	Min
	
	
	-0.568
	0.1063
	2.8382
	-0.3757
	-0.7438
	-0.0033

	Base
	88
	20
	Serv8
	Combination
	
	
	
	-0.3401
	0.114
	1.7123
	-0.1076
	-0.444
	-0.0015

	Base
	88
	20
	Serv9
	Combination
	Max
	
	
	-0.3358
	0.1285
	1.7133
	-0.0735
	-0.4288
	0.0007

	Base
	88
	20
	Serv9
	Combination
	Min
	
	
	-0.3445
	0.0995
	1.7114
	-0.1417
	-0.4592
	-0.0038

	Base
	88
	20
	Serv10
	Combination
	Max
	
	
	-0.3387
	0.2256
	1.7332
	0.1541
	-0.439
	-0.0005

	Base
	88
	20
	Serv10
	Combination
	Min
	
	
	-0.3416
	0.0024
	1.6915
	-0.3694
	-0.4491
	-0.0025

	Base
	88
	20
	ENVSERV
	Combination
	Max
	
	
	-0.3358
	0.3016
	2.8747
	0.1541
	-0.4288
	0.0007

	Base
	88
	20
	ENVSERV
	Combination
	Min
	
	
	-0.5712
	0.0024
	1.6915
	-0.4412
	-0.7552
	-0.0048

	Base
	89
	19
	Dead
	LinStatic
	
	
	
	-1.211
	-0.2354
	4.3715
	0.385
	-1.5838
	-0.001

	Base
	89
	19
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	89
	19
	FHEx
	LinStatic
	
	
	
	-0.1257
	-0.1664
	-0.0373
	0.3777
	-0.4221
	0.0309

	Base
	89
	19
	FHEy
	LinStatic
	
	
	
	-0.0378
	-1.1432
	0.026
	2.6557
	-0.0425
	0.002

	Base
	89
	19
	Sx
	LinRespSpec
	Max
	
	
	0.1033
	0.1845
	0.0304
	0.4203
	0.3453
	0.0303

	Base
	89
	19
	Sy
	LinRespSpec
	Max
	
	
	0.038
	1.1552
	0.0266
	2.6844
	0.0742
	0.0063

	Base
	89
	19
	Comb1
	Combination
	
	
	
	-1.6954
	-0.3296
	6.1202
	0.539
	-2.2173
	-0.0014

	Base
	89
	19
	Comb2
	Combination
	
	
	
	-1.4532
	-0.2825
	5.2459
	0.462
	-1.9006
	-0.0012

	Base
	89
	19
	Comb3
	Combination
	
	
	
	-1.4532
	-0.2825
	5.2459
	0.462
	-1.9006
	-0.0012

	Base
	89
	19
	Comb4
	Combination
	Max
	
	
	-1.4384
	-0.2561
	5.2502
	0.5221
	-1.8512
	0.0031

	Base
	89
	19
	Comb4
	Combination
	Min
	
	
	-1.4679
	-0.3088
	5.2415
	0.402
	-1.9499
	-0.0055

	Base
	89
	19
	Comb5
	Combination
	Max
	
	
	-1.4477
	-0.1174
	5.2497
	0.8456
	-1.89
	-0.0003

	Base
	89
	19
	Comb5
	Combination
	Min
	
	
	-1.4586
	-0.4476
	5.242
	0.0784
	-1.9112
	-0.0021

	Base
	89
	19
	Comb6
	Combination
	
	
	
	-1.0899
	-0.2119
	3.9344
	0.3465
	-1.4254
	-0.0009

	Base
	89
	19
	Comb7
	Combination
	Max
	
	
	-1.0751
	-0.1855
	3.9387
	0.4066
	-1.3761
	0.0034

	Base
	89
	19
	Comb7
	Combination
	Min
	
	
	-1.1046
	-0.2382
	3.93
	0.2865
	-1.4748
	-0.0052

	Base
	89
	19
	Comb8
	Combination
	Max
	
	
	-1.0845
	-0.0468
	3.9382
	0.7301
	-1.4148
	-5.916E-06

	Base
	89
	19
	Comb8
	Combination
	Min
	
	
	-1.0953
	-0.377
	3.9306
	-0.0371
	-1.436
	-0.0018

	Base
	89
	19
	ENVDIS
	Combination
	Max
	
	
	-1.0751
	-0.0468
	6.1202
	0.8456
	-1.3761
	0.0034

	Base
	89
	19
	ENVDIS
	Combination
	Min
	
	
	-1.6954
	-0.4476
	3.93
	-0.0371
	-2.2173
	-0.0055

	Base
	89
	19
	Serv1
	Combination
	
	
	
	-1.211
	-0.2354
	4.3715
	0.385
	-1.5838
	-0.001

	Base
	89
	19
	Serv2
	Combination
	
	
	
	-1.211
	-0.2354
	4.3715
	0.385
	-1.5838
	-0.001

	Base
	89
	19
	Serv3
	Combination
	
	
	
	-1.211
	-0.2354
	4.3715
	0.385
	-1.5838
	-0.001

	Base
	89
	19
	Serv4
	Combination
	Max
	
	
	-1.2006
	-0.217
	4.3746
	0.427
	-1.5493
	0.002

	Base
	89
	19
	Serv4
	Combination
	Min
	
	
	-1.2213
	-0.2539
	4.3685
	0.343
	-1.6183
	-0.004

	Base
	89
	19
	Serv5
	Combination
	Max
	
	
	-1.2072
	-0.1199
	4.3742
	0.6534
	-1.5764
	-0.0004

	Base
	89
	19
	Serv5
	Combination
	Min
	
	
	-1.2148
	-0.3509
	4.3689
	0.1166
	-1.5912
	-0.0016

	Base
	89
	19
	Serv6
	Combination
	Max
	
	
	-1.2032
	-0.2216
	4.3738
	0.4165
	-1.5579
	0.0013

	Base
	89
	19
	Serv6
	Combination
	Min
	
	
	-1.2187
	-0.2492
	4.3693
	0.3535
	-1.6097
	-0.0033

	Base
	89
	19
	Serv7
	Combination
	Max
	
	
	-1.2081
	-0.1488
	4.3735
	0.5863
	-1.5782
	-0.0005

	Base
	89
	19
	Serv7
	Combination
	Min
	
	
	-1.2138
	-0.3221
	4.3695
	0.1837
	-1.5894
	-0.0015

	Base
	89
	19
	Serv8
	Combination
	
	
	
	-0.7266
	-0.1412
	2.6229
	0.231
	-0.9503
	-0.0006

	Base
	89
	19
	Serv9
	Combination
	Max
	
	
	-0.7163
	-0.1228
	2.626
	0.273
	-0.9158
	0.0024

	Base
	89
	19
	Serv9
	Combination
	Min
	
	
	-0.7369
	-0.1597
	2.6199
	0.189
	-0.9848
	-0.0036

	Base
	89
	19
	Serv10
	Combination
	Max
	
	
	-0.7228
	-0.0257
	2.6256
	0.4994
	-0.9429
	2.592E-05

	Base
	89
	19
	Serv10
	Combination
	Min
	
	
	-0.7304
	-0.2568
	2.6203
	-0.0374
	-0.9577
	-0.0012

	Base
	89
	19
	ENVSERV
	Combination
	Max
	
	
	-0.7163
	-0.0257
	4.3746
	0.6534
	-0.9158
	0.0024

	Base
	89
	19
	ENVSERV
	Combination
	Min
	
	
	-1.2213
	-0.3509
	2.6199
	-0.0374
	-1.6183
	-0.004

	Base
	90
	10
	Dead
	LinStatic
	
	
	
	-0.718
	-0.0456
	3.4438
	0.1394
	-0.929
	-0.0021

	Base
	90
	10
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	90
	10
	FHEx
	LinStatic
	
	
	
	-0.1838
	-0.1862
	-0.0523
	0.427
	-0.6321
	0.033

	Base
	90
	10
	FHEy
	LinStatic
	
	
	
	-0.0033
	-1.1393
	0.0061
	2.6611
	2.972E-05
	1.172E-05

	Base
	90
	10
	Sx
	LinRespSpec
	Max
	
	
	0.1579
	0.204
	0.046
	0.4687
	0.5437
	0.0324

	Base
	90
	10
	Sy
	LinRespSpec
	Max
	
	
	0.0322
	1.1541
	0.0119
	2.696
	0.1128
	0.0066

	Base
	90
	10
	Comb1
	Combination
	
	
	
	-1.0051
	-0.0639
	4.8214
	0.1952
	-1.3006
	-0.0029

	Base
	90
	10
	Comb2
	Combination
	
	
	
	-0.8616
	-0.0548
	4.1326
	0.1673
	-1.1148
	-0.0025

	Base
	90
	10
	Comb3
	Combination
	
	
	
	-0.8616
	-0.0548
	4.1326
	0.1673
	-1.1148
	-0.0025

	Base
	90
	10
	Comb4
	Combination
	Max
	
	
	-0.839
	-0.0256
	4.1392
	0.2343
	-1.0371
	0.0021

	Base
	90
	10
	Comb4
	Combination
	Min
	
	
	-0.8841
	-0.0839
	4.126
	0.1004
	-1.1924
	-0.0071

	Base
	90
	10
	Comb5
	Combination
	Max
	
	
	-0.857
	0.1102
	4.1343
	0.5526
	-1.0986
	-0.0016

	Base
	90
	10
	Comb5
	Combination
	Min
	
	
	-0.8662
	-0.2197
	4.1309
	-0.2179
	-1.1309
	-0.0035

	Base
	90
	10
	Comb6
	Combination
	
	
	
	-0.6462
	-0.0411
	3.0995
	0.1255
	-0.8361
	-0.0019

	Base
	90
	10
	Comb7
	Combination
	Max
	
	
	-0.6236
	-0.0119
	3.106
	0.1925
	-0.7584
	0.0027

	Base
	90
	10
	Comb7
	Combination
	Min
	
	
	-0.6687
	-0.0702
	3.0929
	0.0585
	-0.9137
	-0.0065

	Base
	90
	10
	Comb8
	Combination
	Max
	
	
	-0.6416
	0.1239
	3.1012
	0.5108
	-0.8199
	-0.0009

	Base
	90
	10
	Comb8
	Combination
	Min
	
	
	-0.6508
	-0.206
	3.0978
	-0.2598
	-0.8522
	-0.0028

	Base
	90
	10
	ENVDIS
	Combination
	Max
	
	
	-0.6236
	0.1239
	4.8214
	0.5526
	-0.7584
	0.0027

	Base
	90
	10
	ENVDIS
	Combination
	Min
	
	
	-1.0051
	-0.2197
	3.0929
	-0.2598
	-1.3006
	-0.0071

	Base
	90
	10
	Serv1
	Combination
	
	
	
	-0.718
	-0.0456
	3.4438
	0.1394
	-0.929
	-0.0021

	Base
	90
	10
	Serv2
	Combination
	
	
	
	-0.718
	-0.0456
	3.4438
	0.1394
	-0.929
	-0.0021

	Base
	90
	10
	Serv3
	Combination
	
	
	
	-0.718
	-0.0456
	3.4438
	0.1394
	-0.929
	-0.0021

	Base
	90
	10
	Serv4
	Combination
	Max
	
	
	-0.7022
	-0.0252
	3.4484
	0.1863
	-0.8746
	0.0011

	Base
	90
	10
	Serv4
	Combination
	Min
	
	
	-0.7337
	-0.066
	3.4392
	0.0926
	-0.9833
	-0.0053

	Base
	90
	10
	Serv5
	Combination
	Max
	
	
	-0.7147
	0.0698
	3.445
	0.409
	-0.9177
	-0.0014

	Base
	90
	10
	Serv5
	Combination
	Min
	
	
	-0.7212
	-0.161
	3.4427
	-0.1302
	-0.9402
	-0.0028

	Base
	90
	10
	Serv6
	Combination
	Max
	
	
	-0.7061
	-0.0303
	3.4473
	0.1746
	-0.8882
	0.0003

	Base
	90
	10
	Serv6
	Combination
	Min
	
	
	-0.7298
	-0.0609
	3.4404
	0.1043
	-0.9697
	-0.0045

	Base
	90
	10
	Serv7
	Combination
	Max
	
	
	-0.7155
	0.0409
	3.4447
	0.3416
	-0.9205
	-0.0016

	Base
	90
	10
	Serv7
	Combination
	Min
	
	
	-0.7204
	-0.1322
	3.4429
	-0.0628
	-0.9374
	-0.0026

	Base
	90
	10
	Serv8
	Combination
	
	
	
	-0.4308
	-0.0274
	2.0663
	0.0837
	-0.5574
	-0.0013

	Base
	90
	10
	Serv9
	Combination
	Max
	
	
	-0.415
	-0.007
	2.0709
	0.1305
	-0.503
	0.002

	Base
	90
	10
	Serv9
	Combination
	Min
	
	
	-0.4466
	-0.0478
	2.0617
	0.0368
	-0.6118
	-0.0045

	Base
	90
	10
	Serv10
	Combination
	Max
	
	
	-0.4276
	0.088
	2.0675
	0.3533
	-0.5461
	-0.0006

	Base
	90
	10
	Serv10
	Combination
	Min
	
	
	-0.434
	-0.1428
	2.0651
	-0.1859
	-0.5687
	-0.0019

	Base
	90
	10
	ENVSERV
	Combination
	Max
	
	
	-0.415
	0.088
	3.4484
	0.409
	-0.503
	0.002

	Base
	90
	10
	ENVSERV
	Combination
	Min
	
	
	-0.7337
	-0.161
	2.0617
	-0.1859
	-0.9833
	-0.0053

	Base
	91
	8
	Dead
	LinStatic
	
	
	
	-1.505
	0.0137
	1.7218
	0.0657
	-1.9574
	-0.0026

	Base
	91
	8
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	91
	8
	FHEx
	LinStatic
	
	
	
	-0.2565
	-0.1995
	-0.0803
	0.4595
	-0.8664
	0.0346

	Base
	91
	8
	FHEy
	LinStatic
	
	
	
	0.0112
	-1.1579
	-0.1133
	2.6948
	0.0197
	0.0008

	Base
	91
	8
	Sx
	LinRespSpec
	Max
	
	
	0.2285
	0.2195
	0.0766
	0.5059
	0.7721
	0.0353

	Base
	91
	8
	Sy
	LinRespSpec
	Max
	
	
	0.0508
	1.1753
	0.1147
	2.7352
	0.1647
	0.0072

	Base
	91
	8
	Comb1
	Combination
	
	
	
	-2.1071
	0.0191
	2.4106
	0.092
	-2.7404
	-0.0036

	Base
	91
	8
	Comb2
	Combination
	
	
	
	-1.8061
	0.0164
	2.0662
	0.0788
	-2.3489
	-0.0031

	Base
	91
	8
	Comb3
	Combination
	
	
	
	-1.8061
	0.0164
	2.0662
	0.0788
	-2.3489
	-0.0031

	Base
	91
	8
	Comb4
	Combination
	Max
	
	
	-1.7734
	0.0478
	2.0772
	0.1511
	-2.2386
	0.002

	Base
	91
	8
	Comb4
	Combination
	Min
	
	
	-1.8387
	-0.0149
	2.0553
	0.0066
	-2.4592
	-0.0081

	Base
	91
	8
	Comb5
	Combination
	Max
	
	
	-1.7988
	0.1844
	2.0826
	0.4697
	-2.3253
	-0.0021

	Base
	91
	8
	Comb5
	Combination
	Min
	
	
	-1.8133
	-0.1515
	2.0498
	-0.312
	-2.3724
	-0.0041

	Base
	91
	8
	Comb6
	Combination
	
	
	
	-1.3545
	0.0123
	1.5497
	0.0591
	-1.7617
	-0.0023

	Base
	91
	8
	Comb7
	Combination
	Max
	
	
	-1.3219
	0.0437
	1.5606
	0.1314
	-1.6514
	0.0027

	Base
	91
	8
	Comb7
	Combination
	Min
	
	
	-1.3872
	-0.019
	1.5387
	-0.0131
	-1.872
	-0.0074

	Base
	91
	8
	Comb8
	Combination
	Max
	
	
	-1.3473
	0.1803
	1.5661
	0.45
	-1.7381
	-0.0013

	Base
	91
	8
	Comb8
	Combination
	Min
	
	
	-1.3618
	-0.1556
	1.5333
	-0.3317
	-1.7852
	-0.0033

	Base
	91
	8
	ENVDIS
	Combination
	Max
	
	
	-1.3219
	0.1844
	2.4106
	0.4697
	-1.6514
	0.0027

	Base
	91
	8
	ENVDIS
	Combination
	Min
	
	
	-2.1071
	-0.1556
	1.5333
	-0.3317
	-2.7404
	-0.0081

	Base
	91
	8
	Serv1
	Combination
	
	
	
	-1.505
	0.0137
	1.7218
	0.0657
	-1.9574
	-0.0026

	Base
	91
	8
	Serv2
	Combination
	
	
	
	-1.505
	0.0137
	1.7218
	0.0657
	-1.9574
	-0.0026

	Base
	91
	8
	Serv3
	Combination
	
	
	
	-1.505
	0.0137
	1.7218
	0.0657
	-1.9574
	-0.0026

	Base
	91
	8
	Serv4
	Combination
	Max
	
	
	-1.4822
	0.0356
	1.7295
	0.1163
	-1.8802
	0.001

	Base
	91
	8
	Serv4
	Combination
	Min
	
	
	-1.5279
	-0.0083
	1.7142
	0.0151
	-2.0346
	-0.0061

	Base
	91
	8
	Serv5
	Combination
	Max
	
	
	-1.5
	0.1312
	1.7333
	0.3392
	-1.9409
	-0.0019

	Base
	91
	8
	Serv5
	Combination
	Min
	
	
	-1.5101
	-0.1039
	1.7104
	-0.2078
	-1.9739
	-0.0033

	Base
	91
	8
	Serv6
	Combination
	Max
	
	
	-1.4879
	0.0301
	1.7276
	0.1036
	-1.8995
	0.0001

	Base
	91
	8
	Serv6
	Combination
	Min
	
	
	-1.5222
	-0.0028
	1.7161
	0.0278
	-2.0153
	-0.0052

	Base
	91
	8
	Serv7
	Combination
	Max
	
	
	-1.5012
	0.1018
	1.7305
	0.2708
	-1.9451
	-0.002

	Base
	91
	8
	Serv7
	Combination
	Min
	
	
	-1.5089
	-0.0745
	1.7132
	-0.1394
	-1.9698
	-0.0031

	Base
	91
	8
	Serv8
	Combination
	
	
	
	-0.903
	0.0082
	1.0331
	0.0394
	-1.1744
	-0.0015

	Base
	91
	8
	Serv9
	Combination
	Max
	
	
	-0.8802
	0.0302
	1.0408
	0.09
	-1.0972
	0.002

	Base
	91
	8
	Serv9
	Combination
	Min
	
	
	-0.9259
	-0.0137
	1.0255
	-0.0112
	-1.2517
	-0.0051

	Base
	91
	8
	Serv10
	Combination
	Max
	
	
	-0.8979
	0.1257
	1.0446
	0.3129
	-1.158
	-0.0008

	Base
	91
	8
	Serv10
	Combination
	Min
	
	
	-0.9081
	-0.1093
	1.0216
	-0.2341
	-1.1909
	-0.0023

	Base
	91
	8
	ENVSERV
	Combination
	Max
	
	
	-0.8802
	0.1312
	1.7333
	0.3392
	-1.0972
	0.002

	Base
	91
	8
	ENVSERV
	Combination
	Min
	
	
	-1.5279
	-0.1093
	1.0216
	-0.2341
	-2.0346
	-0.0061

	Base
	92
	9
	Dead
	LinStatic
	
	
	
	0.0907
	-1.2303
	-1.1106
	1.7129
	0.1436
	-0.0022

	Base
	92
	9
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	92
	9
	FHEx
	LinStatic
	
	
	
	-0.2857
	-0.0704
	0.0278
	0.1724
	-0.9031
	0.0334

	Base
	92
	9
	FHEy
	LinStatic
	
	
	
	0.0022
	-1.0662
	-0.0614
	2.5677
	0.0066
	0.0002

	Base
	92
	9
	Sx
	LinRespSpec
	Max
	
	
	0.2547
	0.0851
	0.0239
	0.2076
	0.8056
	0.0338

	Base
	92
	9
	Sy
	LinRespSpec
	Max
	
	
	0.053
	1.0845
	0.0642
	2.6118
	0.1675
	0.0069

	Base
	92
	9
	Comb1
	Combination
	
	
	
	0.127
	-1.7225
	-1.5548
	2.3981
	0.2011
	-0.003

	Base
	92
	9
	Comb2
	Combination
	
	
	
	0.1088
	-1.4764
	-1.3327
	2.0555
	0.1724
	-0.0026

	Base
	92
	9
	Comb3
	Combination
	
	
	
	0.1088
	-1.4764
	-1.3327
	2.0555
	0.1724
	-0.0026

	Base
	92
	9
	Comb4
	Combination
	Max
	
	
	0.1452
	-1.4642
	-1.3293
	2.0851
	0.2874
	0.0022

	Base
	92
	9
	Comb4
	Combination
	Min
	
	
	0.0724
	-1.4885
	-1.3361
	2.0258
	0.0573
	-0.0074

	Base
	92
	9
	Comb5
	Combination
	Max
	
	
	0.1164
	-1.3214
	-1.3235
	2.4287
	0.1963
	-0.0016

	Base
	92
	9
	Comb5
	Combination
	Min
	
	
	0.1012
	-1.6314
	-1.3419
	1.6823
	0.1484
	-0.0036

	Base
	92
	9
	Comb6
	Combination
	
	
	
	0.0816
	-1.1073
	-0.9995
	1.5416
	0.1293
	-0.002

	Base
	92
	9
	Comb7
	Combination
	Max
	
	
	0.118
	-1.0951
	-0.9961
	1.5713
	0.2443
	0.0029

	Base
	92
	9
	Comb7
	Combination
	Min
	
	
	0.0452
	-1.1194
	-1.0029
	1.512
	0.0142
	-0.0068

	Base
	92
	9
	Comb8
	Combination
	Max
	
	
	0.0892
	-0.9523
	-0.9903
	1.9148
	0.1532
	-0.001

	Base
	92
	9
	Comb8
	Combination
	Min
	
	
	0.074
	-1.2623
	-1.0087
	1.1684
	0.1053
	-0.0029

	Base
	92
	9
	ENVDIS
	Combination
	Max
	
	
	0.1452
	-0.9523
	-0.9903
	2.4287
	0.2874
	0.0029

	Base
	92
	9
	ENVDIS
	Combination
	Min
	
	
	0.0452
	-1.7225
	-1.5548
	1.1684
	0.0142
	-0.0074

	Base
	92
	9
	Serv1
	Combination
	
	
	
	0.0907
	-1.2303
	-1.1106
	1.7129
	0.1436
	-0.0022

	Base
	92
	9
	Serv2
	Combination
	
	
	
	0.0907
	-1.2303
	-1.1106
	1.7129
	0.1436
	-0.0022

	Base
	92
	9
	Serv3
	Combination
	
	
	
	0.0907
	-1.2303
	-1.1106
	1.7129
	0.1436
	-0.0022

	Base
	92
	9
	Serv4
	Combination
	Max
	
	
	0.1162
	-1.2218
	-1.1082
	1.7337
	0.2242
	0.0012

	Base
	92
	9
	Serv4
	Combination
	Min
	
	
	0.0652
	-1.2388
	-1.113
	1.6921
	0.0631
	-0.0055

	Base
	92
	9
	Serv5
	Combination
	Max
	
	
	0.096
	-1.1219
	-1.1041
	1.9741
	0.1604
	-0.0015

	Base
	92
	9
	Serv5
	Combination
	Min
	
	
	0.0854
	-1.3388
	-1.117
	1.4517
	0.1269
	-0.0029

	Base
	92
	9
	Serv6
	Combination
	Max
	
	
	0.1098
	-1.2239
	-1.1088
	1.7285
	0.204
	0.0004

	Base
	92
	9
	Serv6
	Combination
	Min
	
	
	0.0716
	-1.2367
	-1.1124
	1.6973
	0.0832
	-0.0047

	Base
	92
	9
	Serv7
	Combination
	Max
	
	
	0.0947
	-1.149
	-1.1058
	1.9088
	0.1562
	-0.0017

	Base
	92
	9
	Serv7
	Combination
	Min
	
	
	0.0867
	-1.3117
	-1.1154
	1.517
	0.1311
	-0.0027

	Base
	92
	9
	Serv8
	Combination
	
	
	
	0.0544
	-0.7382
	-0.6663
	1.0277
	0.0862
	-0.0013

	Base
	92
	9
	Serv9
	Combination
	Max
	
	
	0.0799
	-0.7297
	-0.664
	1.0485
	0.1667
	0.0021

	Base
	92
	9
	Serv9
	Combination
	Min
	
	
	0.0289
	-0.7467
	-0.6687
	1.007
	0.0056
	-0.0047

	Base
	92
	9
	Serv10
	Combination
	Max
	
	
	0.0597
	-0.6297
	-0.6599
	1.2889
	0.1029
	-0.0006

	Base
	92
	9
	Serv10
	Combination
	Min
	
	
	0.0491
	-0.8466
	-0.6728
	0.7666
	0.0694
	-0.002

	Base
	92
	9
	ENVSERV
	Combination
	Max
	
	
	0.1162
	-0.6297
	-0.6599
	1.9741
	0.2242
	0.0021

	Base
	92
	9
	ENVSERV
	Combination
	Min
	
	
	0.0289
	-1.3388
	-1.117
	0.7666
	0.0056
	-0.0055

	Base
	93
	12
	Dead
	LinStatic
	
	
	
	-0.062
	-1.1669
	-0.8506
	1.6377
	-0.058
	-0.0014

	Base
	93
	12
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	93
	12
	FHEx
	LinStatic
	
	
	
	-0.2849
	0.0542
	-0.0248
	-0.1324
	-0.9015
	0.0335

	Base
	93
	12
	FHEy
	LinStatic
	
	
	
	-0.001
	-1.0663
	-0.0686
	2.5674
	-0.0006
	-0.0003

	Base
	93
	12
	Sx
	LinRespSpec
	Max
	
	
	0.2541
	0.0541
	0.0219
	0.1319
	0.8044
	0.0346

	Base
	93
	12
	Sy
	LinRespSpec
	Max
	
	
	0.0521
	1.0894
	0.0695
	2.6232
	0.1654
	0.0072

	Base
	93
	12
	Comb1
	Combination
	
	
	
	-0.0868
	-1.6337
	-1.1908
	2.2928
	-0.0812
	-0.002

	Base
	93
	12
	Comb2
	Combination
	
	
	
	-0.0744
	-1.4003
	-1.0207
	1.9653
	-0.0696
	-0.0017

	Base
	93
	12
	Comb3
	Combination
	
	
	
	-0.0744
	-1.4003
	-1.0207
	1.9653
	-0.0696
	-0.0017

	Base
	93
	12
	Comb4
	Combination
	Max
	
	
	-0.0381
	-1.3926
	-1.0176
	1.9841
	0.0453
	0.0033

	Base
	93
	12
	Comb4
	Combination
	Min
	
	
	-0.1107
	-1.408
	-1.0239
	1.9464
	-0.1845
	-0.0066

	Base
	93
	12
	Comb5
	Combination
	Max
	
	
	-0.067
	-1.2446
	-1.0108
	2.3401
	-0.0459
	-0.0007

	Base
	93
	12
	Comb5
	Combination
	Min
	
	
	-0.0818
	-1.556
	-1.0307
	1.5904
	-0.0932
	-0.0027

	Base
	93
	12
	Comb6
	Combination
	
	
	
	-0.0558
	-1.0502
	-0.7655
	1.474
	-0.0522
	-0.0013

	Base
	93
	12
	Comb7
	Combination
	Max
	
	
	-0.0195
	-1.0425
	-0.7624
	1.4928
	0.0627
	0.0037

	Base
	93
	12
	Comb7
	Combination
	Min
	
	
	-0.0921
	-1.058
	-0.7687
	1.4551
	-0.1671
	-0.0062

	Base
	93
	12
	Comb8
	Combination
	Max
	
	
	-0.0484
	-0.8946
	-0.7556
	1.8488
	-0.0285
	-0.0002

	Base
	93
	12
	Comb8
	Combination
	Min
	
	
	-0.0632
	-1.2059
	-0.7755
	1.0991
	-0.0758
	-0.0023

	Base
	93
	12
	ENVDIS
	Combination
	Max
	
	
	-0.0195
	-0.8946
	-0.7556
	2.3401
	0.0627
	0.0037

	Base
	93
	12
	ENVDIS
	Combination
	Min
	
	
	-0.1107
	-1.6337
	-1.1908
	1.0991
	-0.1845
	-0.0066

	Base
	93
	12
	Serv1
	Combination
	
	
	
	-0.062
	-1.1669
	-0.8506
	1.6377
	-0.058
	-0.0014

	Base
	93
	12
	Serv2
	Combination
	
	
	
	-0.062
	-1.1669
	-0.8506
	1.6377
	-0.058
	-0.0014

	Base
	93
	12
	Serv3
	Combination
	
	
	
	-0.062
	-1.1669
	-0.8506
	1.6377
	-0.058
	-0.0014

	Base
	93
	12
	Serv4
	Combination
	Max
	
	
	-0.0366
	-1.1615
	-0.8484
	1.6509
	0.0225
	0.0021

	Base
	93
	12
	Serv4
	Combination
	Min
	
	
	-0.0874
	-1.1723
	-0.8528
	1.6245
	-0.1384
	-0.0049

	Base
	93
	12
	Serv5
	Combination
	Max
	
	
	-0.0568
	-1.058
	-0.8436
	1.9
	-0.0414
	-0.0007

	Base
	93
	12
	Serv5
	Combination
	Min
	
	
	-0.0672
	-1.2759
	-0.8576
	1.3754
	-0.0745
	-0.0021

	Base
	93
	12
	Serv6
	Combination
	Max
	
	
	-0.0429
	-1.1629
	-0.849
	1.6476
	0.0024
	0.0012

	Base
	93
	12
	Serv6
	Combination
	Min
	
	
	-0.0811
	-1.171
	-0.8522
	1.6278
	-0.1183
	-0.004

	Base
	93
	12
	Serv7
	Combination
	Max
	
	
	-0.0581
	-1.0852
	-0.8454
	1.8345
	-0.0456
	-0.0009

	Base
	93
	12
	Serv7
	Combination
	Min
	
	
	-0.0659
	-1.2486
	-0.8558
	1.441
	-0.0704
	-0.0019

	Base
	93
	12
	Serv8
	Combination
	
	
	
	-0.0372
	-0.7002
	-0.5104
	0.9826
	-0.0348
	-0.0008

	Base
	93
	12
	Serv9
	Combination
	Max
	
	
	-0.0118
	-0.6947
	-0.5082
	0.9958
	0.0457
	0.0026

	Base
	93
	12
	Serv9
	Combination
	Min
	
	
	-0.0626
	-0.7056
	-0.5126
	0.9694
	-0.1152
	-0.0043

	Base
	93
	12
	Serv10
	Combination
	Max
	
	
	-0.032
	-0.5912
	-0.5034
	1.245
	-0.0182
	-0.0001

	Base
	93
	12
	Serv10
	Combination
	Min
	
	
	-0.0424
	-0.8091
	-0.5173
	0.7203
	-0.0513
	-0.0016

	Base
	93
	12
	ENVSERV
	Combination
	Max
	
	
	-0.0118
	-0.5912
	-0.5034
	1.9
	0.0457
	0.0026

	Base
	93
	12
	ENVSERV
	Combination
	Min
	
	
	-0.0874
	-1.2759
	-0.8576
	0.7203
	-0.1384
	-0.0049

	Base
	95
	11
	Dead
	LinStatic
	
	
	
	0.0671
	0.0262
	2.7095
	0.0523
	0.1052
	-0.0013

	Base
	95
	11
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	95
	11
	FHEx
	LinStatic
	
	
	
	-0.2093
	-0.0661
	0.0162
	0.1607
	-0.6625
	0.0314

	Base
	95
	11
	FHEy
	LinStatic
	
	
	
	0.0021
	-1.0368
	-0.0028
	2.5236
	0.0067
	0.0006

	Base
	95
	11
	Sx
	LinRespSpec
	Max
	
	
	0.1801
	0.0799
	0.0137
	0.1942
	0.5705
	0.032

	Base
	95
	11
	Sy
	LinRespSpec
	Max
	
	
	0.0379
	1.0535
	0.0049
	2.5644
	0.1199
	0.0065

	Base
	95
	11
	Comb1
	Combination
	
	
	
	0.094
	0.0367
	3.7933
	0.0732
	0.1473
	-0.0019

	Base
	95
	11
	Comb2
	Combination
	
	
	
	0.0806
	0.0314
	3.2514
	0.0627
	0.1263
	-0.0016

	Base
	95
	11
	Comb3
	Combination
	
	
	
	0.0806
	0.0314
	3.2514
	0.0627
	0.1263
	-0.0016

	Base
	95
	11
	Comb4
	Combination
	Max
	
	
	0.1063
	0.0428
	3.2534
	0.0905
	0.2078
	0.003

	Base
	95
	11
	Comb4
	Combination
	Min
	
	
	0.0548
	0.02
	3.2495
	0.035
	0.0448
	-0.0062

	Base
	95
	11
	Comb5
	Combination
	Max
	
	
	0.086
	0.182
	3.2521
	0.4292
	0.1434
	-0.0007

	Base
	95
	11
	Comb5
	Combination
	Min
	
	
	0.0752
	-0.1191
	3.2507
	-0.3037
	0.1091
	-0.0025

	Base
	95
	11
	Comb6
	Combination
	
	
	
	0.0604
	0.0236
	2.4386
	0.047
	0.0947
	-0.0012

	Base
	95
	11
	Comb7
	Combination
	Max
	
	
	0.0862
	0.035
	2.4405
	0.0748
	0.1762
	0.0034

	Base
	95
	11
	Comb7
	Combination
	Min
	
	
	0.0347
	0.0122
	2.4366
	0.0193
	0.0132
	-0.0058

	Base
	95
	11
	Comb8
	Combination
	Max
	
	
	0.0658
	0.1741
	2.4393
	0.4135
	0.1118
	-0.0003

	Base
	95
	11
	Comb8
	Combination
	Min
	
	
	0.055
	-0.127
	2.4379
	-0.3194
	0.0776
	-0.0021

	Base
	95
	11
	ENVDIS
	Combination
	Max
	
	
	0.1063
	0.182
	3.7933
	0.4292
	0.2078
	0.0034

	Base
	95
	11
	ENVDIS
	Combination
	Min
	
	
	0.0347
	-0.127
	2.4366
	-0.3194
	0.0132
	-0.0062

	Base
	95
	11
	Serv1
	Combination
	
	
	
	0.0671
	0.0262
	2.7095
	0.0523
	0.1052
	-0.0013

	Base
	95
	11
	Serv2
	Combination
	
	
	
	0.0671
	0.0262
	2.7095
	0.0523
	0.1052
	-0.0013

	Base
	95
	11
	Serv3
	Combination
	
	
	
	0.0671
	0.0262
	2.7095
	0.0523
	0.1052
	-0.0013

	Base
	95
	11
	Serv4
	Combination
	Max
	
	
	0.0852
	0.0342
	2.7109
	0.0717
	0.1623
	0.0019

	Base
	95
	11
	Serv4
	Combination
	Min
	
	
	0.0491
	0.0182
	2.7081
	0.0328
	0.0482
	-0.0045

	Base
	95
	11
	Serv5
	Combination
	Max
	
	
	0.0709
	0.1315
	2.71
	0.3087
	0.1172
	-0.0007

	Base
	95
	11
	Serv5
	Combination
	Min
	
	
	0.0634
	-0.0792
	2.709
	-0.2042
	0.0932
	-0.002

	Base
	95
	11
	Serv6
	Combination
	Max
	
	
	0.0806
	0.0322
	2.7105
	0.0668
	0.148
	0.0011

	Base
	95
	11
	Serv6
	Combination
	Min
	
	
	0.0536
	0.0202
	2.7085
	0.0377
	0.0624
	-0.0037

	Base
	95
	11
	Serv7
	Combination
	Max
	
	
	0.07
	0.1052
	2.7099
	0.2446
	0.1142
	-0.0009

	Base
	95
	11
	Serv7
	Combination
	Min
	
	
	0.0643
	-0.0528
	2.7091
	-0.1401
	0.0962
	-0.0018

	Base
	95
	11
	Serv8
	Combination
	
	
	
	0.0403
	0.0157
	1.6257
	0.0314
	0.0631
	-0.0008

	Base
	95
	11
	Serv9
	Combination
	Max
	
	
	0.0583
	0.0237
	1.6271
	0.0508
	0.1202
	0.0024

	Base
	95
	11
	Serv9
	Combination
	Min
	
	
	0.0223
	0.0077
	1.6243
	0.0119
	0.0061
	-0.004

	Base
	95
	11
	Serv10
	Combination
	Max
	
	
	0.0441
	0.1211
	1.6262
	0.2878
	0.0751
	-0.0002

	Base
	95
	11
	Serv10
	Combination
	Min
	
	
	0.0365
	-0.0896
	1.6252
	-0.2251
	0.0511
	-0.0015

	Base
	95
	11
	ENVSERV
	Combination
	Max
	
	
	0.0852
	0.1315
	2.7109
	0.3087
	0.1623
	0.0024

	Base
	95
	11
	ENVSERV
	Combination
	Min
	
	
	0.0223
	-0.0896
	1.6243
	-0.2251
	0.0061
	-0.0045

	Base
	96
	13
	Dead
	LinStatic
	
	
	
	-0.0608
	0.0177
	2.6489
	0.0707
	-0.0634
	-0.002

	Base
	96
	13
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	96
	13
	FHEx
	LinStatic
	
	
	
	-0.2091
	0.0496
	-0.0165
	-0.1206
	-0.6621
	0.0314

	Base
	96
	13
	FHEy
	LinStatic
	
	
	
	0.0006
	-1.0379
	0.0008
	2.5249
	0.0023
	0.0001

	Base
	96
	13
	Sx
	LinRespSpec
	Max
	
	
	0.1801
	0.0496
	0.014
	0.1206
	0.5704
	0.0311

	Base
	96
	13
	Sy
	LinRespSpec
	Max
	
	
	0.0373
	1.0595
	0.0031
	2.5775
	0.1184
	0.0064

	Base
	96
	13
	Comb1
	Combination
	
	
	
	-0.0851
	0.0248
	3.7084
	0.099
	-0.0887
	-0.0028

	Base
	96
	13
	Comb2
	Combination
	
	
	
	-0.0729
	0.0213
	3.1786
	0.0848
	-0.0761
	-0.0024

	Base
	96
	13
	Comb3
	Combination
	
	
	
	-0.0729
	0.0213
	3.1786
	0.0848
	-0.0761
	-0.0024

	Base
	96
	13
	Comb4
	Combination
	Max
	
	
	-0.0472
	0.0284
	3.1806
	0.1021
	0.0054
	0.0021

	Base
	96
	13
	Comb4
	Combination
	Min
	
	
	-0.0987
	0.0142
	3.1766
	0.0676
	-0.1576
	-0.0068

	Base
	96
	13
	Comb5
	Combination
	Max
	
	
	-0.0676
	0.1727
	3.1791
	0.4532
	-0.0592
	-0.0015

	Base
	96
	13
	Comb5
	Combination
	Min
	
	
	-0.0783
	-0.1301
	3.1782
	-0.2835
	-0.093
	-0.0033

	Base
	96
	13
	Comb6
	Combination
	
	
	
	-0.0547
	0.016
	2.384
	0.0636
	-0.0571
	-0.0018

	Base
	96
	13
	Comb7
	Combination
	Max
	
	
	-0.029
	0.0231
	2.386
	0.0809
	0.0244
	0.0027

	Base
	96
	13
	Comb7
	Combination
	Min
	
	
	-0.0804
	0.0089
	2.382
	0.0464
	-0.1385
	-0.0062

	Base
	96
	13
	Comb8
	Combination
	Max
	
	
	-0.0494
	0.1674
	2.3844
	0.432
	-0.0401
	-0.0009

	Base
	96
	13
	Comb8
	Combination
	Min
	
	
	-0.06
	-0.1354
	2.3835
	-0.3047
	-0.074
	-0.0027

	Base
	96
	13
	ENVDIS
	Combination
	Max
	
	
	-0.029
	0.1727
	3.7084
	0.4532
	0.0244
	0.0027

	Base
	96
	13
	ENVDIS
	Combination
	Min
	
	
	-0.0987
	-0.1354
	2.382
	-0.3047
	-0.1576
	-0.0068

	Base
	96
	13
	Serv1
	Combination
	
	
	
	-0.0608
	0.0177
	2.6489
	0.0707
	-0.0634
	-0.002

	Base
	96
	13
	Serv2
	Combination
	
	
	
	-0.0608
	0.0177
	2.6489
	0.0707
	-0.0634
	-0.002

	Base
	96
	13
	Serv3
	Combination
	
	
	
	-0.0608
	0.0177
	2.6489
	0.0707
	-0.0634
	-0.002

	Base
	96
	13
	Serv4
	Combination
	Max
	
	
	-0.0428
	0.0227
	2.6503
	0.0828
	-0.0064
	0.0011

	Base
	96
	13
	Serv4
	Combination
	Min
	
	
	-0.0788
	0.0128
	2.6475
	0.0586
	-0.1204
	-0.0051

	Base
	96
	13
	Serv5
	Combination
	Max
	
	
	-0.057
	0.1237
	2.6492
	0.3285
	-0.0516
	-0.0014

	Base
	96
	13
	Serv5
	Combination
	Min
	
	
	-0.0645
	-0.0882
	2.6485
	-0.187
	-0.0752
	-0.0026

	Base
	96
	13
	Serv6
	Combination
	Max
	
	
	-0.0473
	0.0215
	2.6499
	0.0797
	-0.0206
	0.0003

	Base
	96
	13
	Serv6
	Combination
	Min
	
	
	-0.0743
	0.014
	2.6478
	0.0617
	-0.1062
	-0.0043

	Base
	96
	13
	Serv7
	Combination
	Max
	
	
	-0.058
	0.0972
	2.6491
	0.264
	-0.0545
	-0.0015

	Base
	96
	13
	Serv7
	Combination
	Min
	
	
	-0.0636
	-0.0617
	2.6486
	-0.1226
	-0.0723
	-0.0025

	Base
	96
	13
	Serv8
	Combination
	
	
	
	-0.0365
	0.0106
	1.5893
	0.0424
	-0.038
	-0.0012

	Base
	96
	13
	Serv9
	Combination
	Max
	
	
	-0.0185
	0.0156
	1.5907
	0.0545
	0.019
	0.0019

	Base
	96
	13
	Serv9
	Combination
	Min
	
	
	-0.0545
	0.0057
	1.5879
	0.0304
	-0.0951
	-0.0043

	Base
	96
	13
	Serv10
	Combination
	Max
	
	
	-0.0327
	0.1166
	1.5896
	0.3002
	-0.0262
	-0.0006

	Base
	96
	13
	Serv10
	Combination
	Min
	
	
	-0.0402
	-0.0953
	1.589
	-0.2153
	-0.0499
	-0.0018

	Base
	96
	13
	ENVSERV
	Combination
	Max
	
	
	-0.0185
	0.1237
	2.6503
	0.3285
	0.019
	0.0019

	Base
	96
	13
	ENVSERV
	Combination
	Min
	
	
	-0.0788
	-0.0953
	1.5879
	-0.2153
	-0.1204
	-0.0051

	Base
	98
	18
	Dead
	LinStatic
	
	
	
	0.0756
	-0.0505
	2.1838
	0.1483
	0.11
	-0.0024

	Base
	98
	18
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	98
	18
	FHEx
	LinStatic
	
	
	
	-0.1366
	-0.0596
	0.0132
	0.1435
	-0.4336
	0.0283

	Base
	98
	18
	FHEy
	LinStatic
	
	
	
	0.0041
	-1.0565
	0.0574
	2.5434
	0.0109
	-0.0008

	Base
	98
	18
	Sx
	LinRespSpec
	Max
	
	
	0.1114
	0.0741
	0.0118
	0.1783
	0.3541
	0.0275

	Base
	98
	18
	Sy
	LinRespSpec
	Max
	
	
	0.0248
	1.0726
	0.0575
	2.582
	0.0779
	0.006

	Base
	98
	18
	Comb1
	Combination
	
	
	
	0.1058
	-0.0707
	3.0573
	0.2076
	0.1541
	-0.0033

	Base
	98
	18
	Comb2
	Combination
	
	
	
	0.0907
	-0.0606
	2.6205
	0.1779
	0.1321
	-0.0028

	Base
	98
	18
	Comb3
	Combination
	
	
	
	0.0907
	-0.0606
	2.6205
	0.1779
	0.1321
	-0.0028

	Base
	98
	18
	Comb4
	Combination
	Max
	
	
	0.1066
	-0.05
	2.6222
	0.2034
	0.1826
	0.0011

	Base
	98
	18
	Comb4
	Combination
	Min
	
	
	0.0748
	-0.0712
	2.6188
	0.1525
	0.0815
	-0.0067

	Base
	98
	18
	Comb5
	Combination
	Max
	
	
	0.0942
	0.0927
	2.6287
	0.5469
	0.1432
	-0.002

	Base
	98
	18
	Comb5
	Combination
	Min
	
	
	0.0871
	-0.2139
	2.6123
	-0.191
	0.1209
	-0.0037

	Base
	98
	18
	Comb6
	Combination
	
	
	
	0.068
	-0.0454
	1.9654
	0.1335
	0.099
	-0.0021

	Base
	98
	18
	Comb7
	Combination
	Max
	
	
	0.0839
	-0.0349
	1.9671
	0.1589
	0.1496
	0.0018

	Base
	98
	18
	Comb7
	Combination
	Min
	
	
	0.0521
	-0.056
	1.9637
	0.108
	0.0485
	-0.006

	Base
	98
	18
	Comb8
	Combination
	Max
	
	
	0.0716
	0.1078
	1.9736
	0.5024
	0.1102
	-0.0013

	Base
	98
	18
	Comb8
	Combination
	Min
	
	
	0.0645
	-0.1987
	1.9572
	-0.2355
	0.0879
	-0.003

	Base
	98
	18
	ENVDIS
	Combination
	Max
	
	
	0.1066
	0.1078
	3.0573
	0.5469
	0.1826
	0.0018

	Base
	98
	18
	ENVDIS
	Combination
	Min
	
	
	0.0521
	-0.2139
	1.9572
	-0.2355
	0.0485
	-0.0067

	Base
	98
	18
	Serv1
	Combination
	
	
	
	0.0756
	-0.0505
	2.1838
	0.1483
	0.11
	-0.0024

	Base
	98
	18
	Serv2
	Combination
	
	
	
	0.0756
	-0.0505
	2.1838
	0.1483
	0.11
	-0.0024

	Base
	98
	18
	Serv3
	Combination
	
	
	
	0.0756
	-0.0505
	2.1838
	0.1483
	0.11
	-0.0024

	Base
	98
	18
	Serv4
	Combination
	Max
	
	
	0.0867
	-0.0431
	2.1849
	0.1661
	0.1455
	0.0004

	Base
	98
	18
	Serv4
	Combination
	Min
	
	
	0.0644
	-0.0579
	2.1826
	0.1305
	0.0746
	-0.0051

	Base
	98
	18
	Serv5
	Combination
	Max
	
	
	0.0781
	0.0568
	2.1895
	0.4065
	0.1178
	-0.0018

	Base
	98
	18
	Serv5
	Combination
	Min
	
	
	0.0731
	-0.1578
	2.178
	-0.1099
	0.1023
	-0.0029

	Base
	98
	18
	Serv6
	Combination
	Max
	
	
	0.0839
	-0.0449
	2.1847
	0.1617
	0.1366
	-0.0003

	Base
	98
	18
	Serv6
	Combination
	Min
	
	
	0.0672
	-0.056
	2.1829
	0.1349
	0.0835
	-0.0044

	Base
	98
	18
	Serv7
	Combination
	Max
	
	
	0.0774
	0.03
	2.1881
	0.3419
	0.1159
	-0.0019

	Base
	98
	18
	Serv7
	Combination
	Min
	
	
	0.0737
	-0.1309
	2.1795
	-0.0454
	0.1042
	-0.0028

	Base
	98
	18
	Serv8
	Combination
	
	
	
	0.0453
	-0.0303
	1.3103
	0.089
	0.066
	-0.0014

	Base
	98
	18
	Serv9
	Combination
	Max
	
	
	0.0565
	-0.0229
	1.3114
	0.1068
	0.1014
	0.0013

	Base
	98
	18
	Serv9
	Combination
	Min
	
	
	0.0342
	-0.0377
	1.3091
	0.0711
	0.0306
	-0.0042

	Base
	98
	18
	Serv10
	Combination
	Max
	
	
	0.0478
	0.077
	1.316
	0.3472
	0.0738
	-0.0008

	Base
	98
	18
	Serv10
	Combination
	Min
	
	
	0.0429
	-0.1376
	1.3045
	-0.1692
	0.0582
	-0.002

	Base
	98
	18
	ENVSERV
	Combination
	Max
	
	
	0.0867
	0.077
	2.1895
	0.4065
	0.1455
	0.0013

	Base
	98
	18
	ENVSERV
	Combination
	Min
	
	
	0.0342
	-0.1578
	1.3045
	-0.1692
	0.0306
	-0.0051

	Base
	99
	17
	Dead
	LinStatic
	
	
	
	-0.0733
	-0.0868
	2.2596
	0.2024
	-0.0866
	-0.0006

	Base
	99
	17
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	99
	17
	FHEx
	LinStatic
	
	
	
	-0.1376
	0.0421
	-0.0103
	-0.102
	-0.4364
	0.0272

	Base
	99
	17
	FHEy
	LinStatic
	
	
	
	-0.002
	-1.0448
	0.0215
	2.5281
	-0.0029
	-0.0015

	Base
	99
	17
	Sx
	LinRespSpec
	Max
	
	
	0.1122
	0.0436
	0.0087
	0.1053
	0.3563
	0.0278

	Base
	99
	17
	Sy
	LinRespSpec
	Max
	
	
	0.0229
	1.0654
	0.0219
	2.5778
	0.0733
	0.0064

	Base
	99
	17
	Comb1
	Combination
	
	
	
	-0.1027
	-0.1215
	3.1635
	0.2833
	-0.1213
	-0.0008

	Base
	99
	17
	Comb2
	Combination
	
	
	
	-0.088
	-0.1041
	2.7115
	0.2429
	-0.1039
	-0.0007

	Base
	99
	17
	Comb3
	Combination
	
	
	
	-0.088
	-0.1041
	2.7115
	0.2429
	-0.1039
	-0.0007

	Base
	99
	17
	Comb4
	Combination
	Max
	
	
	-0.072
	-0.0979
	2.7128
	0.2579
	-0.053
	0.0033

	Base
	99
	17
	Comb4
	Combination
	Min
	
	
	-0.104
	-0.1104
	2.7103
	0.2278
	-0.1548
	-0.0047

	Base
	99
	17
	Comb5
	Combination
	Max
	
	
	-0.0847
	0.0481
	2.7147
	0.6112
	-0.0935
	0.0002

	Base
	99
	17
	Comb5
	Combination
	Min
	
	
	-0.0913
	-0.2564
	2.7084
	-0.1255
	-0.1144
	-0.0016

	Base
	99
	17
	Comb6
	Combination
	
	
	
	-0.066
	-0.0781
	2.0337
	0.1822
	-0.078
	-0.0005

	Base
	99
	17
	Comb7
	Combination
	Max
	
	
	-0.05
	-0.0719
	2.0349
	0.1972
	-0.0271
	0.0034

	Base
	99
	17
	Comb7
	Combination
	Min
	
	
	-0.082
	-0.0843
	2.0324
	0.1671
	-0.1289
	-0.0045

	Base
	99
	17
	Comb8
	Combination
	Max
	
	
	-0.0627
	0.0741
	2.0368
	0.5505
	-0.0675
	0.0004

	Base
	99
	17
	Comb8
	Combination
	Min
	
	
	-0.0693
	-0.2303
	2.0305
	-0.1862
	-0.0884
	-0.0014

	Base
	99
	17
	ENVDIS
	Combination
	Max
	
	
	-0.05
	0.0741
	3.1635
	0.6112
	-0.0271
	0.0034

	Base
	99
	17
	ENVDIS
	Combination
	Min
	
	
	-0.104
	-0.2564
	2.0305
	-0.1862
	-0.1548
	-0.0047

	Base
	99
	17
	Serv1
	Combination
	
	
	
	-0.0733
	-0.0868
	2.2596
	0.2024
	-0.0866
	-0.0006

	Base
	99
	17
	Serv2
	Combination
	
	
	
	-0.0733
	-0.0868
	2.2596
	0.2024
	-0.0866
	-0.0006

	Base
	99
	17
	Serv3
	Combination
	
	
	
	-0.0733
	-0.0868
	2.2596
	0.2024
	-0.0866
	-0.0006

	Base
	99
	17
	Serv4
	Combination
	Max
	
	
	-0.0621
	-0.0824
	2.2605
	0.2129
	-0.051
	0.0022

	Base
	99
	17
	Serv4
	Combination
	Min
	
	
	-0.0845
	-0.0911
	2.2587
	0.1919
	-0.1222
	-0.0034

	Base
	99
	17
	Serv5
	Combination
	Max
	
	
	-0.071
	0.0198
	2.2618
	0.4602
	-0.0793
	4.787E-05

	Base
	99
	17
	Serv5
	Combination
	Min
	
	
	-0.0756
	-0.1933
	2.2574
	-0.0554
	-0.094
	-0.0012

	Base
	99
	17
	Serv6
	Combination
	Max
	
	
	-0.0649
	-0.0835
	2.2603
	0.2103
	-0.0599
	0.0015

	Base
	99
	17
	Serv6
	Combination
	Min
	
	
	-0.0817
	-0.09
	2.259
	0.1945
	-0.1133
	-0.0027

	Base
	99
	17
	Serv7
	Combination
	Max
	
	
	-0.0716
	-0.0069
	2.2613
	0.3957
	-0.0811
	-0.0001

	Base
	99
	17
	Serv7
	Combination
	Min
	
	
	-0.075
	-0.1667
	2.258
	0.0091
	-0.0921
	-0.0011

	Base
	99
	17
	Serv8
	Combination
	
	
	
	-0.044
	-0.0521
	1.3558
	0.1214
	-0.052
	-0.0004

	Base
	99
	17
	Serv9
	Combination
	Max
	
	
	-0.0328
	-0.0477
	1.3566
	0.132
	-0.0163
	0.0024

	Base
	99
	17
	Serv9
	Combination
	Min
	
	
	-0.0552
	-0.0564
	1.3549
	0.1109
	-0.0876
	-0.0031

	Base
	99
	17
	Serv10
	Combination
	Max
	
	
	-0.0417
	0.0545
	1.358
	0.3792
	-0.0446
	0.0003

	Base
	99
	17
	Serv10
	Combination
	Min
	
	
	-0.0463
	-0.1586
	1.3536
	-0.1363
	-0.0593
	-0.001

	Base
	99
	17
	ENVSERV
	Combination
	Max
	
	
	-0.0328
	0.0545
	2.2618
	0.4602
	-0.0163
	0.0024

	Base
	99
	17
	ENVSERV
	Combination
	Min
	
	
	-0.0845
	-0.1933
	1.3536
	-0.1363
	-0.1222
	-0.0034

	Base
	104
	116
	Dead
	LinStatic
	
	
	
	-1.4511
	-1.7459
	13.3729
	0.1006
	0.0244
	0.0139

	Base
	104
	116
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	104
	116
	FHEx
	LinStatic
	
	
	
	-0.4096
	-1.0133
	11.6783
	-0.31
	-1.199
	-0.6188

	Base
	104
	116
	FHEy
	LinStatic
	
	
	
	-3.3057
	-5.0361
	44.6263
	2.8743
	-0.8466
	0.7888

	Base
	104
	116
	Sx
	LinRespSpec
	Max
	
	
	2.5877
	0.9807
	12.3885
	0.3387
	0.9693
	1.9015

	Base
	104
	116
	Sy
	LinRespSpec
	Max
	
	
	2.0736
	5.3948
	37.0986
	1.8572
	1.2303
	1.2985

	Base
	104
	116
	Comb1
	Combination
	
	
	
	-2.0316
	-2.4442
	18.722
	0.1409
	0.0342
	0.0194

	Base
	104
	116
	Comb2
	Combination
	
	
	
	-1.7414
	-2.095
	16.0475
	0.1208
	0.0293
	0.0166

	Base
	104
	116
	Comb3
	Combination
	
	
	
	-1.7414
	-2.095
	16.0475
	0.1208
	0.0293
	0.0166

	Base
	104
	116
	Comb4
	Combination
	Max
	
	
	-1.3717
	-1.9549
	17.8173
	0.1691
	0.1678
	0.2883

	Base
	104
	116
	Comb4
	Combination
	Min
	
	
	-2.111
	-2.2351
	14.2777
	0.0724
	-0.1092
	-0.255

	Base
	104
	116
	Comb5
	Combination
	Max
	
	
	-1.4451
	-1.3241
	21.3489
	0.3862
	0.2051
	0.2022

	Base
	104
	116
	Comb5
	Combination
	Min
	
	
	-2.0377
	-2.866
	10.7461
	-0.1446
	-0.1465
	-0.1689

	Base
	104
	116
	Comb6
	Combination
	
	
	
	-1.306
	-1.5713
	12.0356
	0.0906
	0.022
	0.0125

	Base
	104
	116
	Comb7
	Combination
	Max
	
	
	-0.9364
	-1.4312
	13.8054
	0.139
	0.1605
	0.2841

	Base
	104
	116
	Comb7
	Combination
	Min
	
	
	-1.6757
	-1.7114
	10.2658
	0.0422
	-0.1165
	-0.2592

	Base
	104
	116
	Comb8
	Combination
	Max
	
	
	-1.0097
	-0.8004
	17.337
	0.356
	0.1978
	0.198

	Base
	104
	116
	Comb8
	Combination
	Min
	
	
	-1.6023
	-2.3422
	6.7342
	-0.1748
	-0.1538
	-0.1731

	Base
	104
	116
	ENVDIS
	Combination
	Max
	
	
	-0.9364
	-0.8004
	21.3489
	0.3862
	0.2051
	0.2883

	Base
	104
	116
	ENVDIS
	Combination
	Min
	
	
	-2.111
	-2.866
	6.7342
	-0.1748
	-0.1538
	-0.2592

	Base
	104
	116
	Serv1
	Combination
	
	
	
	-1.4511
	-1.7459
	13.3729
	0.1006
	0.0244
	0.0139

	Base
	104
	116
	Serv2
	Combination
	
	
	
	-1.4511
	-1.7459
	13.3729
	0.1006
	0.0244
	0.0139

	Base
	104
	116
	Serv3
	Combination
	
	
	
	-1.4511
	-1.7459
	13.3729
	0.1006
	0.0244
	0.0139

	Base
	104
	116
	Serv4
	Combination
	Max
	
	
	-1.1924
	-1.6478
	14.6117
	0.1345
	0.1214
	0.204

	Base
	104
	116
	Serv4
	Combination
	Min
	
	
	-1.7099
	-1.8439
	12.134
	0.0668
	-0.0725
	-0.1763

	Base
	104
	116
	Serv5
	Combination
	Max
	
	
	-1.2438
	-1.2064
	17.0828
	0.2864
	0.1475
	0.1437

	Base
	104
	116
	Serv5
	Combination
	Min
	
	
	-1.6585
	-2.2853
	9.663
	-0.0851
	-0.0986
	-0.116

	Base
	104
	116
	Serv6
	Combination
	Max
	
	
	-1.2571
	-1.6723
	14.302
	0.126
	0.0971
	0.1565

	Base
	104
	116
	Serv6
	Combination
	Min
	
	
	-1.6452
	-1.8194
	12.4438
	0.0752
	-0.0483
	-0.1288

	Base
	104
	116
	Serv7
	Combination
	Max
	
	
	-1.2956
	-1.3413
	16.1553
	0.2399
	0.1167
	0.1112

	Base
	104
	116
	Serv7
	Combination
	Min
	
	
	-1.6067
	-2.1505
	10.5905
	-0.0387
	-0.0679
	-0.0835

	Base
	104
	116
	Serv8
	Combination
	
	
	
	-0.8707
	-1.0475
	8.0237
	0.0604
	0.0147
	0.0083

	Base
	104
	116
	Serv9
	Combination
	Max
	
	
	-0.6119
	-0.9494
	9.2626
	0.0943
	0.1116
	0.1985

	Base
	104
	116
	Serv9
	Combination
	Min
	
	
	-1.1295
	-1.1456
	6.7849
	0.0265
	-0.0823
	-0.1818

	Base
	104
	116
	Serv10
	Combination
	Max
	
	
	-0.6633
	-0.508
	11.7336
	0.2461
	0.1377
	0.1382

	Base
	104
	116
	Serv10
	Combination
	Min
	
	
	-1.078
	-1.587
	4.3139
	-0.1253
	-0.1084
	-0.1215

	Base
	104
	116
	ENVSERV
	Combination
	Max
	
	
	-0.6119
	-0.508
	17.0828
	0.2864
	0.1475
	0.204

	Base
	104
	116
	ENVSERV
	Combination
	Min
	
	
	-1.7099
	-2.2853
	4.3139
	-0.1253
	-0.1084
	-0.1818

	Base
	105
	128
	Dead
	LinStatic
	
	
	
	0.0089
	-1.7534
	7.3512
	0.0602
	0.0039
	0.0033

	Base
	105
	128
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	105
	128
	FHEx
	LinStatic
	
	
	
	-0.5322
	-0.02
	-1.8943
	-0.135
	-0.0595
	-0.6241

	Base
	105
	128
	FHEy
	LinStatic
	
	
	
	0.1414
	-5.5534
	26.6786
	2.1242
	0.0706
	0.0815

	Base
	105
	128
	Sx
	LinRespSpec
	Max
	
	
	1.1773
	0.7416
	5.4648
	0.4244
	0.0662
	1.3517

	Base
	105
	128
	Sy
	LinRespSpec
	Max
	
	
	0.2545
	4.723
	18.7172
	1.4908
	0.0714
	0.2475

	Base
	105
	128
	Comb1
	Combination
	
	
	
	0.0124
	-2.4548
	10.2917
	0.0842
	0.0055
	0.0046

	Base
	105
	128
	Comb2
	Combination
	
	
	
	0.0106
	-2.1041
	8.8215
	0.0722
	0.0047
	0.004

	Base
	105
	128
	Comb3
	Combination
	
	
	
	0.0106
	-2.1041
	8.8215
	0.0722
	0.0047
	0.004

	Base
	105
	128
	Comb4
	Combination
	Max
	
	
	0.1788
	-1.9981
	9.6021
	0.1328
	0.0141
	0.1971

	Base
	105
	128
	Comb4
	Combination
	Min
	
	
	-0.1575
	-2.21
	8.0408
	0.0116
	-0.0048
	-0.1891

	Base
	105
	128
	Comb5
	Combination
	Max
	
	
	0.047
	-1.4292
	11.4962
	0.2852
	0.0149
	0.0393

	Base
	105
	128
	Comb5
	Combination
	Min
	
	
	-0.0257
	-2.779
	6.1468
	-0.1408
	-0.0055
	-0.0314

	Base
	105
	128
	Comb6
	Combination
	
	
	
	0.008
	-1.5781
	6.6161
	0.0542
	0.0035
	0.003

	Base
	105
	128
	Comb7
	Combination
	Max
	
	
	0.1762
	-1.4721
	7.3968
	0.1148
	0.013
	0.1961

	Base
	105
	128
	Comb7
	Combination
	Min
	
	
	-0.1602
	-1.684
	5.8354
	-0.0065
	-0.0059
	-0.1901

	Base
	105
	128
	Comb8
	Combination
	Max
	
	
	0.0443
	-0.9031
	9.2908
	0.2672
	0.0137
	0.0383

	Base
	105
	128
	Comb8
	Combination
	Min
	
	
	-0.0284
	-2.253
	3.9414
	-0.1589
	-0.0067
	-0.0324

	Base
	105
	128
	ENVDIS
	Combination
	Max
	
	
	0.1788
	-0.9031
	11.4962
	0.2852
	0.0149
	0.1971

	Base
	105
	128
	ENVDIS
	Combination
	Min
	
	
	-0.1602
	-2.779
	3.9414
	-0.1589
	-0.0067
	-0.1901

	Base
	105
	128
	Serv1
	Combination
	
	
	
	0.0089
	-1.7534
	7.3512
	0.0602
	0.0039
	0.0033

	Base
	105
	128
	Serv2
	Combination
	
	
	
	0.0089
	-1.7534
	7.3512
	0.0602
	0.0039
	0.0033

	Base
	105
	128
	Serv3
	Combination
	
	
	
	0.0089
	-1.7534
	7.3512
	0.0602
	0.0039
	0.0033

	Base
	105
	128
	Serv4
	Combination
	Max
	
	
	0.1266
	-1.6792
	7.8977
	0.1026
	0.0105
	0.1385

	Base
	105
	128
	Serv4
	Combination
	Min
	
	
	-0.1089
	-1.8276
	6.8047
	0.0177
	-0.0027
	-0.1319

	Base
	105
	128
	Serv5
	Combination
	Max
	
	
	0.0343
	-1.2811
	9.2229
	0.2092
	0.011
	0.0281

	Base
	105
	128
	Serv5
	Combination
	Min
	
	
	-0.0166
	-2.2257
	5.4795
	-0.0889
	-0.0032
	-0.0214

	Base
	105
	128
	Serv6
	Combination
	Max
	
	
	0.0972
	-1.6978
	7.7611
	0.092
	0.0089
	0.1047

	Base
	105
	128
	Serv6
	Combination
	Min
	
	
	-0.0794
	-1.809
	6.9414
	0.0283
	-0.0011
	-0.0981

	Base
	105
	128
	Serv7
	Combination
	Max
	
	
	0.028
	-1.3992
	8.755
	0.172
	0.0093
	0.0219

	Base
	105
	128
	Serv7
	Combination
	Min
	
	
	-0.0102
	-2.1076
	5.9474
	-0.0516
	-0.0015
	-0.0153

	Base
	105
	128
	Serv8
	Combination
	
	
	
	0.0053
	-1.052
	4.4107
	0.0361
	0.0023
	0.002

	Base
	105
	128
	Serv9
	Combination
	Max
	
	
	0.1231
	-0.9779
	4.9572
	0.0785
	0.009
	0.1371

	Base
	105
	128
	Serv9
	Combination
	Min
	
	
	-0.1124
	-1.1262
	3.8643
	-0.0063
	-0.0043
	-0.1332

	Base
	105
	128
	Serv10
	Combination
	Max
	
	
	0.0308
	-0.5797
	6.2825
	0.1852
	0.0095
	0.0267

	Base
	105
	128
	Serv10
	Combination
	Min
	
	
	-0.0201
	-1.5243
	2.539
	-0.113
	-0.0048
	-0.0228

	Base
	105
	128
	ENVSERV
	Combination
	Max
	
	
	0.1266
	-0.5797
	9.2229
	0.2092
	0.011
	0.1385

	Base
	105
	128
	ENVSERV
	Combination
	Min
	
	
	-0.1124
	-2.2257
	2.539
	-0.113
	-0.0048
	-0.1332

	Base
	106
	88
	Dead
	LinStatic
	
	
	
	5.3515
	0.0396
	39.6055
	-0.0032
	1.1349
	0.1024

	Base
	106
	88
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	106
	88
	FHEx
	LinStatic
	
	
	
	-30.9821
	1.5591
	-36.2163
	-0.8009
	-10.6154
	2.259

	Base
	106
	88
	FHEy
	LinStatic
	
	
	
	29.0626
	4.6673
	149.5366
	-7.6995
	13.6691
	0.7337

	Base
	106
	88
	Sx
	LinRespSpec
	Max
	
	
	10.0595
	1.3315
	20.7649
	0.7845
	5.3772
	2.2147

	Base
	106
	88
	Sy
	LinRespSpec
	Max
	
	
	31.8986
	5.1892
	148.8936
	8.0799
	14.9047
	2.1265

	Base
	106
	88
	Comb1
	Combination
	
	
	
	7.4921
	0.0554
	55.4477
	-0.0045
	1.5889
	0.1434

	Base
	106
	88
	Comb2
	Combination
	
	
	
	6.4218
	0.0475
	47.5266
	-0.0039
	1.3619
	0.1229

	Base
	106
	88
	Comb3
	Combination
	
	
	
	6.4218
	0.0475
	47.5266
	-0.0039
	1.3619
	0.1229

	Base
	106
	88
	Comb4
	Combination
	Max
	
	
	7.8589
	0.2377
	50.493
	0.1082
	2.1301
	0.4393

	Base
	106
	88
	Comb4
	Combination
	Min
	
	
	4.9848
	-0.1427
	44.5602
	-0.116
	0.5938
	-0.1935

	Base
	106
	88
	Comb5
	Combination
	Max
	
	
	10.9802
	0.789
	68.8035
	1.1507
	3.4918
	0.4268

	Base
	106
	88
	Comb5
	Combination
	Min
	
	
	1.8635
	-0.694
	26.2497
	-1.1585
	-0.768
	-0.181

	Base
	106
	88
	Comb6
	Combination
	
	
	
	4.8164
	0.0356
	35.645
	-0.0029
	1.0214
	0.0922

	Base
	106
	88
	Comb7
	Combination
	Max
	
	
	6.2535
	0.2258
	38.6114
	0.1092
	1.7896
	0.4086

	Base
	106
	88
	Comb7
	Combination
	Min
	
	
	3.3793
	-0.1546
	32.6786
	-0.115
	0.2533
	-0.2242

	Base
	106
	88
	Comb8
	Combination
	Max
	
	
	9.3747
	0.7772
	56.9219
	1.1517
	3.1513
	0.396

	Base
	106
	88
	Comb8
	Combination
	Min
	
	
	0.2581
	-0.7059
	14.3681
	-1.1575
	-1.1084
	-0.2117

	Base
	106
	88
	ENVDIS
	Combination
	Max
	
	
	10.9802
	0.789
	68.8035
	1.1517
	3.4918
	0.4393

	Base
	106
	88
	ENVDIS
	Combination
	Min
	
	
	0.2581
	-0.7059
	14.3681
	-1.1585
	-1.1084
	-0.2242

	Base
	106
	88
	Serv1
	Combination
	
	
	
	5.3515
	0.0396
	39.6055
	-0.0032
	1.1349
	0.1024

	Base
	106
	88
	Serv2
	Combination
	
	
	
	5.3515
	0.0396
	39.6055
	-0.0032
	1.1349
	0.1024

	Base
	106
	88
	Serv3
	Combination
	
	
	
	5.3515
	0.0396
	39.6055
	-0.0032
	1.1349
	0.1024

	Base
	106
	88
	Serv4
	Combination
	Max
	
	
	6.3575
	0.1727
	41.682
	0.0752
	1.6727
	0.3239

	Base
	106
	88
	Serv4
	Combination
	Min
	
	
	4.3456
	-0.0936
	37.529
	-0.0817
	0.5972
	-0.1191

	Base
	106
	88
	Serv5
	Combination
	Max
	
	
	8.5414
	0.5585
	54.4949
	0.8048
	2.6254
	0.3151

	Base
	106
	88
	Serv5
	Combination
	Min
	
	
	2.1617
	-0.4793
	24.7162
	-0.8112
	-0.3555
	-0.1102

	Base
	106
	88
	Serv6
	Combination
	Max
	
	
	6.106
	0.1395
	41.1629
	0.0556
	1.5382
	0.2685

	Base
	106
	88
	Serv6
	Combination
	Min
	
	
	4.5971
	-0.0603
	38.0482
	-0.0621
	0.7317
	-0.0637

	Base
	106
	88
	Serv7
	Combination
	Max
	
	
	7.7439
	0.4288
	50.7725
	0.6028
	2.2528
	0.2619

	Base
	106
	88
	Serv7
	Combination
	Min
	
	
	2.9591
	-0.3496
	28.4385
	-0.6092
	0.0171
	-0.0571

	Base
	106
	88
	Serv8
	Combination
	
	
	
	3.2109
	0.0238
	23.7633
	-0.0019
	0.681
	0.0615

	Base
	106
	88
	Serv9
	Combination
	Max
	
	
	4.2169
	0.1569
	25.8398
	0.0765
	1.2187
	0.2829

	Base
	106
	88
	Serv9
	Combination
	Min
	
	
	2.205
	-0.1094
	21.6868
	-0.0804
	0.1432
	-0.16

	Base
	106
	88
	Serv10
	Combination
	Max
	
	
	6.4008
	0.5427
	38.6527
	0.806
	2.1714
	0.2741

	Base
	106
	88
	Serv10
	Combination
	Min
	
	
	0.0211
	-0.4952
	8.8739
	-0.8099
	-0.8095
	-0.1512

	Base
	106
	88
	ENVSERV
	Combination
	Max
	
	
	8.5414
	0.5585
	54.4949
	0.806
	2.6254
	0.3239

	Base
	106
	88
	ENVSERV
	Combination
	Min
	
	
	0.0211
	-0.4952
	8.8739
	-0.8112
	-0.8095
	-0.16

	Base
	107
	81
	Dead
	LinStatic
	
	
	
	4.1294
	2.4158
	18.8483
	-2.1918
	-0.1446
	-1.0987

	Base
	107
	81
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	107
	81
	FHEx
	LinStatic
	
	
	
	-34.3062
	-4.9271
	-69.2751
	-1.2211
	-12.9622
	-0.7909

	Base
	107
	81
	FHEy
	LinStatic
	
	
	
	6.8112
	-3.8763
	-265.0443
	-7.9387
	15.0798
	-4.2789

	Base
	107
	81
	Sx
	LinRespSpec
	Max
	
	
	10.7217
	4.268
	43.7538
	1.3317
	5.8808
	3.5687

	Base
	107
	81
	Sy
	LinRespSpec
	Max
	
	
	7.6539
	2.6734
	254.2903
	8.5554
	15.3952
	5.0335

	Base
	107
	81
	Comb1
	Combination
	
	
	
	5.7811
	3.3821
	26.3876
	-3.0685
	-0.2024
	-1.5382

	Base
	107
	81
	Comb2
	Combination
	
	
	
	4.9552
	2.899
	22.6179
	-2.6302
	-0.1735
	-1.3185

	Base
	107
	81
	Comb3
	Combination
	
	
	
	4.9552
	2.899
	22.6179
	-2.6302
	-0.1735
	-1.3185

	Base
	107
	81
	Comb4
	Combination
	Max
	
	
	6.4869
	3.5087
	28.8685
	-2.4399
	0.6666
	-0.8087

	Base
	107
	81
	Comb4
	Combination
	Min
	
	
	3.4236
	2.2893
	16.3674
	-2.8204
	-1.0136
	-1.8283

	Base
	107
	81
	Comb5
	Combination
	Max
	
	
	6.049
	3.281
	58.956
	-1.4076
	2.0265
	-0.5992

	Base
	107
	81
	Comb5
	Combination
	Min
	
	
	3.8615
	2.5169
	-13.7202
	-3.8527
	-2.3735
	-2.0378

	Base
	107
	81
	Comb6
	Combination
	
	
	
	3.7164
	2.1742
	16.9634
	-1.9726
	-0.1301
	-0.9889

	Base
	107
	81
	Comb7
	Combination
	Max
	
	
	5.2481
	2.7839
	23.214
	-1.7824
	0.71
	-0.479

	Base
	107
	81
	Comb7
	Combination
	Min
	
	
	2.1848
	1.5645
	10.7129
	-2.1629
	-0.9702
	-1.4987

	Base
	107
	81
	Comb8
	Combination
	Max
	
	
	4.8102
	2.5563
	53.3015
	-0.7501
	2.0699
	-0.2696

	Base
	107
	81
	Comb8
	Combination
	Min
	
	
	2.6227
	1.7922
	-19.3747
	-3.1952
	-2.3301
	-1.7081

	Base
	107
	81
	ENVDIS
	Combination
	Max
	
	
	6.4869
	3.5087
	58.956
	-0.7501
	2.0699
	-0.2696

	Base
	107
	81
	ENVDIS
	Combination
	Min
	
	
	2.1848
	1.5645
	-19.3747
	-3.8527
	-2.3735
	-2.0378

	Base
	107
	81
	Serv1
	Combination
	
	
	
	4.1294
	2.4158
	18.8483
	-2.1918
	-0.1446
	-1.0987

	Base
	107
	81
	Serv2
	Combination
	
	
	
	4.1294
	2.4158
	18.8483
	-2.1918
	-0.1446
	-1.0987

	Base
	107
	81
	Serv3
	Combination
	
	
	
	4.1294
	2.4158
	18.8483
	-2.1918
	-0.1446
	-1.0987

	Base
	107
	81
	Serv4
	Combination
	Max
	
	
	5.2015
	2.8426
	23.2236
	-2.0586
	0.4435
	-0.7419

	Base
	107
	81
	Serv4
	Combination
	Min
	
	
	3.0572
	1.989
	14.4729
	-2.325
	-0.7327
	-1.4556

	Base
	107
	81
	Serv5
	Combination
	Max
	
	
	4.8948
	2.6832
	44.2773
	-1.3363
	1.3949
	-0.5954

	Base
	107
	81
	Serv5
	Combination
	Min
	
	
	3.364
	2.1485
	-6.5808
	-3.0473
	-1.6841
	-1.6021

	Base
	107
	81
	Serv6
	Combination
	Max
	
	
	4.9335
	2.7359
	22.1298
	-2.0919
	0.2965
	-0.8311

	Base
	107
	81
	Serv6
	Combination
	Min
	
	
	3.3252
	2.0957
	15.5667
	-2.2917
	-0.5856
	-1.3664

	Base
	107
	81
	Serv7
	Combination
	Max
	
	
	4.7034
	2.6163
	37.92
	-1.5502
	1.0101
	-0.7212

	Base
	107
	81
	Serv7
	Combination
	Min
	
	
	3.5553
	2.2153
	-0.2235
	-2.8335
	-1.2992
	-1.4762

	Base
	107
	81
	Serv8
	Combination
	
	
	
	2.4776
	1.4495
	11.309
	-1.3151
	-0.0867
	-0.6592

	Base
	107
	81
	Serv9
	Combination
	Max
	
	
	3.5498
	1.8763
	15.6843
	-1.1819
	0.5013
	-0.3024

	Base
	107
	81
	Serv9
	Combination
	Min
	
	
	1.4054
	1.0227
	6.9336
	-1.4483
	-0.6748
	-1.0161

	Base
	107
	81
	Serv10
	Combination
	Max
	
	
	3.243
	1.7168
	36.738
	-0.4595
	1.4528
	-0.1559

	Base
	107
	81
	Serv10
	Combination
	Min
	
	
	1.7122
	1.1821
	-14.1201
	-2.1706
	-1.6263
	-1.1626

	Base
	107
	81
	ENVSERV
	Combination
	Max
	
	
	5.2015
	2.8426
	44.2773
	-0.4595
	1.4528
	-0.1559

	Base
	107
	81
	ENVSERV
	Combination
	Min
	
	
	1.4054
	1.0227
	-14.1201
	-3.0473
	-1.6841
	-1.6021

	Base
	108
	78
	Dead
	LinStatic
	
	
	
	-1.3508
	0.0027
	-5.2056
	-0.0306
	0.0412
	0.012

	Base
	108
	78
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	108
	78
	FHEx
	LinStatic
	
	
	
	4.6616
	-0.0026
	18.3445
	0.0259
	-0.1349
	0.0119

	Base
	108
	78
	FHEy
	LinStatic
	
	
	
	-5.3817
	2.4199
	-19.7158
	0.1511
	0.1574
	0.2213

	Base
	108
	78
	Sx
	LinRespSpec
	Max
	
	
	0.7065
	1.0807
	8.1654
	0.0349
	0.0604
	0.03

	Base
	108
	78
	Sy
	LinRespSpec
	Max
	
	
	4.9863
	2.3237
	20.3294
	0.1461
	0.1615
	0.213

	Base
	108
	78
	Comb1
	Combination
	
	
	
	-1.8911
	0.0038
	-7.2878
	-0.0428
	0.0577
	0.0168

	Base
	108
	78
	Comb2
	Combination
	
	
	
	-1.621
	0.0033
	-6.2467
	-0.0367
	0.0494
	0.0144

	Base
	108
	78
	Comb3
	Combination
	
	
	
	-1.621
	0.0033
	-6.2467
	-0.0367
	0.0494
	0.0144

	Base
	108
	78
	Comb4
	Combination
	Max
	
	
	-1.52
	0.1577
	-5.0802
	-0.0317
	0.0581
	0.0187

	Base
	108
	78
	Comb4
	Combination
	Min
	
	
	-1.7219
	-0.1511
	-7.4132
	-0.0417
	0.0408
	0.0101

	Base
	108
	78
	Comb5
	Combination
	Max
	
	
	-0.9084
	0.3354
	-3.3416
	-0.0158
	0.0725
	0.0448

	Base
	108
	78
	Comb5
	Combination
	Min
	
	
	-2.3335
	-0.3288
	-9.1518
	-0.0576
	0.0264
	-0.016

	Base
	108
	78
	Comb6
	Combination
	
	
	
	-1.2157
	0.0025
	-4.685
	-0.0275
	0.0371
	0.0108

	Base
	108
	78
	Comb7
	Combination
	Max
	
	
	-1.1148
	0.1569
	-3.5185
	-0.0225
	0.0457
	0.0151

	Base
	108
	78
	Comb7
	Combination
	Min
	
	
	-1.3167
	-0.1519
	-5.8515
	-0.0325
	0.0284
	0.0065

	Base
	108
	78
	Comb8
	Combination
	Max
	
	
	-0.5032
	0.3345
	-1.7799
	-0.0066
	0.0602
	0.0412

	Base
	108
	78
	Comb8
	Combination
	Min
	
	
	-1.9283
	-0.3296
	-7.5901
	-0.0484
	0.014
	-0.0196

	Base
	108
	78
	ENVDIS
	Combination
	Max
	
	
	-0.5032
	0.3354
	-1.7799
	-0.0066
	0.0725
	0.0448

	Base
	108
	78
	ENVDIS
	Combination
	Min
	
	
	-2.3335
	-0.3296
	-9.1518
	-0.0576
	0.014
	-0.0196

	Base
	108
	78
	Serv1
	Combination
	
	
	
	-1.3508
	0.0027
	-5.2056
	-0.0306
	0.0412
	0.012

	Base
	108
	78
	Serv2
	Combination
	
	
	
	-1.3508
	0.0027
	-5.2056
	-0.0306
	0.0412
	0.012

	Base
	108
	78
	Serv3
	Combination
	
	
	
	-1.3508
	0.0027
	-5.2056
	-0.0306
	0.0412
	0.012

	Base
	108
	78
	Serv4
	Combination
	Max
	
	
	-1.2802
	0.1108
	-4.389
	-0.0271
	0.0472
	0.015

	Base
	108
	78
	Serv4
	Combination
	Min
	
	
	-1.4215
	-0.1053
	-6.0221
	-0.0341
	0.0352
	0.009

	Base
	108
	78
	Serv5
	Combination
	Max
	
	
	-0.8522
	0.2351
	-3.1726
	-0.016
	0.0573
	0.0333

	Base
	108
	78
	Serv5
	Combination
	Min
	
	
	-1.8494
	-0.2296
	-7.2385
	-0.0452
	0.0251
	-0.0093

	Base
	108
	78
	Serv6
	Combination
	Max
	
	
	-1.2978
	0.0838
	-4.5932
	-0.028
	0.0457
	0.0142

	Base
	108
	78
	Serv6
	Combination
	Min
	
	
	-1.4038
	-0.0783
	-5.818
	-0.0332
	0.0367
	0.0097

	Base
	108
	78
	Serv7
	Combination
	Max
	
	
	-0.9768
	0.177
	-3.6809
	-0.0196
	0.0533
	0.028

	Base
	108
	78
	Serv7
	Combination
	Min
	
	
	-1.7248
	-0.1715
	-6.7303
	-0.0415
	0.0291
	-0.004

	Base
	108
	78
	Serv8
	Combination
	
	
	
	-0.8105
	0.0016
	-3.1233
	-0.0183
	0.0247
	0.0072

	Base
	108
	78
	Serv9
	Combination
	Max
	
	
	-0.7398
	0.1097
	-2.3068
	-0.0149
	0.0308
	0.0102

	Base
	108
	78
	Serv9
	Combination
	Min
	
	
	-0.8811
	-0.1064
	-3.9399
	-0.0218
	0.0187
	0.0042

	Base
	108
	78
	Serv10
	Combination
	Max
	
	
	-0.3119
	0.234
	-1.0904
	-0.0037
	0.0409
	0.0285

	Base
	108
	78
	Serv10
	Combination
	Min
	
	
	-1.3091
	-0.2307
	-5.1563
	-0.033
	0.0086
	-0.0141

	Base
	108
	78
	ENVSERV
	Combination
	Max
	
	
	-0.3119
	0.2351
	-1.0904
	-0.0037
	0.0573
	0.0333

	Base
	108
	78
	ENVSERV
	Combination
	Min
	
	
	-1.8494
	-0.2307
	-7.2385
	-0.0452
	0.0086
	-0.0141

	Base
	109
	85
	Dead
	LinStatic
	
	
	
	-2.261
	-4.0037
	61.2477
	0.6529
	-0.9678
	0.2229

	Base
	109
	85
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	109
	85
	FHEx
	LinStatic
	
	
	
	-40.8128
	-5.1948
	76.608
	-0.5675
	-15.0439
	-0.397

	Base
	109
	85
	FHEy
	LinStatic
	
	
	
	21.3903
	-11.398
	340.4657
	-1.131
	8.0446
	3.3055

	Base
	109
	85
	Sx
	LinRespSpec
	Max
	
	
	14.6761
	2.1357
	44.5425
	1.0784
	6.5743
	0.844

	Base
	109
	85
	Sy
	LinRespSpec
	Max
	
	
	24.8976
	10.7383
	341.2031
	0.9756
	9.4493
	3.5477

	Base
	109
	85
	Comb1
	Combination
	
	
	
	-3.1654
	-5.6052
	85.7468
	0.9141
	-1.355
	0.3121

	Base
	109
	85
	Comb2
	Combination
	
	
	
	-2.7132
	-4.8044
	73.4972
	0.7835
	-1.1614
	0.2675

	Base
	109
	85
	Comb3
	Combination
	
	
	
	-2.7132
	-4.8044
	73.4972
	0.7835
	-1.1614
	0.2675

	Base
	109
	85
	Comb4
	Combination
	Max
	
	
	-0.6166
	-4.4994
	79.8604
	0.9376
	-0.2222
	0.3881

	Base
	109
	85
	Comb4
	Combination
	Min
	
	
	-4.8098
	-5.1095
	67.134
	0.6294
	-2.1006
	0.147

	Base
	109
	85
	Comb5
	Combination
	Max
	
	
	0.8447
	-3.2699
	122.2551
	0.9229
	0.1889
	0.7745

	Base
	109
	85
	Comb5
	Combination
	Min
	
	
	-6.2711
	-6.3389
	24.7393
	0.6441
	-2.5117
	-0.2394

	Base
	109
	85
	Comb6
	Combination
	
	
	
	-2.0349
	-3.6033
	55.1229
	0.5876
	-0.8711
	0.2007

	Base
	109
	85
	Comb7
	Combination
	Max
	
	
	0.0617
	-3.2982
	61.4861
	0.7417
	0.0681
	0.3212

	Base
	109
	85
	Comb7
	Combination
	Min
	
	
	-4.1315
	-3.9084
	48.7597
	0.4336
	-1.8102
	0.0801

	Base
	109
	85
	Comb8
	Combination
	Max
	
	
	1.523
	-2.0688
	103.8808
	0.727
	0.4792
	0.7076

	Base
	109
	85
	Comb8
	Combination
	Min
	
	
	-5.5928
	-5.1378
	6.365
	0.4482
	-2.2214
	-0.3063

	Base
	109
	85
	ENVDIS
	Combination
	Max
	
	
	1.523
	-2.0688
	122.2551
	0.9376
	0.4792
	0.7745

	Base
	109
	85
	ENVDIS
	Combination
	Min
	
	
	-6.2711
	-6.3389
	6.365
	0.4336
	-2.5117
	-0.3063

	Base
	109
	85
	Serv1
	Combination
	
	
	
	-2.261
	-4.0037
	61.2477
	0.6529
	-0.9678
	0.2229

	Base
	109
	85
	Serv2
	Combination
	
	
	
	-2.261
	-4.0037
	61.2477
	0.6529
	-0.9678
	0.2229

	Base
	109
	85
	Serv3
	Combination
	
	
	
	-2.261
	-4.0037
	61.2477
	0.6529
	-0.9678
	0.2229

	Base
	109
	85
	Serv4
	Combination
	Max
	
	
	-0.7934
	-3.7901
	65.7019
	0.7608
	-0.3104
	0.3074

	Base
	109
	85
	Serv4
	Combination
	Min
	
	
	-3.7286
	-4.2173
	56.7934
	0.5451
	-1.6253
	0.1385

	Base
	109
	85
	Serv5
	Combination
	Max
	
	
	0.2287
	-2.9299
	95.368
	0.7505
	-0.0229
	0.5777

	Base
	109
	85
	Serv5
	Combination
	Min
	
	
	-4.7508
	-5.0775
	27.1274
	0.5554
	-1.9128
	-0.1318

	Base
	109
	85
	Serv6
	Combination
	Max
	
	
	-1.1603
	-3.8435
	64.5884
	0.7338
	-0.4748
	0.2863

	Base
	109
	85
	Serv6
	Combination
	Min
	
	
	-3.3617
	-4.1639
	57.907
	0.572
	-1.4609
	0.1596

	Base
	109
	85
	Serv7
	Combination
	Max
	
	
	-0.3937
	-3.1983
	86.8379
	0.7261
	-0.2591
	0.489

	Base
	109
	85
	Serv7
	Combination
	Min
	
	
	-4.1283
	-4.8091
	35.6575
	0.5797
	-1.6765
	-0.0431

	Base
	109
	85
	Serv8
	Combination
	
	
	
	-1.3566
	-2.4022
	36.7486
	0.3917
	-0.5807
	0.1338

	Base
	109
	85
	Serv9
	Combination
	Max
	
	
	0.111
	-2.1887
	41.2029
	0.4996
	0.0767
	0.2182

	Base
	109
	85
	Serv9
	Combination
	Min
	
	
	-2.8242
	-2.6158
	32.2944
	0.2839
	-1.2381
	0.0494

	Base
	109
	85
	Serv10
	Combination
	Max
	
	
	1.1332
	-1.3284
	70.8689
	0.4893
	0.3642
	0.4885

	Base
	109
	85
	Serv10
	Combination
	Min
	
	
	-3.8464
	-3.476
	2.6283
	0.2942
	-1.5256
	-0.221

	Base
	109
	85
	ENVSERV
	Combination
	Max
	
	
	1.1332
	-1.3284
	95.368
	0.7608
	0.3642
	0.5777

	Base
	109
	85
	ENVSERV
	Combination
	Min
	
	
	-4.7508
	-5.0775
	2.6283
	0.2839
	-1.9128
	-0.221

	Base
	110
	84
	Dead
	LinStatic
	
	
	
	-3.1988
	2.1179
	15.6973
	-1.4754
	-2.0477
	0.8188

	Base
	110
	84
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	110
	84
	FHEx
	LinStatic
	
	
	
	-37.9522
	4.4955
	23.2702
	-0.1309
	-11.8235
	-2.485

	Base
	110
	84
	FHEy
	LinStatic
	
	
	
	19.3073
	-18.0559
	-378.7743
	-1.4079
	-2.8165
	4.8898

	Base
	110
	84
	Sx
	LinRespSpec
	Max
	
	
	11.726
	2.5236
	32.7535
	0.9299
	3.3819
	1.87

	Base
	110
	84
	Sy
	LinRespSpec
	Max
	
	
	20.4634
	19.8535
	384.349
	1.1993
	3.0687
	5.0975

	Base
	110
	84
	Comb1
	Combination
	
	
	
	-4.4783
	2.965
	21.9763
	-2.0656
	-2.8667
	1.1463

	Base
	110
	84
	Comb2
	Combination
	
	
	
	-3.8385
	2.5414
	18.8368
	-1.7705
	-2.4572
	0.9825

	Base
	110
	84
	Comb3
	Combination
	
	
	
	-3.8385
	2.5414
	18.8368
	-1.7705
	-2.4572
	0.9825

	Base
	110
	84
	Comb4
	Combination
	Max
	
	
	-2.1634
	2.9019
	23.5159
	-1.6377
	-1.9741
	1.2497

	Base
	110
	84
	Comb4
	Combination
	Min
	
	
	-5.5137
	2.1809
	14.1577
	-1.9034
	-2.9403
	0.7154

	Base
	110
	84
	Comb5
	Combination
	Max
	
	
	-0.9143
	5.3785
	73.7603
	-1.5991
	-2.0187
	1.711

	Base
	110
	84
	Comb5
	Combination
	Min
	
	
	-6.7627
	-0.2956
	-36.0867
	-1.9419
	-2.8957
	0.2541

	Base
	110
	84
	Comb6
	Combination
	
	
	
	-2.8789
	1.9061
	14.1276
	-1.3279
	-1.8429
	0.7369

	Base
	110
	84
	Comb7
	Combination
	Max
	
	
	-1.2038
	2.2666
	18.8067
	-1.195
	-1.3598
	1.004

	Base
	110
	84
	Comb7
	Combination
	Min
	
	
	-4.554
	1.5456
	9.4485
	-1.4607
	-2.326
	0.4698

	Base
	110
	84
	Comb8
	Combination
	Max
	
	
	0.0453
	4.7431
	69.0511
	-1.1565
	-1.4044
	1.4653

	Base
	110
	84
	Comb8
	Combination
	Min
	
	
	-5.8031
	-0.931
	-40.7959
	-1.4993
	-2.2814
	0.0085

	Base
	110
	84
	ENVDIS
	Combination
	Max
	
	
	0.0453
	5.3785
	73.7603
	-1.1565
	-1.3598
	1.711

	Base
	110
	84
	ENVDIS
	Combination
	Min
	
	
	-6.7627
	-0.931
	-40.7959
	-2.0656
	-2.9403
	0.0085

	Base
	110
	84
	Serv1
	Combination
	
	
	
	-3.1988
	2.1179
	15.6973
	-1.4754
	-2.0477
	0.8188

	Base
	110
	84
	Serv2
	Combination
	
	
	
	-3.1988
	2.1179
	15.6973
	-1.4754
	-2.0477
	0.8188

	Base
	110
	84
	Serv3
	Combination
	
	
	
	-3.1988
	2.1179
	15.6973
	-1.4754
	-2.0477
	0.8188

	Base
	110
	84
	Serv4
	Combination
	Max
	
	
	-2.0262
	2.3702
	18.9727
	-1.3824
	-1.7095
	1.0058

	Base
	110
	84
	Serv4
	Combination
	Min
	
	
	-4.3714
	1.8655
	12.422
	-1.5684
	-2.3858
	0.6318

	Base
	110
	84
	Serv5
	Combination
	Max
	
	
	-1.1524
	4.1032
	54.1322
	-1.3555
	-1.7408
	1.3285

	Base
	110
	84
	Serv5
	Combination
	Min
	
	
	-5.2451
	0.1325
	-22.7376
	-1.5954
	-2.3545
	0.309

	Base
	110
	84
	Serv6
	Combination
	Max
	
	
	-2.3193
	2.3071
	18.1538
	-1.4057
	-1.794
	0.959

	Base
	110
	84
	Serv6
	Combination
	Min
	
	
	-4.0782
	1.9286
	13.2408
	-1.5452
	-2.3013
	0.6785

	Base
	110
	84
	Serv7
	Combination
	Max
	
	
	-1.664
	3.6069
	44.5235
	-1.3855
	-1.8175
	1.2011

	Base
	110
	84
	Serv7
	Combination
	Min
	
	
	-4.7335
	0.6289
	-13.1288
	-1.5654
	-2.2778
	0.4365

	Base
	110
	84
	Serv8
	Combination
	
	
	
	-1.9193
	1.2707
	9.4184
	-0.8853
	-1.2286
	0.4913

	Base
	110
	84
	Serv9
	Combination
	Max
	
	
	-0.7467
	1.5231
	12.6937
	-0.7923
	-0.8904
	0.6783

	Base
	110
	84
	Serv9
	Combination
	Min
	
	
	-3.0919
	1.0184
	6.1431
	-0.9782
	-1.5668
	0.3043

	Base
	110
	84
	Serv10
	Combination
	Max
	
	
	0.1271
	3.2561
	47.8533
	-0.7653
	-0.9217
	1.001

	Base
	110
	84
	Serv10
	Combination
	Min
	
	
	-3.9656
	-0.7146
	-29.0165
	-1.0052
	-1.5355
	-0.0185

	Base
	110
	84
	ENVSERV
	Combination
	Max
	
	
	0.1271
	4.1032
	54.1322
	-0.7653
	-0.8904
	1.3285

	Base
	110
	84
	ENVSERV
	Combination
	Min
	
	
	-5.2451
	-0.7146
	-29.0165
	-1.5954
	-2.3858
	-0.0185

	Base
	113
	107
	Dead
	LinStatic
	
	
	
	-1.6762
	1.1884
	9.5984
	0.0676
	0.1235
	0.0113

	Base
	113
	107
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	113
	107
	FHEx
	LinStatic
	
	
	
	-0.7962
	1.5215
	16.3888
	0.2602
	-1.2921
	-0.2202

	Base
	113
	107
	FHEy
	LinStatic
	
	
	
	4.4945
	-2.9454
	-48.5821
	1.7768
	1.4982
	-0.2546

	Base
	113
	107
	Sx
	LinRespSpec
	Max
	
	
	0.2412
	0.8293
	13.393
	0.3374
	0.9169
	0.3511

	Base
	113
	107
	Sy
	LinRespSpec
	Max
	
	
	3.9028
	4.9206
	42.689
	1.2146
	1.8149
	0.2998

	Base
	113
	107
	Comb1
	Combination
	
	
	
	-2.3467
	1.6638
	13.4378
	0.0946
	0.1729
	0.0159

	Base
	113
	107
	Comb2
	Combination
	
	
	
	-2.0115
	1.4261
	11.5181
	0.0811
	0.1482
	0.0136

	Base
	113
	107
	Comb3
	Combination
	
	
	
	-2.0115
	1.4261
	11.5181
	0.0811
	0.1482
	0.0136

	Base
	113
	107
	Comb4
	Combination
	Max
	
	
	-1.977
	1.5445
	13.4314
	0.1293
	0.2792
	0.0638

	Base
	113
	107
	Comb4
	Combination
	Min
	
	
	-2.0459
	1.3076
	9.6048
	0.0329
	0.0172
	-0.0366

	Base
	113
	107
	Comb5
	Combination
	Max
	
	
	-1.4538
	2.1292
	17.6184
	0.2546
	0.4076
	0.0564

	Base
	113
	107
	Comb5
	Combination
	Min
	
	
	-2.5692
	0.7229
	5.4179
	-0.0925
	-0.1111
	-0.0293

	Base
	113
	107
	Comb6
	Combination
	
	
	
	-1.5086
	1.0696
	8.6386
	0.0608
	0.1112
	0.0102

	Base
	113
	107
	Comb7
	Combination
	Max
	
	
	-1.4742
	1.188
	10.5519
	0.109
	0.2421
	0.0604

	Base
	113
	107
	Comb7
	Combination
	Min
	
	
	-1.5431
	0.9511
	6.7253
	0.0126
	-0.0198
	-0.04

	Base
	113
	107
	Comb8
	Combination
	Max
	
	
	-0.9509
	1.7727
	14.7389
	0.2344
	0.3705
	0.053

	Base
	113
	107
	Comb8
	Combination
	Min
	
	
	-2.0663
	0.3664
	2.5384
	-0.1127
	-0.1482
	-0.0326

	Base
	113
	107
	ENVDIS
	Combination
	Max
	
	
	-0.9509
	2.1292
	17.6184
	0.2546
	0.4076
	0.0638

	Base
	113
	107
	ENVDIS
	Combination
	Min
	
	
	-2.5692
	0.3664
	2.5384
	-0.1127
	-0.1482
	-0.04

	Base
	113
	107
	Serv1
	Combination
	
	
	
	-1.6762
	1.1884
	9.5984
	0.0676
	0.1235
	0.0113

	Base
	113
	107
	Serv2
	Combination
	
	
	
	-1.6762
	1.1884
	9.5984
	0.0676
	0.1235
	0.0113

	Base
	113
	107
	Serv3
	Combination
	
	
	
	-1.6762
	1.1884
	9.5984
	0.0676
	0.1235
	0.0113

	Base
	113
	107
	Serv4
	Combination
	Max
	
	
	-1.6521
	1.2713
	10.9378
	0.1013
	0.2152
	0.0464

	Base
	113
	107
	Serv4
	Combination
	Min
	
	
	-1.7004
	1.1055
	8.2591
	0.0338
	0.0318
	-0.0238

	Base
	113
	107
	Serv5
	Combination
	Max
	
	
	-1.286
	1.6805
	13.8673
	0.189
	0.305
	0.0413

	Base
	113
	107
	Serv5
	Combination
	Min
	
	
	-2.0665
	0.6963
	5.3296
	-0.0539
	-0.058
	-0.0187

	Base
	113
	107
	Serv6
	Combination
	Max
	
	
	-1.6582
	1.2506
	10.6029
	0.0929
	0.1923
	0.0377

	Base
	113
	107
	Serv6
	Combination
	Min
	
	
	-1.6943
	1.1262
	8.594
	0.0423
	0.0548
	-0.015

	Base
	113
	107
	Serv7
	Combination
	Max
	
	
	-1.3835
	1.5574
	12.8001
	0.1587
	0.2596
	0.0338

	Base
	113
	107
	Serv7
	Combination
	Min
	
	
	-1.969
	0.8194
	6.3968
	-0.0235
	-0.0126
	-0.0112

	Base
	113
	107
	Serv8
	Combination
	
	
	
	-1.0057
	0.713
	5.7591
	0.0405
	0.0741
	0.0068

	Base
	113
	107
	Serv9
	Combination
	Max
	
	
	-0.9816
	0.796
	7.0984
	0.0743
	0.1658
	0.0419

	Base
	113
	107
	Serv9
	Combination
	Min
	
	
	-1.0299
	0.6301
	4.4198
	0.0068
	-0.0176
	-0.0283

	Base
	113
	107
	Serv10
	Combination
	Max
	
	
	-0.6155
	1.2051
	10.028
	0.162
	0.2556
	0.0368

	Base
	113
	107
	Serv10
	Combination
	Min
	
	
	-1.396
	0.221
	1.4902
	-0.0809
	-0.1074
	-0.0232

	Base
	113
	107
	ENVSERV
	Combination
	Max
	
	
	-0.6155
	1.6805
	13.8673
	0.189
	0.305
	0.0464

	Base
	113
	107
	ENVSERV
	Combination
	Min
	
	
	-2.0665
	0.221
	1.4902
	-0.0809
	-0.1074
	-0.0283

	Base
	114
	65
	Dead
	LinStatic
	
	
	
	3.5384
	-6.5524
	25.4645
	1.438
	-2.082
	0.445

	Base
	114
	65
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	114
	65
	FHEx
	LinStatic
	
	
	
	-21.7034
	17.0452
	-57.3202
	-2.3412
	-2.636
	-0.7041

	Base
	114
	65
	FHEy
	LinStatic
	
	
	
	8.0998
	-25.571
	98.292
	3.8515
	-33.104
	1.1954

	Base
	114
	65
	Sx
	LinRespSpec
	Max
	
	
	18.215
	14.2335
	47.1064
	2.0423
	4.9576
	0.514

	Base
	114
	65
	Sy
	LinRespSpec
	Max
	
	
	21.719
	26.3735
	99.5409
	4.0324
	25.9661
	1.836

	Base
	114
	65
	Comb1
	Combination
	
	
	
	4.9538
	-9.1733
	35.6503
	2.0132
	-2.9149
	0.623

	Base
	114
	65
	Comb2
	Combination
	
	
	
	4.2461
	-7.8629
	30.5574
	1.7256
	-2.4984
	0.534

	Base
	114
	65
	Comb3
	Combination
	
	
	
	4.2461
	-7.8629
	30.5574
	1.7256
	-2.4984
	0.534

	Base
	114
	65
	Comb4
	Combination
	Max
	
	
	6.8482
	-5.8295
	37.2869
	2.0174
	-1.7902
	0.6074

	Base
	114
	65
	Comb4
	Combination
	Min
	
	
	1.6439
	-9.8962
	23.8279
	1.4339
	-3.2067
	0.4606

	Base
	114
	65
	Comb5
	Combination
	Max
	
	
	7.3497
	-4.0941
	44.7818
	2.3019
	1.2121
	0.7964

	Base
	114
	65
	Comb5
	Combination
	Min
	
	
	1.1424
	-11.6316
	16.333
	1.1494
	-6.209
	0.2716

	Base
	114
	65
	Comb6
	Combination
	
	
	
	3.1846
	-5.8971
	22.9181
	1.2942
	-1.8738
	0.4005

	Base
	114
	65
	Comb7
	Combination
	Max
	
	
	5.7867
	-3.8638
	29.6476
	1.586
	-1.1656
	0.4739

	Base
	114
	65
	Comb7
	Combination
	Min
	
	
	0.5824
	-7.9305
	16.1886
	1.0025
	-2.5821
	0.3271

	Base
	114
	65
	Comb8
	Combination
	Max
	
	
	6.2882
	-2.1284
	37.1425
	1.8705
	1.8367
	0.6629

	Base
	114
	65
	Comb8
	Combination
	Min
	
	
	0.0809
	-9.6659
	8.6937
	0.718
	-5.5844
	0.1381

	Base
	114
	65
	ENVDIS
	Combination
	Max
	
	
	7.3497
	-2.1284
	44.7818
	2.3019
	1.8367
	0.7964

	Base
	114
	65
	ENVDIS
	Combination
	Min
	
	
	0.0809
	-11.6316
	8.6937
	0.718
	-6.209
	0.1381

	Base
	114
	65
	Serv1
	Combination
	
	
	
	3.5384
	-6.5524
	25.4645
	1.438
	-2.082
	0.445

	Base
	114
	65
	Serv2
	Combination
	
	
	
	3.5384
	-6.5524
	25.4645
	1.438
	-2.082
	0.445

	Base
	114
	65
	Serv3
	Combination
	
	
	
	3.5384
	-6.5524
	25.4645
	1.438
	-2.082
	0.445

	Base
	114
	65
	Serv4
	Combination
	Max
	
	
	5.3599
	-5.129
	30.1752
	1.6422
	-1.5863
	0.4964

	Base
	114
	65
	Serv4
	Combination
	Min
	
	
	1.7169
	-7.9757
	20.7539
	1.2338
	-2.5778
	0.3936

	Base
	114
	65
	Serv5
	Combination
	Max
	
	
	5.7103
	-3.915
	35.4186
	1.8413
	0.5146
	0.6286

	Base
	114
	65
	Serv5
	Combination
	Min
	
	
	1.3665
	-9.1897
	15.5104
	1.0348
	-4.6786
	0.2614

	Base
	114
	65
	Serv6
	Combination
	Max
	
	
	4.9045
	-5.4849
	28.9975
	1.5912
	-1.7102
	0.4835

	Base
	114
	65
	Serv6
	Combination
	Min
	
	
	2.1723
	-7.6199
	21.9315
	1.2848
	-2.4539
	0.4064

	Base
	114
	65
	Serv7
	Combination
	Max
	
	
	5.1673
	-4.5744
	32.9301
	1.7405
	-0.1346
	0.5827

	Base
	114
	65
	Serv7
	Combination
	Min
	
	
	1.9095
	-8.5304
	17.999
	1.1356
	-4.0295
	0.3073

	Base
	114
	65
	Serv8
	Combination
	
	
	
	2.123
	-3.9314
	15.2787
	0.8628
	-1.2492
	0.267

	Base
	114
	65
	Serv9
	Combination
	Max
	
	
	3.9445
	-2.5081
	19.9894
	1.067
	-0.7535
	0.3184

	Base
	114
	65
	Serv9
	Combination
	Min
	
	
	0.3015
	-5.3548
	10.5681
	0.6586
	-1.745
	0.2156

	Base
	114
	65
	Serv10
	Combination
	Max
	
	
	4.2949
	-1.2941
	25.2328
	1.2661
	1.3474
	0.4506

	Base
	114
	65
	Serv10
	Combination
	Min
	
	
	-0.0489
	-6.5688
	5.3246
	0.4596
	-3.8458
	0.0834

	Base
	114
	65
	ENVSERV
	Combination
	Max
	
	
	5.7103
	-1.2941
	35.4186
	1.8413
	1.3474
	0.6286

	Base
	114
	65
	ENVSERV
	Combination
	Min
	
	
	-0.0489
	-9.1897
	5.3246
	0.4596
	-4.6786
	0.0834

	Base
	115
	66
	Dead
	LinStatic
	
	
	
	-4.9513
	1.5424
	25.3573
	-1.0047
	-0.2936
	0.1347

	Base
	115
	66
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	115
	66
	FHEx
	LinStatic
	
	
	
	-7.8431
	-6.2772
	28.3801
	3.9007
	-7.4804
	-0.8005

	Base
	115
	66
	FHEy
	LinStatic
	
	
	
	-17.9722
	-36.2228
	-93.8395
	13.9691
	1.3653
	4.4612

	Base
	115
	66
	Sx
	LinRespSpec
	Max
	
	
	7.2158
	8.2409
	22.9364
	4.0728
	6.3218
	1.0787

	Base
	115
	66
	Sy
	LinRespSpec
	Max
	
	
	13.6823
	28.9258
	83.0824
	8.4471
	5.8252
	4.2162

	Base
	115
	66
	Comb1
	Combination
	
	
	
	-6.9318
	2.1594
	35.5002
	-1.4066
	-0.4111
	0.1886

	Base
	115
	66
	Comb2
	Combination
	
	
	
	-5.9415
	1.8509
	30.4288
	-1.2057
	-0.3523
	0.1617

	Base
	115
	66
	Comb3
	Combination
	
	
	
	-5.9415
	1.8509
	30.4288
	-1.2057
	-0.3523
	0.1617

	Base
	115
	66
	Comb4
	Combination
	Max
	
	
	-4.9107
	3.0282
	33.7054
	-0.6238
	0.5508
	0.3158

	Base
	115
	66
	Comb4
	Combination
	Min
	
	
	-6.9724
	0.6736
	27.1521
	-1.7875
	-1.2555
	0.0076

	Base
	115
	66
	Comb5
	Combination
	Max
	
	
	-3.9863
	5.9844
	42.3012
	0.0014
	0.4801
	0.7642

	Base
	115
	66
	Comb5
	Combination
	Min
	
	
	-7.8967
	-2.2826
	18.5563
	-2.4127
	-1.1848
	-0.4408

	Base
	115
	66
	Comb6
	Combination
	
	
	
	-4.4562
	1.3882
	22.8216
	-0.9042
	-0.2643
	0.1213

	Base
	115
	66
	Comb7
	Combination
	Max
	
	
	-3.4253
	2.5654
	26.0982
	-0.3224
	0.6389
	0.2754

	Base
	115
	66
	Comb7
	Combination
	Min
	
	
	-5.487
	0.2109
	19.5449
	-1.4861
	-1.1674
	-0.0329

	Base
	115
	66
	Comb8
	Combination
	Max
	
	
	-2.501
	5.5217
	34.6941
	0.3029
	0.5682
	0.7237

	Base
	115
	66
	Comb8
	Combination
	Min
	
	
	-6.4113
	-2.7453
	10.9491
	-2.1113
	-1.0967
	-0.4812

	Base
	115
	66
	ENVDIS
	Combination
	Max
	
	
	-2.501
	5.9844
	42.3012
	0.3029
	0.6389
	0.7642

	Base
	115
	66
	ENVDIS
	Combination
	Min
	
	
	-7.8967
	-2.7453
	10.9491
	-2.4127
	-1.2555
	-0.4812

	Base
	115
	66
	Serv1
	Combination
	
	
	
	-4.9513
	1.5424
	25.3573
	-1.0047
	-0.2936
	0.1347

	Base
	115
	66
	Serv2
	Combination
	
	
	
	-4.9513
	1.5424
	25.3573
	-1.0047
	-0.2936
	0.1347

	Base
	115
	66
	Serv3
	Combination
	
	
	
	-4.9513
	1.5424
	25.3573
	-1.0047
	-0.2936
	0.1347

	Base
	115
	66
	Serv4
	Combination
	Max
	
	
	-4.2297
	2.3665
	27.651
	-0.5974
	0.3386
	0.2426

	Base
	115
	66
	Serv4
	Combination
	Min
	
	
	-5.6729
	0.7183
	23.0637
	-1.412
	-0.9258
	0.0268

	Base
	115
	66
	Serv5
	Combination
	Max
	
	
	-3.5831
	4.435
	33.6656
	-0.16
	0.2889
	0.5563

	Base
	115
	66
	Serv5
	Combination
	Min
	
	
	-6.3195
	-1.3502
	17.0491
	-1.8494
	-0.8761
	-0.2869

	Base
	115
	66
	Serv6
	Combination
	Max
	
	
	-4.4101
	2.1605
	27.0775
	-0.6992
	0.1805
	0.2156

	Base
	115
	66
	Serv6
	Combination
	Min
	
	
	-5.4925
	0.9243
	23.6371
	-1.3102
	-0.7678
	0.0538

	Base
	115
	66
	Serv7
	Combination
	Max
	
	
	-3.9251
	3.7118
	31.5885
	-0.3712
	0.1433
	0.4509

	Base
	115
	66
	Serv7
	Combination
	Min
	
	
	-5.9774
	-0.627
	19.1261
	-1.6382
	-0.7305
	-0.1815

	Base
	115
	66
	Serv8
	Combination
	
	
	
	-2.9708
	0.9254
	15.2144
	-0.6028
	-0.1762
	0.0808

	Base
	115
	66
	Serv9
	Combination
	Max
	
	
	-2.2492
	1.7495
	17.508
	-0.1955
	0.456
	0.1887

	Base
	115
	66
	Serv9
	Combination
	Min
	
	
	-3.6923
	0.1014
	12.9207
	-1.0101
	-0.8084
	-0.027

	Base
	115
	66
	Serv10
	Combination
	Max
	
	
	-1.6025
	3.818
	23.5226
	0.2419
	0.4063
	0.5025

	Base
	115
	66
	Serv10
	Combination
	Min
	
	
	-4.339
	-1.9671
	6.9062
	-1.4475
	-0.7587
	-0.3408

	Base
	115
	66
	ENVSERV
	Combination
	Max
	
	
	-1.6025
	4.435
	33.6656
	0.2419
	0.456
	0.5563

	Base
	115
	66
	ENVSERV
	Combination
	Min
	
	
	-6.3195
	-1.9671
	6.9062
	-1.8494
	-0.9258
	-0.3408

	Base
	116
	67
	Dead
	LinStatic
	
	
	
	5.0574
	-1.675
	19.9617
	-0.2284
	0.5087
	-0.2558

	Base
	116
	67
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	116
	67
	FHEx
	LinStatic
	
	
	
	-3.3042
	-7.52
	-11.6746
	6.8791
	0.2861
	-0.0614

	Base
	116
	67
	FHEy
	LinStatic
	
	
	
	55.643
	-33.5927
	142.8892
	16.3327
	2.0185
	4.4424

	Base
	116
	67
	Sx
	LinRespSpec
	Max
	
	
	6.7454
	7.7822
	16.9004
	6.2192
	0.4564
	0.8758

	Base
	116
	67
	Sy
	LinRespSpec
	Max
	
	
	43.8278
	18.6174
	107.0199
	12.0763
	0.8389
	3.8695

	Base
	116
	67
	Comb1
	Combination
	
	
	
	7.0803
	-2.3449
	27.9463
	-0.3198
	0.7122
	-0.3581

	Base
	116
	67
	Comb2
	Combination
	
	
	
	6.0688
	-2.0099
	23.954
	-0.2741
	0.6105
	-0.307

	Base
	116
	67
	Comb3
	Combination
	
	
	
	6.0688
	-2.0099
	23.954
	-0.2741
	0.6105
	-0.307

	Base
	116
	67
	Comb4
	Combination
	Max
	
	
	7.0324
	-0.8982
	26.3683
	0.6143
	0.6757
	-0.1819

	Base
	116
	67
	Comb4
	Combination
	Min
	
	
	5.1052
	-3.1217
	21.5396
	-1.1626
	0.5453
	-0.4321

	Base
	116
	67
	Comb5
	Combination
	Max
	
	
	12.3318
	0.6505
	39.2471
	1.4516
	0.7303
	0.246

	Base
	116
	67
	Comb5
	Combination
	Min
	
	
	-0.1942
	-4.6704
	8.6608
	-1.9998
	0.4906
	-0.8599

	Base
	116
	67
	Comb6
	Combination
	
	
	
	4.5516
	-1.5075
	17.9655
	-0.2056
	0.4578
	-0.2302

	Base
	116
	67
	Comb7
	Combination
	Max
	
	
	5.5152
	-0.3957
	20.3798
	0.6829
	0.523
	-0.1051

	Base
	116
	67
	Comb7
	Combination
	Min
	
	
	3.588
	-2.6192
	15.5512
	-1.0941
	0.3926
	-0.3553

	Base
	116
	67
	Comb8
	Combination
	Max
	
	
	10.8146
	1.153
	33.2586
	1.5201
	0.5777
	0.3227

	Base
	116
	67
	Comb8
	Combination
	Min
	
	
	-1.7114
	-4.1679
	2.6723
	-1.9313
	0.338
	-0.7832

	Base
	116
	67
	ENVDIS
	Combination
	Max
	
	
	12.3318
	1.153
	39.2471
	1.5201
	0.7303
	0.3227

	Base
	116
	67
	ENVDIS
	Combination
	Min
	
	
	-1.7114
	-4.6704
	2.6723
	-1.9998
	0.338
	-0.8599

	Base
	116
	67
	Serv1
	Combination
	
	
	
	5.0574
	-1.675
	19.9617
	-0.2284
	0.5087
	-0.2558

	Base
	116
	67
	Serv2
	Combination
	
	
	
	5.0574
	-1.675
	19.9617
	-0.2284
	0.5087
	-0.2558

	Base
	116
	67
	Serv3
	Combination
	
	
	
	5.0574
	-1.675
	19.9617
	-0.2284
	0.5087
	-0.2558

	Base
	116
	67
	Serv4
	Combination
	Max
	
	
	5.7319
	-0.8967
	21.6517
	0.3935
	0.5544
	-0.1682

	Base
	116
	67
	Serv4
	Combination
	Min
	
	
	4.3828
	-2.4532
	18.2716
	-0.8504
	0.4631
	-0.3434

	Base
	116
	67
	Serv5
	Combination
	Max
	
	
	9.4401
	0.1868
	30.6636
	0.9792
	0.5926
	0.1311

	Base
	116
	67
	Serv5
	Combination
	Min
	
	
	0.6746
	-3.5367
	9.2597
	-1.4361
	0.4248
	-0.6427

	Base
	116
	67
	Serv6
	Combination
	Max
	
	
	5.5633
	-1.0913
	21.2292
	0.238
	0.5429
	-0.1901

	Base
	116
	67
	Serv6
	Combination
	Min
	
	
	4.5515
	-2.2586
	18.6941
	-0.6949
	0.4745
	-0.3215

	Base
	116
	67
	Serv7
	Combination
	Max
	
	
	8.3444
	-0.2787
	27.9881
	0.6773
	0.5716
	0.0344

	Base
	116
	67
	Serv7
	Combination
	Min
	
	
	1.7703
	-3.0713
	11.9352
	-1.1342
	0.4458
	-0.546

	Base
	116
	67
	Serv8
	Combination
	
	
	
	3.0344
	-1.005
	11.977
	-0.1371
	0.3052
	-0.1535

	Base
	116
	67
	Serv9
	Combination
	Max
	
	
	3.7089
	-0.2267
	13.667
	0.4848
	0.3509
	-0.0659

	Base
	116
	67
	Serv9
	Combination
	Min
	
	
	2.3599
	-1.7832
	10.287
	-0.759
	0.2596
	-0.2411

	Base
	116
	67
	Serv10
	Combination
	Max
	
	
	7.4172
	0.8568
	22.679
	1.0706
	0.3891
	0.2335

	Base
	116
	67
	Serv10
	Combination
	Min
	
	
	-1.3484
	-2.8667
	1.275
	-1.3447
	0.2213
	-0.5404

	Base
	116
	67
	ENVSERV
	Combination
	Max
	
	
	9.4401
	0.8568
	30.6636
	1.0706
	0.5926
	0.2335

	Base
	116
	67
	ENVSERV
	Combination
	Min
	
	
	-1.3484
	-3.5367
	1.275
	-1.4361
	0.2213
	-0.6427

	Base
	117
	64
	Dead
	LinStatic
	
	
	
	3.4506
	5.5159
	22.225
	0.8456
	2.0733
	0.2187

	Base
	117
	64
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	117
	64
	FHEx
	LinStatic
	
	
	
	-23.6882
	-16.9251
	-63.53
	0.402
	-12.1492
	-0.1038

	Base
	117
	64
	FHEy
	LinStatic
	
	
	
	17.3291
	12.4108
	-19.0131
	-0.7251
	46.2161
	-3.6432

	Base
	117
	64
	Sx
	LinRespSpec
	Max
	
	
	19.24
	13.8554
	53.1286
	0.4175
	10.7271
	0.8569

	Base
	117
	64
	Sy
	LinRespSpec
	Max
	
	
	24.5327
	18.6467
	35.1884
	0.5426
	42.4838
	2.6091

	Base
	117
	64
	Comb1
	Combination
	
	
	
	4.8308
	7.7222
	31.115
	1.1839
	2.9026
	0.3062

	Base
	117
	64
	Comb2
	Combination
	
	
	
	4.1407
	6.6191
	26.67
	1.0148
	2.488
	0.2624

	Base
	117
	64
	Comb3
	Combination
	
	
	
	4.1407
	6.6191
	26.67
	1.0148
	2.488
	0.2624

	Base
	117
	64
	Comb4
	Combination
	Max
	
	
	6.8893
	8.5984
	34.2598
	1.0744
	4.0204
	0.3849

	Base
	117
	64
	Comb4
	Combination
	Min
	
	
	1.3921
	4.6397
	19.0802
	0.9551
	0.9555
	0.14

	Base
	117
	64
	Comb5
	Combination
	Max
	
	
	7.6464
	9.2837
	31.6984
	1.0923
	8.5589
	0.6353

	Base
	117
	64
	Comb5
	Combination
	Min
	
	
	0.635
	3.9545
	21.6416
	0.9372
	-3.583
	-0.1104

	Base
	117
	64
	Comb6
	Combination
	
	
	
	3.1055
	4.9643
	20.0025
	0.7611
	1.866
	0.1968

	Base
	117
	64
	Comb7
	Combination
	Max
	
	
	5.8541
	6.9436
	27.5923
	0.8207
	3.3984
	0.3192

	Base
	117
	64
	Comb7
	Combination
	Min
	
	
	0.357
	2.985
	12.4127
	0.7014
	0.3335
	0.0744

	Base
	117
	64
	Comb8
	Combination
	Max
	
	
	6.6112
	7.6289
	25.0309
	0.8386
	7.9369
	0.5697

	Base
	117
	64
	Comb8
	Combination
	Min
	
	
	-0.4002
	2.2997
	14.9741
	0.6835
	-4.205
	-0.176

	Base
	117
	64
	ENVDIS
	Combination
	Max
	
	
	7.6464
	9.2837
	34.2598
	1.1839
	8.5589
	0.6353

	Base
	117
	64
	ENVDIS
	Combination
	Min
	
	
	-0.4002
	2.2997
	12.4127
	0.6835
	-4.205
	-0.176

	Base
	117
	64
	Serv1
	Combination
	
	
	
	3.4506
	5.5159
	22.225
	0.8456
	2.0733
	0.2187

	Base
	117
	64
	Serv2
	Combination
	
	
	
	3.4506
	5.5159
	22.225
	0.8456
	2.0733
	0.2187

	Base
	117
	64
	Serv3
	Combination
	
	
	
	3.4506
	5.5159
	22.225
	0.8456
	2.0733
	0.2187

	Base
	117
	64
	Serv4
	Combination
	Max
	
	
	5.3746
	6.9014
	27.5378
	0.8874
	3.146
	0.3044

	Base
	117
	64
	Serv4
	Combination
	Min
	
	
	1.5266
	4.1304
	16.9121
	0.8039
	1.0006
	0.133

	Base
	117
	64
	Serv5
	Combination
	Max
	
	
	5.9038
	7.3806
	25.7438
	0.8999
	6.3217
	0.4796

	Base
	117
	64
	Serv5
	Combination
	Min
	
	
	0.9973
	3.6512
	18.7061
	0.7914
	-2.1751
	-0.0422

	Base
	117
	64
	Serv6
	Combination
	Max
	
	
	4.8936
	6.555
	26.2096
	0.8769
	2.8778
	0.283

	Base
	117
	64
	Serv6
	Combination
	Min
	
	
	2.0076
	4.4767
	18.2403
	0.8143
	1.2688
	0.1544

	Base
	117
	64
	Serv7
	Combination
	Max
	
	
	5.2905
	6.9144
	24.8641
	0.8863
	5.2596
	0.4144

	Base
	117
	64
	Serv7
	Combination
	Min
	
	
	1.6106
	4.1174
	19.5858
	0.8049
	-1.113
	0.023

	Base
	117
	64
	Serv8
	Combination
	
	
	
	2.0703
	3.3095
	13.335
	0.5074
	1.244
	0.1312

	Base
	117
	64
	Serv9
	Combination
	Max
	
	
	3.9943
	4.6951
	18.6478
	0.5491
	2.3167
	0.2169

	Base
	117
	64
	Serv9
	Combination
	Min
	
	
	0.1464
	1.924
	8.0221
	0.4656
	0.1713
	0.0455

	Base
	117
	64
	Serv10
	Combination
	Max
	
	
	4.5236
	5.1742
	16.8538
	0.5616
	5.4924
	0.3921

	Base
	117
	64
	Serv10
	Combination
	Min
	
	
	-0.3829
	1.4449
	9.8161
	0.4531
	-3.0044
	-0.1297

	Base
	117
	64
	ENVSERV
	Combination
	Max
	
	
	5.9038
	7.3806
	27.5378
	0.8999
	6.3217
	0.4796

	Base
	117
	64
	ENVSERV
	Combination
	Min
	
	
	-0.3829
	1.4449
	8.0221
	0.4531
	-3.0044
	-0.1297

	Base
	118
	63
	Dead
	LinStatic
	
	
	
	-1.8689
	0.7633
	21.7303
	-0.1925
	0.8391
	0.1058

	Base
	118
	63
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	118
	63
	FHEx
	LinStatic
	
	
	
	-16.3518
	1.9056
	58.5874
	-0.4105
	-10.6267
	-1.0551

	Base
	118
	63
	FHEy
	LinStatic
	
	
	
	36.6052
	-43.3537
	-201.5241
	21.1615
	16.7772
	-1.827

	Base
	118
	63
	Sx
	LinRespSpec
	Max
	
	
	13.4849
	4.9454
	48.4821
	2.4305
	8.7042
	1.2644

	Base
	118
	63
	Sy
	LinRespSpec
	Max
	
	
	37.1631
	32.7425
	172.5361
	13.8896
	18.425
	2.7448

	Base
	118
	63
	Comb1
	Combination
	
	
	
	-2.6164
	1.0686
	30.4224
	-0.2695
	1.1747
	0.1481

	Base
	118
	63
	Comb2
	Combination
	
	
	
	-2.2426
	0.916
	26.0764
	-0.231
	1.0069
	0.127

	Base
	118
	63
	Comb3
	Combination
	
	
	
	-2.2426
	0.916
	26.0764
	-0.231
	1.0069
	0.127

	Base
	118
	63
	Comb4
	Combination
	Max
	
	
	-0.3162
	1.6224
	33.0024
	0.1162
	2.2504
	0.3076

	Base
	118
	63
	Comb4
	Combination
	Min
	
	
	-4.169
	0.2095
	19.1504
	-0.5782
	-0.2365
	-0.0537

	Base
	118
	63
	Comb5
	Combination
	Max
	
	
	3.068
	5.5949
	50.7318
	1.7538
	3.6398
	0.5192

	Base
	118
	63
	Comb5
	Combination
	Min
	
	
	-7.5532
	-3.7629
	1.421
	-2.2158
	-1.626
	-0.2653

	Base
	118
	63
	Comb6
	Combination
	
	
	
	-1.682
	0.687
	19.5573
	-0.1733
	0.7552
	0.0952

	Base
	118
	63
	Comb7
	Combination
	Max
	
	
	0.2444
	1.3935
	26.4833
	0.174
	1.9986
	0.2759

	Base
	118
	63
	Comb7
	Combination
	Min
	
	
	-3.6084
	-0.0195
	12.6313
	-0.5205
	-0.4883
	-0.0854

	Base
	118
	63
	Comb8
	Combination
	Max
	
	
	3.6286
	5.3659
	44.2127
	1.8116
	3.3881
	0.4875

	Base
	118
	63
	Comb8
	Combination
	Min
	
	
	-6.9926
	-3.9919
	-5.0981
	-2.1581
	-1.8778
	-0.297

	Base
	118
	63
	ENVDIS
	Combination
	Max
	
	
	3.6286
	5.5949
	50.7318
	1.8116
	3.6398
	0.5192

	Base
	118
	63
	ENVDIS
	Combination
	Min
	
	
	-7.5532
	-3.9919
	-5.0981
	-2.2158
	-1.8778
	-0.297

	Base
	118
	63
	Serv1
	Combination
	
	
	
	-1.8689
	0.7633
	21.7303
	-0.1925
	0.8391
	0.1058

	Base
	118
	63
	Serv2
	Combination
	
	
	
	-1.8689
	0.7633
	21.7303
	-0.1925
	0.8391
	0.1058

	Base
	118
	63
	Serv3
	Combination
	
	
	
	-1.8689
	0.7633
	21.7303
	-0.1925
	0.8391
	0.1058

	Base
	118
	63
	Serv4
	Combination
	Max
	
	
	-0.5204
	1.2578
	26.5785
	0.0505
	1.7095
	0.2323

	Base
	118
	63
	Serv4
	Combination
	Min
	
	
	-3.2173
	0.2688
	16.8821
	-0.4356
	-0.0313
	-0.0206

	Base
	118
	63
	Serv5
	Combination
	Max
	
	
	1.8475
	4.0376
	38.9839
	1.1964
	2.6816
	0.3803

	Base
	118
	63
	Serv5
	Combination
	Min
	
	
	-5.5852
	-2.5109
	4.4767
	-1.5815
	-1.0034
	-0.1687

	Base
	118
	63
	Serv6
	Combination
	Max
	
	
	-0.8575
	1.1342
	25.3665
	-0.0102
	1.4919
	0.2006

	Base
	118
	63
	Serv6
	Combination
	Min
	
	
	-2.8802
	0.3924
	18.0941
	-0.3748
	0.1863
	0.011

	Base
	118
	63
	Serv7
	Combination
	Max
	
	
	0.9184
	3.219
	34.6705
	0.8492
	2.221
	0.3117

	Base
	118
	63
	Serv7
	Combination
	Min
	
	
	-4.6561
	-1.6924
	8.7901
	-1.2342
	-0.5428
	-0.1001

	Base
	118
	63
	Serv8
	Combination
	
	
	
	-1.1213
	0.458
	13.0382
	-0.1155
	0.5035
	0.0635

	Base
	118
	63
	Serv9
	Combination
	Max
	
	
	0.2272
	0.9525
	17.8864
	0.1275
	1.3739
	0.1899

	Base
	118
	63
	Serv9
	Combination
	Min
	
	
	-2.4698
	-0.0366
	8.19
	-0.3586
	-0.367
	-0.063

	Base
	118
	63
	Serv10
	Combination
	Max
	
	
	2.595
	3.7322
	30.2918
	1.2735
	2.346
	0.338

	Base
	118
	63
	Serv10
	Combination
	Min
	
	
	-4.8376
	-2.8163
	-4.2154
	-1.5045
	-1.339
	-0.211

	Base
	118
	63
	ENVSERV
	Combination
	Max
	
	
	2.595
	4.0376
	38.9839
	1.2735
	2.6816
	0.3803

	Base
	118
	63
	ENVSERV
	Combination
	Min
	
	
	-5.5852
	-2.8163
	-4.2154
	-1.5815
	-1.339
	-0.211

	Base
	119
	62
	Dead
	LinStatic
	
	
	
	-5.0341
	-2.1436
	19.108
	1.0078
	-0.0907
	-0.0514

	Base
	119
	62
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	119
	62
	FHEx
	LinStatic
	
	
	
	0.0583
	-5.4445
	40.1608
	-4.8528
	1.47
	-0.8737

	Base
	119
	62
	FHEy
	LinStatic
	
	
	
	-47.9837
	-34.8326
	87.0315
	18.7298
	-4.8237
	3.1929

	Base
	119
	62
	Sx
	LinRespSpec
	Max
	
	
	6.293
	6.1411
	38.0303
	3.682
	1.2606
	0.9386

	Base
	119
	62
	Sy
	LinRespSpec
	Max
	
	
	36.9371
	19.4118
	46.4825
	12.3498
	4.8782
	3.2979

	Base
	119
	62
	Comb1
	Combination
	
	
	
	-7.0477
	-3.0011
	26.7511
	1.4109
	-0.1269
	-0.0719

	Base
	119
	62
	Comb2
	Combination
	
	
	
	-6.0409
	-2.5723
	22.9296
	1.2094
	-0.1088
	-0.0616

	Base
	119
	62
	Comb3
	Combination
	
	
	
	-6.0409
	-2.5723
	22.9296
	1.2094
	-0.1088
	-0.0616

	Base
	119
	62
	Comb4
	Combination
	Max
	
	
	-5.1419
	-1.695
	28.3625
	1.7354
	0.0713
	0.0724

	Base
	119
	62
	Comb4
	Combination
	Min
	
	
	-6.9399
	-3.4496
	17.4967
	0.6834
	-0.2889
	-0.1957

	Base
	119
	62
	Comb5
	Combination
	Max
	
	
	-0.7626
	0.2016
	29.5719
	2.9742
	0.5883
	0.4096

	Base
	119
	62
	Comb5
	Combination
	Min
	
	
	-11.3192
	-5.3463
	16.2872
	-0.5554
	-0.8059
	-0.5329

	Base
	119
	62
	Comb6
	Combination
	
	
	
	-4.5306
	-1.9293
	17.1972
	0.907
	-0.0816
	-0.0462

	Base
	119
	62
	Comb7
	Combination
	Max
	
	
	-3.6316
	-1.0519
	22.6301
	1.433
	0.0985
	0.0879

	Base
	119
	62
	Comb7
	Combination
	Min
	
	
	-5.4297
	-2.8066
	11.7643
	0.381
	-0.2617
	-0.1803

	Base
	119
	62
	Comb8
	Combination
	Max
	
	
	0.7477
	0.8447
	23.8395
	2.6718
	0.6155
	0.425

	Base
	119
	62
	Comb8
	Combination
	Min
	
	
	-9.809
	-4.7032
	10.5548
	-0.8578
	-0.7787
	-0.5175

	Base
	119
	62
	ENVDIS
	Combination
	Max
	
	
	0.7477
	0.8447
	29.5719
	2.9742
	0.6155
	0.425

	Base
	119
	62
	ENVDIS
	Combination
	Min
	
	
	-11.3192
	-5.3463
	10.5548
	-0.8578
	-0.8059
	-0.5329

	Base
	119
	62
	Serv1
	Combination
	
	
	
	-5.0341
	-2.1436
	19.108
	1.0078
	-0.0907
	-0.0514

	Base
	119
	62
	Serv2
	Combination
	
	
	
	-5.0341
	-2.1436
	19.108
	1.0078
	-0.0907
	-0.0514

	Base
	119
	62
	Serv3
	Combination
	
	
	
	-5.0341
	-2.1436
	19.108
	1.0078
	-0.0907
	-0.0514

	Base
	119
	62
	Serv4
	Combination
	Max
	
	
	-4.4048
	-1.5295
	22.911
	1.376
	0.0354
	0.0425

	Base
	119
	62
	Serv4
	Combination
	Min
	
	
	-5.6634
	-2.7577
	15.3049
	0.6396
	-0.2167
	-0.1452

	Base
	119
	62
	Serv5
	Combination
	Max
	
	
	-1.3403
	-0.2024
	23.7562
	2.2428
	0.3972
	0.2784

	Base
	119
	62
	Serv5
	Combination
	Min
	
	
	-8.7278
	-4.0848
	14.4597
	-0.2272
	-0.5785
	-0.3811

	Base
	119
	62
	Serv6
	Combination
	Max
	
	
	-4.5621
	-1.683
	21.9602
	1.284
	0.0039
	0.019

	Base
	119
	62
	Serv6
	Combination
	Min
	
	
	-5.506
	-2.6042
	16.2557
	0.7317
	-0.1852
	-0.1218

	Base
	119
	62
	Serv7
	Combination
	Max
	
	
	-2.2638
	-0.6877
	22.5942
	1.934
	0.2752
	0.196

	Base
	119
	62
	Serv7
	Combination
	Min
	
	
	-7.8043
	-3.5995
	15.6218
	0.0816
	-0.4565
	-0.2987

	Base
	119
	62
	Serv8
	Combination
	
	
	
	-3.0204
	-1.2862
	11.4648
	0.6047
	-0.0544
	-0.0308

	Base
	119
	62
	Serv9
	Combination
	Max
	
	
	-2.3911
	-0.6721
	15.2678
	0.9729
	0.0717
	0.063

	Base
	119
	62
	Serv9
	Combination
	Min
	
	
	-3.6497
	-1.9003
	7.6617
	0.2365
	-0.1805
	-0.1247

	Base
	119
	62
	Serv10
	Combination
	Max
	
	
	0.6733
	0.655
	16.113
	1.8397
	0.4334
	0.299

	Base
	119
	62
	Serv10
	Combination
	Min
	
	
	-6.7141
	-3.2274
	6.8165
	-0.6303
	-0.5422
	-0.3606

	Base
	119
	62
	ENVSERV
	Combination
	Max
	
	
	0.6733
	0.655
	23.7562
	2.2428
	0.4334
	0.299

	Base
	119
	62
	ENVSERV
	Combination
	Min
	
	
	-8.7278
	-4.0848
	6.8165
	-0.6303
	-0.5785
	-0.3811

	Base
	120
	56
	Dead
	LinStatic
	
	
	
	0.7816
	-4.2887
	20.3796
	-0.3046
	-1.8171
	-0.106

	Base
	120
	56
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	120
	56
	FHEx
	LinStatic
	
	
	
	-20.4923
	12.7718
	-54.9571
	-0.9234
	-6.9558
	-0.1493

	Base
	120
	56
	FHEy
	LinStatic
	
	
	
	-12.7578
	8.2328
	31.9292
	-0.3021
	-45.8082
	-3.8474

	Base
	120
	56
	Sx
	LinRespSpec
	Max
	
	
	14.1986
	10.8699
	42.0278
	1.0871
	9.0734
	0.8297

	Base
	120
	56
	Sy
	LinRespSpec
	Max
	
	
	18.718
	12.4098
	17.7582
	1.5763
	42.8026
	2.9639

	Base
	120
	56
	Comb1
	Combination
	
	
	
	1.0943
	-6.0042
	28.5314
	-0.4264
	-2.5439
	-0.1484

	Base
	120
	56
	Comb2
	Combination
	
	
	
	0.9379
	-5.1465
	24.4555
	-0.3655
	-2.1805
	-0.1272

	Base
	120
	56
	Comb3
	Combination
	
	
	
	0.9379
	-5.1465
	24.4555
	-0.3655
	-2.1805
	-0.1272

	Base
	120
	56
	Comb4
	Combination
	Max
	
	
	2.9663
	-3.5937
	30.4594
	-0.2102
	-0.8843
	-0.0087

	Base
	120
	56
	Comb4
	Combination
	Min
	
	
	-1.0904
	-6.6993
	18.4515
	-0.5208
	-3.4767
	-0.2458

	Base
	120
	56
	Comb5
	Combination
	Max
	
	
	3.6127
	-3.3731
	26.9931
	-0.1403
	3.936
	0.2963

	Base
	120
	56
	Comb5
	Combination
	Min
	
	
	-1.7369
	-6.9199
	21.9178
	-0.5908
	-8.297
	-0.5508

	Base
	120
	56
	Comb6
	Combination
	
	
	
	0.7035
	-3.8599
	18.3416
	-0.2741
	-1.6354
	-0.0954

	Base
	120
	56
	Comb7
	Combination
	Max
	
	
	2.7318
	-2.307
	24.3456
	-0.1188
	-0.3392
	0.0231

	Base
	120
	56
	Comb7
	Combination
	Min
	
	
	-1.3249
	-5.4127
	12.3376
	-0.4294
	-2.9316
	-0.2139

	Base
	120
	56
	Comb8
	Combination
	Max
	
	
	3.3783
	-2.0865
	20.8793
	-0.0489
	4.4811
	0.3281

	Base
	120
	56
	Comb8
	Combination
	Min
	
	
	-1.9713
	-5.6332
	15.804
	-0.4994
	-7.7519
	-0.519

	Base
	120
	56
	ENVDIS
	Combination
	Max
	
	
	3.6127
	-2.0865
	30.4594
	-0.0489
	4.4811
	0.3281

	Base
	120
	56
	ENVDIS
	Combination
	Min
	
	
	-1.9713
	-6.9199
	12.3376
	-0.5908
	-8.297
	-0.5508

	Base
	120
	56
	Serv1
	Combination
	
	
	
	0.7816
	-4.2887
	20.3796
	-0.3046
	-1.8171
	-0.106

	Base
	120
	56
	Serv2
	Combination
	
	
	
	0.7816
	-4.2887
	20.3796
	-0.3046
	-1.8171
	-0.106

	Base
	120
	56
	Serv3
	Combination
	
	
	
	0.7816
	-4.2887
	20.3796
	-0.3046
	-1.8171
	-0.106

	Base
	120
	56
	Serv4
	Combination
	Max
	
	
	2.2015
	-3.2018
	24.5823
	-0.1959
	-0.9097
	-0.0231

	Base
	120
	56
	Serv4
	Combination
	Min
	
	
	-0.6382
	-5.3757
	16.1768
	-0.4133
	-2.7244
	-0.189

	Base
	120
	56
	Serv5
	Combination
	Max
	
	
	2.6534
	-3.0478
	22.1554
	-0.147
	2.4632
	0.1904

	Base
	120
	56
	Serv5
	Combination
	Min
	
	
	-1.0902
	-5.5297
	18.6037
	-0.4622
	-6.0973
	-0.4024

	Base
	120
	56
	Serv6
	Combination
	Max
	
	
	1.8465
	-3.4735
	23.5317
	-0.2231
	-1.1366
	-0.0438

	Base
	120
	56
	Serv6
	Combination
	Min
	
	
	-0.2833
	-5.104
	17.2275
	-0.3861
	-2.4976
	-0.1682

	Base
	120
	56
	Serv7
	Combination
	Max
	
	
	2.1855
	-3.358
	21.7114
	-0.1864
	1.3931
	0.1163

	Base
	120
	56
	Serv7
	Combination
	Min
	
	
	-0.6222
	-5.2195
	19.0477
	-0.4228
	-5.0273
	-0.3283

	Base
	120
	56
	Serv8
	Combination
	
	
	
	0.469
	-2.5732
	12.2277
	-0.1828
	-1.0902
	-0.0636

	Base
	120
	56
	Serv9
	Combination
	Max
	
	
	1.8888
	-1.4863
	16.4305
	-0.074
	-0.1829
	0.0194

	Base
	120
	56
	Serv9
	Combination
	Min
	
	
	-0.9509
	-3.6602
	8.025
	-0.2915
	-1.9976
	-0.1466

	Base
	120
	56
	Serv10
	Combination
	Max
	
	
	2.3408
	-1.3323
	14.0036
	-0.0251
	3.19
	0.2328

	Base
	120
	56
	Serv10
	Combination
	Min
	
	
	-1.4028
	-3.8142
	10.4519
	-0.3404
	-5.3705
	-0.36

	Base
	120
	56
	ENVSERV
	Combination
	Max
	
	
	2.6534
	-1.3323
	24.5823
	-0.0251
	3.19
	0.2328

	Base
	120
	56
	ENVSERV
	Combination
	Min
	
	
	-1.4028
	-5.5297
	8.025
	-0.4622
	-6.0973
	-0.4024

	Base
	121
	57
	Dead
	LinStatic
	
	
	
	-6.0697
	-3.7955
	37.5658
	1.0468
	-1.0411
	0.281

	Base
	121
	57
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	121
	57
	FHEx
	LinStatic
	
	
	
	-9.9102
	-0.2521
	42.9781
	0.422
	-8.2129
	1.0232

	Base
	121
	57
	FHEy
	LinStatic
	
	
	
	-33.9268
	-35.7919
	182.4405
	19.6667
	-14.915
	-2.8178

	Base
	121
	57
	Sx
	LinRespSpec
	Max
	
	
	11.0156
	4.7413
	46.3968
	3.0165
	6.9943
	1.9553

	Base
	121
	57
	Sy
	LinRespSpec
	Max
	
	
	34.3957
	24.9708
	150.9922
	12.1215
	16.3348
	3.2333

	Base
	121
	57
	Comb1
	Combination
	
	
	
	-8.4976
	-5.3137
	52.5921
	1.4656
	-1.4576
	0.3934

	Base
	121
	57
	Comb2
	Combination
	
	
	
	-7.2836
	-4.5546
	45.079
	1.2562
	-1.2494
	0.3372

	Base
	121
	57
	Comb3
	Combination
	
	
	
	-7.2836
	-4.5546
	45.079
	1.2562
	-1.2494
	0.3372

	Base
	121
	57
	Comb4
	Combination
	Max
	
	
	-5.71
	-3.8773
	51.7071
	1.6871
	-0.2502
	0.6165

	Base
	121
	57
	Comb4
	Combination
	Min
	
	
	-8.8573
	-5.2319
	38.4509
	0.8253
	-2.2485
	0.0579

	Base
	121
	57
	Comb5
	Combination
	Max
	
	
	-2.3685
	-0.9863
	66.6558
	2.9884
	1.0849
	0.7993

	Base
	121
	57
	Comb5
	Combination
	Min
	
	
	-12.1988
	-8.1229
	23.5022
	-0.476
	-3.5836
	-0.1248

	Base
	121
	57
	Comb6
	Combination
	
	
	
	-5.4627
	-3.4159
	33.8092
	0.9422
	-0.937
	0.2529

	Base
	121
	57
	Comb7
	Combination
	Max
	
	
	-3.8891
	-2.7386
	40.4373
	1.3731
	0.0622
	0.5322

	Base
	121
	57
	Comb7
	Combination
	Min
	
	
	-7.0364
	-4.0933
	27.1811
	0.5112
	-1.9362
	-0.0264

	Base
	121
	57
	Comb8
	Combination
	Max
	
	
	-0.5476
	0.1524
	55.386
	2.6743
	1.3972
	0.715

	Base
	121
	57
	Comb8
	Combination
	Min
	
	
	-10.3779
	-6.9843
	12.2324
	-0.79
	-3.2713
	-0.2091

	Base
	121
	57
	ENVDIS
	Combination
	Max
	
	
	-0.5476
	0.1524
	66.6558
	2.9884
	1.3972
	0.7993

	Base
	121
	57
	ENVDIS
	Combination
	Min
	
	
	-12.1988
	-8.1229
	12.2324
	-0.79
	-3.5836
	-0.2091

	Base
	121
	57
	Serv1
	Combination
	
	
	
	-6.0697
	-3.7955
	37.5658
	1.0468
	-1.0411
	0.281

	Base
	121
	57
	Serv2
	Combination
	
	
	
	-6.0697
	-3.7955
	37.5658
	1.0468
	-1.0411
	0.281

	Base
	121
	57
	Serv3
	Combination
	
	
	
	-6.0697
	-3.7955
	37.5658
	1.0468
	-1.0411
	0.281

	Base
	121
	57
	Serv4
	Combination
	Max
	
	
	-4.9681
	-3.3214
	42.2055
	1.3485
	-0.3417
	0.4765

	Base
	121
	57
	Serv4
	Combination
	Min
	
	
	-7.1713
	-4.2696
	32.9261
	0.7452
	-1.7406
	0.0855

	Base
	121
	57
	Serv5
	Combination
	Max
	
	
	-2.6301
	-1.2984
	52.665
	2.259
	0.5923
	0.6043

	Base
	121
	57
	Serv5
	Combination
	Min
	
	
	-9.5093
	-6.2926
	22.4666
	-0.1653
	-2.6746
	-0.0423

	Base
	121
	57
	Serv6
	Combination
	Max
	
	
	-5.2435
	-3.4399
	41.0456
	1.2731
	-0.5166
	0.4277

	Base
	121
	57
	Serv6
	Combination
	Min
	
	
	-6.8959
	-4.1511
	34.086
	0.8206
	-1.5657
	0.1344

	Base
	121
	57
	Serv7
	Combination
	Max
	
	
	-3.49
	-1.9227
	48.8902
	1.956
	0.184
	0.5235

	Base
	121
	57
	Serv7
	Combination
	Min
	
	
	-8.6494
	-5.6683
	26.2414
	0.1377
	-2.2662
	0.0385

	Base
	121
	57
	Serv8
	Combination
	
	
	
	-3.6418
	-2.2773
	22.5395
	0.6281
	-0.6247
	0.1686

	Base
	121
	57
	Serv9
	Combination
	Max
	
	
	-2.5403
	-1.8032
	27.1792
	0.9298
	0.0747
	0.3641

	Base
	121
	57
	Serv9
	Combination
	Min
	
	
	-4.7434
	-2.7514
	17.8998
	0.3265
	-1.3241
	-0.0269

	Base
	121
	57
	Serv10
	Combination
	Max
	
	
	-0.2023
	0.2198
	37.6387
	1.8403
	1.0088
	0.4919

	Base
	121
	57
	Serv10
	Combination
	Min
	
	
	-7.0814
	-4.7744
	7.4403
	-0.584
	-2.2582
	-0.1547

	Base
	121
	57
	ENVSERV
	Combination
	Max
	
	
	-0.2023
	0.2198
	52.665
	2.259
	1.0088
	0.6043

	Base
	121
	57
	ENVSERV
	Combination
	Min
	
	
	-9.5093
	-6.2926
	7.4403
	-0.584
	-2.6746
	-0.1547

	Base
	122
	58
	Dead
	LinStatic
	
	
	
	-0.7868
	0.1862
	14.679
	-0.3837
	0.4311
	0.4356

	Base
	122
	58
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	122
	58
	FHEx
	LinStatic
	
	
	
	-0.324
	4.7544
	36.7448
	4.0446
	0.9421
	1.0005

	Base
	122
	58
	FHEy
	LinStatic
	
	
	
	54.6664
	-36.2531
	-93.9375
	12.7829
	4.9401
	2.73

	Base
	122
	58
	Sx
	LinRespSpec
	Max
	
	
	6.3987
	4.3473
	26.3469
	4.2641
	0.9605
	1.5723

	Base
	122
	58
	Sy
	LinRespSpec
	Max
	
	
	43.8202
	19.6841
	50.2862
	6.8226
	5.0437
	3.228

	Base
	122
	58
	Comb1
	Combination
	
	
	
	-1.1015
	0.2606
	20.5506
	-0.5372
	0.6036
	0.6099

	Base
	122
	58
	Comb2
	Combination
	
	
	
	-0.9441
	0.2234
	17.6148
	-0.4605
	0.5173
	0.5227

	Base
	122
	58
	Comb3
	Combination
	
	
	
	-0.9441
	0.2234
	17.6148
	-0.4605
	0.5173
	0.5227

	Base
	122
	58
	Comb4
	Combination
	Max
	
	
	-0.03
	0.8444
	21.3787
	0.1487
	0.6546
	0.7474

	Base
	122
	58
	Comb4
	Combination
	Min
	
	
	-1.8582
	-0.3977
	13.851
	-1.0696
	0.3801
	0.2981

	Base
	122
	58
	Comb5
	Combination
	Max
	
	
	5.3178
	3.0362
	24.8007
	0.5145
	1.2381
	0.984

	Base
	122
	58
	Comb5
	Combination
	Min
	
	
	-7.206
	-2.5895
	10.4289
	-1.4354
	-0.2034
	0.0615

	Base
	122
	58
	Comb6
	Combination
	
	
	
	-0.7081
	0.1675
	13.2111
	-0.3454
	0.388
	0.3921

	Base
	122
	58
	Comb7
	Combination
	Max
	
	
	0.206
	0.7886
	16.975
	0.2638
	0.5252
	0.6167

	Base
	122
	58
	Comb7
	Combination
	Min
	
	
	-1.6222
	-0.4535
	9.4473
	-0.9545
	0.2508
	0.1674

	Base
	122
	58
	Comb8
	Combination
	Max
	
	
	5.5538
	2.9804
	20.397
	0.6296
	1.1088
	0.8533

	Base
	122
	58
	Comb8
	Combination
	Min
	
	
	-6.97
	-2.6453
	6.0252
	-1.3203
	-0.3327
	-0.0692

	Base
	122
	58
	ENVDIS
	Combination
	Max
	
	
	5.5538
	3.0362
	24.8007
	0.6296
	1.2381
	0.984

	Base
	122
	58
	ENVDIS
	Combination
	Min
	
	
	-7.206
	-2.6453
	6.0252
	-1.4354
	-0.3327
	-0.0692

	Base
	122
	58
	Serv1
	Combination
	
	
	
	-0.7868
	0.1862
	14.679
	-0.3837
	0.4311
	0.4356

	Base
	122
	58
	Serv2
	Combination
	
	
	
	-0.7868
	0.1862
	14.679
	-0.3837
	0.4311
	0.4356

	Base
	122
	58
	Serv3
	Combination
	
	
	
	-0.7868
	0.1862
	14.679
	-0.3837
	0.4311
	0.4356

	Base
	122
	58
	Serv4
	Combination
	Max
	
	
	-0.1469
	0.6209
	17.3137
	0.0427
	0.5272
	0.5929

	Base
	122
	58
	Serv4
	Combination
	Min
	
	
	-1.4266
	-0.2486
	12.0443
	-0.8101
	0.3351
	0.2784

	Base
	122
	58
	Serv5
	Combination
	Max
	
	
	3.5953
	2.1546
	19.7076
	0.2985
	0.9355
	0.7584

	Base
	122
	58
	Serv5
	Combination
	Min
	
	
	-5.1688
	-1.7823
	9.6504
	-1.066
	-0.0733
	0.1128

	Base
	122
	58
	Serv6
	Combination
	Max
	
	
	-0.3069
	0.5122
	16.655
	-0.0639
	0.5032
	0.5535

	Base
	122
	58
	Serv6
	Combination
	Min
	
	
	-1.2667
	-0.1399
	12.703
	-0.7035
	0.3591
	0.3177

	Base
	122
	58
	Serv7
	Combination
	Max
	
	
	2.4998
	1.6625
	18.4505
	0.128
	0.8094
	0.6777

	Base
	122
	58
	Serv7
	Combination
	Min
	
	
	-4.0733
	-1.2902
	10.9075
	-0.8954
	0.0528
	0.1935

	Base
	122
	58
	Serv8
	Combination
	
	
	
	-0.4721
	0.1117
	8.8074
	-0.2302
	0.2587
	0.2614

	Base
	122
	58
	Serv9
	Combination
	Max
	
	
	0.1678
	0.5464
	11.4421
	0.1962
	0.3547
	0.4186

	Base
	122
	58
	Serv9
	Combination
	Min
	
	
	-1.1119
	-0.323
	6.1727
	-0.6566
	0.1626
	0.1041

	Base
	122
	58
	Serv10
	Combination
	Max
	
	
	3.91
	2.0801
	13.836
	0.452
	0.763
	0.5842

	Base
	122
	58
	Serv10
	Combination
	Min
	
	
	-4.8541
	-1.8567
	3.7788
	-0.9125
	-0.2457
	-0.0614

	Base
	122
	58
	ENVSERV
	Combination
	Max
	
	
	3.91
	2.1546
	19.7076
	0.452
	0.9355
	0.7584

	Base
	122
	58
	ENVSERV
	Combination
	Min
	
	
	-5.1688
	-1.8567
	3.7788
	-1.066
	-0.2457
	-0.0614

	Base
	123
	61
	Dead
	LinStatic
	
	
	
	-0.5009
	4.2819
	14.1146
	-0.6716
	-0.7519
	-0.1664

	Base
	123
	61
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	123
	61
	FHEx
	LinStatic
	
	
	
	-21.187
	-12.2926
	-45.0816
	1.7778
	-5.1434
	0.5201

	Base
	123
	61
	FHEy
	LinStatic
	
	
	
	-12.2934
	-21.4755
	-86.1914
	3.4881
	35.8803
	1.5513

	Base
	123
	61
	Sx
	LinRespSpec
	Max
	
	
	22.7656
	10.6573
	41.0713
	1.8713
	4.609
	0.7903

	Base
	123
	61
	Sy
	LinRespSpec
	Max
	
	
	26.6372
	21.1291
	85.3082
	3.7621
	29.4351
	2.3789

	Base
	123
	61
	Comb1
	Combination
	
	
	
	-0.7012
	5.9947
	19.7604
	-0.9402
	-1.0526
	-0.233

	Base
	123
	61
	Comb2
	Combination
	
	
	
	-0.6011
	5.1383
	16.9375
	-0.8059
	-0.9022
	-0.1997

	Base
	123
	61
	Comb3
	Combination
	
	
	
	-0.6011
	5.1383
	16.9375
	-0.8059
	-0.9022
	-0.1997

	Base
	123
	61
	Comb4
	Combination
	Max
	
	
	2.6512
	6.6608
	22.8048
	-0.5385
	-0.2438
	-0.0868

	Base
	123
	61
	Comb4
	Combination
	Min
	
	
	-3.8533
	3.6159
	11.0702
	-1.0732
	-1.5607
	-0.3126

	Base
	123
	61
	Comb5
	Combination
	Max
	
	
	3.2054
	8.1577
	29.128
	-0.2683
	3.304
	0.1403

	Base
	123
	61
	Comb5
	Combination
	Min
	
	
	-4.4075
	2.119
	4.7469
	-1.3435
	-5.1085
	-0.5396

	Base
	123
	61
	Comb6
	Combination
	
	
	
	-0.4508
	3.8537
	12.7031
	-0.6044
	-0.6767
	-0.1498

	Base
	123
	61
	Comb7
	Combination
	Max
	
	
	2.8014
	5.3762
	18.5704
	-0.3371
	-0.0183
	-0.0369

	Base
	123
	61
	Comb7
	Combination
	Min
	
	
	-3.703
	2.3313
	6.8358
	-0.8717
	-1.3351
	-0.2627

	Base
	123
	61
	Comb8
	Combination
	Max
	
	
	3.3557
	6.8731
	24.8937
	-0.0668
	3.5296
	0.1902

	Base
	123
	61
	Comb8
	Combination
	Min
	
	
	-4.2572
	0.8344
	0.5126
	-1.142
	-4.883
	-0.4897

	Base
	123
	61
	ENVDIS
	Combination
	Max
	
	
	3.3557
	8.1577
	29.128
	-0.0668
	3.5296
	0.1902

	Base
	123
	61
	ENVDIS
	Combination
	Min
	
	
	-4.4075
	0.8344
	0.5126
	-1.3435
	-5.1085
	-0.5396

	Base
	123
	61
	Serv1
	Combination
	
	
	
	-0.5009
	4.2819
	14.1146
	-0.6716
	-0.7519
	-0.1664

	Base
	123
	61
	Serv2
	Combination
	
	
	
	-0.5009
	4.2819
	14.1146
	-0.6716
	-0.7519
	-0.1664

	Base
	123
	61
	Serv3
	Combination
	
	
	
	-0.5009
	4.2819
	14.1146
	-0.6716
	-0.7519
	-0.1664

	Base
	123
	61
	Serv4
	Combination
	Max
	
	
	1.7757
	5.3477
	18.2217
	-0.4844
	-0.291
	-0.0874

	Base
	123
	61
	Serv4
	Combination
	Min
	
	
	-2.7774
	3.2162
	10.0074
	-0.8587
	-1.2128
	-0.2454

	Base
	123
	61
	Serv5
	Combination
	Max
	
	
	2.1628
	6.3948
	22.6454
	-0.2954
	2.1916
	0.0715

	Base
	123
	61
	Serv5
	Combination
	Min
	
	
	-3.1646
	2.169
	5.5837
	-1.0478
	-3.6954
	-0.4043

	Base
	123
	61
	Serv6
	Combination
	Max
	
	
	1.2065
	5.0812
	17.1949
	-0.5312
	-0.4062
	-0.1071

	Base
	123
	61
	Serv6
	Combination
	Min
	
	
	-2.2083
	3.4826
	11.0342
	-0.8119
	-1.0975
	-0.2257

	Base
	123
	61
	Serv7
	Combination
	Max
	
	
	1.4969
	5.8666
	20.5127
	-0.3894
	1.4558
	0.012

	Base
	123
	61
	Serv7
	Combination
	Min
	
	
	-2.4987
	2.6972
	7.7165
	-0.9537
	-2.9595
	-0.3448

	Base
	123
	61
	Serv8
	Combination
	
	
	
	-0.3005
	2.5692
	8.4687
	-0.4029
	-0.4511
	-0.0998

	Base
	123
	61
	Serv9
	Combination
	Max
	
	
	1.976
	3.6349
	12.5759
	-0.2158
	0.0098
	-0.0208

	Base
	123
	61
	Serv9
	Combination
	Min
	
	
	-2.5771
	1.5034
	4.3616
	-0.5901
	-0.912
	-0.1789

	Base
	123
	61
	Serv10
	Combination
	Max
	
	
	2.3632
	4.6821
	16.9996
	-0.0267
	2.4924
	0.138

	Base
	123
	61
	Serv10
	Combination
	Min
	
	
	-2.9642
	0.4562
	-0.0621
	-0.7791
	-3.3946
	-0.3377

	Base
	123
	61
	ENVSERV
	Combination
	Max
	
	
	2.3632
	6.3948
	22.6454
	-0.0267
	2.4924
	0.138

	Base
	123
	61
	ENVSERV
	Combination
	Min
	
	
	-3.1646
	0.4562
	-0.0621
	-1.0478
	-3.6954
	-0.4043

	Base
	124
	60
	Dead
	LinStatic
	
	
	
	-3.6159
	-5.4112
	34.4308
	1.5338
	-1.232
	0.3311

	Base
	124
	60
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	124
	60
	FHEx
	LinStatic
	
	
	
	-5.7061
	5.702
	24.095
	-3.6697
	-6.878
	0.7853

	Base
	124
	60
	FHEy
	LinStatic
	
	
	
	26.8101
	-37.853
	89.4603
	14.5348
	-0.6695
	3.7871

	Base
	124
	60
	Sx
	LinRespSpec
	Max
	
	
	3.4525
	4.6136
	26.8976
	3.1102
	6.1647
	1.2102

	Base
	124
	60
	Sy
	LinRespSpec
	Max
	
	
	24.1632
	32.441
	76.3926
	8.799
	5.0712
	4.4034

	Base
	124
	60
	Comb1
	Combination
	
	
	
	-5.0623
	-7.5756
	48.2031
	2.1473
	-1.7248
	0.4636

	Base
	124
	60
	Comb2
	Combination
	
	
	
	-4.3391
	-6.4934
	41.3169
	1.8405
	-1.4784
	0.3974

	Base
	124
	60
	Comb3
	Combination
	
	
	
	-4.3391
	-6.4934
	41.3169
	1.8405
	-1.4784
	0.3974

	Base
	124
	60
	Comb4
	Combination
	Max
	
	
	-3.8459
	-5.8343
	45.1594
	2.2848
	-0.5977
	0.5703

	Base
	124
	60
	Comb4
	Combination
	Min
	
	
	-4.8323
	-7.1525
	37.4744
	1.3962
	-2.359
	0.2245

	Base
	124
	60
	Comb5
	Combination
	Max
	
	
	-0.8862
	-1.8576
	52.2334
	3.0979
	-0.7537
	1.0266

	Base
	124
	60
	Comb5
	Combination
	Min
	
	
	-7.792
	-11.1292
	30.4004
	0.5832
	-2.203
	-0.2319

	Base
	124
	60
	Comb6
	Combination
	
	
	
	-3.2543
	-4.87
	30.9877
	1.3804
	-1.1088
	0.298

	Base
	124
	60
	Comb7
	Combination
	Max
	
	
	-2.7611
	-4.211
	34.8302
	1.8247
	-0.2281
	0.4709

	Base
	124
	60
	Comb7
	Combination
	Min
	
	
	-3.7475
	-5.5291
	27.1452
	0.9361
	-1.9894
	0.1251

	Base
	124
	60
	Comb8
	Combination
	Max
	
	
	0.1986
	-0.2342
	41.9042
	2.6378
	-0.3841
	0.9273

	Base
	124
	60
	Comb8
	Combination
	Min
	
	
	-6.7073
	-9.5059
	20.0712
	0.123
	-1.8334
	-0.3312

	Base
	124
	60
	ENVDIS
	Combination
	Max
	
	
	0.1986
	-0.2342
	52.2334
	3.0979
	-0.2281
	1.0266

	Base
	124
	60
	ENVDIS
	Combination
	Min
	
	
	-7.792
	-11.1292
	20.0712
	0.123
	-2.359
	-0.3312

	Base
	124
	60
	Serv1
	Combination
	
	
	
	-3.6159
	-5.4112
	34.4308
	1.5338
	-1.232
	0.3311

	Base
	124
	60
	Serv2
	Combination
	
	
	
	-3.6159
	-5.4112
	34.4308
	1.5338
	-1.232
	0.3311

	Base
	124
	60
	Serv3
	Combination
	
	
	
	-3.6159
	-5.4112
	34.4308
	1.5338
	-1.232
	0.3311

	Base
	124
	60
	Serv4
	Combination
	Max
	
	
	-3.2707
	-4.9498
	37.1205
	1.8448
	-0.6155
	0.4522

	Base
	124
	60
	Serv4
	Combination
	Min
	
	
	-3.9612
	-5.8725
	31.741
	1.2228
	-1.8484
	0.2101

	Base
	124
	60
	Serv5
	Combination
	Max
	
	
	-1.1996
	-2.1671
	42.07
	2.4137
	-0.7248
	0.7715

	Base
	124
	60
	Serv5
	Combination
	Min
	
	
	-6.0322
	-8.6553
	26.7915
	0.6539
	-1.7391
	-0.1092

	Base
	124
	60
	Serv6
	Combination
	Max
	
	
	-3.357
	-5.0651
	36.4481
	1.767
	-0.7696
	0.4219

	Base
	124
	60
	Serv6
	Combination
	Min
	
	
	-3.8749
	-5.7572
	32.4134
	1.3005
	-1.6943
	0.2404

	Base
	124
	60
	Serv7
	Combination
	Max
	
	
	-1.8037
	-2.9781
	40.1602
	2.1937
	-0.8516
	0.6614

	Base
	124
	60
	Serv7
	Combination
	Min
	
	
	-5.4282
	-7.8442
	28.7013
	0.8739
	-1.6123
	0.0009

	Base
	124
	60
	Serv8
	Combination
	
	
	
	-2.1696
	-3.2467
	20.6585
	0.9203
	-0.7392
	0.1987

	Base
	124
	60
	Serv9
	Combination
	Max
	
	
	-1.8243
	-2.7853
	23.3482
	1.2313
	-0.1227
	0.3197

	Base
	124
	60
	Serv9
	Combination
	Min
	
	
	-2.5148
	-3.7081
	17.9687
	0.6092
	-1.3557
	0.0777

	Base
	124
	60
	Serv10
	Combination
	Max
	
	
	0.2468
	-0.0026
	28.2977
	1.8002
	-0.2321
	0.639

	Base
	124
	60
	Serv10
	Combination
	Min
	
	
	-4.5859
	-6.4908
	13.0192
	0.0404
	-1.2463
	-0.2417

	Base
	124
	60
	ENVSERV
	Combination
	Max
	
	
	0.2468
	-0.0026
	42.07
	2.4137
	-0.1227
	0.7715

	Base
	124
	60
	ENVSERV
	Combination
	Min
	
	
	-6.0322
	-8.6553
	13.0192
	0.0404
	-1.8484
	-0.2417

	Base
	125
	59
	Dead
	LinStatic
	
	
	
	0.2844
	0.5527
	9.023
	2.0135
	0.6903
	0.556

	Base
	125
	59
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	125
	59
	FHEx
	LinStatic
	
	
	
	-2.7074
	8.2799
	-6.7029
	-6.645
	0.6179
	0.124

	Base
	125
	59
	FHEy
	LinStatic
	
	
	
	-59.5212
	-35.1169
	-133.6929
	21.3488
	-1.2111
	3.6884

	Base
	125
	59
	Sx
	LinRespSpec
	Max
	
	
	8.0744
	8.9072
	18.9833
	4.4245
	1.0325
	0.6323

	Base
	125
	59
	Sy
	LinRespSpec
	Max
	
	
	48.563
	19.5242
	97.0446
	17.9602
	1.3103
	3.6995

	Base
	125
	59
	Comb1
	Combination
	
	
	
	0.3982
	0.7737
	12.6322
	2.8189
	0.9665
	0.7783

	Base
	125
	59
	Comb2
	Combination
	
	
	
	0.3413
	0.6632
	10.8276
	2.4162
	0.8284
	0.6672

	Base
	125
	59
	Comb3
	Combination
	
	
	
	0.3413
	0.6632
	10.8276
	2.4162
	0.8284
	0.6672

	Base
	125
	59
	Comb4
	Combination
	Max
	
	
	1.4948
	1.9357
	13.5395
	3.0482
	0.9759
	0.7575

	Base
	125
	59
	Comb4
	Combination
	Min
	
	
	-0.8121
	-0.6093
	8.1157
	1.7841
	0.6809
	0.5768

	Base
	125
	59
	Comb5
	Combination
	Max
	
	
	7.281
	3.4532
	24.6953
	4.9827
	1.0156
	1.1958

	Base
	125
	59
	Comb5
	Combination
	Min
	
	
	-6.5983
	-2.1268
	-3.0401
	-0.1503
	0.6412
	0.1385

	Base
	125
	59
	Comb6
	Combination
	
	
	
	0.256
	0.4974
	8.1207
	1.8121
	0.6213
	0.5004

	Base
	125
	59
	Comb7
	Combination
	Max
	
	
	1.4095
	1.7699
	10.8326
	2.4442
	0.7688
	0.5907

	Base
	125
	59
	Comb7
	Combination
	Min
	
	
	-0.8975
	-0.7751
	5.4088
	1.18
	0.4738
	0.41

	Base
	125
	59
	Comb8
	Combination
	Max
	
	
	7.1957
	3.2874
	21.9884
	4.3786
	0.8085
	1.029

	Base
	125
	59
	Comb8
	Combination
	Min
	
	
	-6.6837
	-2.2926
	-5.747
	-0.7544
	0.4341
	-0.0283

	Base
	125
	59
	ENVDIS
	Combination
	Max
	
	
	7.281
	3.4532
	24.6953
	4.9827
	1.0156
	1.1958

	Base
	125
	59
	ENVDIS
	Combination
	Min
	
	
	-6.6837
	-2.2926
	-5.747
	-0.7544
	0.4341
	-0.0283

	Base
	125
	59
	Serv1
	Combination
	
	
	
	0.2844
	0.5527
	9.023
	2.0135
	0.6903
	0.556

	Base
	125
	59
	Serv2
	Combination
	
	
	
	0.2844
	0.5527
	9.023
	2.0135
	0.6903
	0.556

	Base
	125
	59
	Serv3
	Combination
	
	
	
	0.2844
	0.5527
	9.023
	2.0135
	0.6903
	0.556

	Base
	125
	59
	Serv4
	Combination
	Max
	
	
	1.0919
	1.4434
	10.9213
	2.4559
	0.7936
	0.6192

	Base
	125
	59
	Serv4
	Combination
	Min
	
	
	-0.523
	-0.3381
	7.1247
	1.571
	0.5871
	0.4927

	Base
	125
	59
	Serv5
	Combination
	Max
	
	
	5.1407
	2.5051
	18.7275
	3.8095
	0.8214
	0.9259

	Base
	125
	59
	Serv5
	Combination
	Min
	
	
	-4.5719
	-1.3998
	-0.6814
	0.2175
	0.5593
	0.186

	Base
	125
	59
	Serv6
	Combination
	Max
	
	
	0.89
	1.2207
	10.4468
	2.3453
	0.7678
	0.6034

	Base
	125
	59
	Serv6
	Combination
	Min
	
	
	-0.3211
	-0.1154
	7.5993
	1.6816
	0.6129
	0.5085

	Base
	125
	59
	Serv7
	Combination
	Max
	
	
	3.9267
	2.017
	16.3014
	3.3605
	0.7886
	0.8334

	Base
	125
	59
	Serv7
	Combination
	Min
	
	
	-3.3578
	-0.9117
	1.7447
	0.6665
	0.5921
	0.2785

	Base
	125
	59
	Serv8
	Combination
	
	
	
	0.1707
	0.3316
	5.4138
	1.2081
	0.4142
	0.3336

	Base
	125
	59
	Serv9
	Combination
	Max
	
	
	0.9781
	1.2223
	7.3121
	1.6505
	0.5175
	0.3968

	Base
	125
	59
	Serv9
	Combination
	Min
	
	
	-0.6368
	-0.5591
	3.5155
	0.7656
	0.3109
	0.2703

	Base
	125
	59
	Serv10
	Combination
	Max
	
	
	5.027
	2.284
	15.1183
	3.0041
	0.5452
	0.7035

	Base
	125
	59
	Serv10
	Combination
	Min
	
	
	-4.6856
	-1.6208
	-4.2907
	-0.5879
	0.2832
	-0.0364

	Base
	125
	59
	ENVSERV
	Combination
	Max
	
	
	5.1407
	2.5051
	18.7275
	3.8095
	0.8214
	0.9259

	Base
	125
	59
	ENVSERV
	Combination
	Min
	
	
	-4.6856
	-1.6208
	-4.2907
	-0.5879
	0.2832
	-0.0364

	Base
	128
	89
	Dead
	LinStatic
	
	
	
	4.1145
	-4.1296
	57.9752
	4.3232
	2.5167
	1.5523

	Base
	128
	89
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	128
	89
	FHEx
	LinStatic
	
	
	
	-41.5769
	4.6135
	-69.6498
	0.8116
	-17.5411
	-0.9125

	Base
	128
	89
	FHEy
	LinStatic
	
	
	
	-15.4616
	-21.0682
	347.9877
	-1.5695
	1.5691
	-15.7124

	Base
	128
	89
	Sx
	LinRespSpec
	Max
	
	
	13.1221
	2.8692
	36.036
	1.2226
	8.4315
	3.9094

	Base
	128
	89
	Sy
	LinRespSpec
	Max
	
	
	16.8663
	23.4229
	354.1956
	1.695
	2.195
	18.3741

	Base
	128
	89
	Comb1
	Combination
	
	
	
	5.7603
	-5.7815
	81.1652
	6.0525
	3.5234
	2.1732

	Base
	128
	89
	Comb2
	Combination
	
	
	
	4.9374
	-4.9556
	69.5702
	5.1879
	3.0201
	1.8627

	Base
	128
	89
	Comb3
	Combination
	
	
	
	4.9374
	-4.9556
	69.5702
	5.1879
	3.0201
	1.8627

	Base
	128
	89
	Comb4
	Combination
	Max
	
	
	6.812
	-4.5457
	74.7182
	5.3625
	4.2246
	2.4212

	Base
	128
	89
	Comb4
	Combination
	Min
	
	
	3.0628
	-5.3655
	64.4222
	5.0132
	1.8156
	1.3043

	Base
	128
	89
	Comb5
	Combination
	Max
	
	
	7.3476
	-1.6084
	120.1848
	5.4301
	3.3337
	4.4884

	Base
	128
	89
	Comb5
	Combination
	Min
	
	
	2.5272
	-8.3027
	18.9556
	4.9457
	2.7064
	-0.7629

	Base
	128
	89
	Comb6
	Combination
	
	
	
	3.7031
	-3.7167
	52.1776
	3.8909
	2.265
	1.3971

	Base
	128
	89
	Comb7
	Combination
	Max
	
	
	5.5777
	-3.3068
	57.3256
	4.0656
	3.4695
	1.9555

	Base
	128
	89
	Comb7
	Combination
	Min
	
	
	1.8285
	-4.1266
	47.0296
	3.7162
	1.0605
	0.8386

	Base
	128
	89
	Comb8
	Combination
	Max
	
	
	6.1133
	-0.3695
	102.7922
	4.1331
	2.5787
	4.0227

	Base
	128
	89
	Comb8
	Combination
	Min
	
	
	1.2929
	-7.0638
	1.5631
	3.6487
	1.9514
	-1.2286

	Base
	128
	89
	ENVDIS
	Combination
	Max
	
	
	7.3476
	-0.3695
	120.1848
	6.0525
	4.2246
	4.4884

	Base
	128
	89
	ENVDIS
	Combination
	Min
	
	
	1.2929
	-8.3027
	1.5631
	3.6487
	1.0605
	-1.2286

	Base
	128
	89
	Serv1
	Combination
	
	
	
	4.1145
	-4.1296
	57.9752
	4.3232
	2.5167
	1.5523

	Base
	128
	89
	Serv2
	Combination
	
	
	
	4.1145
	-4.1296
	57.9752
	4.3232
	2.5167
	1.5523

	Base
	128
	89
	Serv3
	Combination
	
	
	
	4.1145
	-4.1296
	57.9752
	4.3232
	2.5167
	1.5523

	Base
	128
	89
	Serv4
	Combination
	Max
	
	
	5.4267
	-3.8427
	61.5788
	4.4455
	3.3599
	1.9432

	Base
	128
	89
	Serv4
	Combination
	Min
	
	
	2.8023
	-4.4166
	54.3716
	4.201
	1.6736
	1.1613

	Base
	128
	89
	Serv5
	Combination
	Max
	
	
	5.8011
	-1.7874
	93.3947
	4.4927
	2.7362
	3.3897

	Base
	128
	89
	Serv5
	Combination
	Min
	
	
	2.4279
	-6.4719
	22.5556
	4.1537
	2.2972
	-0.2851

	Base
	128
	89
	Serv6
	Combination
	Max
	
	
	5.0987
	-3.9145
	60.6779
	4.4149
	3.1491
	1.8455

	Base
	128
	89
	Serv6
	Combination
	Min
	
	
	3.1304
	-4.3448
	55.2725
	4.2315
	1.8844
	1.2591

	Base
	128
	89
	Serv7
	Combination
	Max
	
	
	5.3795
	-2.3729
	84.5398
	4.4503
	2.6813
	2.9303

	Base
	128
	89
	Serv7
	Combination
	Min
	
	
	2.8495
	-5.8864
	31.4105
	4.1961
	2.3521
	0.1742

	Base
	128
	89
	Serv8
	Combination
	
	
	
	2.4687
	-2.4778
	34.7851
	2.5939
	1.51
	0.9314

	Base
	128
	89
	Serv9
	Combination
	Max
	
	
	3.7809
	-2.1909
	38.3887
	2.7162
	2.3532
	1.3223

	Base
	128
	89
	Serv9
	Combination
	Min
	
	
	1.1565
	-2.7647
	31.1815
	2.4717
	0.6669
	0.5404

	Base
	128
	89
	Serv10
	Combination
	Max
	
	
	4.1553
	-0.1355
	70.2047
	2.7634
	1.7295
	2.7688

	Base
	128
	89
	Serv10
	Combination
	Min
	
	
	0.7821
	-4.8201
	-0.6345
	2.4244
	1.2905
	-0.906

	Base
	128
	89
	ENVSERV
	Combination
	Max
	
	
	5.8011
	-0.1355
	93.3947
	4.4927
	3.3599
	3.3897

	Base
	128
	89
	ENVSERV
	Combination
	Min
	
	
	0.7821
	-6.4719
	-0.6345
	2.4244
	0.6669
	-0.906

	Base
	129
	92
	Dead
	LinStatic
	
	
	
	-5.9242
	-4.5778
	47.5935
	3.9768
	-1.7655
	-1.3785

	Base
	129
	92
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	129
	92
	FHEx
	LinStatic
	
	
	
	-31.916
	-2.9725
	19.1794
	0.229
	-11.1374
	1.1424

	Base
	129
	92
	FHEy
	LinStatic
	
	
	
	-16.3216
	-25.6475
	359.6202
	-5.5335
	4.8312
	15.923

	Base
	129
	92
	Sx
	LinRespSpec
	Max
	
	
	10.0145
	5.8148
	38.0369
	0.7314
	5.14
	6.2944

	Base
	129
	92
	Sy
	LinRespSpec
	Max
	
	
	17.0365
	27.1907
	367.8444
	5.7041
	4.5894
	18.2086

	Base
	129
	92
	Comb1
	Combination
	
	
	
	-8.2938
	-6.4089
	66.6309
	5.5676
	-2.4718
	-1.9299

	Base
	129
	92
	Comb2
	Combination
	
	
	
	-7.109
	-5.4934
	57.1122
	4.7722
	-2.1186
	-1.6542

	Base
	129
	92
	Comb3
	Combination
	
	
	
	-7.109
	-5.4934
	57.1122
	4.7722
	-2.1186
	-1.6542

	Base
	129
	92
	Comb4
	Combination
	Max
	
	
	-5.6784
	-4.6627
	62.546
	4.8767
	-1.3844
	-0.755

	Base
	129
	92
	Comb4
	Combination
	Min
	
	
	-8.5397
	-6.3241
	51.6783
	4.6677
	-2.8529
	-2.5534

	Base
	129
	92
	Comb5
	Combination
	Max
	
	
	-4.6745
	-1.6078
	109.6772
	5.5873
	-1.4628
	0.9478

	Base
	129
	92
	Comb5
	Combination
	Min
	
	
	-9.5435
	-9.3789
	4.5472
	3.9571
	-2.7745
	-4.2562

	Base
	129
	92
	Comb6
	Combination
	
	
	
	-5.3318
	-4.12
	42.8341
	3.5791
	-1.589
	-1.2407

	Base
	129
	92
	Comb7
	Combination
	Max
	
	
	-3.9011
	-3.2894
	48.268
	3.6836
	-0.8547
	-0.3415

	Base
	129
	92
	Comb7
	Combination
	Min
	
	
	-6.7624
	-4.9507
	37.4003
	3.4747
	-2.3233
	-2.1399

	Base
	129
	92
	Comb8
	Combination
	Max
	
	
	-2.8972
	-0.2345
	95.3991
	4.3943
	-0.9332
	1.3613

	Base
	129
	92
	Comb8
	Combination
	Min
	
	
	-7.7663
	-8.0056
	-9.7308
	2.764
	-2.2448
	-3.8427

	Base
	129
	92
	ENVDIS
	Combination
	Max
	
	
	-2.8972
	-0.2345
	109.6772
	5.5873
	-0.8547
	1.3613

	Base
	129
	92
	ENVDIS
	Combination
	Min
	
	
	-9.5435
	-9.3789
	-9.7308
	2.764
	-2.8529
	-4.2562

	Base
	129
	92
	Serv1
	Combination
	
	
	
	-5.9242
	-4.5778
	47.5935
	3.9768
	-1.7655
	-1.3785

	Base
	129
	92
	Serv2
	Combination
	
	
	
	-5.9242
	-4.5778
	47.5935
	3.9768
	-1.7655
	-1.3785

	Base
	129
	92
	Serv3
	Combination
	
	
	
	-5.9242
	-4.5778
	47.5935
	3.9768
	-1.7655
	-1.3785

	Base
	129
	92
	Serv4
	Combination
	Max
	
	
	-4.9227
	-3.9963
	51.3972
	4.05
	-1.2515
	-0.7491

	Base
	129
	92
	Serv4
	Combination
	Min
	
	
	-6.9256
	-5.1593
	43.7898
	3.9037
	-2.2795
	-2.008

	Base
	129
	92
	Serv5
	Combination
	Max
	
	
	-4.2205
	-1.8587
	84.3779
	4.5472
	-1.3066
	0.4423

	Base
	129
	92
	Serv5
	Combination
	Min
	
	
	-7.6278
	-7.2969
	10.809
	3.4064
	-2.2245
	-3.1994

	Base
	129
	92
	Serv6
	Combination
	Max
	
	
	-5.1731
	-4.1417
	50.4463
	4.0317
	-1.38
	-0.9064

	Base
	129
	92
	Serv6
	Combination
	Min
	
	
	-6.6753
	-5.0139
	44.7407
	3.922
	-2.151
	-1.8506

	Base
	129
	92
	Serv7
	Combination
	Max
	
	
	-4.6464
	-2.5385
	75.1818
	4.4046
	-1.4213
	-0.0129

	Base
	129
	92
	Serv7
	Combination
	Min
	
	
	-7.2019
	-6.6171
	20.0051
	3.549
	-2.1097
	-2.7442

	Base
	129
	92
	Serv8
	Combination
	
	
	
	-3.5545
	-2.7467
	28.5561
	2.3861
	-1.0593
	-0.8271

	Base
	129
	92
	Serv9
	Combination
	Max
	
	
	-2.5531
	-2.1652
	32.3598
	2.4592
	-0.5453
	-0.1977

	Base
	129
	92
	Serv9
	Combination
	Min
	
	
	-4.556
	-3.3282
	24.7524
	2.313
	-1.5733
	-1.4566

	Base
	129
	92
	Serv10
	Combination
	Max
	
	
	-1.8509
	-0.0276
	65.3405
	2.9565
	-0.6004
	0.9938

	Base
	129
	92
	Serv10
	Combination
	Min
	
	
	-5.2582
	-5.4658
	-8.2284
	1.8157
	-1.5183
	-2.648

	Base
	129
	92
	ENVSERV
	Combination
	Max
	
	
	-1.8509
	-0.0276
	84.3779
	4.5472
	-0.5453
	0.9938

	Base
	129
	92
	ENVSERV
	Combination
	Min
	
	
	-7.6278
	-7.2969
	-8.2284
	1.8157
	-2.2795
	-3.1994

	Base
	130
	93
	Dead
	LinStatic
	
	
	
	-3.4106
	3.886
	26.4821
	-1.8877
	-0.7919
	0.4047

	Base
	130
	93
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	130
	93
	FHEx
	LinStatic
	
	
	
	-32.119
	4.5259
	71.4245
	0.3813
	-10.4095
	-0.6878

	Base
	130
	93
	FHEy
	LinStatic
	
	
	
	-23.3731
	-6.9858
	-300.9608
	-5.5618
	-19.6721
	10.5197

	Base
	130
	93
	Sx
	LinRespSpec
	Max
	
	
	10.6043
	2.7809
	43.1486
	0.9313
	5.2088
	4.3982

	Base
	130
	93
	Sy
	LinRespSpec
	Max
	
	
	26.2358
	7.3421
	305.3106
	5.7319
	19.9642
	12.2207

	Base
	130
	93
	Comb1
	Combination
	
	
	
	-4.7748
	5.4403
	37.0749
	-2.6427
	-1.1086
	0.5666

	Base
	130
	93
	Comb2
	Combination
	
	
	
	-4.0927
	4.6632
	31.7785
	-2.2652
	-0.9502
	0.4856

	Base
	130
	93
	Comb3
	Combination
	
	
	
	-4.0927
	4.6632
	31.7785
	-2.2652
	-0.9502
	0.4856

	Base
	130
	93
	Comb4
	Combination
	Max
	
	
	-2.5778
	5.0604
	37.9426
	-2.1321
	-0.2061
	1.1139

	Base
	130
	93
	Comb4
	Combination
	Min
	
	
	-5.6076
	4.2659
	25.6144
	-2.3982
	-1.6944
	-0.1427

	Base
	130
	93
	Comb5
	Combination
	Max
	
	
	-0.3436
	5.7123
	75.4074
	-1.4461
	1.9026
	2.232

	Base
	130
	93
	Comb5
	Combination
	Min
	
	
	-7.8418
	3.614
	-11.8504
	-3.0843
	-3.8031
	-1.2607

	Base
	130
	93
	Comb6
	Combination
	
	
	
	-3.0695
	3.4974
	23.8339
	-1.6989
	-0.7127
	0.3642

	Base
	130
	93
	Comb7
	Combination
	Max
	
	
	-1.5546
	3.8946
	29.998
	-1.5658
	0.0314
	0.9925

	Base
	130
	93
	Comb7
	Combination
	Min
	
	
	-4.5844
	3.1001
	17.6698
	-1.8319
	-1.4568
	-0.2641

	Base
	130
	93
	Comb8
	Combination
	Max
	
	
	0.6796
	4.5465
	67.4628
	-0.8798
	2.1402
	2.1106

	Base
	130
	93
	Comb8
	Combination
	Min
	
	
	-6.8186
	2.4482
	-19.795
	-2.518
	-3.5656
	-1.3821

	Base
	130
	93
	ENVDIS
	Combination
	Max
	
	
	0.6796
	5.7123
	75.4074
	-0.8798
	2.1402
	2.232

	Base
	130
	93
	ENVDIS
	Combination
	Min
	
	
	-7.8418
	2.4482
	-19.795
	-3.0843
	-3.8031
	-1.3821

	Base
	130
	93
	Serv1
	Combination
	
	
	
	-3.4106
	3.886
	26.4821
	-1.8877
	-0.7919
	0.4047

	Base
	130
	93
	Serv2
	Combination
	
	
	
	-3.4106
	3.886
	26.4821
	-1.8877
	-0.7919
	0.4047

	Base
	130
	93
	Serv3
	Combination
	
	
	
	-3.4106
	3.886
	26.4821
	-1.8877
	-0.7919
	0.4047

	Base
	130
	93
	Serv4
	Combination
	Max
	
	
	-2.3501
	4.164
	30.7969
	-1.7945
	-0.271
	0.8445

	Base
	130
	93
	Serv4
	Combination
	Min
	
	
	-4.471
	3.6079
	22.1672
	-1.9808
	-1.3127
	-0.0351

	Base
	130
	93
	Serv5
	Combination
	Max
	
	
	-0.787
	4.6202
	57.0132
	-1.3145
	1.2046
	1.6268

	Base
	130
	93
	Serv5
	Combination
	Min
	
	
	-6.0342
	3.1518
	-4.049
	-2.4608
	-2.7883
	-0.8174

	Base
	130
	93
	Serv6
	Combination
	Max
	
	
	-2.6153
	4.0945
	29.7182
	-1.8178
	-0.4012
	0.7346

	Base
	130
	93
	Serv6
	Combination
	Min
	
	
	-4.2059
	3.6774
	23.2459
	-1.9575
	-1.1825
	0.0748

	Base
	130
	93
	Serv7
	Combination
	Max
	
	
	-1.4429
	4.4366
	49.3804
	-1.4578
	0.7054
	1.3212

	Base
	130
	93
	Serv7
	Combination
	Min
	
	
	-5.3783
	3.3353
	3.5838
	-2.3175
	-2.2892
	-0.5119

	Base
	130
	93
	Serv8
	Combination
	
	
	
	-2.0463
	2.3316
	15.8893
	-1.1326
	-0.4751
	0.2428

	Base
	130
	93
	Serv9
	Combination
	Max
	
	
	-0.9859
	2.6097
	20.2041
	-1.0395
	0.0458
	0.6826

	Base
	130
	93
	Serv9
	Combination
	Min
	
	
	-3.1068
	2.0535
	11.5744
	-1.2257
	-0.996
	-0.197

	Base
	130
	93
	Serv10
	Combination
	Max
	
	
	0.5772
	3.0658
	46.4203
	-0.5594
	1.5213
	1.4649

	Base
	130
	93
	Serv10
	Combination
	Min
	
	
	-4.6699
	1.5974
	-14.6418
	-1.7058
	-2.4715
	-0.9793

	Base
	130
	93
	ENVSERV
	Combination
	Max
	
	
	0.5772
	4.6202
	57.0132
	-0.5594
	1.5213
	1.6268

	Base
	130
	93
	ENVSERV
	Combination
	Min
	
	
	-6.0342
	1.5974
	-14.6418
	-2.4608
	-2.7883
	-0.9793

	Base
	131
	96
	Dead
	LinStatic
	
	
	
	2.2298
	2.4695
	22.1617
	-0.8703
	0.9648
	-0.0508

	Base
	131
	96
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	131
	96
	FHEx
	LinStatic
	
	
	
	-36.6098
	-4.145
	-27.4156
	0.8326
	-8.8483
	0.2577

	Base
	131
	96
	FHEy
	LinStatic
	
	
	
	-31.8105
	-12.4256
	-392.2163
	-0.9726
	-8.1979
	-5.0688

	Base
	131
	96
	Sx
	LinRespSpec
	Max
	
	
	11.325
	2.0893
	23.0246
	1.0989
	3.4756
	0.8221

	Base
	131
	96
	Sy
	LinRespSpec
	Max
	
	
	34.2426
	11.8075
	401.3301
	0.9183
	8.2515
	5.567

	Base
	131
	96
	Comb1
	Combination
	
	
	
	3.1217
	3.4572
	31.0264
	-1.2184
	1.3507
	-0.0712

	Base
	131
	96
	Comb2
	Combination
	
	
	
	2.6757
	2.9633
	26.5941
	-1.0444
	1.1577
	-0.061

	Base
	131
	96
	Comb3
	Combination
	
	
	
	2.6757
	2.9633
	26.5941
	-1.0444
	1.1577
	-0.061

	Base
	131
	96
	Comb4
	Combination
	Max
	
	
	4.2936
	3.2618
	29.8833
	-0.8874
	1.6543
	0.0564

	Base
	131
	96
	Comb4
	Combination
	Min
	
	
	1.0579
	2.6649
	23.3049
	-1.2014
	0.6612
	-0.1785

	Base
	131
	96
	Comb5
	Combination
	Max
	
	
	7.569
	4.6506
	83.9442
	-0.9132
	2.3369
	0.7345

	Base
	131
	96
	Comb5
	Combination
	Min
	
	
	-2.2175
	1.276
	-30.756
	-1.1756
	-0.0214
	-0.8565

	Base
	131
	96
	Comb6
	Combination
	
	
	
	2.0068
	2.2225
	19.9456
	-0.7833
	0.8683
	-0.0458

	Base
	131
	96
	Comb7
	Combination
	Max
	
	
	3.6247
	2.521
	23.2348
	-0.6263
	1.3648
	0.0717

	Base
	131
	96
	Comb7
	Combination
	Min
	
	
	0.3889
	1.924
	16.6563
	-0.9403
	0.3718
	-0.1632

	Base
	131
	96
	Comb8
	Combination
	Max
	
	
	6.9001
	3.9098
	77.2956
	-0.6521
	2.0474
	0.7498

	Base
	131
	96
	Comb8
	Combination
	Min
	
	
	-2.8865
	0.5352
	-37.4045
	-0.9145
	-0.3108
	-0.8413

	Base
	131
	96
	ENVDIS
	Combination
	Max
	
	
	7.569
	4.6506
	83.9442
	-0.6263
	2.3369
	0.7498

	Base
	131
	96
	ENVDIS
	Combination
	Min
	
	
	-2.8865
	0.5352
	-37.4045
	-1.2184
	-0.3108
	-0.8565

	Base
	131
	96
	Serv1
	Combination
	
	
	
	2.2298
	2.4695
	22.1617
	-0.8703
	0.9648
	-0.0508

	Base
	131
	96
	Serv2
	Combination
	
	
	
	2.2298
	2.4695
	22.1617
	-0.8703
	0.9648
	-0.0508

	Base
	131
	96
	Serv3
	Combination
	
	
	
	2.2298
	2.4695
	22.1617
	-0.8703
	0.9648
	-0.0508

	Base
	131
	96
	Serv4
	Combination
	Max
	
	
	3.3623
	2.6784
	24.4642
	-0.7604
	1.3123
	0.0314

	Base
	131
	96
	Serv4
	Combination
	Min
	
	
	1.0973
	2.2605
	19.8593
	-0.9802
	0.6172
	-0.1331

	Base
	131
	96
	Serv5
	Combination
	Max
	
	
	5.654
	3.6502
	62.2948
	-0.7785
	1.7899
	0.5059

	Base
	131
	96
	Serv5
	Combination
	Min
	
	
	-1.1945
	1.2887
	-17.9713
	-0.9621
	0.1396
	-0.6075

	Base
	131
	96
	Serv6
	Combination
	Max
	
	
	3.0792
	2.6261
	23.8886
	-0.7879
	1.2255
	0.0108

	Base
	131
	96
	Serv6
	Combination
	Min
	
	
	1.3804
	2.3128
	20.4349
	-0.9527
	0.7041
	-0.1125

	Base
	131
	96
	Serv7
	Combination
	Max
	
	
	4.798
	3.355
	52.2615
	-0.8014
	1.5837
	0.3667

	Base
	131
	96
	Serv7
	Combination
	Min
	
	
	-0.3384
	1.5839
	-7.938
	-0.9392
	0.3459
	-0.4684

	Base
	131
	96
	Serv8
	Combination
	
	
	
	1.3379
	1.4817
	13.297
	-0.5222
	0.5789
	-0.0305

	Base
	131
	96
	Serv9
	Combination
	Max
	
	
	2.4704
	1.6906
	15.5995
	-0.4123
	0.9264
	0.0517

	Base
	131
	96
	Serv9
	Combination
	Min
	
	
	0.2054
	1.2727
	10.9946
	-0.6321
	0.2313
	-0.1127

	Base
	131
	96
	Serv10
	Combination
	Max
	
	
	4.7621
	2.6624
	53.4301
	-0.4304
	1.404
	0.5262

	Base
	131
	96
	Serv10
	Combination
	Min
	
	
	-2.0864
	0.3009
	-26.836
	-0.614
	-0.2463
	-0.5872

	Base
	131
	96
	ENVSERV
	Combination
	Max
	
	
	5.654
	3.6502
	62.2948
	-0.4123
	1.7899
	0.5262

	Base
	131
	96
	ENVSERV
	Combination
	Min
	
	
	-2.0864
	0.3009
	-26.836
	-0.9802
	-0.2463
	-0.6075

	Base
	140
	103
	Dead
	LinStatic
	
	
	
	6.0615
	-3.0625
	27.8779
	0.1423
	-0.0181
	0.1474

	Base
	140
	103
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	140
	103
	FHEx
	LinStatic
	
	
	
	-12.9038
	11.6682
	-40.3351
	-0.2003
	-5.3722
	-0.1473

	Base
	140
	103
	FHEy
	LinStatic
	
	
	
	35.7398
	-19.2831
	169.9883
	5.8571
	-9.5022
	-0.4815

	Base
	140
	103
	Sx
	LinRespSpec
	Max
	
	
	8.3733
	11.2304
	34.6304
	1.6272
	7.326
	2.3045

	Base
	140
	103
	Sy
	LinRespSpec
	Max
	
	
	36.9669
	20.16
	171.4303
	6.0917
	10.8433
	1.6908

	Base
	140
	103
	Comb1
	Combination
	
	
	
	8.4861
	-4.2875
	39.0291
	0.1992
	-0.0254
	0.2064

	Base
	140
	103
	Comb2
	Combination
	
	
	
	7.2738
	-3.675
	33.4535
	0.1707
	-0.0218
	0.1769

	Base
	140
	103
	Comb3
	Combination
	
	
	
	7.2738
	-3.675
	33.4535
	0.1707
	-0.0218
	0.1769

	Base
	140
	103
	Comb4
	Combination
	Max
	
	
	8.47
	-2.0706
	38.4007
	0.4032
	1.0248
	0.5061

	Base
	140
	103
	Comb4
	Combination
	Min
	
	
	6.0776
	-5.2793
	28.5063
	-0.0617
	-1.0683
	-0.1523

	Base
	140
	103
	Comb5
	Combination
	Max
	
	
	12.5564
	-0.7941
	57.9509
	1.0412
	1.5277
	0.4185

	Base
	140
	103
	Comb5
	Combination
	Min
	
	
	1.9912
	-6.5558
	8.9561
	-0.6998
	-1.5713
	-0.0647

	Base
	140
	103
	Comb6
	Combination
	
	
	
	5.4553
	-2.7562
	25.0901
	0.128
	-0.0163
	0.1327

	Base
	140
	103
	Comb7
	Combination
	Max
	
	
	6.6515
	-1.1519
	30.0374
	0.3605
	1.0302
	0.4619

	Base
	140
	103
	Comb7
	Combination
	Min
	
	
	4.2592
	-4.3606
	20.1429
	-0.1044
	-1.0629
	-0.1966

	Base
	140
	103
	Comb8
	Combination
	Max
	
	
	10.7379
	0.1246
	49.5875
	0.9986
	1.5332
	0.3743

	Base
	140
	103
	Comb8
	Combination
	Min
	
	
	0.1728
	-5.6371
	0.5928
	-0.7425
	-1.5658
	-0.109

	Base
	140
	103
	ENVDIS
	Combination
	Max
	
	
	12.5564
	0.1246
	57.9509
	1.0412
	1.5332
	0.5061

	Base
	140
	103
	ENVDIS
	Combination
	Min
	
	
	0.1728
	-6.5558
	0.5928
	-0.7425
	-1.5713
	-0.1966

	Base
	140
	103
	Serv1
	Combination
	
	
	
	6.0615
	-3.0625
	27.8779
	0.1423
	-0.0181
	0.1474

	Base
	140
	103
	Serv2
	Combination
	
	
	
	6.0615
	-3.0625
	27.8779
	0.1423
	-0.0181
	0.1474

	Base
	140
	103
	Serv3
	Combination
	
	
	
	6.0615
	-3.0625
	27.8779
	0.1423
	-0.0181
	0.1474

	Base
	140
	103
	Serv4
	Combination
	Max
	
	
	6.8988
	-1.9394
	31.341
	0.305
	0.7145
	0.3779

	Base
	140
	103
	Serv4
	Combination
	Min
	
	
	5.2242
	-4.1855
	24.4149
	-0.0204
	-0.7507
	-0.083

	Base
	140
	103
	Serv5
	Combination
	Max
	
	
	9.7582
	-1.0465
	45.021
	0.7514
	1.0662
	0.3165

	Base
	140
	103
	Serv5
	Combination
	Min
	
	
	2.3648
	-5.0785
	10.7349
	-0.4669
	-1.1025
	-0.0217

	Base
	140
	103
	Serv6
	Combination
	Max
	
	
	6.6895
	-2.2202
	30.4752
	0.2643
	0.5313
	0.3202

	Base
	140
	103
	Serv6
	Combination
	Min
	
	
	5.4335
	-3.9048
	25.2807
	0.0202
	-0.5676
	-0.0254

	Base
	140
	103
	Serv7
	Combination
	Max
	
	
	8.834
	-1.5505
	40.7352
	0.5992
	0.7951
	0.2742

	Base
	140
	103
	Serv7
	Combination
	Min
	
	
	3.289
	-4.5745
	15.0207
	-0.3146
	-0.8314
	0.0206

	Base
	140
	103
	Serv8
	Combination
	
	
	
	3.6369
	-1.8375
	16.7268
	0.0854
	-0.0109
	0.0884

	Base
	140
	103
	Serv9
	Combination
	Max
	
	
	4.4742
	-0.7144
	20.1898
	0.2481
	0.7217
	0.3189

	Base
	140
	103
	Serv9
	Combination
	Min
	
	
	2.7996
	-2.9605
	13.2637
	-0.0774
	-0.7435
	-0.142

	Base
	140
	103
	Serv10
	Combination
	Max
	
	
	7.3336
	0.1785
	33.8698
	0.6945
	1.0734
	0.2575

	Base
	140
	103
	Serv10
	Combination
	Min
	
	
	-0.0598
	-3.8535
	-0.4163
	-0.5238
	-1.0952
	-0.0806

	Base
	140
	103
	ENVSERV
	Combination
	Max
	
	
	9.7582
	0.1785
	45.021
	0.7514
	1.0734
	0.3779

	Base
	140
	103
	ENVSERV
	Combination
	Min
	
	
	-0.0598
	-5.0785
	-0.4163
	-0.5238
	-1.1025
	-0.142

	Base
	141
	104
	Dead
	LinStatic
	
	
	
	-2.8317
	-1.9097
	20.2818
	0.2295
	0.0855
	0.1187

	Base
	141
	104
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	141
	104
	FHEx
	LinStatic
	
	
	
	-8.5502
	-11.5922
	30.5149
	0.0278
	-5.187
	-0.13

	Base
	141
	104
	FHEy
	LinStatic
	
	
	
	-23.7542
	11.5232
	81.192
	-0.7607
	-11.2931
	0.0418

	Base
	141
	104
	Sx
	LinRespSpec
	Max
	
	
	9.5639
	10.2411
	32.2676
	1.206
	6.7054
	1.7326

	Base
	141
	104
	Sy
	LinRespSpec
	Max
	
	
	23.2941
	13.4017
	75.1399
	1.1996
	12.318
	1.345

	Base
	141
	104
	Comb1
	Combination
	
	
	
	-3.9643
	-2.6736
	28.3945
	0.3213
	0.1197
	0.1662

	Base
	141
	104
	Comb2
	Combination
	
	
	
	-3.398
	-2.2917
	24.3381
	0.2754
	0.1026
	0.1425

	Base
	141
	104
	Comb3
	Combination
	
	
	
	-3.398
	-2.2917
	24.3381
	0.2754
	0.1026
	0.1425

	Base
	141
	104
	Comb4
	Combination
	Max
	
	
	-2.0317
	-0.8287
	28.9478
	0.4477
	1.0605
	0.39

	Base
	141
	104
	Comb4
	Combination
	Min
	
	
	-4.7643
	-3.7547
	19.7284
	0.1031
	-0.8553
	-0.1051

	Base
	141
	104
	Comb5
	Combination
	Max
	
	
	-0.0693
	-0.3766
	35.0756
	0.4469
	1.8628
	0.3347

	Base
	141
	104
	Comb5
	Combination
	Min
	
	
	-6.7267
	-4.2068
	13.6006
	0.104
	-1.6576
	-0.0497

	Base
	141
	104
	Comb6
	Combination
	
	
	
	-2.5485
	-1.7188
	18.2536
	0.2066
	0.0769
	0.1068

	Base
	141
	104
	Comb7
	Combination
	Max
	
	
	-1.1822
	-0.2557
	22.8632
	0.3789
	1.0349
	0.3544

	Base
	141
	104
	Comb7
	Combination
	Min
	
	
	-3.9148
	-3.1818
	13.6439
	0.0343
	-0.881
	-0.1407

	Base
	141
	104
	Comb8
	Combination
	Max
	
	
	0.7802
	0.1963
	28.9911
	0.378
	1.8372
	0.299

	Base
	141
	104
	Comb8
	Combination
	Min
	
	
	-5.8772
	-3.6339
	7.5161
	0.0352
	-1.6833
	-0.0854

	Base
	141
	104
	ENVDIS
	Combination
	Max
	
	
	0.7802
	0.1963
	35.0756
	0.4477
	1.8628
	0.39

	Base
	141
	104
	ENVDIS
	Combination
	Min
	
	
	-6.7267
	-4.2068
	7.5161
	0.0343
	-1.6833
	-0.1407

	Base
	141
	104
	Serv1
	Combination
	
	
	
	-2.8317
	-1.9097
	20.2818
	0.2295
	0.0855
	0.1187

	Base
	141
	104
	Serv2
	Combination
	
	
	
	-2.8317
	-1.9097
	20.2818
	0.2295
	0.0855
	0.1187

	Base
	141
	104
	Serv3
	Combination
	
	
	
	-2.8317
	-1.9097
	20.2818
	0.2295
	0.0855
	0.1187

	Base
	141
	104
	Serv4
	Combination
	Max
	
	
	-1.8753
	-0.8856
	23.5085
	0.3501
	0.756
	0.292

	Base
	141
	104
	Serv4
	Combination
	Min
	
	
	-3.7881
	-2.9338
	17.055
	0.1089
	-0.585
	-0.0545

	Base
	141
	104
	Serv5
	Combination
	Max
	
	
	-0.5022
	-0.5696
	27.7957
	0.3495
	1.3173
	0.2532

	Base
	141
	104
	Serv5
	Combination
	Min
	
	
	-5.1611
	-3.2499
	12.7678
	0.1096
	-1.1463
	-0.0158

	Base
	141
	104
	Serv6
	Combination
	Max
	
	
	-2.1144
	-1.1416
	22.7018
	0.32
	0.5884
	0.2487

	Base
	141
	104
	Serv6
	Combination
	Min
	
	
	-3.549
	-2.6778
	17.8617
	0.1391
	-0.4174
	-0.0112

	Base
	141
	104
	Serv7
	Combination
	Max
	
	
	-1.0846
	-0.9046
	25.9172
	0.3195
	1.0093
	0.2196

	Base
	141
	104
	Serv7
	Combination
	Min
	
	
	-4.5787
	-2.9149
	14.6463
	0.1396
	-0.8384
	0.0178

	Base
	141
	104
	Serv8
	Combination
	
	
	
	-1.699
	-1.1458
	12.1691
	0.1377
	0.0513
	0.0712

	Base
	141
	104
	Serv9
	Combination
	Max
	
	
	-0.7426
	-0.1217
	15.3958
	0.2583
	0.7218
	0.2445

	Base
	141
	104
	Serv9
	Combination
	Min
	
	
	-2.6554
	-2.1699
	8.9423
	0.0171
	-0.6192
	-0.102

	Base
	141
	104
	Serv10
	Combination
	Max
	
	
	0.6304
	0.1943
	19.683
	0.2577
	1.2831
	0.2057

	Base
	141
	104
	Serv10
	Combination
	Min
	
	
	-4.0284
	-2.486
	4.6551
	0.0178
	-1.1805
	-0.0633

	Base
	141
	104
	ENVSERV
	Combination
	Max
	
	
	0.6304
	0.1943
	27.7957
	0.3501
	1.3173
	0.292

	Base
	141
	104
	ENVSERV
	Combination
	Min
	
	
	-5.1611
	-3.2499
	4.6551
	0.0171
	-1.1805
	-0.102

	Base
	142
	106
	Dead
	LinStatic
	
	
	
	3.8186
	2.5057
	12.3341
	0.0449
	1.4657
	0.0057

	Base
	142
	106
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	142
	106
	FHEx
	LinStatic
	
	
	
	-10.5947
	-11.5663
	-30.122
	0.1346
	-4.4018
	0.0249

	Base
	142
	106
	FHEy
	LinStatic
	
	
	
	5.3296
	3.3951
	-80.1374
	4.7014
	21.8609
	-1.4254

	Base
	142
	106
	Sx
	LinRespSpec
	Max
	
	
	10.7052
	9.2937
	31.4189
	0.7448
	10.2132
	2.6539

	Base
	142
	106
	Sy
	LinRespSpec
	Max
	
	
	7.7725
	6.4653
	73.6559
	4.8331
	23.6248
	2.1168

	Base
	142
	106
	Comb1
	Combination
	
	
	
	5.3461
	3.5079
	17.2677
	0.0628
	2.052
	0.008

	Base
	142
	106
	Comb2
	Combination
	
	
	
	4.5824
	3.0068
	14.8009
	0.0539
	1.7588
	0.0069

	Base
	142
	106
	Comb3
	Combination
	
	
	
	4.5824
	3.0068
	14.8009
	0.0539
	1.7588
	0.0069

	Base
	142
	106
	Comb4
	Combination
	Max
	
	
	6.1117
	4.3345
	19.2893
	0.1602
	3.2178
	0.386

	Base
	142
	106
	Comb4
	Combination
	Min
	
	
	3.053
	1.6791
	10.3125
	-0.0525
	0.2998
	-0.3722

	Base
	142
	106
	Comb5
	Combination
	Max
	
	
	5.693
	3.9307
	25.3263
	0.7445
	5.1348
	0.3094

	Base
	142
	106
	Comb5
	Combination
	Min
	
	
	3.4717
	2.0829
	4.2755
	-0.6368
	-1.6172
	-0.2956

	Base
	142
	106
	Comb6
	Combination
	
	
	
	3.4368
	2.2551
	11.1007
	0.0404
	1.3191
	0.0052

	Base
	142
	106
	Comb7
	Combination
	Max
	
	
	4.9661
	3.5828
	15.5891
	0.1468
	2.7781
	0.3843

	Base
	142
	106
	Comb7
	Combination
	Min
	
	
	1.9074
	0.9274
	6.6123
	-0.066
	-0.1399
	-0.374

	Base
	142
	106
	Comb8
	Combination
	Max
	
	
	4.5474
	3.179
	21.6261
	0.731
	4.6951
	0.3077

	Base
	142
	106
	Comb8
	Combination
	Min
	
	
	2.3261
	1.3312
	0.5753
	-0.6503
	-2.0569
	-0.2973

	Base
	142
	106
	ENVDIS
	Combination
	Max
	
	
	6.1117
	4.3345
	25.3263
	0.7445
	5.1348
	0.386

	Base
	142
	106
	ENVDIS
	Combination
	Min
	
	
	1.9074
	0.9274
	0.5753
	-0.6503
	-2.0569
	-0.374

	Base
	142
	106
	Serv1
	Combination
	
	
	
	3.8186
	2.5057
	12.3341
	0.0449
	1.4657
	0.0057

	Base
	142
	106
	Serv2
	Combination
	
	
	
	3.8186
	2.5057
	12.3341
	0.0449
	1.4657
	0.0057

	Base
	142
	106
	Serv3
	Combination
	
	
	
	3.8186
	2.5057
	12.3341
	0.0449
	1.4657
	0.0057

	Base
	142
	106
	Serv4
	Combination
	Max
	
	
	4.8891
	3.435
	15.476
	0.1194
	2.487
	0.2711

	Base
	142
	106
	Serv4
	Combination
	Min
	
	
	2.7481
	1.5763
	9.1922
	-0.0296
	0.4444
	-0.2597

	Base
	142
	106
	Serv5
	Combination
	Max
	
	
	4.5959
	3.1522
	19.6997
	0.5282
	3.8282
	0.2174

	Base
	142
	106
	Serv5
	Combination
	Min
	
	
	3.0414
	1.8591
	4.9685
	-0.4384
	-0.8968
	-0.2059

	Base
	142
	106
	Serv6
	Combination
	Max
	
	
	4.6215
	3.2027
	14.6905
	0.1007
	2.2317
	0.2048

	Base
	142
	106
	Serv6
	Combination
	Min
	
	
	3.0157
	1.8086
	9.9777
	-0.011
	0.6997
	-0.1933

	Base
	142
	106
	Serv7
	Combination
	Max
	
	
	4.4016
	2.9906
	17.8583
	0.4074
	3.2375
	0.1645

	Base
	142
	106
	Serv7
	Combination
	Min
	
	
	3.2357
	2.0208
	6.8099
	-0.3176
	-0.3062
	-0.153

	Base
	142
	106
	Serv8
	Combination
	
	
	
	2.2912
	1.5034
	7.4004
	0.0269
	0.8794
	0.0034

	Base
	142
	106
	Serv9
	Combination
	Max
	
	
	3.3617
	2.4328
	10.5423
	0.1014
	1.9007
	0.2688

	Base
	142
	106
	Serv9
	Combination
	Min
	
	
	1.2207
	0.574
	4.2586
	-0.0476
	-0.1419
	-0.2619

	Base
	142
	106
	Serv10
	Combination
	Max
	
	
	3.0684
	2.1499
	14.766
	0.5102
	3.2419
	0.2151

	Base
	142
	106
	Serv10
	Combination
	Min
	
	
	1.5139
	0.8569
	0.0349
	-0.4564
	-1.4831
	-0.2082

	Base
	142
	106
	ENVSERV
	Combination
	Max
	
	
	4.8891
	3.435
	19.6997
	0.5282
	3.8282
	0.2711

	Base
	142
	106
	ENVSERV
	Combination
	Min
	
	
	1.2207
	0.574
	0.0349
	-0.4564
	-1.4831
	-0.2619

	Base
	143
	105
	Dead
	LinStatic
	
	
	
	0.7812
	0.8379
	2.8513
	0.3367
	1.7249
	0.0705

	Base
	143
	105
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	143
	105
	FHEx
	LinStatic
	
	
	
	-10.2653
	12.2466
	40.9512
	-0.3455
	-4.5686
	-0.0195

	Base
	143
	105
	FHEy
	LinStatic
	
	
	
	36.6208
	-16.0224
	-172.221
	0.4379
	23.8448
	-0.6301

	Base
	143
	105
	Sx
	LinRespSpec
	Max
	
	
	10.6023
	8.8845
	31.9437
	0.4362
	9.3535
	2.9067

	Base
	143
	105
	Sy
	LinRespSpec
	Max
	
	
	37.6696
	18.7418
	174.6086
	0.289
	25.5756
	2.011

	Base
	143
	105
	Comb1
	Combination
	
	
	
	1.0937
	1.173
	3.9918
	0.4714
	2.4148
	0.0987

	Base
	143
	105
	Comb2
	Combination
	
	
	
	0.9375
	1.0054
	3.4216
	0.4041
	2.0698
	0.0846

	Base
	143
	105
	Comb3
	Combination
	
	
	
	0.9375
	1.0054
	3.4216
	0.4041
	2.0698
	0.0846

	Base
	143
	105
	Comb4
	Combination
	Max
	
	
	2.4521
	2.2746
	7.9849
	0.4664
	3.406
	0.4999

	Base
	143
	105
	Comb4
	Combination
	Min
	
	
	-0.5772
	-0.2638
	-1.1418
	0.3418
	0.7336
	-0.3306

	Base
	143
	105
	Comb5
	Combination
	Max
	
	
	6.3205
	3.6836
	28.3731
	0.4454
	5.7246
	0.372

	Base
	143
	105
	Comb5
	Combination
	Min
	
	
	-4.4455
	-1.6728
	-21.53
	0.3628
	-1.5849
	-0.2028

	Base
	143
	105
	Comb6
	Combination
	
	
	
	0.7031
	0.7541
	2.5662
	0.3031
	1.5524
	0.0635

	Base
	143
	105
	Comb7
	Combination
	Max
	
	
	2.2177
	2.0233
	7.1296
	0.3654
	2.8886
	0.4787

	Base
	143
	105
	Comb7
	Combination
	Min
	
	
	-0.8115
	-0.5151
	-1.9972
	0.2407
	0.2162
	-0.3518

	Base
	143
	105
	Comb8
	Combination
	Max
	
	
	6.0861
	3.4323
	27.5177
	0.3444
	5.2071
	0.3508

	Base
	143
	105
	Comb8
	Combination
	Min
	
	
	-4.6799
	-1.9241
	-22.3854
	0.2618
	-2.1024
	-0.2239

	Base
	143
	105
	ENVDIS
	Combination
	Max
	
	
	6.3205
	3.6836
	28.3731
	0.4714
	5.7246
	0.4999

	Base
	143
	105
	ENVDIS
	Combination
	Min
	
	
	-4.6799
	-1.9241
	-22.3854
	0.2407
	-2.1024
	-0.3518

	Base
	143
	105
	Serv1
	Combination
	
	
	
	0.7812
	0.8379
	2.8513
	0.3367
	1.7249
	0.0705

	Base
	143
	105
	Serv2
	Combination
	
	
	
	0.7812
	0.8379
	2.8513
	0.3367
	1.7249
	0.0705

	Base
	143
	105
	Serv3
	Combination
	
	
	
	0.7812
	0.8379
	2.8513
	0.3367
	1.7249
	0.0705

	Base
	143
	105
	Serv4
	Combination
	Max
	
	
	1.8415
	1.7263
	6.0457
	0.3804
	2.6602
	0.3612

	Base
	143
	105
	Serv4
	Combination
	Min
	
	
	-0.279
	-0.0506
	-0.3431
	0.2931
	0.7895
	-0.2202

	Base
	143
	105
	Serv5
	Combination
	Max
	
	
	4.5482
	2.712
	20.3122
	0.3656
	4.2824
	0.2716

	Base
	143
	105
	Serv5
	Combination
	Min
	
	
	-2.9857
	-1.0363
	-14.6096
	0.3078
	-0.8327
	-0.1306

	Base
	143
	105
	Serv6
	Combination
	Max
	
	
	1.5764
	1.5042
	5.2471
	0.3694
	2.4264
	0.2885

	Base
	143
	105
	Serv6
	Combination
	Min
	
	
	-0.014
	0.1715
	0.4555
	0.304
	1.0233
	-0.1475

	Base
	143
	105
	Serv7
	Combination
	Max
	
	
	3.6064
	2.2435
	15.9469
	0.3584
	3.643
	0.2213

	Base
	143
	105
	Serv7
	Combination
	Min
	
	
	-2.044
	-0.5678
	-10.2443
	0.315
	-0.1933
	-0.0803

	Base
	143
	105
	Serv8
	Combination
	
	
	
	0.4687
	0.5027
	1.7108
	0.202
	1.0349
	0.0423

	Base
	143
	105
	Serv9
	Combination
	Max
	
	
	1.529
	1.3912
	4.9051
	0.2457
	1.9703
	0.333

	Base
	143
	105
	Serv9
	Combination
	Min
	
	
	-0.5915
	-0.3857
	-1.4836
	0.1584
	0.0996
	-0.2484

	Base
	143
	105
	Serv10
	Combination
	Max
	
	
	4.2357
	2.3769
	19.1716
	0.2309
	3.5925
	0.2434

	Base
	143
	105
	Serv10
	Combination
	Min
	
	
	-3.2982
	-1.3715
	-15.7501
	0.1731
	-1.5226
	-0.1588

	Base
	143
	105
	ENVSERV
	Combination
	Max
	
	
	4.5482
	2.712
	20.3122
	0.3804
	4.2824
	0.3612

	Base
	143
	105
	ENVSERV
	Combination
	Min
	
	
	-3.2982
	-1.3715
	-15.7501
	0.1584
	-1.5226
	-0.2484

	Base
	168
	102
	Dead
	LinStatic
	
	
	
	-1.4152
	-1.5494
	16.6479
	0.0778
	1.8424
	0.0503

	Base
	168
	102
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	168
	102
	FHEx
	LinStatic
	
	
	
	-20.6775
	-11.0699
	50.1668
	0.9832
	-6.9596
	-0.4381

	Base
	168
	102
	FHEy
	LinStatic
	
	
	
	8.1214
	6.8129
	48.1941
	-0.2357
	39.6093
	3.0003

	Base
	168
	102
	Sx
	LinRespSpec
	Max
	
	
	14.7914
	8.9429
	32.9915
	1.6163
	8.6069
	1.0837

	Base
	168
	102
	Sy
	LinRespSpec
	Max
	
	
	14.9845
	9.2615
	15.8777
	1.7146
	36.2426
	1.5614

	Base
	168
	102
	Comb1
	Combination
	
	
	
	-1.9813
	-2.1691
	23.3071
	0.1089
	2.5794
	0.0704

	Base
	168
	102
	Comb2
	Combination
	
	
	
	-1.6982
	-1.8592
	19.9775
	0.0934
	2.2109
	0.0604

	Base
	168
	102
	Comb3
	Combination
	
	
	
	-1.6982
	-1.8592
	19.9775
	0.0934
	2.2109
	0.0604

	Base
	168
	102
	Comb4
	Combination
	Max
	
	
	0.4148
	-0.5817
	24.6905
	0.3243
	3.4405
	0.2152

	Base
	168
	102
	Comb4
	Combination
	Min
	
	
	-3.8113
	-3.1368
	15.2644
	-0.1375
	0.9813
	-0.0945

	Base
	168
	102
	Comb5
	Combination
	Max
	
	
	0.443
	-0.5358
	22.2464
	0.3384
	7.39
	0.2835

	Base
	168
	102
	Comb5
	Combination
	Min
	
	
	-3.8395
	-3.1827
	17.7086
	-0.1517
	-2.9682
	-0.1628

	Base
	168
	102
	Comb6
	Combination
	
	
	
	-1.2737
	-1.3944
	14.9831
	0.07
	1.6582
	0.0453

	Base
	168
	102
	Comb7
	Combination
	Max
	
	
	0.8394
	-0.1169
	19.6962
	0.3009
	2.8877
	0.2001

	Base
	168
	102
	Comb7
	Combination
	Min
	
	
	-3.3867
	-2.672
	10.27
	-0.1609
	0.4286
	-0.1095

	Base
	168
	102
	Comb8
	Combination
	Max
	
	
	0.8676
	-0.0709
	17.252
	0.315
	6.8372
	0.2684

	Base
	168
	102
	Comb8
	Combination
	Min
	
	
	-3.415
	-2.7179
	12.7142
	-0.175
	-3.5209
	-0.1779

	Base
	168
	102
	ENVDIS
	Combination
	Max
	
	
	0.8676
	-0.0709
	24.6905
	0.3384
	7.39
	0.2835

	Base
	168
	102
	ENVDIS
	Combination
	Min
	
	
	-3.8395
	-3.1827
	10.27
	-0.175
	-3.5209
	-0.1779

	Base
	168
	102
	Serv1
	Combination
	
	
	
	-1.4152
	-1.5494
	16.6479
	0.0778
	1.8424
	0.0503

	Base
	168
	102
	Serv2
	Combination
	
	
	
	-1.4152
	-1.5494
	16.6479
	0.0778
	1.8424
	0.0503

	Base
	168
	102
	Serv3
	Combination
	
	
	
	-1.4152
	-1.5494
	16.6479
	0.0778
	1.8424
	0.0503

	Base
	168
	102
	Serv4
	Combination
	Max
	
	
	0.0639
	-0.6551
	19.947
	0.2394
	2.7031
	0.1587

	Base
	168
	102
	Serv4
	Combination
	Min
	
	
	-2.8943
	-2.4436
	13.3487
	-0.0838
	0.9817
	-0.0581

	Base
	168
	102
	Serv5
	Combination
	Max
	
	
	0.0832
	-0.6232
	18.2357
	0.2493
	5.4667
	0.2064

	Base
	168
	102
	Serv5
	Combination
	Min
	
	
	-2.9137
	-2.4755
	15.0601
	-0.0937
	-1.7818
	-0.1058

	Base
	168
	102
	Serv6
	Combination
	Max
	
	
	-0.3059
	-0.8786
	19.1223
	0.199
	2.4879
	0.1316

	Base
	168
	102
	Serv6
	Combination
	Min
	
	
	-2.5246
	-2.2201
	14.1735
	-0.0434
	1.1969
	-0.031

	Base
	168
	102
	Serv7
	Combination
	Max
	
	
	-0.2914
	-0.8547
	17.8387
	0.2064
	4.5606
	0.1674

	Base
	168
	102
	Serv7
	Combination
	Min
	
	
	-2.539
	-2.244
	15.4571
	-0.0508
	-0.8758
	-0.0668

	Base
	168
	102
	Serv8
	Combination
	
	
	
	-0.8491
	-0.9296
	9.9887
	0.0467
	1.1054
	0.0302

	Base
	168
	102
	Serv9
	Combination
	Max
	
	
	0.63
	-0.0353
	13.2879
	0.2083
	1.9661
	0.1386

	Base
	168
	102
	Serv9
	Combination
	Min
	
	
	-2.3283
	-1.8239
	6.6896
	-0.1149
	0.2448
	-0.0782

	Base
	168
	102
	Serv10
	Combination
	Max
	
	
	0.6493
	-0.0035
	11.5765
	0.2181
	4.7297
	0.1863

	Base
	168
	102
	Serv10
	Combination
	Min
	
	
	-2.3476
	-1.8558
	8.401
	-0.1248
	-2.5188
	-0.126

	Base
	168
	102
	ENVSERV
	Combination
	Max
	
	
	0.6493
	-0.0035
	19.947
	0.2493
	5.4667
	0.2064

	Base
	168
	102
	ENVSERV
	Combination
	Min
	
	
	-2.9137
	-2.4755
	6.6896
	-0.1248
	-2.5188
	-0.126

	Base
	169
	97
	Dead
	LinStatic
	
	
	
	3.4906
	-3.6005
	36.8945
	0.621
	0.8533
	-0.1222

	Base
	169
	97
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	169
	97
	FHEx
	LinStatic
	
	
	
	-8.832
	1.5183
	-42.9889
	-0.6411
	-7.7789
	0.5699

	Base
	169
	97
	FHEy
	LinStatic
	
	
	
	28.6129
	-40.9987
	180.7334
	21.1948
	13.3351
	0.1497

	Base
	169
	97
	Sx
	LinRespSpec
	Max
	
	
	8.8206
	7.3825
	54.3602
	4.749
	6.4704
	0.9419

	Base
	169
	97
	Sy
	LinRespSpec
	Max
	
	
	28.2929
	28.5816
	142.8411
	12.4369
	14.7787
	2.2257

	Base
	169
	97
	Comb1
	Combination
	
	
	
	4.8868
	-5.0407
	51.6522
	0.8694
	1.1946
	-0.1711

	Base
	169
	97
	Comb2
	Combination
	
	
	
	4.1887
	-4.3206
	44.2734
	0.7452
	1.024
	-0.1467

	Base
	169
	97
	Comb3
	Combination
	
	
	
	4.1887
	-4.3206
	44.2734
	0.7452
	1.024
	-0.1467

	Base
	169
	97
	Comb4
	Combination
	Max
	
	
	5.4488
	-3.266
	52.0391
	1.4236
	1.9483
	-0.0121

	Base
	169
	97
	Comb4
	Combination
	Min
	
	
	2.9286
	-5.3753
	36.5076
	0.0667
	0.0996
	-0.2812

	Base
	169
	97
	Comb5
	Combination
	Max
	
	
	8.2318
	-0.2363
	64.6854
	2.5224
	3.1359
	0.1714

	Base
	169
	97
	Comb5
	Combination
	Min
	
	
	0.1456
	-8.405
	23.8614
	-1.0321
	-1.0879
	-0.4647

	Base
	169
	97
	Comb6
	Combination
	
	
	
	3.1415
	-3.2405
	33.205
	0.5589
	0.768
	-0.11

	Base
	169
	97
	Comb7
	Combination
	Max
	
	
	4.4016
	-2.1858
	40.9708
	1.2373
	1.6923
	0.0245

	Base
	169
	97
	Comb7
	Combination
	Min
	
	
	1.8814
	-4.2951
	25.4393
	-0.1196
	-0.1564
	-0.2446

	Base
	169
	97
	Comb8
	Combination
	Max
	
	
	7.1846
	0.8438
	53.617
	2.3361
	2.8799
	0.208

	Base
	169
	97
	Comb8
	Combination
	Min
	
	
	-0.9015
	-7.3248
	12.793
	-1.2184
	-1.3439
	-0.4281

	Base
	169
	97
	ENVDIS
	Combination
	Max
	
	
	8.2318
	0.8438
	64.6854
	2.5224
	3.1359
	0.208

	Base
	169
	97
	ENVDIS
	Combination
	Min
	
	
	-0.9015
	-8.405
	12.793
	-1.2184
	-1.3439
	-0.4647

	Base
	169
	97
	Serv1
	Combination
	
	
	
	3.4906
	-3.6005
	36.8945
	0.621
	0.8533
	-0.1222

	Base
	169
	97
	Serv2
	Combination
	
	
	
	3.4906
	-3.6005
	36.8945
	0.621
	0.8533
	-0.1222

	Base
	169
	97
	Serv3
	Combination
	
	
	
	3.4906
	-3.6005
	36.8945
	0.621
	0.8533
	-0.1222

	Base
	169
	97
	Serv4
	Combination
	Max
	
	
	4.3727
	-2.8623
	42.3305
	1.0959
	1.5004
	-0.028

	Base
	169
	97
	Serv4
	Combination
	Min
	
	
	2.6085
	-4.3388
	31.4584
	0.1461
	0.2063
	-0.2164

	Base
	169
	97
	Serv5
	Combination
	Max
	
	
	6.3199
	-0.7424
	51.1786
	1.8647
	2.3312
	0.1003

	Base
	169
	97
	Serv5
	Combination
	Min
	
	
	0.6613
	-6.4587
	22.6103
	-0.6227
	-0.6246
	-0.3448

	Base
	169
	97
	Serv6
	Combination
	Max
	
	
	4.1521
	-3.0468
	40.9715
	0.9771
	1.3386
	-0.0516

	Base
	169
	97
	Serv6
	Combination
	Min
	
	
	2.829
	-4.1542
	32.8174
	0.2648
	0.368
	-0.1929

	Base
	169
	97
	Serv7
	Combination
	Max
	
	
	5.6126
	-1.4569
	47.6075
	1.5537
	1.9617
	0.0447

	Base
	169
	97
	Serv7
	Combination
	Min
	
	
	1.3686
	-5.7442
	26.1814
	-0.3118
	-0.2551
	-0.2892

	Base
	169
	97
	Serv8
	Combination
	
	
	
	2.0944
	-2.1603
	22.1367
	0.3726
	0.512
	-0.0733

	Base
	169
	97
	Serv9
	Combination
	Max
	
	
	2.9764
	-1.4221
	27.5727
	0.8475
	1.159
	0.0208

	Base
	169
	97
	Serv9
	Combination
	Min
	
	
	1.2123
	-2.8986
	16.7007
	-0.1023
	-0.1351
	-0.1675

	Base
	169
	97
	Serv10
	Combination
	Max
	
	
	4.9237
	0.6978
	36.4208
	1.6163
	1.9899
	0.1492

	Base
	169
	97
	Serv10
	Combination
	Min
	
	
	-0.7349
	-5.0185
	7.8526
	-0.8711
	-0.9659
	-0.2959

	Base
	169
	97
	ENVSERV
	Combination
	Max
	
	
	6.3199
	0.6978
	51.1786
	1.8647
	2.3312
	0.1492

	Base
	169
	97
	ENVSERV
	Combination
	Min
	
	
	-0.7349
	-6.4587
	7.8526
	-0.8711
	-0.9659
	-0.3448

	Base
	170
	98
	Dead
	LinStatic
	
	
	
	1.397
	1.1483
	16.233
	-0.0153
	-0.3644
	-0.2567

	Base
	170
	98
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	170
	98
	FHEx
	LinStatic
	
	
	
	-0.8415
	-5.0837
	-35.7393
	-5.0252
	0.7711
	0.806

	Base
	170
	98
	FHEy
	LinStatic
	
	
	
	-42.3662
	-40.7974
	-105.3525
	17.3828
	-5.171
	-4.1787

	Base
	170
	98
	Sx
	LinRespSpec
	Max
	
	
	5.8907
	6.322
	22.3434
	7.9732
	0.8308
	1.4479

	Base
	170
	98
	Sy
	LinRespSpec
	Max
	
	
	29.7959
	21.6811
	57.4985
	9.4552
	5.5965
	4.3181

	Base
	170
	98
	Comb1
	Combination
	
	
	
	1.9558
	1.6076
	22.7262
	-0.0214
	-0.5101
	-0.3594

	Base
	170
	98
	Comb2
	Combination
	
	
	
	1.6764
	1.3779
	19.4796
	-0.0183
	-0.4373
	-0.3081

	Base
	170
	98
	Comb3
	Combination
	
	
	
	1.6764
	1.3779
	19.4796
	-0.0183
	-0.4373
	-0.3081

	Base
	170
	98
	Comb4
	Combination
	Max
	
	
	2.518
	2.2811
	22.6715
	1.1207
	-0.3186
	-0.1012

	Base
	170
	98
	Comb4
	Combination
	Min
	
	
	0.8349
	0.4748
	16.2877
	-1.1574
	-0.5559
	-0.5149

	Base
	170
	98
	Comb5
	Combination
	Max
	
	
	5.9343
	4.4761
	27.6961
	1.3328
	0.3625
	0.309

	Base
	170
	98
	Comb5
	Combination
	Min
	
	
	-2.5814
	-1.7203
	11.2631
	-1.3695
	-1.237
	-0.9251

	Base
	170
	98
	Comb6
	Combination
	
	
	
	1.2573
	1.0334
	14.6097
	-0.0138
	-0.3279
	-0.2311

	Base
	170
	98
	Comb7
	Combination
	Max
	
	
	2.0989
	1.9366
	17.8016
	1.1253
	-0.2093
	-0.0242

	Base
	170
	98
	Comb7
	Combination
	Min
	
	
	0.4158
	0.1303
	11.4178
	-1.1528
	-0.4466
	-0.4379

	Base
	170
	98
	Comb8
	Combination
	Max
	
	
	5.5152
	4.1317
	22.8262
	1.3374
	0.4718
	0.386

	Base
	170
	98
	Comb8
	Combination
	Min
	
	
	-3.0005
	-2.0648
	6.3932
	-1.3649
	-1.1277
	-0.8481

	Base
	170
	98
	ENVDIS
	Combination
	Max
	
	
	5.9343
	4.4761
	27.6961
	1.3374
	0.4718
	0.386

	Base
	170
	98
	ENVDIS
	Combination
	Min
	
	
	-3.0005
	-2.0648
	6.3932
	-1.3695
	-1.237
	-0.9251

	Base
	170
	98
	Serv1
	Combination
	
	
	
	1.397
	1.1483
	16.233
	-0.0153
	-0.3644
	-0.2567

	Base
	170
	98
	Serv2
	Combination
	
	
	
	1.397
	1.1483
	16.233
	-0.0153
	-0.3644
	-0.2567

	Base
	170
	98
	Serv3
	Combination
	
	
	
	1.397
	1.1483
	16.233
	-0.0153
	-0.3644
	-0.2567

	Base
	170
	98
	Serv4
	Combination
	Max
	
	
	1.9861
	1.7805
	18.4673
	0.782
	-0.2813
	-0.1119

	Base
	170
	98
	Serv4
	Combination
	Min
	
	
	0.808
	0.5161
	13.9987
	-0.8126
	-0.4475
	-0.4015

	Base
	170
	98
	Serv5
	Combination
	Max
	
	
	4.3766
	3.3164
	21.9829
	0.9302
	0.1953
	0.1751

	Base
	170
	98
	Serv5
	Combination
	Min
	
	
	-1.5826
	-1.0199
	10.4831
	-0.9608
	-0.924
	-0.6885

	Base
	170
	98
	Serv6
	Combination
	Max
	
	
	1.8388
	1.6224
	17.9088
	0.5827
	-0.3021
	-0.1481

	Base
	170
	98
	Serv6
	Combination
	Min
	
	
	0.9552
	0.6741
	14.5572
	-0.6133
	-0.4267
	-0.3653

	Base
	170
	98
	Serv7
	Combination
	Max
	
	
	3.6317
	2.7743
	20.5454
	0.6939
	0.0554
	0.0671

	Base
	170
	98
	Serv7
	Combination
	Min
	
	
	-0.8377
	-0.4778
	11.9206
	-0.7244
	-0.7841
	-0.5806

	Base
	170
	98
	Serv8
	Combination
	
	
	
	0.8382
	0.689
	9.7398
	-0.0092
	-0.2186
	-0.154

	Base
	170
	98
	Serv9
	Combination
	Max
	
	
	1.4273
	1.3212
	11.9741
	0.7881
	-0.1355
	-0.0092

	Base
	170
	98
	Serv9
	Combination
	Min
	
	
	0.2491
	0.0568
	7.5055
	-0.8065
	-0.3017
	-0.2988

	Base
	170
	98
	Serv10
	Combination
	Max
	
	
	3.8178
	2.8571
	15.4897
	0.9363
	0.341
	0.2778

	Base
	170
	98
	Serv10
	Combination
	Min
	
	
	-2.1414
	-1.4792
	3.9899
	-0.9547
	-0.7783
	-0.5858

	Base
	170
	98
	ENVSERV
	Combination
	Max
	
	
	4.3766
	3.3164
	21.9829
	0.9363
	0.341
	0.2778

	Base
	170
	98
	ENVSERV
	Combination
	Min
	
	
	-2.1414
	-1.4792
	3.9899
	-0.9608
	-0.924
	-0.6885

	Base
	171
	101
	Dead
	LinStatic
	
	
	
	-2.0342
	1.0273
	10.2596
	-0.0001
	-1.5704
	0.0326

	Base
	171
	101
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	171
	101
	FHEx
	LinStatic
	
	
	
	-20.7068
	11.1788
	42.7191
	-1.9493
	-4.4793
	0.3082

	Base
	171
	101
	FHEy
	LinStatic
	
	
	
	-6.2282
	-19.8876
	-72.411
	1.7385
	-32.5939
	0.1071

	Base
	171
	101
	Sx
	LinRespSpec
	Max
	
	
	18.2686
	10.2879
	40.0333
	1.7831
	4.5138
	0.1949

	Base
	171
	101
	Sy
	LinRespSpec
	Max
	
	
	2.9909
	18.8052
	69.3059
	1.9765
	26.1993
	0.0527

	Base
	171
	101
	Comb1
	Combination
	
	
	
	-2.8479
	1.4382
	14.3634
	-0.0001
	-2.1986
	0.0457

	Base
	171
	101
	Comb2
	Combination
	
	
	
	-2.441
	1.2328
	12.3115
	-0.0001
	-1.8845
	0.0392

	Base
	171
	101
	Comb3
	Combination
	
	
	
	-2.441
	1.2328
	12.3115
	-0.0001
	-1.8845
	0.0392

	Base
	171
	101
	Comb4
	Combination
	Max
	
	
	0.1687
	2.7025
	18.0305
	0.2546
	-1.2397
	0.067

	Base
	171
	101
	Comb4
	Combination
	Min
	
	
	-5.0508
	-0.237
	6.5925
	-0.2548
	-2.5293
	0.0113

	Base
	171
	101
	Comb5
	Combination
	Max
	
	
	-2.0136
	3.92
	22.2153
	0.2823
	1.8594
	0.0467

	Base
	171
	101
	Comb5
	Combination
	Min
	
	
	-2.8684
	-1.4545
	2.4077
	-0.2826
	-5.6284
	0.0316

	Base
	171
	101
	Comb6
	Combination
	
	
	
	-1.8308
	0.9246
	9.2336
	-0.0001
	-1.4134
	0.0294

	Base
	171
	101
	Comb7
	Combination
	Max
	
	
	0.779
	2.3943
	14.9527
	0.2546
	-0.7686
	0.0572

	Base
	171
	101
	Comb7
	Combination
	Min
	
	
	-4.4406
	-0.5451
	3.5146
	-0.2548
	-2.0582
	0.0015

	Base
	171
	101
	Comb8
	Combination
	Max
	
	
	-1.4034
	3.6118
	19.1374
	0.2824
	2.3305
	0.0369

	Base
	171
	101
	Comb8
	Combination
	Min
	
	
	-2.2582
	-1.7627
	-0.6702
	-0.2825
	-5.1573
	0.0218

	Base
	171
	101
	ENVDIS
	Combination
	Max
	
	
	0.779
	3.92
	22.2153
	0.2824
	2.3305
	0.067

	Base
	171
	101
	ENVDIS
	Combination
	Min
	
	
	-5.0508
	-1.7627
	-0.6702
	-0.2826
	-5.6284
	0.0015

	Base
	171
	101
	Serv1
	Combination
	
	
	
	-2.0342
	1.0273
	10.2596
	-0.0001
	-1.5704
	0.0326

	Base
	171
	101
	Serv2
	Combination
	
	
	
	-2.0342
	1.0273
	10.2596
	-0.0001
	-1.5704
	0.0326

	Base
	171
	101
	Serv3
	Combination
	
	
	
	-2.0342
	1.0273
	10.2596
	-0.0001
	-1.5704
	0.0326

	Base
	171
	101
	Serv4
	Combination
	Max
	
	
	-0.2073
	2.0561
	14.2629
	0.1782
	-1.119
	0.0521

	Base
	171
	101
	Serv4
	Combination
	Min
	
	
	-3.8611
	-0.0015
	6.2563
	-0.1784
	-2.0218
	0.0131

	Base
	171
	101
	Serv5
	Combination
	Max
	
	
	-1.7351
	2.9078
	17.1902
	0.1975
	1.0495
	0.0379

	Base
	171
	101
	Serv5
	Combination
	Min
	
	
	-2.3333
	-0.8532
	3.329
	-0.1978
	-4.1904
	0.0274

	Base
	171
	101
	Serv6
	Combination
	Max
	
	
	-0.6641
	1.7989
	13.2621
	0.1336
	-1.2319
	0.0472

	Base
	171
	101
	Serv6
	Combination
	Min
	
	
	-3.4043
	0.2557
	7.2571
	-0.1338
	-1.909
	0.018

	Base
	171
	101
	Serv7
	Combination
	Max
	
	
	-1.8099
	2.4377
	15.4575
	0.1481
	0.3945
	0.0366

	Base
	171
	101
	Serv7
	Combination
	Min
	
	
	-2.2585
	-0.3831
	5.0616
	-0.1483
	-3.5354
	0.0287

	Base
	171
	101
	Serv8
	Combination
	
	
	
	-1.2205
	0.6164
	6.1557
	-0.0001
	-0.9423
	0.0196

	Base
	171
	101
	Serv9
	Combination
	Max
	
	
	0.6063
	1.6452
	10.1591
	0.1782
	-0.4909
	0.0391

	Base
	171
	101
	Serv9
	Combination
	Min
	
	
	-3.0474
	-0.4124
	2.1524
	-0.1784
	-1.3936
	0.0001

	Base
	171
	101
	Serv10
	Combination
	Max
	
	
	-0.9214
	2.4969
	13.0863
	0.1976
	1.6777
	0.0249

	Base
	171
	101
	Serv10
	Combination
	Min
	
	
	-1.5196
	-1.2641
	-0.7748
	-0.1977
	-3.5622
	0.0143

	Base
	171
	101
	ENVSERV
	Combination
	Max
	
	
	0.6063
	2.9078
	17.1902
	0.1976
	1.6777
	0.0521

	Base
	171
	101
	ENVSERV
	Combination
	Min
	
	
	-3.8611
	-1.2641
	-0.7748
	-0.1978
	-4.1904
	0.0001

	Base
	172
	100
	Dead
	LinStatic
	
	
	
	1.2971
	-3.9805
	30.0382
	0.7048
	0.029
	-0.0644

	Base
	172
	100
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	172
	100
	FHEx
	LinStatic
	
	
	
	-4.4167
	-5.9247
	-21.2736
	3.8452
	-6.3562
	0.6218

	Base
	172
	100
	FHEy
	LinStatic
	
	
	
	-15.0591
	-33.9755
	86.3555
	17.082
	-2.6659
	-2.4911

	Base
	172
	100
	Sx
	LinRespSpec
	Max
	
	
	2.2783
	5.0146
	26.6285
	2.7681
	4.936
	0.9784

	Base
	172
	100
	Sy
	LinRespSpec
	Max
	
	
	9.5438
	25.6893
	67.6198
	10.6327
	0.5837
	1.5443

	Base
	172
	100
	Comb1
	Combination
	
	
	
	1.816
	-5.5727
	42.0535
	0.9868
	0.0406
	-0.0901

	Base
	172
	100
	Comb2
	Combination
	
	
	
	1.5566
	-4.7766
	36.0458
	0.8458
	0.0348
	-0.0773

	Base
	172
	100
	Comb3
	Combination
	
	
	
	1.5566
	-4.7766
	36.0458
	0.8458
	0.0348
	-0.0773

	Base
	172
	100
	Comb4
	Combination
	Max
	
	
	1.882
	-4.0602
	39.8499
	1.2413
	0.7399
	0.0625

	Base
	172
	100
	Comb4
	Combination
	Min
	
	
	1.2311
	-5.493
	32.2418
	0.4504
	-0.6704
	-0.217

	Base
	172
	100
	Comb5
	Combination
	Max
	
	
	2.9204
	-1.1056
	45.7087
	2.3652
	0.1182
	0.1434

	Base
	172
	100
	Comb5
	Combination
	Min
	
	
	0.1927
	-8.4476
	26.383
	-0.6736
	-0.0486
	-0.2979

	Base
	172
	100
	Comb6
	Combination
	
	
	
	1.1674
	-3.5825
	27.0344
	0.6344
	0.0261
	-0.0579

	Base
	172
	100
	Comb7
	Combination
	Max
	
	
	1.4929
	-2.8661
	30.8385
	1.0298
	0.7312
	0.0818

	Base
	172
	100
	Comb7
	Combination
	Min
	
	
	0.8419
	-4.2988
	23.2303
	0.2389
	-0.6791
	-0.1977

	Base
	172
	100
	Comb8
	Combination
	Max
	
	
	2.5312
	0.0885
	36.6972
	2.1538
	0.1095
	0.1627

	Base
	172
	100
	Comb8
	Combination
	Min
	
	
	-0.1964
	-7.2535
	17.3715
	-0.8851
	-0.0573
	-0.2786

	Base
	172
	100
	ENVDIS
	Combination
	Max
	
	
	2.9204
	0.0885
	45.7087
	2.3652
	0.7399
	0.1627

	Base
	172
	100
	ENVDIS
	Combination
	Min
	
	
	-0.1964
	-8.4476
	17.3715
	-0.8851
	-0.6791
	-0.2979

	Base
	172
	100
	Serv1
	Combination
	
	
	
	1.2971
	-3.9805
	30.0382
	0.7048
	0.029
	-0.0644

	Base
	172
	100
	Serv2
	Combination
	
	
	
	1.2971
	-3.9805
	30.0382
	0.7048
	0.029
	-0.0644

	Base
	172
	100
	Serv3
	Combination
	
	
	
	1.2971
	-3.9805
	30.0382
	0.7048
	0.029
	-0.0644

	Base
	172
	100
	Serv4
	Combination
	Max
	
	
	1.525
	-3.4791
	32.7011
	0.9817
	0.5226
	0.0335

	Base
	172
	100
	Serv4
	Combination
	Min
	
	
	1.0693
	-4.482
	27.3754
	0.428
	-0.4646
	-0.1622

	Base
	172
	100
	Serv5
	Combination
	Max
	
	
	2.2515
	-1.4116
	36.8002
	1.7681
	0.0873
	0.09

	Base
	172
	100
	Serv5
	Combination
	Min
	
	
	0.3428
	-6.5494
	23.2762
	-0.3584
	-0.0294
	-0.2188

	Base
	172
	100
	Serv6
	Combination
	Max
	
	
	1.468
	-3.6044
	32.0353
	0.9125
	0.3992
	0.009

	Base
	172
	100
	Serv6
	Combination
	Min
	
	
	1.1263
	-4.3566
	28.0411
	0.4972
	-0.3412
	-0.1378

	Base
	172
	100
	Serv7
	Combination
	Max
	
	
	2.0129
	-2.0538
	35.1097
	1.5023
	0.0728
	0.0514

	Base
	172
	100
	Serv7
	Combination
	Min
	
	
	0.5813
	-5.9072
	24.9667
	-0.0926
	-0.0148
	-0.1802

	Base
	172
	100
	Serv8
	Combination
	
	
	
	0.7783
	-2.3883
	18.0229
	0.4229
	0.0174
	-0.0386

	Base
	172
	100
	Serv9
	Combination
	Max
	
	
	1.0061
	-1.8868
	20.6858
	0.6997
	0.511
	0.0592

	Base
	172
	100
	Serv9
	Combination
	Min
	
	
	0.5504
	-2.8898
	15.3601
	0.1461
	-0.4762
	-0.1365

	Base
	172
	100
	Serv10
	Combination
	Max
	
	
	1.7327
	0.1806
	24.7849
	1.4862
	0.0758
	0.1158

	Base
	172
	100
	Serv10
	Combination
	Min
	
	
	-0.1761
	-4.9572
	11.2609
	-0.6404
	-0.041
	-0.1931

	Base
	172
	100
	ENVSERV
	Combination
	Max
	
	
	2.2515
	0.1806
	36.8002
	1.7681
	0.5226
	0.1158

	Base
	172
	100
	ENVSERV
	Combination
	Min
	
	
	-0.1761
	-6.5494
	11.2609
	-0.6404
	-0.4762
	-0.2188

	Base
	173
	99
	Dead
	LinStatic
	
	
	
	-1.1529
	0.9749
	12.1251
	1.236
	0.0642
	-0.1536

	Base
	173
	99
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	173
	99
	FHEx
	LinStatic
	
	
	
	-2.2738
	-8.3354
	7.4879
	7.4341
	0.4051
	0.0931

	Base
	173
	99
	FHEy
	LinStatic
	
	
	
	49.1432
	-42.4108
	-141.7459
	18.9476
	3.2037
	-3.5057

	Base
	173
	99
	Sx
	LinRespSpec
	Max
	
	
	8.4405
	6.3234
	27.417
	6.2353
	0.3856
	0.7287

	Base
	173
	99
	Sy
	LinRespSpec
	Max
	
	
	35.1548
	24.1424
	98.9297
	14.7662
	2.3342
	2.2735

	Base
	173
	99
	Comb1
	Combination
	
	
	
	-1.614
	1.3648
	16.9751
	1.7304
	0.0898
	-0.215

	Base
	173
	99
	Comb2
	Combination
	
	
	
	-1.3835
	1.1699
	14.5501
	1.4832
	0.077
	-0.1843

	Base
	173
	99
	Comb3
	Combination
	
	
	
	-1.3835
	1.1699
	14.5501
	1.4832
	0.077
	-0.1843

	Base
	173
	99
	Comb4
	Combination
	Max
	
	
	-0.1777
	2.0732
	18.4668
	2.3739
	0.1321
	-0.0802

	Base
	173
	99
	Comb4
	Combination
	Min
	
	
	-2.5893
	0.2665
	10.6334
	0.5924
	0.0219
	-0.2884

	Base
	173
	99
	Comb5
	Combination
	Max
	
	
	3.6402
	4.6198
	28.6871
	3.5933
	0.4106
	0.1406

	Base
	173
	99
	Comb5
	Combination
	Min
	
	
	-6.4071
	-2.2801
	0.413
	-0.6269
	-0.2566
	-0.5092

	Base
	173
	99
	Comb6
	Combination
	
	
	
	-1.0376
	0.8774
	10.9126
	1.1124
	0.0578
	-0.1382

	Base
	173
	99
	Comb7
	Combination
	Max
	
	
	0.1682
	1.7807
	14.8293
	2.0031
	0.1128
	-0.0341

	Base
	173
	99
	Comb7
	Combination
	Min
	
	
	-2.2434
	-0.026
	6.9958
	0.2216
	0.0027
	-0.2423

	Base
	173
	99
	Comb8
	Combination
	Max
	
	
	3.986
	4.3273
	25.0496
	3.2225
	0.3913
	0.1867

	Base
	173
	99
	Comb8
	Combination
	Min
	
	
	-6.0612
	-2.5726
	-3.2245
	-0.9977
	-0.2758
	-0.4631

	Base
	173
	99
	ENVDIS
	Combination
	Max
	
	
	3.986
	4.6198
	28.6871
	3.5933
	0.4106
	0.1867

	Base
	173
	99
	ENVDIS
	Combination
	Min
	
	
	-6.4071
	-2.5726
	-3.2245
	-0.9977
	-0.2758
	-0.5092

	Base
	173
	99
	Serv1
	Combination
	
	
	
	-1.1529
	0.9749
	12.1251
	1.236
	0.0642
	-0.1536

	Base
	173
	99
	Serv2
	Combination
	
	
	
	-1.1529
	0.9749
	12.1251
	1.236
	0.0642
	-0.1536

	Base
	173
	99
	Serv3
	Combination
	
	
	
	-1.1529
	0.9749
	12.1251
	1.236
	0.0642
	-0.1536

	Base
	173
	99
	Serv4
	Combination
	Max
	
	
	-0.3088
	1.6072
	14.8668
	1.8595
	0.1027
	-0.0807

	Base
	173
	99
	Serv4
	Combination
	Min
	
	
	-1.9969
	0.3425
	9.3834
	0.6124
	0.0256
	-0.2265

	Base
	173
	99
	Serv5
	Combination
	Max
	
	
	2.3626
	3.3891
	22.018
	2.7126
	0.2976
	0.0738

	Base
	173
	99
	Serv5
	Combination
	Min
	
	
	-4.6684
	-1.4394
	2.2321
	-0.2406
	-0.1693
	-0.3809

	Base
	173
	99
	Serv6
	Combination
	Max
	
	
	-0.5198
	1.4491
	14.1813
	1.7036
	0.0931
	-0.0989

	Base
	173
	99
	Serv6
	Combination
	Min
	
	
	-1.7859
	0.5006
	10.0688
	0.7683
	0.0352
	-0.2082

	Base
	173
	99
	Serv7
	Combination
	Max
	
	
	1.4837
	2.7856
	19.5448
	2.3434
	0.2392
	0.0169

	Base
	173
	99
	Serv7
	Combination
	Min
	
	
	-3.7895
	-0.8358
	4.7053
	0.1285
	-0.1109
	-0.3241

	Base
	173
	99
	Serv8
	Combination
	
	
	
	-0.6917
	0.5849
	7.275
	0.7416
	0.0385
	-0.0922

	Base
	173
	99
	Serv9
	Combination
	Max
	
	
	0.1523
	1.2173
	10.0167
	1.3651
	0.0771
	-0.0193

	Base
	173
	99
	Serv9
	Combination
	Min
	
	
	-1.5358
	-0.0474
	4.5333
	0.118
	-0.0001
	-0.165

	Base
	173
	99
	Serv10
	Combination
	Max
	
	
	2.8237
	2.9992
	17.168
	2.2182
	0.2719
	0.1352

	Base
	173
	99
	Serv10
	Combination
	Min
	
	
	-4.2072
	-1.8293
	-2.6179
	-0.735
	-0.1949
	-0.3195

	Base
	173
	99
	ENVSERV
	Combination
	Max
	
	
	2.8237
	3.3891
	22.018
	2.7126
	0.2976
	0.1352

	Base
	173
	99
	ENVSERV
	Combination
	Min
	
	
	-4.6684
	-1.8293
	-2.6179
	-0.735
	-0.1949
	-0.3809

	Base
	174
	70
	Dead
	LinStatic
	
	
	
	-3.4254
	3.179
	17.8911
	0.7788
	-1.7015
	-0.1928

	Base
	174
	70
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	174
	70
	FHEx
	LinStatic
	
	
	
	-24.3005
	15.5619
	61.9927
	-0.6788
	-12.0228
	0.2334

	Base
	174
	70
	FHEy
	LinStatic
	
	
	
	-17.4494
	14.2465
	-21.1557
	0.1789
	-45.0249
	3.0534

	Base
	174
	70
	Sx
	LinRespSpec
	Max
	
	
	24.9503
	15.1519
	59.7093
	1.2639
	11.9899
	1.3145

	Base
	174
	70
	Sy
	LinRespSpec
	Max
	
	
	24.1067
	18.2131
	34.6041
	1.5795
	41.9584
	2.3235

	Base
	174
	70
	Comb1
	Combination
	
	
	
	-4.7955
	4.4506
	25.0475
	1.0903
	-2.3822
	-0.27

	Base
	174
	70
	Comb2
	Combination
	
	
	
	-4.1105
	3.8148
	21.4693
	0.9345
	-2.0419
	-0.2314

	Base
	174
	70
	Comb3
	Combination
	
	
	
	-4.1105
	3.8148
	21.4693
	0.9345
	-2.0419
	-0.2314

	Base
	174
	70
	Comb4
	Combination
	Max
	
	
	-0.5461
	5.9793
	29.9992
	1.1151
	-0.329
	-0.0436

	Base
	174
	70
	Comb4
	Combination
	Min
	
	
	-7.6748
	1.6502
	12.9394
	0.754
	-3.7547
	-0.4192

	Base
	174
	70
	Comb5
	Combination
	Max
	
	
	-0.6656
	6.4174
	26.4142
	1.1602
	3.954
	0.1006

	Base
	174
	70
	Comb5
	Combination
	Min
	
	
	-7.5553
	1.2121
	16.5243
	0.7088
	-8.0377
	-0.5634

	Base
	174
	70
	Comb6
	Combination
	
	
	
	-3.0828
	2.8611
	16.1019
	0.7009
	-1.5314
	-0.1735

	Base
	174
	70
	Comb7
	Combination
	Max
	
	
	0.4815
	5.0256
	24.6318
	0.8814
	0.1815
	0.0142

	Base
	174
	70
	Comb7
	Combination
	Min
	
	
	-6.6472
	0.6965
	7.572
	0.5203
	-3.2442
	-0.3613

	Base
	174
	70
	Comb8
	Combination
	Max
	
	
	0.362
	5.4637
	21.0469
	0.9266
	4.4645
	0.1585

	Base
	174
	70
	Comb8
	Combination
	Min
	
	
	-6.5277
	0.2584
	11.157
	0.4752
	-7.5272
	-0.5056

	Base
	174
	70
	ENVDIS
	Combination
	Max
	
	
	0.4815
	6.4174
	29.9992
	1.1602
	4.4645
	0.1585

	Base
	174
	70
	ENVDIS
	Combination
	Min
	
	
	-7.6748
	0.2584
	7.572
	0.4752
	-8.0377
	-0.5634

	Base
	174
	70
	Serv1
	Combination
	
	
	
	-3.4254
	3.179
	17.8911
	0.7788
	-1.7015
	-0.1928

	Base
	174
	70
	Serv2
	Combination
	
	
	
	-3.4254
	3.179
	17.8911
	0.7788
	-1.7015
	-0.1928

	Base
	174
	70
	Serv3
	Combination
	
	
	
	-3.4254
	3.179
	17.8911
	0.7788
	-1.7015
	-0.1928

	Base
	174
	70
	Serv4
	Combination
	Max
	
	
	-0.9303
	4.6942
	23.862
	0.9052
	-0.5026
	-0.0614

	Base
	174
	70
	Serv4
	Combination
	Min
	
	
	-5.9204
	1.6638
	11.9201
	0.6524
	-2.9005
	-0.3243

	Base
	174
	70
	Serv5
	Combination
	Max
	
	
	-1.0147
	5.0003
	21.3515
	0.9367
	2.4943
	0.0395

	Base
	174
	70
	Serv5
	Combination
	Min
	
	
	-5.8361
	1.3577
	14.4306
	0.6208
	-5.8974
	-0.4252

	Base
	174
	70
	Serv6
	Combination
	Max
	
	
	-1.5541
	4.3154
	22.3693
	0.8736
	-0.8023
	-0.0942

	Base
	174
	70
	Serv6
	Combination
	Min
	
	
	-5.2967
	2.0426
	13.4129
	0.684
	-2.6008
	-0.2914

	Base
	174
	70
	Serv7
	Combination
	Max
	
	
	-1.6174
	4.545
	20.4864
	0.8972
	1.4453
	-0.0186

	Base
	174
	70
	Serv7
	Combination
	Min
	
	
	-5.2334
	1.813
	15.2957
	0.6603
	-4.8484
	-0.3671

	Base
	174
	70
	Serv8
	Combination
	
	
	
	-2.0552
	1.9074
	10.7346
	0.4673
	-1.0209
	-0.1157

	Base
	174
	70
	Serv9
	Combination
	Max
	
	
	0.4398
	3.4226
	16.7056
	0.5936
	0.1781
	0.0158

	Base
	174
	70
	Serv9
	Combination
	Min
	
	
	-4.5503
	0.3922
	4.7637
	0.3409
	-2.2199
	-0.2471

	Base
	174
	70
	Serv10
	Combination
	Max
	
	
	0.3554
	3.7287
	14.195
	0.6252
	3.1749
	0.1167

	Base
	174
	70
	Serv10
	Combination
	Min
	
	
	-4.4659
	0.0861
	7.2742
	0.3093
	-5.2168
	-0.348

	Base
	174
	70
	ENVSERV
	Combination
	Max
	
	
	0.4398
	5.0003
	23.862
	0.9367
	3.1749
	0.1167

	Base
	174
	70
	ENVSERV
	Combination
	Min
	
	
	-5.9204
	0.0861
	4.7637
	0.3093
	-5.8974
	-0.4252

	Base
	175
	69
	Dead
	LinStatic
	
	
	
	0.4641
	1.0799
	23.0822
	-0.2433
	-0.7942
	-0.2334

	Base
	175
	69
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	175
	69
	FHEx
	LinStatic
	
	
	
	-15.2085
	-3.2027
	-60.7259
	1.1144
	-10.6372
	-1.1808

	Base
	175
	69
	FHEy
	LinStatic
	
	
	
	-36.2242
	-42.4021
	-199.289
	20.3418
	-17.2879
	0.4276

	Base
	175
	69
	Sx
	LinRespSpec
	Max
	
	
	13.0588
	6.5152
	65.3765
	4.0169
	10.1642
	1.2728

	Base
	175
	69
	Sy
	LinRespSpec
	Max
	
	
	38.5309
	30.0609
	166.9747
	12.5453
	19.3377
	2.7701

	Base
	175
	69
	Comb1
	Combination
	
	
	
	0.6497
	1.5119
	32.315
	-0.3406
	-1.1119
	-0.3268

	Base
	175
	69
	Comb2
	Combination
	
	
	
	0.5569
	1.2959
	27.6986
	-0.292
	-0.953
	-0.2801

	Base
	175
	69
	Comb3
	Combination
	
	
	
	0.5569
	1.2959
	27.6986
	-0.292
	-0.953
	-0.2801

	Base
	175
	69
	Comb4
	Combination
	Max
	
	
	2.4224
	2.2267
	37.0381
	0.2819
	0.499
	-0.0983

	Base
	175
	69
	Comb4
	Combination
	Min
	
	
	-1.3086
	0.3652
	18.3591
	-0.8658
	-2.4051
	-0.4619

	Base
	175
	69
	Comb5
	Combination
	Max
	
	
	6.063
	5.5916
	51.5593
	1.5007
	1.8103
	0.1158

	Base
	175
	69
	Comb5
	Combination
	Min
	
	
	-4.9492
	-2.9998
	3.8379
	-2.0847
	-3.7164
	-0.6759

	Base
	175
	69
	Comb6
	Combination
	
	
	
	0.4177
	0.972
	20.7739
	-0.219
	-0.7148
	-0.2101

	Base
	175
	69
	Comb7
	Combination
	Max
	
	
	2.2832
	1.9027
	30.1134
	0.3549
	0.7372
	-0.0282

	Base
	175
	69
	Comb7
	Combination
	Min
	
	
	-1.4479
	0.0412
	11.4344
	-0.7928
	-2.1668
	-0.3919

	Base
	175
	69
	Comb8
	Combination
	Max
	
	
	5.9237
	5.2677
	44.6346
	1.5737
	2.0486
	0.1858

	Base
	175
	69
	Comb8
	Combination
	Min
	
	
	-5.0884
	-3.3237
	-3.0867
	-2.0117
	-3.4781
	-0.6059

	Base
	175
	69
	ENVDIS
	Combination
	Max
	
	
	6.063
	5.5916
	51.5593
	1.5737
	2.0486
	0.1858

	Base
	175
	69
	ENVDIS
	Combination
	Min
	
	
	-5.0884
	-3.3237
	-3.0867
	-2.0847
	-3.7164
	-0.6759

	Base
	175
	69
	Serv1
	Combination
	
	
	
	0.4641
	1.0799
	23.0822
	-0.2433
	-0.7942
	-0.2334

	Base
	175
	69
	Serv2
	Combination
	
	
	
	0.4641
	1.0799
	23.0822
	-0.2433
	-0.7942
	-0.2334

	Base
	175
	69
	Serv3
	Combination
	
	
	
	0.4641
	1.0799
	23.0822
	-0.2433
	-0.7942
	-0.2334

	Base
	175
	69
	Serv4
	Combination
	Max
	
	
	1.77
	1.7315
	29.6198
	0.1584
	0.2222
	-0.1061

	Base
	175
	69
	Serv4
	Combination
	Min
	
	
	-0.8418
	0.4284
	16.5445
	-0.645
	-1.8106
	-0.3607

	Base
	175
	69
	Serv5
	Combination
	Max
	
	
	4.3172
	4.086
	39.7796
	1.0112
	1.1396
	0.0436

	Base
	175
	69
	Serv5
	Combination
	Min
	
	
	-3.389
	-1.9261
	6.3847
	-1.4978
	-2.728
	-0.5104

	Base
	175
	69
	Serv6
	Combination
	Max
	
	
	1.4435
	1.5686
	27.9854
	0.058
	-0.0319
	-0.1379

	Base
	175
	69
	Serv6
	Combination
	Min
	
	
	-0.5153
	0.5913
	18.1789
	-0.5446
	-1.5565
	-0.3289

	Base
	175
	69
	Serv7
	Combination
	Max
	
	
	3.3539
	3.3345
	35.6053
	0.6976
	0.6561
	-0.0256

	Base
	175
	69
	Serv7
	Combination
	Min
	
	
	-2.4257
	-1.1746
	10.5591
	-1.1842
	-2.2445
	-0.4412

	Base
	175
	69
	Serv8
	Combination
	
	
	
	0.2784
	0.648
	13.8493
	-0.146
	-0.4765
	-0.14

	Base
	175
	69
	Serv9
	Combination
	Max
	
	
	1.5843
	1.2995
	20.3869
	0.2557
	0.5399
	-0.0128

	Base
	175
	69
	Serv9
	Combination
	Min
	
	
	-1.0274
	-0.0036
	7.3116
	-0.5477
	-1.4929
	-0.2673

	Base
	175
	69
	Serv10
	Combination
	Max
	
	
	4.1315
	3.6541
	30.5468
	1.1085
	1.4572
	0.137

	Base
	175
	69
	Serv10
	Combination
	Min
	
	
	-3.5746
	-2.3581
	-2.8482
	-1.4005
	-2.4103
	-0.4171

	Base
	175
	69
	ENVSERV
	Combination
	Max
	
	
	4.3172
	4.086
	39.7796
	1.1085
	1.4572
	0.137

	Base
	175
	69
	ENVSERV
	Combination
	Min
	
	
	-3.5746
	-2.3581
	-2.8482
	-1.4978
	-2.728
	-0.5104

	Base
	176
	68
	Dead
	LinStatic
	
	
	
	3.9699
	-2.511
	19.4993
	0.8269
	0.1729
	-0.0716

	Base
	176
	68
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	176
	68
	FHEx
	LinStatic
	
	
	
	-0.2723
	4.7191
	-38.509
	5.7021
	1.5461
	-1.3102

	Base
	176
	68
	FHEy
	LinStatic
	
	
	
	42.662
	-35.8455
	89.3531
	18.5006
	5.698
	-3.8583

	Base
	176
	68
	Sx
	LinRespSpec
	Max
	
	
	6.6812
	6.9651
	40.2102
	7.5281
	1.3824
	1.4164

	Base
	176
	68
	Sy
	LinRespSpec
	Max
	
	
	29.9649
	19.1936
	45.9522
	11.5269
	6.034
	3.9791

	Base
	176
	68
	Comb1
	Combination
	
	
	
	5.5579
	-3.5153
	27.299
	1.1576
	0.2421
	-0.1002

	Base
	176
	68
	Comb2
	Combination
	
	
	
	4.7639
	-3.0131
	23.3992
	0.9922
	0.2075
	-0.0859

	Base
	176
	68
	Comb3
	Combination
	
	
	
	4.7639
	-3.0131
	23.3992
	0.9922
	0.2075
	-0.0859

	Base
	176
	68
	Comb4
	Combination
	Max
	
	
	5.7184
	-2.0181
	29.1435
	2.0677
	0.405
	0.1165

	Base
	176
	68
	Comb4
	Combination
	Min
	
	
	3.8095
	-4.0082
	17.6549
	-0.0832
	0.01
	-0.2882

	Base
	176
	68
	Comb5
	Combination
	Max
	
	
	9.0459
	-0.2704
	29.9657
	2.6394
	1.0698
	0.4827

	Base
	176
	68
	Comb5
	Combination
	Min
	
	
	0.4819
	-5.7559
	16.8326
	-0.655
	-0.6547
	-0.6545

	Base
	176
	68
	Comb6
	Combination
	
	
	
	3.5729
	-2.2599
	17.5494
	0.7442
	0.1556
	-0.0644

	Base
	176
	68
	Comb7
	Combination
	Max
	
	
	4.5274
	-1.2648
	23.2937
	1.8196
	0.3531
	0.1379

	Base
	176
	68
	Comb7
	Combination
	Min
	
	
	2.6185
	-3.2549
	11.8051
	-0.3313
	-0.0419
	-0.2668

	Base
	176
	68
	Comb8
	Combination
	Max
	
	
	7.8549
	0.4829
	24.1159
	2.3914
	1.0179
	0.5042

	Base
	176
	68
	Comb8
	Combination
	Min
	
	
	-0.709
	-5.0026
	10.9828
	-0.903
	-0.7066
	-0.633

	Base
	176
	68
	ENVDIS
	Combination
	Max
	
	
	9.0459
	0.4829
	29.9657
	2.6394
	1.0698
	0.5042

	Base
	176
	68
	ENVDIS
	Combination
	Min
	
	
	-0.709
	-5.7559
	10.9828
	-0.903
	-0.7066
	-0.6545

	Base
	176
	68
	Serv1
	Combination
	
	
	
	3.9699
	-2.511
	19.4993
	0.8269
	0.1729
	-0.0716

	Base
	176
	68
	Serv2
	Combination
	
	
	
	3.9699
	-2.511
	19.4993
	0.8269
	0.1729
	-0.0716

	Base
	176
	68
	Serv3
	Combination
	
	
	
	3.9699
	-2.511
	19.4993
	0.8269
	0.1729
	-0.0716

	Base
	176
	68
	Serv4
	Combination
	Max
	
	
	4.638
	-1.8144
	23.5203
	1.5797
	0.3112
	0.0701

	Base
	176
	68
	Serv4
	Combination
	Min
	
	
	3.3018
	-3.2075
	15.4783
	0.0741
	0.0347
	-0.2132

	Base
	176
	68
	Serv5
	Combination
	Max
	
	
	6.9664
	-0.5916
	24.0945
	1.9796
	0.7763
	0.3263

	Base
	176
	68
	Serv5
	Combination
	Min
	
	
	0.9734
	-4.4303
	14.9041
	-0.3258
	-0.4305
	-0.4695

	Base
	176
	68
	Serv6
	Combination
	Max
	
	
	4.471
	-1.9886
	22.5151
	1.3915
	0.2766
	0.0347

	Base
	176
	68
	Serv6
	Combination
	Min
	
	
	3.4688
	-3.0333
	16.4835
	0.2623
	0.0692
	-0.1778

	Base
	176
	68
	Serv7
	Combination
	Max
	
	
	6.2173
	-1.0714
	22.9457
	1.6914
	0.6255
	0.2269

	Base
	176
	68
	Serv7
	Combination
	Min
	
	
	1.7226
	-3.9505
	16.0529
	-0.0377
	-0.2796
	-0.37

	Base
	176
	68
	Serv8
	Combination
	
	
	
	2.382
	-1.5066
	11.6996
	0.4961
	0.1038
	-0.0429

	Base
	176
	68
	Serv9
	Combination
	Max
	
	
	3.0501
	-0.8101
	15.7206
	1.2489
	0.242
	0.0987

	Base
	176
	68
	Serv9
	Combination
	Min
	
	
	1.7138
	-2.2031
	7.6786
	-0.2567
	-0.0345
	-0.1846

	Base
	176
	68
	Serv10
	Combination
	Max
	
	
	5.3784
	0.4128
	16.2948
	1.6488
	0.7072
	0.355

	Base
	176
	68
	Serv10
	Combination
	Min
	
	
	-0.6145
	-3.4259
	7.1044
	-0.6566
	-0.4996
	-0.4408

	Base
	176
	68
	ENVSERV
	Combination
	Max
	
	
	6.9664
	0.4128
	24.0945
	1.9796
	0.7763
	0.355

	Base
	176
	68
	ENVSERV
	Combination
	Min
	
	
	-0.6145
	-4.4303
	7.1044
	-0.6566
	-0.4996
	-0.4695

	Base
	177
	71
	Dead
	LinStatic
	
	
	
	-2.7866
	-4.1019
	21.0298
	1.0296
	0.5871
	-0.2182

	Base
	177
	71
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	177
	71
	FHEx
	LinStatic
	
	
	
	-21.5592
	-16.1681
	58.1038
	2.3551
	-2.8418
	-0.4452

	Base
	177
	71
	FHEy
	LinStatic
	
	
	
	6.3217
	-27.6479
	95.1585
	2.4153
	32.0696
	-0.0957

	Base
	177
	71
	Sx
	LinRespSpec
	Max
	
	
	22.2929
	16.1792
	58.1232
	2.319
	5.9803
	0.4282

	Base
	177
	71
	Sy
	LinRespSpec
	Max
	
	
	12.6178
	27.5519
	97.0549
	3.0398
	24.9245
	0.4639

	Base
	177
	71
	Comb1
	Combination
	
	
	
	-3.9012
	-5.7427
	29.4417
	1.4414
	0.822
	-0.3055

	Base
	177
	71
	Comb2
	Combination
	
	
	
	-3.3439
	-4.9223
	25.2358
	1.2355
	0.7045
	-0.2619

	Base
	177
	71
	Comb3
	Combination
	
	
	
	-3.3439
	-4.9223
	25.2358
	1.2355
	0.7045
	-0.2619

	Base
	177
	71
	Comb4
	Combination
	Max
	
	
	-0.1592
	-2.611
	33.5391
	1.5668
	1.5589
	-0.2007

	Base
	177
	71
	Comb4
	Combination
	Min
	
	
	-6.5286
	-7.2336
	16.9325
	0.9042
	-0.1498
	-0.323

	Base
	177
	71
	Comb5
	Combination
	Max
	
	
	-1.5408
	-0.9851
	39.1049
	1.6699
	4.2662
	-0.1956

	Base
	177
	71
	Comb5
	Combination
	Min
	
	
	-5.147
	-8.8595
	11.3666
	0.8011
	-2.8572
	-0.3281

	Base
	177
	71
	Comb6
	Combination
	
	
	
	-2.5079
	-3.6917
	18.9268
	0.9266
	0.5284
	-0.1964

	Base
	177
	71
	Comb7
	Combination
	Max
	
	
	0.6768
	-1.3804
	27.2302
	1.2579
	1.3827
	-0.1352

	Base
	177
	71
	Comb7
	Combination
	Min
	
	
	-5.6926
	-6.003
	10.6235
	0.5953
	-0.3259
	-0.2576

	Base
	177
	71
	Comb8
	Combination
	Max
	
	
	-0.7048
	0.2454
	32.796
	1.361
	4.0901
	-0.1301

	Base
	177
	71
	Comb8
	Combination
	Min
	
	
	-4.311
	-7.6289
	5.0577
	0.4922
	-3.0333
	-0.2627

	Base
	177
	71
	ENVDIS
	Combination
	Max
	
	
	0.6768
	0.2454
	39.1049
	1.6699
	4.2662
	-0.1301

	Base
	177
	71
	ENVDIS
	Combination
	Min
	
	
	-6.5286
	-8.8595
	5.0577
	0.4922
	-3.0333
	-0.3281

	Base
	177
	71
	Serv1
	Combination
	
	
	
	-2.7866
	-4.1019
	21.0298
	1.0296
	0.5871
	-0.2182

	Base
	177
	71
	Serv2
	Combination
	
	
	
	-2.7866
	-4.1019
	21.0298
	1.0296
	0.5871
	-0.2182

	Base
	177
	71
	Serv3
	Combination
	
	
	
	-2.7866
	-4.1019
	21.0298
	1.0296
	0.5871
	-0.2182

	Base
	177
	71
	Serv4
	Combination
	Max
	
	
	-0.5573
	-2.484
	26.8421
	1.2615
	1.1851
	-0.1754

	Base
	177
	71
	Serv4
	Combination
	Min
	
	
	-5.0159
	-5.7198
	15.2175
	0.7977
	-0.0109
	-0.261

	Base
	177
	71
	Serv5
	Combination
	Max
	
	
	-1.5248
	-1.3467
	30.7353
	1.3336
	3.0796
	-0.1718

	Base
	177
	71
	Serv5
	Combination
	Min
	
	
	-4.0484
	-6.8571
	11.3243
	0.7256
	-1.9053
	-0.2646

	Base
	177
	71
	Serv6
	Combination
	Max
	
	
	-1.1146
	-2.8885
	25.3891
	1.2035
	1.0356
	-0.1861

	Base
	177
	71
	Serv6
	Combination
	Min
	
	
	-4.4586
	-5.3154
	16.6706
	0.8557
	0.1386
	-0.2503

	Base
	177
	71
	Serv7
	Combination
	Max
	
	
	-1.8403
	-2.0355
	28.3089
	1.2576
	2.4564
	-0.1834

	Base
	177
	71
	Serv7
	Combination
	Min
	
	
	-3.7329
	-6.1683
	13.7507
	0.8016
	-1.2822
	-0.253

	Base
	177
	71
	Serv8
	Combination
	
	
	
	-1.6719
	-2.4611
	12.6179
	0.6177
	0.3523
	-0.1309

	Base
	177
	71
	Serv9
	Combination
	Max
	
	
	0.5573
	-0.8432
	18.4302
	0.8496
	0.9503
	-0.0881

	Base
	177
	71
	Serv9
	Combination
	Min
	
	
	-3.9012
	-4.0791
	6.8056
	0.3859
	-0.2458
	-0.1737

	Base
	177
	71
	Serv10
	Combination
	Max
	
	
	-0.4102
	0.294
	22.3234
	0.9217
	2.8447
	-0.0845

	Base
	177
	71
	Serv10
	Combination
	Min
	
	
	-2.9337
	-5.2163
	2.9124
	0.3138
	-2.1402
	-0.1773

	Base
	177
	71
	ENVSERV
	Combination
	Max
	
	
	0.5573
	0.294
	30.7353
	1.3336
	3.0796
	-0.0845

	Base
	177
	71
	ENVSERV
	Combination
	Min
	
	
	-5.0159
	-6.8571
	2.9124
	0.3138
	-2.1402
	-0.2646

	Base
	178
	72
	Dead
	LinStatic
	
	
	
	1.5502
	1.9184
	23.6472
	-0.6281
	-0.1229
	-0.0301

	Base
	178
	72
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	178
	72
	FHEx
	LinStatic
	
	
	
	-7.6086
	5.4179
	-29.276
	-3.6399
	-7.3199
	-0.7588

	Base
	178
	72
	FHEy
	LinStatic
	
	
	
	6.2542
	-30.4606
	-92.8218
	15.8117
	0.3489
	-3.3352

	Base
	178
	72
	Sx
	LinRespSpec
	Max
	
	
	6.7341
	8.2689
	31.732
	4.3746
	7.4491
	1.7191

	Base
	178
	72
	Sy
	LinRespSpec
	Max
	
	
	2.7133
	22.0911
	77.3473
	9.4845
	3.6674
	2.7064

	Base
	178
	72
	Comb1
	Combination
	
	
	
	2.1703
	2.6857
	33.1061
	-0.8793
	-0.172
	-0.0421

	Base
	178
	72
	Comb2
	Combination
	
	
	
	1.8603
	2.3021
	28.3767
	-0.7537
	-0.1474
	-0.0361

	Base
	178
	72
	Comb3
	Combination
	
	
	
	1.8603
	2.3021
	28.3767
	-0.7537
	-0.1474
	-0.0361

	Base
	178
	72
	Comb4
	Combination
	Max
	
	
	2.8223
	3.4833
	32.9098
	-0.1287
	0.9167
	0.2095

	Base
	178
	72
	Comb4
	Combination
	Min
	
	
	0.8983
	1.1208
	23.8435
	-1.3786
	-1.2116
	-0.2817

	Base
	178
	72
	Comb5
	Combination
	Max
	
	
	2.248
	5.4589
	39.4296
	0.6017
	0.3766
	0.3507

	Base
	178
	72
	Comb5
	Combination
	Min
	
	
	1.4725
	-0.8548
	17.3237
	-2.109
	-0.6715
	-0.4228

	Base
	178
	72
	Comb6
	Combination
	
	
	
	1.3952
	1.7265
	21.2825
	-0.5653
	-0.1106
	-0.027

	Base
	178
	72
	Comb7
	Combination
	Max
	
	
	2.3572
	2.9078
	25.8156
	0.0597
	0.9536
	0.2185

	Base
	178
	72
	Comb7
	Combination
	Min
	
	
	0.4332
	0.5453
	16.7494
	-1.1902
	-1.1747
	-0.2726

	Base
	178
	72
	Comb8
	Combination
	Max
	
	
	1.7829
	4.8834
	32.3354
	0.7901
	0.4135
	0.3597

	Base
	178
	72
	Comb8
	Combination
	Min
	
	
	1.0075
	-1.4303
	10.2296
	-1.9206
	-0.6346
	-0.4138

	Base
	178
	72
	ENVDIS
	Combination
	Max
	
	
	2.8223
	5.4589
	39.4296
	0.7901
	0.9536
	0.3597

	Base
	178
	72
	ENVDIS
	Combination
	Min
	
	
	0.4332
	-1.4303
	10.2296
	-2.109
	-1.2116
	-0.4228

	Base
	178
	72
	Serv1
	Combination
	
	
	
	1.5502
	1.9184
	23.6472
	-0.6281
	-0.1229
	-0.0301

	Base
	178
	72
	Serv2
	Combination
	
	
	
	1.5502
	1.9184
	23.6472
	-0.6281
	-0.1229
	-0.0301

	Base
	178
	72
	Serv3
	Combination
	
	
	
	1.5502
	1.9184
	23.6472
	-0.6281
	-0.1229
	-0.0301

	Base
	178
	72
	Serv4
	Combination
	Max
	
	
	2.2236
	2.7453
	26.8204
	-0.1906
	0.6221
	0.1419

	Base
	178
	72
	Serv4
	Combination
	Min
	
	
	0.8768
	1.0915
	20.474
	-1.0655
	-0.8678
	-0.202

	Base
	178
	72
	Serv5
	Combination
	Max
	
	
	1.8216
	4.1275
	31.382
	0.3204
	0.2439
	0.2406

	Base
	178
	72
	Serv5
	Combination
	Min
	
	
	1.2789
	-0.2907
	15.9125
	-1.5765
	-0.4896
	-0.3007

	Base
	178
	72
	Serv6
	Combination
	Max
	
	
	2.0553
	2.5385
	26.0271
	-0.3
	0.4358
	0.0989

	Base
	178
	72
	Serv6
	Combination
	Min
	
	
	1.0452
	1.2982
	21.2673
	-0.9562
	-0.6815
	-0.159

	Base
	178
	72
	Serv7
	Combination
	Max
	
	
	1.7537
	3.5752
	29.4483
	0.0833
	0.1522
	0.1729

	Base
	178
	72
	Serv7
	Combination
	Min
	
	
	1.3467
	0.2615
	17.8462
	-1.3394
	-0.3979
	-0.233

	Base
	178
	72
	Serv8
	Combination
	
	
	
	0.9301
	1.151
	14.1883
	-0.3768
	-0.0737
	-0.018

	Base
	178
	72
	Serv9
	Combination
	Max
	
	
	1.6035
	1.9779
	17.3615
	0.0606
	0.6712
	0.1539

	Base
	178
	72
	Serv9
	Combination
	Min
	
	
	0.2567
	0.3241
	11.0151
	-0.8143
	-0.8186
	-0.1899

	Base
	178
	72
	Serv10
	Combination
	Max
	
	
	1.2015
	3.3601
	21.9231
	0.5716
	0.293
	0.2526

	Base
	178
	72
	Serv10
	Combination
	Min
	
	
	0.6588
	-1.0581
	6.4536
	-1.3253
	-0.4405
	-0.2887

	Base
	178
	72
	ENVSERV
	Combination
	Max
	
	
	2.2236
	4.1275
	31.382
	0.5716
	0.6712
	0.2526

	Base
	178
	72
	ENVSERV
	Combination
	Min
	
	
	0.2567
	-1.0581
	6.4536
	-1.5765
	-0.8678
	-0.3007

	Base
	179
	73
	Dead
	LinStatic
	
	
	
	-4.0405
	-2.5016
	20.4489
	-0.1289
	-0.245
	0.19

	Base
	179
	73
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	179
	73
	FHEx
	LinStatic
	
	
	
	-3.569
	7.404
	15.0184
	-7.0115
	0.1273
	-0.1802

	Base
	179
	73
	FHEy
	LinStatic
	
	
	
	-50.5527
	-41.1394
	144.6304
	16.6977
	-3.1962
	-4.1921

	Base
	179
	73
	Sx
	LinRespSpec
	Max
	
	
	8.7466
	9.7302
	27.6692
	8.1659
	0.4357
	1.5476

	Base
	179
	73
	Sy
	LinRespSpec
	Max
	
	
	36.3594
	24.6337
	103.7672
	11.7469
	2.4391
	3.2721

	Base
	179
	73
	Comb1
	Combination
	
	
	
	-5.6567
	-3.5022
	28.6284
	-0.1805
	-0.3431
	0.2659

	Base
	179
	73
	Comb2
	Combination
	
	
	
	-4.8486
	-3.0019
	24.5386
	-0.1547
	-0.2941
	0.2279

	Base
	179
	73
	Comb3
	Combination
	
	
	
	-4.8486
	-3.0019
	24.5386
	-0.1547
	-0.2941
	0.2279

	Base
	179
	73
	Comb4
	Combination
	Max
	
	
	-3.5991
	-1.6119
	28.4914
	1.0119
	-0.2318
	0.449

	Base
	179
	73
	Comb4
	Combination
	Min
	
	
	-6.0981
	-4.3919
	20.5859
	-1.3212
	-0.3563
	0.0069

	Base
	179
	73
	Comb5
	Combination
	Max
	
	
	0.3472
	0.5183
	39.367
	1.524
	0.0545
	0.6955

	Base
	179
	73
	Comb5
	Combination
	Min
	
	
	-10.0444
	-6.522
	9.7103
	-1.8333
	-0.6426
	-0.2396

	Base
	179
	73
	Comb6
	Combination
	
	
	
	-3.6364
	-2.2514
	18.404
	-0.116
	-0.2205
	0.171

	Base
	179
	73
	Comb7
	Combination
	Max
	
	
	-2.3869
	-0.8614
	22.3567
	1.0505
	-0.1583
	0.392

	Base
	179
	73
	Comb7
	Combination
	Min
	
	
	-4.886
	-3.6414
	14.4512
	-1.2826
	-0.2828
	-0.0501

	Base
	179
	73
	Comb8
	Combination
	Max
	
	
	1.5593
	1.2687
	33.2323
	1.5626
	0.128
	0.6385

	Base
	179
	73
	Comb8
	Combination
	Min
	
	
	-8.8322
	-5.7716
	3.5756
	-1.7946
	-0.5691
	-0.2966

	Base
	179
	73
	ENVDIS
	Combination
	Max
	
	
	1.5593
	1.2687
	39.367
	1.5626
	0.128
	0.6955

	Base
	179
	73
	ENVDIS
	Combination
	Min
	
	
	-10.0444
	-6.522
	3.5756
	-1.8333
	-0.6426
	-0.2966

	Base
	179
	73
	Serv1
	Combination
	
	
	
	-4.0405
	-2.5016
	20.4489
	-0.1289
	-0.245
	0.19

	Base
	179
	73
	Serv2
	Combination
	
	
	
	-4.0405
	-2.5016
	20.4489
	-0.1289
	-0.245
	0.19

	Base
	179
	73
	Serv3
	Combination
	
	
	
	-4.0405
	-2.5016
	20.4489
	-0.1289
	-0.245
	0.19

	Base
	179
	73
	Serv4
	Combination
	Max
	
	
	-3.1658
	-1.5286
	23.2158
	0.6877
	-0.2015
	0.3447

	Base
	179
	73
	Serv4
	Combination
	Min
	
	
	-4.9152
	-3.4746
	17.6819
	-0.9455
	-0.2886
	0.0352

	Base
	179
	73
	Serv5
	Combination
	Max
	
	
	-0.4046
	-0.0382
	30.8256
	1.0458
	-0.0011
	0.5172

	Base
	179
	73
	Serv5
	Combination
	Min
	
	
	-7.6764
	-4.9649
	10.0721
	-1.3036
	-0.489
	-0.1372

	Base
	179
	73
	Serv6
	Combination
	Max
	
	
	-3.3845
	-1.7718
	22.524
	0.4835
	-0.2124
	0.306

	Base
	179
	73
	Serv6
	Combination
	Min
	
	
	-4.6965
	-3.2313
	18.3737
	-0.7413
	-0.2777
	0.0739

	Base
	179
	73
	Serv7
	Combination
	Max
	
	
	-1.3135
	-0.654
	28.2314
	0.7521
	-0.0621
	0.4354

	Base
	179
	73
	Serv7
	Combination
	Min
	
	
	-6.7675
	-4.3491
	12.6663
	-1.0099
	-0.428
	-0.0554

	Base
	179
	73
	Serv8
	Combination
	
	
	
	-2.4243
	-1.5009
	12.2693
	-0.0773
	-0.147
	0.114

	Base
	179
	73
	Serv9
	Combination
	Max
	
	
	-1.5496
	-0.5279
	15.0362
	0.7392
	-0.1035
	0.2687

	Base
	179
	73
	Serv9
	Combination
	Min
	
	
	-3.299
	-2.474
	9.5024
	-0.8939
	-0.1906
	-0.0408

	Base
	179
	73
	Serv10
	Combination
	Max
	
	
	1.2116
	0.9624
	22.646
	1.0974
	0.0969
	0.4412

	Base
	179
	73
	Serv10
	Combination
	Min
	
	
	-6.0602
	-3.9643
	1.8926
	-1.252
	-0.3909
	-0.2132

	Base
	179
	73
	ENVSERV
	Combination
	Max
	
	
	1.2116
	0.9624
	30.8256
	1.0974
	0.0969
	0.5172

	Base
	179
	73
	ENVSERV
	Combination
	Min
	
	
	-7.6764
	-4.9649
	1.8926
	-1.3036
	-0.489
	-0.2132

	Base
	180
	75
	Dead
	LinStatic
	
	
	
	0.1
	0.6965
	5.4148
	0.0307
	-1.4957
	0.0374

	Base
	180
	75
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	180
	75
	FHEx
	LinStatic
	
	
	
	-11.0789
	-12.4373
	-43.7491
	0.273
	-5.5289
	0.0292

	Base
	180
	75
	FHEy
	LinStatic
	
	
	
	-35.7254
	-17.3424
	-177.6189
	1.5893
	-22.1741
	1.155

	Base
	180
	75
	Sx
	LinRespSpec
	Max
	
	
	9.4523
	10.7014
	35.999
	0.186
	5.2725
	0.1801

	Base
	180
	75
	Sy
	LinRespSpec
	Max
	
	
	37.6137
	19.1017
	179.1842
	1.3225
	24.7828
	1.24

	Base
	180
	75
	Comb1
	Combination
	
	
	
	0.1401
	0.975
	7.5807
	0.043
	-2.094
	0.0524

	Base
	180
	75
	Comb2
	Combination
	
	
	
	0.1201
	0.8357
	6.4977
	0.0368
	-1.7948
	0.0449

	Base
	180
	75
	Comb3
	Combination
	
	
	
	0.1201
	0.8357
	6.4977
	0.0368
	-1.7948
	0.0449

	Base
	180
	75
	Comb4
	Combination
	Max
	
	
	1.4704
	2.3645
	11.6404
	0.0634
	-1.0416
	0.0707

	Base
	180
	75
	Comb4
	Combination
	Min
	
	
	-1.2303
	-0.693
	1.355
	0.0103
	-2.548
	0.0192

	Base
	180
	75
	Comb5
	Combination
	Max
	
	
	5.4951
	3.5654
	32.1031
	0.2258
	1.7466
	0.2221

	Base
	180
	75
	Comb5
	Combination
	Min
	
	
	-5.2549
	-1.8939
	-19.1077
	-0.1521
	-5.3363
	-0.1323

	Base
	180
	75
	Comb6
	Combination
	
	
	
	0.09
	0.6268
	4.8733
	0.0276
	-1.3461
	0.0337

	Base
	180
	75
	Comb7
	Combination
	Max
	
	
	1.4404
	2.1556
	10.016
	0.0542
	-0.5929
	0.0594

	Base
	180
	75
	Comb7
	Combination
	Min
	
	
	-1.2603
	-0.902
	-0.2694
	0.0011
	-2.0993
	0.008

	Base
	180
	75
	Comb8
	Combination
	Max
	
	
	5.465
	3.3564
	30.4787
	0.2166
	2.1953
	0.2109

	Base
	180
	75
	Comb8
	Combination
	Min
	
	
	-5.285
	-2.1028
	-20.7321
	-0.1614
	-4.8876
	-0.1435

	Base
	180
	75
	ENVDIS
	Combination
	Max
	
	
	5.4951
	3.5654
	32.1031
	0.2258
	2.1953
	0.2221

	Base
	180
	75
	ENVDIS
	Combination
	Min
	
	
	-5.285
	-2.1028
	-20.7321
	-0.1614
	-5.3363
	-0.1435

	Base
	180
	75
	Serv1
	Combination
	
	
	
	0.1
	0.6965
	5.4148
	0.0307
	-1.4957
	0.0374

	Base
	180
	75
	Serv2
	Combination
	
	
	
	0.1
	0.6965
	5.4148
	0.0307
	-1.4957
	0.0374

	Base
	180
	75
	Serv3
	Combination
	
	
	
	0.1
	0.6965
	5.4148
	0.0307
	-1.4957
	0.0374

	Base
	180
	75
	Serv4
	Combination
	Max
	
	
	1.0453
	1.7666
	9.0147
	0.0493
	-0.9684
	0.0555

	Base
	180
	75
	Serv4
	Combination
	Min
	
	
	-0.8452
	-0.3737
	1.8149
	0.0121
	-2.0229
	0.0194

	Base
	180
	75
	Serv5
	Combination
	Max
	
	
	3.8614
	2.6066
	23.3332
	0.163
	0.9826
	0.1614

	Base
	180
	75
	Serv5
	Combination
	Min
	
	
	-3.6613
	-1.2137
	-12.5037
	-0.1015
	-3.974
	-0.0866

	Base
	180
	75
	Serv6
	Combination
	Max
	
	
	0.809
	1.4991
	8.1147
	0.0447
	-1.1002
	0.051

	Base
	180
	75
	Serv6
	Combination
	Min
	
	
	-0.6089
	-0.1062
	2.7148
	0.0167
	-1.8911
	0.0239

	Base
	180
	75
	Serv7
	Combination
	Max
	
	
	2.9211
	2.1291
	18.8536
	0.1299
	0.363
	0.1304

	Base
	180
	75
	Serv7
	Combination
	Min
	
	
	-2.721
	-0.7362
	-8.0241
	-0.0685
	-3.3544
	-0.0556

	Base
	180
	75
	Serv8
	Combination
	
	
	
	0.06
	0.4179
	3.2489
	0.0184
	-0.8974
	0.0225

	Base
	180
	75
	Serv9
	Combination
	Max
	
	
	1.0053
	1.488
	6.8488
	0.037
	-0.3702
	0.0405

	Base
	180
	75
	Serv9
	Combination
	Min
	
	
	-0.8852
	-0.6523
	-0.351
	-0.0002
	-1.4247
	0.0045

	Base
	180
	75
	Serv10
	Combination
	Max
	
	
	3.8214
	2.328
	21.1673
	0.1507
	1.5809
	0.1465

	Base
	180
	75
	Serv10
	Combination
	Min
	
	
	-3.7013
	-1.4923
	-14.6696
	-0.1138
	-3.3757
	-0.1015

	Base
	180
	75
	ENVSERV
	Combination
	Max
	
	
	3.8614
	2.6066
	23.3332
	0.163
	1.5809
	0.1614

	Base
	180
	75
	ENVSERV
	Combination
	Min
	
	
	-3.7013
	-1.4923
	-14.6696
	-0.1138
	-3.974
	-0.1015

	Base
	181
	74
	Dead
	LinStatic
	
	
	
	3.728
	-0.9586
	18.679
	-0.137
	0.7389
	-0.0985

	Base
	181
	74
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	181
	74
	FHEx
	LinStatic
	
	
	
	-8.0128
	11.8343
	-28.7633
	-0.0389
	-4.7792
	-0.0822

	Base
	181
	74
	FHEy
	LinStatic
	
	
	
	25.4479
	11.2425
	79.9392
	-1.2081
	8.0904
	-1.4424

	Base
	181
	74
	Sx
	LinRespSpec
	Max
	
	
	11.628
	10.61
	34.9823
	0.3691
	4.0601
	0.1398

	Base
	181
	74
	Sy
	LinRespSpec
	Max
	
	
	23.9053
	13.8791
	70.0132
	1.7655
	9.0184
	1.5572

	Base
	181
	74
	Comb1
	Combination
	
	
	
	5.2191
	-1.3421
	26.1506
	-0.1918
	1.0345
	-0.1379

	Base
	181
	74
	Comb2
	Combination
	
	
	
	4.4735
	-1.1504
	22.4148
	-0.1644
	0.8867
	-0.1182

	Base
	181
	74
	Comb3
	Combination
	
	
	
	4.4735
	-1.1504
	22.4148
	-0.1644
	0.8867
	-0.1182

	Base
	181
	74
	Comb4
	Combination
	Max
	
	
	6.1347
	0.3653
	27.4123
	-0.1117
	1.4667
	-0.0982

	Base
	181
	74
	Comb4
	Combination
	Min
	
	
	2.8124
	-2.6661
	17.4174
	-0.2171
	0.3067
	-0.1381

	Base
	181
	74
	Comb5
	Combination
	Max
	
	
	7.8896
	0.833
	32.4197
	0.0879
	2.1754
	0.1044

	Base
	181
	74
	Comb5
	Combination
	Min
	
	
	1.0575
	-3.1337
	12.41
	-0.4167
	-0.402
	-0.3407

	Base
	181
	74
	Comb6
	Combination
	
	
	
	3.3552
	-0.8628
	16.8111
	-0.1233
	0.665
	-0.0886

	Base
	181
	74
	Comb7
	Combination
	Max
	
	
	5.0163
	0.6529
	21.8086
	-0.0706
	1.245
	-0.0687

	Base
	181
	74
	Comb7
	Combination
	Min
	
	
	1.694
	-2.3785
	11.8137
	-0.176
	0.085
	-0.1086

	Base
	181
	74
	Comb8
	Combination
	Max
	
	
	6.7712
	1.1206
	26.816
	0.129
	1.9537
	0.1339

	Base
	181
	74
	Comb8
	Combination
	Min
	
	
	-0.0609
	-2.8461
	6.8062
	-0.3756
	-0.6237
	-0.3111

	Base
	181
	74
	ENVDIS
	Combination
	Max
	
	
	7.8896
	1.1206
	32.4197
	0.129
	2.1754
	0.1339

	Base
	181
	74
	ENVDIS
	Combination
	Min
	
	
	-0.0609
	-3.1337
	6.8062
	-0.4167
	-0.6237
	-0.3407

	Base
	181
	74
	Serv1
	Combination
	
	
	
	3.728
	-0.9586
	18.679
	-0.137
	0.7389
	-0.0985

	Base
	181
	74
	Serv2
	Combination
	
	
	
	3.728
	-0.9586
	18.679
	-0.137
	0.7389
	-0.0985

	Base
	181
	74
	Serv3
	Combination
	
	
	
	3.728
	-0.9586
	18.679
	-0.137
	0.7389
	-0.0985

	Base
	181
	74
	Serv4
	Combination
	Max
	
	
	4.8908
	0.1024
	22.1773
	-0.1001
	1.1449
	-0.0845

	Base
	181
	74
	Serv4
	Combination
	Min
	
	
	2.5651
	-2.0196
	15.1808
	-0.1739
	0.3329
	-0.1124

	Base
	181
	74
	Serv5
	Combination
	Max
	
	
	6.1185
	0.4293
	25.6804
	0.0396
	1.6407
	0.0573

	Base
	181
	74
	Serv5
	Combination
	Min
	
	
	1.3374
	-2.3466
	11.6777
	-0.3135
	-0.1629
	-0.2542

	Base
	181
	74
	Serv6
	Combination
	Max
	
	
	4.6001
	-0.1629
	21.3027
	-0.1093
	1.0434
	-0.088

	Base
	181
	74
	Serv6
	Combination
	Min
	
	
	2.8558
	-1.7544
	16.0554
	-0.1647
	0.4344
	-0.109

	Base
	181
	74
	Serv7
	Combination
	Max
	
	
	5.5209
	0.0823
	23.93
	-0.0046
	1.4153
	0.0183

	Base
	181
	74
	Serv7
	Combination
	Min
	
	
	1.935
	-1.9996
	13.428
	-0.2694
	0.0625
	-0.2153

	Base
	181
	74
	Serv8
	Combination
	
	
	
	2.2368
	-0.5752
	11.2074
	-0.0822
	0.4433
	-0.0591

	Base
	181
	74
	Serv9
	Combination
	Max
	
	
	3.3996
	0.4858
	14.7056
	-0.0453
	0.8493
	-0.0451

	Base
	181
	74
	Serv9
	Combination
	Min
	
	
	1.074
	-1.6362
	7.7092
	-0.1191
	0.0373
	-0.0731

	Base
	181
	74
	Serv10
	Combination
	Max
	
	
	4.6273
	0.8127
	18.2087
	0.0944
	1.3452
	0.0966

	Base
	181
	74
	Serv10
	Combination
	Min
	
	
	-0.1538
	-1.9631
	4.2061
	-0.2587
	-0.4585
	-0.2148

	Base
	181
	74
	ENVSERV
	Combination
	Max
	
	
	6.1185
	0.8127
	25.6804
	0.0944
	1.6407
	0.0966

	Base
	181
	74
	ENVSERV
	Combination
	Min
	
	
	-0.1538
	-2.3466
	4.2061
	-0.3135
	-0.4585
	-0.2542

	Base
	182
	76
	Dead
	LinStatic
	
	
	
	-2.8316
	2.7039
	12.4513
	0.2365
	-1.5566
	0.0633

	Base
	182
	76
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	182
	76
	FHEx
	LinStatic
	
	
	
	-11.6723
	11.1613
	28.342
	0.0308
	-5.0904
	0.0556

	Base
	182
	76
	FHEy
	LinStatic
	
	
	
	-8.4013
	4.1715
	-79.3587
	3.6128
	-20.519
	1.6686

	Base
	182
	76
	Sx
	LinRespSpec
	Max
	
	
	11.2793
	10.9217
	34.547
	0.4246
	4.7373
	0.1181

	Base
	182
	76
	Sy
	LinRespSpec
	Max
	
	
	12.0343
	5.4872
	69.2559
	3.7127
	23.2997
	1.7235

	Base
	182
	76
	Comb1
	Combination
	
	
	
	-3.9642
	3.7855
	17.4318
	0.3311
	-2.1792
	0.0886

	Base
	182
	76
	Comb2
	Combination
	
	
	
	-3.3979
	3.2447
	14.9415
	0.2838
	-1.8679
	0.0759

	Base
	182
	76
	Comb3
	Combination
	
	
	
	-3.3979
	3.2447
	14.9415
	0.2838
	-1.8679
	0.0759

	Base
	182
	76
	Comb4
	Combination
	Max
	
	
	-1.7866
	4.805
	19.8768
	0.3444
	-1.1912
	0.0928

	Base
	182
	76
	Comb4
	Combination
	Min
	
	
	-5.0092
	1.6845
	10.0062
	0.2231
	-2.5447
	0.059

	Base
	182
	76
	Comb5
	Combination
	Max
	
	
	-1.6782
	4.0289
	24.8382
	0.8143
	1.4616
	0.3222

	Base
	182
	76
	Comb5
	Combination
	Min
	
	
	-5.1176
	2.4606
	5.0449
	-0.2468
	-5.1974
	-0.1704

	Base
	182
	76
	Comb6
	Combination
	
	
	
	-2.5484
	2.4336
	11.2062
	0.2128
	-1.4009
	0.0569

	Base
	182
	76
	Comb7
	Combination
	Max
	
	
	-0.9371
	3.9938
	16.1414
	0.2735
	-0.7242
	0.0738

	Base
	182
	76
	Comb7
	Combination
	Min
	
	
	-4.1598
	0.8733
	6.2709
	0.1522
	-2.0777
	0.0401

	Base
	182
	76
	Comb8
	Combination
	Max
	
	
	-0.8287
	3.2177
	21.1028
	0.7434
	1.9286
	0.3032

	Base
	182
	76
	Comb8
	Combination
	Min
	
	
	-4.2681
	1.6494
	1.3095
	-0.3177
	-4.7305
	-0.1894

	Base
	182
	76
	ENVDIS
	Combination
	Max
	
	
	-0.8287
	4.805
	24.8382
	0.8143
	1.9286
	0.3222

	Base
	182
	76
	ENVDIS
	Combination
	Min
	
	
	-5.1176
	0.8733
	1.3095
	-0.3177
	-5.1974
	-0.1894

	Base
	182
	76
	Serv1
	Combination
	
	
	
	-2.8316
	2.7039
	12.4513
	0.2365
	-1.5566
	0.0633

	Base
	182
	76
	Serv2
	Combination
	
	
	
	-2.8316
	2.7039
	12.4513
	0.2365
	-1.5566
	0.0633

	Base
	182
	76
	Serv3
	Combination
	
	
	
	-2.8316
	2.7039
	12.4513
	0.2365
	-1.5566
	0.0633

	Base
	182
	76
	Serv4
	Combination
	Max
	
	
	-1.7037
	3.7961
	15.906
	0.2789
	-1.0829
	0.0751

	Base
	182
	76
	Serv4
	Combination
	Min
	
	
	-3.9595
	1.6118
	8.9966
	0.194
	-2.0303
	0.0514

	Base
	182
	76
	Serv5
	Combination
	Max
	
	
	-1.6282
	3.2527
	19.3769
	0.6078
	0.7734
	0.2356

	Base
	182
	76
	Serv5
	Combination
	Min
	
	
	-4.035
	2.1552
	5.5257
	-0.1348
	-3.8866
	-0.1091

	Base
	182
	76
	Serv6
	Combination
	Max
	
	
	-1.9856
	3.5231
	15.0423
	0.2683
	-1.2013
	0.0721

	Base
	182
	76
	Serv6
	Combination
	Min
	
	
	-3.6775
	1.8848
	9.8603
	0.2046
	-1.9119
	0.0544

	Base
	182
	76
	Serv7
	Combination
	Max
	
	
	-1.929
	3.1155
	17.6455
	0.5149
	0.1909
	0.1925

	Base
	182
	76
	Serv7
	Combination
	Min
	
	
	-3.7342
	2.2924
	7.2571
	-0.042
	-3.3041
	-0.066

	Base
	182
	76
	Serv8
	Combination
	
	
	
	-1.699
	1.6224
	7.4708
	0.1419
	-0.934
	0.038

	Base
	182
	76
	Serv9
	Combination
	Max
	
	
	-0.571
	2.7145
	10.9255
	0.1843
	-0.4602
	0.0498

	Base
	182
	76
	Serv9
	Combination
	Min
	
	
	-2.8269
	0.5302
	4.0161
	0.0994
	-1.4077
	0.0261

	Base
	182
	76
	Serv10
	Combination
	Max
	
	
	-0.4955
	2.1711
	14.3964
	0.5132
	1.396
	0.2103

	Base
	182
	76
	Serv10
	Combination
	Min
	
	
	-2.9024
	1.0736
	0.5452
	-0.2294
	-3.2639
	-0.1344

	Base
	182
	76
	ENVSERV
	Combination
	Max
	
	
	-0.4955
	3.7961
	19.3769
	0.6078
	1.396
	0.2356

	Base
	182
	76
	ENVSERV
	Combination
	Min
	
	
	-4.035
	0.5302
	0.5452
	-0.2294
	-3.8866
	-0.1344

	Base
	183
	77
	Dead
	LinStatic
	
	
	
	-4.4013
	-3.4924
	25.3959
	0.4007
	0.6159
	-0.0772

	Base
	183
	77
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	183
	77
	FHEx
	LinStatic
	
	
	
	-14.2507
	-11.7581
	43.2727
	0.3421
	-5.1842
	-0.0818

	Base
	183
	77
	FHEy
	LinStatic
	
	
	
	-41.9627
	-18.6421
	176.038
	6.4074
	6.8536
	-0.7719

	Base
	183
	77
	Sx
	LinRespSpec
	Max
	
	
	12.1468
	10.9297
	35.4532
	0.3819
	4.8482
	0.138

	Base
	183
	77
	Sy
	LinRespSpec
	Max
	
	
	42.4308
	19.9601
	177.2536
	6.7402
	7.9494
	0.9328

	Base
	183
	77
	Comb1
	Combination
	
	
	
	-6.1619
	-4.8894
	35.5542
	0.561
	0.8623
	-0.108

	Base
	183
	77
	Comb2
	Combination
	
	
	
	-5.2816
	-4.1909
	30.475
	0.4809
	0.7391
	-0.0926

	Base
	183
	77
	Comb3
	Combination
	
	
	
	-5.2816
	-4.1909
	30.475
	0.4809
	0.7391
	-0.0926

	Base
	183
	77
	Comb4
	Combination
	Max
	
	
	-3.5463
	-2.6295
	35.5398
	0.5355
	1.4317
	-0.0729

	Base
	183
	77
	Comb4
	Combination
	Min
	
	
	-7.0169
	-5.7523
	25.4103
	0.4263
	0.0465
	-0.1123

	Base
	183
	77
	Comb5
	Combination
	Max
	
	
	0.7818
	-1.3386
	55.8046
	1.4441
	1.8751
	0.0407

	Base
	183
	77
	Comb5
	Combination
	Min
	
	
	-11.345
	-7.0432
	5.1455
	-0.4823
	-0.3969
	-0.2259

	Base
	183
	77
	Comb6
	Combination
	
	
	
	-3.9612
	-3.1432
	22.8563
	0.3607
	0.5543
	-0.0694

	Base
	183
	77
	Comb7
	Combination
	Max
	
	
	-2.2259
	-1.5818
	27.921
	0.4152
	1.2469
	-0.0497

	Base
	183
	77
	Comb7
	Combination
	Min
	
	
	-5.6965
	-4.7046
	17.7916
	0.3061
	-0.1383
	-0.0891

	Base
	183
	77
	Comb8
	Combination
	Max
	
	
	2.1022
	-0.2909
	48.1858
	1.3239
	1.6903
	0.0639

	Base
	183
	77
	Comb8
	Combination
	Min
	
	
	-10.0246
	-5.9955
	-2.4732
	-0.6025
	-0.5817
	-0.2027

	Base
	183
	77
	ENVDIS
	Combination
	Max
	
	
	2.1022
	-0.2909
	55.8046
	1.4441
	1.8751
	0.0639

	Base
	183
	77
	ENVDIS
	Combination
	Min
	
	
	-11.345
	-7.0432
	-2.4732
	-0.6025
	-0.5817
	-0.2259

	Base
	183
	77
	Serv1
	Combination
	
	
	
	-4.4013
	-3.4924
	25.3959
	0.4007
	0.6159
	-0.0772

	Base
	183
	77
	Serv2
	Combination
	
	
	
	-4.4013
	-3.4924
	25.3959
	0.4007
	0.6159
	-0.0772

	Base
	183
	77
	Serv3
	Combination
	
	
	
	-4.4013
	-3.4924
	25.3959
	0.4007
	0.6159
	-0.0772

	Base
	183
	77
	Serv4
	Combination
	Max
	
	
	-3.1867
	-2.3994
	28.9412
	0.4389
	1.1007
	-0.0634

	Base
	183
	77
	Serv4
	Combination
	Min
	
	
	-5.616
	-4.5854
	21.8506
	0.3626
	0.1311
	-0.091

	Base
	183
	77
	Serv5
	Combination
	Max
	
	
	-0.1583
	-1.4964
	43.1212
	1.0748
	1.4108
	0.0161

	Base
	183
	77
	Serv5
	Combination
	Min
	
	
	-8.6444
	-5.4884
	7.6705
	-0.2733
	-0.179
	-0.1704

	Base
	183
	77
	Serv6
	Combination
	Max
	
	
	-3.4903
	-2.6727
	28.0549
	0.4294
	0.9795
	-0.0668

	Base
	183
	77
	Serv6
	Combination
	Min
	
	
	-5.3124
	-4.3121
	22.7369
	0.3721
	0.2523
	-0.0875

	Base
	183
	77
	Serv7
	Combination
	Max
	
	
	-1.219
	-1.9954
	38.6899
	0.9063
	1.2121
	-0.0072

	Base
	183
	77
	Serv7
	Combination
	Min
	
	
	-7.5837
	-4.9894
	12.1019
	-0.1048
	0.0197
	-0.1471

	Base
	183
	77
	Serv8
	Combination
	
	
	
	-2.6408
	-2.0955
	15.2375
	0.2404
	0.3695
	-0.0463

	Base
	183
	77
	Serv9
	Combination
	Max
	
	
	-1.4261
	-1.0025
	18.7828
	0.2786
	0.8544
	-0.0325

	Base
	183
	77
	Serv9
	Combination
	Min
	
	
	-3.8555
	-3.1884
	11.6922
	0.2023
	-0.1153
	-0.0601

	Base
	183
	77
	Serv10
	Combination
	Max
	
	
	1.6023
	-0.0994
	32.9629
	0.9145
	1.1645
	0.047

	Base
	183
	77
	Serv10
	Combination
	Min
	
	
	-6.8839
	-4.0915
	-2.4878
	-0.4336
	-0.4254
	-0.1396

	Base
	183
	77
	ENVSERV
	Combination
	Max
	
	
	1.6023
	-0.0994
	43.1212
	1.0748
	1.4108
	0.047

	Base
	183
	77
	ENVSERV
	Combination
	Min
	
	
	-8.6444
	-5.4884
	-2.4878
	-0.4336
	-0.4254
	-0.1704

	Base
	3
	24
	Dead
	LinStatic
	
	
	
	0.4241
	4.3041
	9.0171
	-5.6447
	0.5647
	-0.0024

	Base
	3
	24
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	3
	24
	FHEx
	LinStatic
	
	
	
	-0.1335
	-0.0066
	0.5021
	0.0331
	-0.2421
	-0.0157

	Base
	3
	24
	FHEy
	LinStatic
	
	
	
	0.2475
	-0.162
	-0.8793
	0.6921
	0.4543
	-0.0253

	Base
	3
	24
	Sx
	LinRespSpec
	Max
	
	
	0.1203
	0.0198
	0.4636
	0.0834
	0.2169
	0.0184

	Base
	3
	24
	Sy
	LinRespSpec
	Max
	
	
	0.2444
	0.1363
	0.8241
	0.5923
	0.4504
	0.0304

	Base
	3
	24
	Comb1
	Combination
	
	
	
	0.5938
	6.0257
	12.624
	-7.9026
	0.7906
	-0.0033

	Base
	3
	24
	Comb2
	Combination
	
	
	
	0.509
	5.1649
	10.8206
	-6.7737
	0.6776
	-0.0029

	Base
	3
	24
	Comb3
	Combination
	
	
	
	0.509
	5.1649
	10.8206
	-6.7737
	0.6776
	-0.0029

	Base
	3
	24
	Comb4
	Combination
	Max
	
	
	0.5262
	5.1677
	10.8868
	-6.7617
	0.7086
	-0.0002

	Base
	3
	24
	Comb4
	Combination
	Min
	
	
	0.4918
	5.1621
	10.7543
	-6.7856
	0.6467
	-0.0055

	Base
	3
	24
	Comb5
	Combination
	Max
	
	
	0.5439
	5.1844
	10.9383
	-6.689
	0.742
	0.0015

	Base
	3
	24
	Comb5
	Combination
	Min
	
	
	0.474
	5.1454
	10.7028
	-6.8583
	0.6133
	-0.0072

	Base
	3
	24
	Comb6
	Combination
	
	
	
	0.3817
	3.8737
	8.1154
	-5.0802
	0.5082
	-0.0021

	Base
	3
	24
	Comb7
	Combination
	Max
	
	
	0.3989
	3.8765
	8.1817
	-5.0683
	0.5392
	0.0005

	Base
	3
	24
	Comb7
	Combination
	Min
	
	
	0.3645
	3.8709
	8.0492
	-5.0922
	0.4772
	-0.0048

	Base
	3
	24
	Comb8
	Combination
	Max
	
	
	0.4166
	3.8932
	8.2332
	-4.9956
	0.5726
	0.0022

	Base
	3
	24
	Comb8
	Combination
	Min
	
	
	0.3468
	3.8542
	7.9977
	-5.1649
	0.4439
	-0.0065

	Base
	3
	24
	ENVDIS
	Combination
	Max
	
	
	0.5938
	6.0257
	12.624
	-4.9956
	0.7906
	0.0022

	Base
	3
	24
	ENVDIS
	Combination
	Min
	
	
	0.3468
	3.8542
	7.9977
	-7.9026
	0.4439
	-0.0072

	Base
	3
	24
	Serv1
	Combination
	
	
	
	0.4241
	4.3041
	9.0171
	-5.6447
	0.5647
	-0.0024

	Base
	3
	24
	Serv2
	Combination
	
	
	
	0.4241
	4.3041
	9.0171
	-5.6447
	0.5647
	-0.0024

	Base
	3
	24
	Serv3
	Combination
	
	
	
	0.4241
	4.3041
	9.0171
	-5.6447
	0.5647
	-0.0024

	Base
	3
	24
	Serv4
	Combination
	Max
	
	
	0.4362
	4.3061
	9.0635
	-5.6364
	0.5864
	-0.0005

	Base
	3
	24
	Serv4
	Combination
	Min
	
	
	0.4121
	4.3021
	8.9708
	-5.6531
	0.543
	-0.0042

	Base
	3
	24
	Serv5
	Combination
	Max
	
	
	0.4486
	4.3177
	9.0996
	-5.5855
	0.6097
	0.0007

	Base
	3
	24
	Serv5
	Combination
	Min
	
	
	0.3997
	4.2904
	8.9347
	-5.7039
	0.5197
	-0.0054

	Base
	3
	24
	Serv6
	Combination
	Max
	
	
	0.4332
	4.3056
	9.0519
	-5.6385
	0.581
	-0.001

	Base
	3
	24
	Serv6
	Combination
	Min
	
	
	0.4151
	4.3026
	8.9824
	-5.651
	0.5484
	-0.0038

	Base
	3
	24
	Serv7
	Combination
	Max
	
	
	0.4425
	4.3143
	9.079
	-5.6003
	0.5985
	-0.0001

	Base
	3
	24
	Serv7
	Combination
	Min
	
	
	0.4058
	4.2939
	8.9553
	-5.6891
	0.5309
	-0.0047

	Base
	3
	24
	Serv8
	Combination
	
	
	
	0.2545
	2.5824
	5.4103
	-3.3868
	0.3388
	-0.0014

	Base
	3
	24
	Serv9
	Combination
	Max
	
	
	0.2665
	2.5844
	5.4566
	-3.3785
	0.3605
	0.0004

	Base
	3
	24
	Serv9
	Combination
	Min
	
	
	0.2425
	2.5805
	5.3639
	-3.3952
	0.3171
	-0.0033

	Base
	3
	24
	Serv10
	Combination
	Max
	
	
	0.2789
	2.5961
	5.4927
	-3.3276
	0.3839
	0.0016

	Base
	3
	24
	Serv10
	Combination
	Min
	
	
	0.23
	2.5688
	5.3279
	-3.4461
	0.2938
	-0.0045

	Base
	3
	24
	ENVSERV
	Combination
	Max
	
	
	0.4486
	4.3177
	9.0996
	-3.3276
	0.6097
	0.0016

	Base
	3
	24
	ENVSERV
	Combination
	Min
	
	
	0.23
	2.5688
	5.3279
	-5.7039
	0.2938
	-0.0054

	Base
	4
	26
	Dead
	LinStatic
	
	
	
	-0.3483
	0.9837
	5.0176
	-1.2573
	-0.4539
	-0.0011

	Base
	4
	26
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	4
	26
	FHEx
	LinStatic
	
	
	
	-0.0661
	-0.0215
	-0.1966
	0.0781
	-0.1315
	0.0005

	Base
	4
	26
	FHEy
	LinStatic
	
	
	
	0.1049
	-0.3048
	0.221
	1.179
	0.2147
	-0.0484

	Base
	4
	26
	Sx
	LinRespSpec
	Max
	
	
	0.0422
	0.0381
	0.125
	0.1453
	0.0867
	0.0125

	Base
	4
	26
	Sy
	LinRespSpec
	Max
	
	
	0.1123
	0.2878
	0.2342
	1.109
	0.2285
	0.0503

	Base
	4
	26
	Comb1
	Combination
	
	
	
	-0.4876
	1.3771
	7.0246
	-1.7602
	-0.6354
	-0.0015

	Base
	4
	26
	Comb2
	Combination
	
	
	
	-0.4179
	1.1804
	6.0211
	-1.5088
	-0.5446
	-0.0013

	Base
	4
	26
	Comb3
	Combination
	
	
	
	-0.4179
	1.1804
	6.0211
	-1.5088
	-0.5446
	-0.0013

	Base
	4
	26
	Comb4
	Combination
	Max
	
	
	-0.4119
	1.1858
	6.0389
	-1.488
	-0.5323
	0.0005

	Base
	4
	26
	Comb4
	Combination
	Min
	
	
	-0.424
	1.1749
	6.0032
	-1.5295
	-0.557
	-0.0031

	Base
	4
	26
	Comb5
	Combination
	Max
	
	
	-0.4019
	1.2215
	6.0545
	-1.3503
	-0.512
	0.0059

	Base
	4
	26
	Comb5
	Combination
	Min
	
	
	-0.434
	1.1393
	5.9876
	-1.6673
	-0.5773
	-0.0085

	Base
	4
	26
	Comb6
	Combination
	
	
	
	-0.3134
	0.8853
	4.5158
	-1.1316
	-0.4085
	-0.001

	Base
	4
	26
	Comb7
	Combination
	Max
	
	
	-0.3074
	0.8907
	4.5337
	-1.1108
	-0.3961
	0.0008

	Base
	4
	26
	Comb7
	Combination
	Min
	
	
	-0.3195
	0.8799
	4.4979
	-1.1523
	-0.4209
	-0.0028

	Base
	4
	26
	Comb8
	Combination
	Max
	
	
	-0.2974
	0.9264
	4.5493
	-0.9731
	-0.3758
	0.0062

	Base
	4
	26
	Comb8
	Combination
	Min
	
	
	-0.3295
	0.8442
	4.4823
	-1.2901
	-0.4411
	-0.0082

	Base
	4
	26
	ENVDIS
	Combination
	Max
	
	
	-0.2974
	1.3771
	7.0246
	-0.9731
	-0.3758
	0.0062

	Base
	4
	26
	ENVDIS
	Combination
	Min
	
	
	-0.4876
	0.8442
	4.4823
	-1.7602
	-0.6354
	-0.0085

	Base
	4
	26
	Serv1
	Combination
	
	
	
	-0.3483
	0.9837
	5.0176
	-1.2573
	-0.4539
	-0.0011

	Base
	4
	26
	Serv2
	Combination
	
	
	
	-0.3483
	0.9837
	5.0176
	-1.2573
	-0.4539
	-0.0011

	Base
	4
	26
	Serv3
	Combination
	
	
	
	-0.3483
	0.9837
	5.0176
	-1.2573
	-0.4539
	-0.0011

	Base
	4
	26
	Serv4
	Combination
	Max
	
	
	-0.3441
	0.9875
	5.0301
	-1.2428
	-0.4452
	0.0002

	Base
	4
	26
	Serv4
	Combination
	Min
	
	
	-0.3525
	0.9799
	5.0051
	-1.2719
	-0.4625
	-0.0023

	Base
	4
	26
	Serv5
	Combination
	Max
	
	
	-0.337
	1.0124
	5.041
	-1.1464
	-0.431
	0.004

	Base
	4
	26
	Serv5
	Combination
	Min
	
	
	-0.3595
	0.9549
	4.9941
	-1.3682
	-0.4767
	-0.0061

	Base
	4
	26
	Serv6
	Combination
	Max
	
	
	-0.3451
	0.9865
	5.0269
	-1.2464
	-0.4474
	-0.0001

	Base
	4
	26
	Serv6
	Combination
	Min
	
	
	-0.3514
	0.9808
	5.0082
	-1.2682
	-0.4604
	-0.002

	Base
	4
	26
	Serv7
	Combination
	Max
	
	
	-0.3399
	1.0052
	5.0351
	-1.1741
	-0.4367
	0.0027

	Base
	4
	26
	Serv7
	Combination
	Min
	
	
	-0.3567
	0.9621
	5
	-1.3405
	-0.471
	-0.0049

	Base
	4
	26
	Serv8
	Combination
	
	
	
	-0.209
	0.5902
	3.0105
	-0.7544
	-0.2723
	-0.0006

	Base
	4
	26
	Serv9
	Combination
	Max
	
	
	-0.2047
	0.594
	3.023
	-0.7399
	-0.2636
	0.0006

	Base
	4
	26
	Serv9
	Combination
	Min
	
	
	-0.2132
	0.5864
	2.998
	-0.7689
	-0.281
	-0.0019

	Base
	4
	26
	Serv10
	Combination
	Max
	
	
	-0.1977
	0.619
	3.034
	-0.6435
	-0.2495
	0.0044

	Base
	4
	26
	Serv10
	Combination
	Min
	
	
	-0.2202
	0.5614
	2.9871
	-0.8653
	-0.2952
	-0.0057

	Base
	4
	26
	ENVSERV
	Combination
	Max
	
	
	-0.1977
	1.0124
	5.041
	-0.6435
	-0.2495
	0.0044

	Base
	4
	26
	ENVSERV
	Combination
	Min
	
	
	-0.3595
	0.5614
	2.9871
	-1.3682
	-0.4767
	-0.0061

	Base
	5
	28
	Dead
	LinStatic
	
	
	
	0.2069
	-3.2572
	12.7774
	4.3068
	0.2602
	-0.0026

	Base
	5
	28
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	5
	28
	FHEx
	LinStatic
	
	
	
	-0.2241
	-0.0056
	1.6129
	0.0232
	-0.4032
	-0.0017

	Base
	5
	28
	FHEy
	LinStatic
	
	
	
	-0.3843
	-0.2021
	2.7106
	0.7648
	-0.6961
	-0.0369

	Base
	5
	28
	Sx
	LinRespSpec
	Max
	
	
	0.214
	0.0258
	1.5875
	0.0964
	0.3825
	0.0048

	Base
	5
	28
	Sy
	LinRespSpec
	Max
	
	
	0.4017
	0.1804
	2.7314
	0.6676
	0.7301
	0.0428

	Base
	5
	28
	Comb1
	Combination
	
	
	
	0.2896
	-4.56
	17.8884
	6.0296
	0.3643
	-0.0037

	Base
	5
	28
	Comb2
	Combination
	
	
	
	0.2483
	-3.9086
	15.3329
	5.1682
	0.3123
	-0.0032

	Base
	5
	28
	Comb3
	Combination
	
	
	
	0.2483
	-3.9086
	15.3329
	5.1682
	0.3123
	-0.0032

	Base
	5
	28
	Comb4
	Combination
	Max
	
	
	0.2788
	-3.9049
	15.5597
	5.182
	0.3669
	-0.0025

	Base
	5
	28
	Comb4
	Combination
	Min
	
	
	0.2177
	-3.9123
	15.1062
	5.1544
	0.2576
	-0.0038

	Base
	5
	28
	Comb5
	Combination
	Max
	
	
	0.3057
	-3.8828
	15.7232
	5.2636
	0.4166
	0.003

	Base
	5
	28
	Comb5
	Combination
	Min
	
	
	0.1908
	-3.9344
	14.9426
	5.0728
	0.2079
	-0.0093

	Base
	5
	28
	Comb6
	Combination
	
	
	
	0.1862
	-2.9315
	11.4997
	3.8761
	0.2342
	-0.0024

	Base
	5
	28
	Comb7
	Combination
	Max
	
	
	0.2168
	-2.9278
	11.7265
	3.8899
	0.2889
	-0.0017

	Base
	5
	28
	Comb7
	Combination
	Min
	
	
	0.1556
	-2.9351
	11.2729
	3.8624
	0.1796
	-0.0031

	Base
	5
	28
	Comb8
	Combination
	Max
	
	
	0.2436
	-2.9057
	11.89
	3.9715
	0.3385
	0.0037

	Base
	5
	28
	Comb8
	Combination
	Min
	
	
	0.1288
	-2.9572
	11.1094
	3.7808
	0.1299
	-0.0085

	Base
	5
	28
	ENVDIS
	Combination
	Max
	
	
	0.3057
	-2.9057
	17.8884
	6.0296
	0.4166
	0.0037

	Base
	5
	28
	ENVDIS
	Combination
	Min
	
	
	0.1288
	-4.56
	11.1094
	3.7808
	0.1299
	-0.0093

	Base
	5
	28
	Serv1
	Combination
	
	
	
	0.2069
	-3.2572
	12.7774
	4.3068
	0.2602
	-0.0026

	Base
	5
	28
	Serv2
	Combination
	
	
	
	0.2069
	-3.2572
	12.7774
	4.3068
	0.2602
	-0.0026

	Base
	5
	28
	Serv3
	Combination
	
	
	
	0.2069
	-3.2572
	12.7774
	4.3068
	0.2602
	-0.0026

	Base
	5
	28
	Serv4
	Combination
	Max
	
	
	0.2283
	-3.2546
	12.9362
	4.3165
	0.2985
	-0.0022

	Base
	5
	28
	Serv4
	Combination
	Min
	
	
	0.1855
	-3.2598
	12.6187
	4.2972
	0.222
	-0.0031

	Base
	5
	28
	Serv5
	Combination
	Max
	
	
	0.2471
	-3.2391
	13.0506
	4.3736
	0.3332
	0.0016

	Base
	5
	28
	Serv5
	Combination
	Min
	
	
	0.1667
	-3.2752
	12.5043
	4.2401
	0.1872
	-0.0069

	Base
	5
	28
	Serv6
	Combination
	Max
	
	
	0.2229
	-3.2552
	12.8965
	4.3141
	0.2889
	-0.0023

	Base
	5
	28
	Serv6
	Combination
	Min
	
	
	0.1908
	-3.2591
	12.6584
	4.2996
	0.2315
	-0.003

	Base
	5
	28
	Serv7
	Combination
	Max
	
	
	0.237
	-3.2436
	12.9823
	4.3569
	0.315
	0.0006

	Base
	5
	28
	Serv7
	Combination
	Min
	
	
	0.1767
	-3.2707
	12.5726
	4.2568
	0.2055
	-0.0058

	Base
	5
	28
	Serv8
	Combination
	
	
	
	0.1241
	-1.9543
	7.6665
	2.5841
	0.1561
	-0.0016

	Base
	5
	28
	Serv9
	Combination
	Max
	
	
	0.1455
	-1.9517
	7.8252
	2.5937
	0.1944
	-0.0011

	Base
	5
	28
	Serv9
	Combination
	Min
	
	
	0.1027
	-1.9569
	7.5077
	2.5745
	0.1179
	-0.0021

	Base
	5
	28
	Serv10
	Combination
	Max
	
	
	0.1643
	-1.9363
	7.9396
	2.6509
	0.2292
	0.0027

	Base
	5
	28
	Serv10
	Combination
	Min
	
	
	0.084
	-1.9723
	7.3933
	2.5173
	0.0831
	-0.0059

	Base
	5
	28
	ENVSERV
	Combination
	Max
	
	
	0.2471
	-1.9363
	13.0506
	4.3736
	0.3332
	0.0027

	Base
	5
	28
	ENVSERV
	Combination
	Min
	
	
	0.084
	-3.2752
	7.3933
	2.5173
	0.0831
	-0.0069

	Base
	13
	30
	Dead
	LinStatic
	
	
	
	-0.2481
	-0.7991
	6.4924
	1.0887
	-0.3381
	-0.0023

	Base
	13
	30
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	13
	30
	FHEx
	LinStatic
	
	
	
	-0.1905
	-0.0125
	-1.2592
	0.0535
	-0.3525
	-0.0011

	Base
	13
	30
	FHEy
	LinStatic
	
	
	
	-0.2908
	-0.3102
	-1.7509
	1.1885
	-0.5452
	-0.0268

	Base
	13
	30
	Sx
	LinRespSpec
	Max
	
	
	0.168
	0.0359
	1.1479
	0.136
	0.3109
	0.0036

	Base
	13
	30
	Sy
	LinRespSpec
	Max
	
	
	0.3229
	0.2941
	1.9366
	1.1216
	0.6037
	0.0297

	Base
	13
	30
	Comb1
	Combination
	
	
	
	-0.3474
	-1.1187
	9.0893
	1.5241
	-0.4733
	-0.0032

	Base
	13
	30
	Comb2
	Combination
	
	
	
	-0.2978
	-0.9589
	7.7909
	1.3064
	-0.4057
	-0.0027

	Base
	13
	30
	Comb3
	Combination
	
	
	
	-0.2978
	-0.9589
	7.7909
	1.3064
	-0.4057
	-0.0027

	Base
	13
	30
	Comb4
	Combination
	Max
	
	
	-0.2738
	-0.9538
	7.9548
	1.3258
	-0.3613
	-0.0022

	Base
	13
	30
	Comb4
	Combination
	Min
	
	
	-0.3218
	-0.964
	7.6269
	1.287
	-0.4501
	-0.0032

	Base
	13
	30
	Comb5
	Combination
	Max
	
	
	-0.2516
	-0.9168
	8.0676
	1.4667
	-0.3195
	0.0015

	Base
	13
	30
	Comb5
	Combination
	Min
	
	
	-0.3439
	-1.0009
	7.5141
	1.1461
	-0.492
	-0.007

	Base
	13
	30
	Comb6
	Combination
	
	
	
	-0.2233
	-0.7192
	5.8431
	0.9798
	-0.3043
	-0.002

	Base
	13
	30
	Comb7
	Combination
	Max
	
	
	-0.1993
	-0.714
	6.0071
	0.9992
	-0.2599
	-0.0015

	Base
	13
	30
	Comb7
	Combination
	Min
	
	
	-0.2473
	-0.7243
	5.6792
	0.9604
	-0.3487
	-0.0026

	Base
	13
	30
	Comb8
	Combination
	Max
	
	
	-0.1772
	-0.6771
	6.1199
	1.1401
	-0.218
	0.0022

	Base
	13
	30
	Comb8
	Combination
	Min
	
	
	-0.2695
	-0.7612
	5.5664
	0.8195
	-0.3906
	-0.0063

	Base
	13
	30
	ENVDIS
	Combination
	Max
	
	
	-0.1772
	-0.6771
	9.0893
	1.5241
	-0.218
	0.0022

	Base
	13
	30
	ENVDIS
	Combination
	Min
	
	
	-0.3474
	-1.1187
	5.5664
	0.8195
	-0.492
	-0.007

	Base
	13
	30
	Serv1
	Combination
	
	
	
	-0.2481
	-0.7991
	6.4924
	1.0887
	-0.3381
	-0.0023

	Base
	13
	30
	Serv2
	Combination
	
	
	
	-0.2481
	-0.7991
	6.4924
	1.0887
	-0.3381
	-0.0023

	Base
	13
	30
	Serv3
	Combination
	
	
	
	-0.2481
	-0.7991
	6.4924
	1.0887
	-0.3381
	-0.0023

	Base
	13
	30
	Serv4
	Combination
	Max
	
	
	-0.2313
	-0.7955
	6.6072
	1.1023
	-0.307
	-0.0019

	Base
	13
	30
	Serv4
	Combination
	Min
	
	
	-0.2649
	-0.8027
	6.3776
	1.0751
	-0.3692
	-0.0026

	Base
	13
	30
	Serv5
	Combination
	Max
	
	
	-0.2158
	-0.7697
	6.686
	1.2008
	-0.2777
	0.0007

	Base
	13
	30
	Serv5
	Combination
	Min
	
	
	-0.2804
	-0.8285
	6.2987
	0.9765
	-0.3985
	-0.0052

	Base
	13
	30
	Serv6
	Combination
	Max
	
	
	-0.2355
	-0.7964
	6.5785
	1.0989
	-0.3148
	-0.002

	Base
	13
	30
	Serv6
	Combination
	Min
	
	
	-0.2607
	-0.8018
	6.4063
	1.0785
	-0.3614
	-0.0025

	Base
	13
	30
	Serv7
	Combination
	Max
	
	
	-0.2239
	-0.777
	6.6376
	1.1728
	-0.2928
	-3.566E-05

	Base
	13
	30
	Serv7
	Combination
	Min
	
	
	-0.2723
	-0.8211
	6.3471
	1.0045
	-0.3834
	-0.0045

	Base
	13
	30
	Serv8
	Combination
	
	
	
	-0.1489
	-0.4794
	3.8954
	0.6532
	-0.2029
	-0.0014

	Base
	13
	30
	Serv9
	Combination
	Max
	
	
	-0.1321
	-0.4759
	4.0102
	0.6668
	-0.1718
	-0.001

	Base
	13
	30
	Serv9
	Combination
	Min
	
	
	-0.1657
	-0.483
	3.7806
	0.6396
	-0.2339
	-0.0017

	Base
	13
	30
	Serv10
	Combination
	Max
	
	
	-0.1166
	-0.45
	4.0891
	0.7654
	-0.1425
	0.0016

	Base
	13
	30
	Serv10
	Combination
	Min
	
	
	-0.1812
	-0.5089
	3.7018
	0.541
	-0.2632
	-0.0043

	Base
	13
	30
	ENVSERV
	Combination
	Max
	
	
	-0.1166
	-0.45
	6.686
	1.2008
	-0.1425
	0.0016

	Base
	13
	30
	ENVSERV
	Combination
	Min
	
	
	-0.2804
	-0.8285
	3.7018
	0.541
	-0.3985
	-0.0052

	Base
	16
	32
	Dead
	LinStatic
	
	
	
	-0.0001
	-0.0013
	0.3589
	0.005
	-0.0006
	0.0001

	Base
	16
	32
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	16
	32
	FHEx
	LinStatic
	
	
	
	-0.002
	-0.002
	6.344E-07
	0.0081
	-0.0082
	0.0016

	Base
	16
	32
	FHEy
	LinStatic
	
	
	
	-0.001
	-0.0266
	7.6E-06
	0.1062
	-0.004
	0.0008

	Base
	16
	32
	Sx
	LinRespSpec
	Max
	
	
	0.0028
	0.003
	8.554E-07
	0.012
	0.0113
	0.0019

	Base
	16
	32
	Sy
	LinRespSpec
	Max
	
	
	0.0014
	0.0255
	7.505E-06
	0.1019
	0.0055
	0.0013

	Base
	16
	32
	Comb1
	Combination
	
	
	
	-0.0002
	-0.0018
	0.5025
	0.007
	-0.0008
	0.0001

	Base
	16
	32
	Comb2
	Combination
	
	
	
	-0.0002
	-0.0015
	0.4307
	0.006
	-0.0007
	0.0001

	Base
	16
	32
	Comb3
	Combination
	
	
	
	-0.0002
	-0.0015
	0.4307
	0.006
	-0.0007
	0.0001

	Base
	16
	32
	Comb4
	Combination
	Max
	
	
	0.0002
	-0.0011
	0.4307
	0.0077
	0.0009
	0.0003

	Base
	16
	32
	Comb4
	Combination
	Min
	
	
	-0.0006
	-0.0019
	0.4307
	0.0043
	-0.0023
	-0.0002

	Base
	16
	32
	Comb5
	Combination
	Max
	
	
	1.713E-05
	0.0021
	0.4307
	0.0206
	0.0001
	0.0002

	Base
	16
	32
	Comb5
	Combination
	Min
	
	
	-0.0004
	-0.0051
	0.4307
	-0.0086
	-0.0015
	-0.0001

	Base
	16
	32
	Comb6
	Combination
	
	
	
	-0.0001
	-0.0011
	0.3231
	0.0045
	-0.0005
	4.796E-05

	Base
	16
	32
	Comb7
	Combination
	Max
	
	
	0.0003
	-0.0007
	0.3231
	0.0062
	0.0011
	0.0003

	Base
	16
	32
	Comb7
	Combination
	Min
	
	
	-0.0005
	-0.0016
	0.3231
	0.0028
	-0.0021
	-0.0002

	Base
	16
	32
	Comb8
	Combination
	Max
	
	
	0.0001
	0.0025
	0.3231
	0.0191
	0.0002
	0.0002

	Base
	16
	32
	Comb8
	Combination
	Min
	
	
	-0.0003
	-0.0048
	0.3231
	-0.0101
	-0.0013
	-0.0001

	Base
	16
	32
	ENVDIS
	Combination
	Max
	
	
	0.0003
	0.0025
	0.5025
	0.0206
	0.0011
	0.0003

	Base
	16
	32
	ENVDIS
	Combination
	Min
	
	
	-0.0006
	-0.0051
	0.3231
	-0.0101
	-0.0023
	-0.0002

	Base
	16
	32
	Serv1
	Combination
	
	
	
	-0.0001
	-0.0013
	0.3589
	0.005
	-0.0006
	0.0001

	Base
	16
	32
	Serv2
	Combination
	
	
	
	-0.0001
	-0.0013
	0.3589
	0.005
	-0.0006
	0.0001

	Base
	16
	32
	Serv3
	Combination
	
	
	
	-0.0001
	-0.0013
	0.3589
	0.005
	-0.0006
	0.0001

	Base
	16
	32
	Serv4
	Combination
	Max
	
	
	0.0001
	-0.001
	0.3589
	0.0062
	0.0005
	0.0002

	Base
	16
	32
	Serv4
	Combination
	Min
	
	
	-0.0004
	-0.0016
	0.3589
	0.0038
	-0.0017
	-0.0001

	Base
	16
	32
	Serv5
	Combination
	Max
	
	
	-1.187E-05
	0.0013
	0.3589
	0.0152
	-4.764E-05
	0.0002

	Base
	16
	32
	Serv5
	Combination
	Min
	
	
	-0.0003
	-0.0038
	0.3589
	-0.0052
	-0.0011
	-0.0001

	Base
	16
	32
	Serv6
	Combination
	Max
	
	
	0.0001
	-0.001
	0.3589
	0.0059
	0.0002
	0.0002

	Base
	16
	32
	Serv6
	Combination
	Min
	
	
	-0.0004
	-0.0015
	0.3589
	0.0041
	-0.0014
	-0.0001

	Base
	16
	32
	Serv7
	Combination
	Max
	
	
	-4.612E-05
	0.0007
	0.3589
	0.0126
	-0.0002
	0.0001

	Base
	16
	32
	Serv7
	Combination
	Min
	
	
	-0.0003
	-0.0032
	0.3589
	-0.0027
	-0.001
	-4.141E-05

	Base
	16
	32
	Serv8
	Combination
	
	
	
	-0.0001
	-0.0008
	0.2154
	0.003
	-0.0004
	3.197E-05

	Base
	16
	32
	Serv9
	Combination
	Max
	
	
	0.0002
	-0.0005
	0.2154
	0.0042
	0.0008
	0.0002

	Base
	16
	32
	Serv9
	Combination
	Min
	
	
	-0.0004
	-0.0011
	0.2154
	0.0018
	-0.0015
	-0.0002

	Base
	16
	32
	Serv10
	Combination
	Max
	
	
	4.768E-05
	0.0018
	0.2154
	0.0132
	0.0002
	0.0002

	Base
	16
	32
	Serv10
	Combination
	Min
	
	
	-0.0002
	-0.0033
	0.2154
	-0.0072
	-0.0009
	-0.0001

	Base
	16
	32
	ENVSERV
	Combination
	Max
	
	
	0.0002
	0.0018
	0.3589
	0.0152
	0.0008
	0.0002

	Base
	16
	32
	ENVSERV
	Combination
	Min
	
	
	-0.0004
	-0.0038
	0.2154
	-0.0072
	-0.0017
	-0.0002

	Base
	19
	34
	Dead
	LinStatic
	
	
	
	-0.0001
	-0.0004
	0.3584
	0.0015
	-0.0003
	-0.0001

	Base
	19
	34
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	19
	34
	FHEx
	LinStatic
	
	
	
	-0.0022
	0.0001
	0
	-0.0004
	-0.0086
	0.0004

	Base
	19
	34
	FHEy
	LinStatic
	
	
	
	-0.0001
	-0.1357
	0
	0.5427
	-0.0005
	-0.0008

	Base
	19
	34
	Sx
	LinRespSpec
	Max
	
	
	0.0029
	0.0001
	0
	0.0006
	0.0115
	0.0006

	Base
	19
	34
	Sy
	LinRespSpec
	Max
	
	
	0.0005
	0.1376
	0
	0.5505
	0.0021
	0.0007

	Base
	19
	34
	Comb1
	Combination
	
	
	
	-0.0001
	-0.0005
	0.5017
	0.0021
	-0.0004
	-0.0001

	Base
	19
	34
	Comb2
	Combination
	
	
	
	-0.0001
	-0.0004
	0.4301
	0.0018
	-0.0004
	-0.0001

	Base
	19
	34
	Comb3
	Combination
	
	
	
	-0.0001
	-0.0004
	0.4301
	0.0018
	-0.0004
	-0.0001

	Base
	19
	34
	Comb4
	Combination
	Max
	
	
	0.0003
	-0.0004
	0.4301
	0.0019
	0.0013
	-8.776E-06

	Base
	19
	34
	Comb4
	Combination
	Min
	
	
	-0.0005
	-0.0005
	0.4301
	0.0017
	-0.002
	-0.0002

	Base
	19
	34
	Comb5
	Combination
	Max
	
	
	-1.392E-05
	0.0192
	0.4301
	0.0804
	-0.0001
	6.79E-06

	Base
	19
	34
	Comb5
	Combination
	Min
	
	
	-0.0002
	-0.0201
	0.4301
	-0.0769
	-0.0007
	-0.0002

	Base
	19
	34
	Comb6
	Combination
	
	
	
	-0.0001
	-0.0003
	0.3225
	0.0013
	-0.0003
	-0.0001

	Base
	19
	34
	Comb7
	Combination
	Max
	
	
	0.0003
	-0.0003
	0.3225
	0.0014
	0.0014
	1.544E-05

	Base
	19
	34
	Comb7
	Combination
	Min
	
	
	-0.0005
	-0.0004
	0.3225
	0.0012
	-0.0019
	-0.0002

	Base
	19
	34
	Comb8
	Combination
	Max
	
	
	8.484E-06
	0.0193
	0.3225
	0.08
	3.395E-05
	3.101E-05

	Base
	19
	34
	Comb8
	Combination
	Min
	
	
	-0.0001
	-0.02
	0.3225
	-0.0773
	-0.0006
	-0.0002

	Base
	19
	34
	ENVDIS
	Combination
	Max
	
	
	0.0003
	0.0193
	0.5017
	0.0804
	0.0014
	3.101E-05

	Base
	19
	34
	ENVDIS
	Combination
	Min
	
	
	-0.0005
	-0.0201
	0.3225
	-0.0773
	-0.002
	-0.0002

	Base
	19
	34
	Serv1
	Combination
	
	
	
	-0.0001
	-0.0004
	0.3584
	0.0015
	-0.0003
	-0.0001

	Base
	19
	34
	Serv2
	Combination
	
	
	
	-0.0001
	-0.0004
	0.3584
	0.0015
	-0.0003
	-0.0001

	Base
	19
	34
	Serv3
	Combination
	
	
	
	-0.0001
	-0.0004
	0.3584
	0.0015
	-0.0003
	-0.0001

	Base
	19
	34
	Serv4
	Combination
	Max
	
	
	0.0002
	-0.0004
	0.3584
	0.0015
	0.0009
	-1.906E-05

	Base
	19
	34
	Serv4
	Combination
	Min
	
	
	-0.0004
	-0.0004
	0.3584
	0.0014
	-0.0015
	-0.0001

	Base
	19
	34
	Serv5
	Combination
	Max
	
	
	-2.17E-05
	0.0134
	0.3584
	0.0565
	-0.0001
	-8.184E-06

	Base
	19
	34
	Serv5
	Combination
	Min
	
	
	-0.0001
	-0.0141
	0.3584
	-0.0536
	-0.0005
	-0.0002

	Base
	19
	34
	Serv6
	Combination
	Max
	
	
	0.0001
	-0.0004
	0.3584
	0.0015
	0.0006
	-3.447E-05

	Base
	19
	34
	Serv6
	Combination
	Min
	
	
	-0.0003
	-0.0004
	0.3584
	0.0014
	-0.0012
	-0.0001

	Base
	19
	34
	Serv7
	Combination
	Max
	
	
	-3.494E-05
	0.01
	0.3584
	0.0428
	-0.0001
	-2.632E-05

	Base
	19
	34
	Serv7
	Combination
	Min
	
	
	-0.0001
	-0.0107
	0.3584
	-0.0398
	-0.0005
	-0.0001

	Base
	19
	34
	Serv8
	Combination
	
	
	
	-4.48E-05
	-0.0002
	0.215
	0.0009
	-0.0002
	-4.843E-05

	Base
	19
	34
	Serv9
	Combination
	Max
	
	
	0.0002
	-0.0002
	0.215
	0.0009
	0.001
	1.323E-05

	Base
	19
	34
	Serv9
	Combination
	Min
	
	
	-0.0003
	-0.0002
	0.215
	0.0008
	-0.0013
	-0.0001

	Base
	19
	34
	Serv10
	Combination
	Max
	
	
	8.163E-06
	0.0135
	0.215
	0.0559
	3.266E-05
	2.41E-05

	Base
	19
	34
	Serv10
	Combination
	Min
	
	
	-0.0001
	-0.014
	0.215
	-0.0542
	-0.0004
	-0.0001

	Base
	19
	34
	ENVSERV
	Combination
	Max
	
	
	0.0002
	0.0135
	0.3584
	0.0565
	0.001
	2.41E-05

	Base
	19
	34
	ENVSERV
	Combination
	Min
	
	
	-0.0004
	-0.0141
	0.215
	-0.0542
	-0.0015
	-0.0002

	Base
	21
	36
	Dead
	LinStatic
	
	
	
	-0.0001
	-0.0039
	0.4988
	0.01
	-0.0002
	-0.0003

	Base
	21
	36
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	21
	36
	FHEx
	LinStatic
	
	
	
	-0.002
	0.0008
	-0.0002
	-0.0033
	-0.0081
	-0.0002

	Base
	21
	36
	FHEy
	LinStatic
	
	
	
	0.0008
	-0.0294
	0.0047
	0.1173
	0.0031
	-0.0021

	Base
	21
	36
	Sx
	LinRespSpec
	Max
	
	
	0.0028
	0.0015
	0.0003
	0.0062
	0.011
	0.0004

	Base
	21
	36
	Sy
	LinRespSpec
	Max
	
	
	0.0009
	0.0295
	0.0047
	0.1178
	0.0035
	0.0025

	Base
	21
	36
	Comb1
	Combination
	
	
	
	-0.0002
	-0.0055
	0.6984
	0.0139
	-0.0002
	-0.0004

	Base
	21
	36
	Comb2
	Combination
	
	
	
	-0.0002
	-0.0047
	0.5986
	0.012
	-0.0002
	-0.0003

	Base
	21
	36
	Comb3
	Combination
	
	
	
	-0.0002
	-0.0047
	0.5986
	0.012
	-0.0002
	-0.0003

	Base
	21
	36
	Comb4
	Combination
	Max
	
	
	0.0002
	-0.0045
	0.5986
	0.0128
	0.0014
	-0.0002

	Base
	21
	36
	Comb4
	Combination
	Min
	
	
	-0.0005
	-0.0049
	0.5986
	0.0111
	-0.0018
	-0.0004

	Base
	21
	36
	Comb5
	Combination
	Max
	
	
	-2.625E-05
	-0.0005
	0.5993
	0.0288
	0.0003
	4.665E-05

	Base
	21
	36
	Comb5
	Combination
	Min
	
	
	-0.0003
	-0.0089
	0.5979
	-0.0049
	-0.0007
	-0.0007

	Base
	21
	36
	Comb6
	Combination
	
	
	
	-0.0001
	-0.0035
	0.4489
	0.009
	-0.0002
	-0.0002

	Base
	21
	36
	Comb7
	Combination
	Max
	
	
	0.0003
	-0.0033
	0.449
	0.0098
	0.0014
	-0.0002

	Base
	21
	36
	Comb7
	Combination
	Min
	
	
	-0.0005
	-0.0038
	0.4489
	0.0081
	-0.0017
	-0.0003

	Base
	21
	36
	Comb8
	Combination
	Max
	
	
	1.164E-05
	0.0007
	0.4496
	0.0258
	0.0004
	0.0001

	Base
	21
	36
	Comb8
	Combination
	Min
	
	
	-0.0002
	-0.0078
	0.4483
	-0.0079
	-0.0007
	-0.0006

	Base
	21
	36
	ENVDIS
	Combination
	Max
	
	
	0.0003
	0.0007
	0.6984
	0.0288
	0.0014
	0.0001

	Base
	21
	36
	ENVDIS
	Combination
	Min
	
	
	-0.0005
	-0.0089
	0.4483
	-0.0079
	-0.0018
	-0.0007

	Base
	21
	36
	Serv1
	Combination
	
	
	
	-0.0001
	-0.0039
	0.4988
	0.01
	-0.0002
	-0.0003

	Base
	21
	36
	Serv2
	Combination
	
	
	
	-0.0001
	-0.0039
	0.4988
	0.01
	-0.0002
	-0.0003

	Base
	21
	36
	Serv3
	Combination
	
	
	
	-0.0001
	-0.0039
	0.4988
	0.01
	-0.0002
	-0.0003

	Base
	21
	36
	Serv4
	Combination
	Max
	
	
	0.0001
	-0.0038
	0.4989
	0.0106
	0.0009
	-0.0002

	Base
	21
	36
	Serv4
	Combination
	Min
	
	
	-0.0004
	-0.0041
	0.4988
	0.0093
	-0.0013
	-0.0003

	Base
	21
	36
	Serv5
	Combination
	Max
	
	
	-3.861E-05
	-0.001
	0.4993
	0.0217
	0.0002
	-8.115E-06

	Base
	21
	36
	Serv5
	Combination
	Min
	
	
	-0.0002
	-0.0069
	0.4984
	-0.0018
	-0.0005
	-0.0005

	Base
	21
	36
	Serv6
	Combination
	Max
	
	
	0.0001
	-0.0038
	0.4988
	0.0104
	0.0007
	-0.0002

	Base
	21
	36
	Serv6
	Combination
	Min
	
	
	-0.0003
	-0.004
	0.4988
	0.0095
	-0.001
	-0.0003

	Base
	21
	36
	Serv7
	Combination
	Max
	
	
	-0.0001
	-0.0017
	0.4992
	0.0188
	0.0001
	-0.0001

	Base
	21
	36
	Serv7
	Combination
	Min
	
	
	-0.0002
	-0.0061
	0.4985
	0.0011
	-0.0004
	-0.0004

	Base
	21
	36
	Serv8
	Combination
	
	
	
	-0.0001
	-0.0024
	0.2993
	0.006
	-0.0001
	-0.0002

	Base
	21
	36
	Serv9
	Combination
	Max
	
	
	0.0002
	-0.0022
	0.2993
	0.0066
	0.001
	-0.0001

	Base
	21
	36
	Serv9
	Combination
	Min
	
	
	-0.0004
	-0.0025
	0.2993
	0.0054
	-0.0012
	-0.0002

	Base
	21
	36
	Serv10
	Combination
	Max
	
	
	1.191E-05
	0.0006
	0.2998
	0.0178
	0.0002
	0.0001

	Base
	21
	36
	Serv10
	Combination
	Min
	
	
	-0.0002
	-0.0053
	0.2988
	-0.0058
	-0.0005
	-0.0004

	Base
	21
	36
	ENVSERV
	Combination
	Max
	
	
	0.0002
	0.0006
	0.4993
	0.0217
	0.001
	0.0001

	Base
	21
	36
	ENVSERV
	Combination
	Min
	
	
	-0.0004
	-0.0069
	0.2988
	-0.0058
	-0.0013
	-0.0005

	Base
	22
	38
	Dead
	LinStatic
	
	
	
	-0.4293
	-0.5434
	32.8004
	2.2564
	-0.7971
	-0.0054

	Base
	22
	38
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	22
	38
	FHEx
	LinStatic
	
	
	
	-2.2622
	-0.437
	1.3033
	1.7398
	-5.3752
	0.4011

	Base
	22
	38
	FHEy
	LinStatic
	
	
	
	-2.4908
	-10.6553
	1.7624
	42.481
	-5.7899
	-0.401

	Base
	22
	38
	Sx
	LinRespSpec
	Max
	
	
	2.1861
	0.8811
	1.1679
	3.5107
	5.2375
	0.6512

	Base
	22
	38
	Sy
	LinRespSpec
	Max
	
	
	2.8784
	10.4927
	1.9889
	41.8324
	6.7141
	0.5384

	Base
	22
	38
	Comb1
	Combination
	
	
	
	-0.601
	-0.7607
	45.9206
	3.1589
	-1.1159
	-0.0076

	Base
	22
	38
	Comb2
	Combination
	
	
	
	-0.5152
	-0.652
	39.3605
	2.7077
	-0.9565
	-0.0065

	Base
	22
	38
	Comb3
	Combination
	
	
	
	-0.5152
	-0.652
	39.3605
	2.7077
	-0.9565
	-0.0065

	Base
	22
	38
	Comb4
	Combination
	Max
	
	
	-0.2029
	-0.5261
	39.5274
	3.2092
	-0.2083
	0.0865

	Base
	22
	38
	Comb4
	Combination
	Min
	
	
	-0.8275
	-0.7779
	39.1937
	2.2061
	-1.7047
	-0.0995

	Base
	22
	38
	Comb5
	Combination
	Max
	
	
	-0.1038
	0.8474
	39.6447
	8.6855
	0.003
	0.0704

	Base
	22
	38
	Comb5
	Combination
	Min
	
	
	-0.9265
	-2.1514
	39.0763
	-3.2702
	-1.9159
	-0.0834

	Base
	22
	38
	Comb6
	Combination
	
	
	
	-0.3864
	-0.489
	29.5204
	2.0307
	-0.7174
	-0.0049

	Base
	22
	38
	Comb7
	Combination
	Max
	
	
	-0.0741
	-0.3631
	29.6872
	2.5323
	0.0309
	0.0882

	Base
	22
	38
	Comb7
	Combination
	Min
	
	
	-0.6987
	-0.6149
	29.3535
	1.5292
	-1.4656
	-0.0979

	Base
	22
	38
	Comb8
	Combination
	Max
	
	
	0.0249
	1.0104
	29.8046
	8.0086
	0.2421
	0.0721

	Base
	22
	38
	Comb8
	Combination
	Min
	
	
	-0.7977
	-1.9884
	29.2362
	-3.9471
	-1.6768
	-0.0818

	Base
	22
	38
	ENVDIS
	Combination
	Max
	
	
	0.0249
	1.0104
	45.9206
	8.6855
	0.2421
	0.0882

	Base
	22
	38
	ENVDIS
	Combination
	Min
	
	
	-0.9265
	-2.1514
	29.2362
	-3.9471
	-1.9159
	-0.0995

	Base
	22
	38
	Serv1
	Combination
	
	
	
	-0.4293
	-0.5434
	32.8004
	2.2564
	-0.7971
	-0.0054

	Base
	22
	38
	Serv2
	Combination
	
	
	
	-0.4293
	-0.5434
	32.8004
	2.2564
	-0.7971
	-0.0054

	Base
	22
	38
	Serv3
	Combination
	
	
	
	-0.4293
	-0.5434
	32.8004
	2.2564
	-0.7971
	-0.0054

	Base
	22
	38
	Serv4
	Combination
	Max
	
	
	-0.2107
	-0.4552
	32.9172
	2.6075
	-0.2733
	0.0597

	Base
	22
	38
	Serv4
	Combination
	Min
	
	
	-0.6479
	-0.6315
	32.6836
	1.9053
	-1.3208
	-0.0705

	Base
	22
	38
	Serv5
	Combination
	Max
	
	
	-0.1415
	0.5059
	32.9993
	6.4396
	-0.1257
	0.0484

	Base
	22
	38
	Serv5
	Combination
	Min
	
	
	-0.7171
	-1.5926
	32.6015
	-1.9269
	-1.4685
	-0.0593

	Base
	22
	38
	Serv6
	Combination
	Max
	
	
	-0.2653
	-0.4773
	32.888
	2.5197
	-0.4043
	0.0434

	Base
	22
	38
	Serv6
	Combination
	Min
	
	
	-0.5933
	-0.6094
	32.7128
	1.9931
	-1.1899
	-0.0543

	Base
	22
	38
	Serv7
	Combination
	Max
	
	
	-0.2134
	0.2436
	32.9496
	5.3938
	-0.2935
	0.035

	Base
	22
	38
	Serv7
	Combination
	Min
	
	
	-0.6452
	-1.3303
	32.6513
	-0.8811
	-1.3006
	-0.0458

	Base
	22
	38
	Serv8
	Combination
	
	
	
	-0.2576
	-0.326
	19.6803
	1.3538
	-0.4782
	-0.0032

	Base
	22
	38
	Serv9
	Combination
	Max
	
	
	-0.039
	-0.2379
	19.797
	1.7049
	0.0455
	0.0619

	Base
	22
	38
	Serv9
	Combination
	Min
	
	
	-0.4762
	-0.4141
	19.5635
	1.0028
	-1.002
	-0.0684

	Base
	22
	38
	Serv10
	Combination
	Max
	
	
	0.0303
	0.7233
	19.8791
	5.5371
	0.1932
	0.0506

	Base
	22
	38
	Serv10
	Combination
	Min
	
	
	-0.5454
	-1.3753
	19.4814
	-2.8294
	-1.1497
	-0.0571

	Base
	22
	38
	ENVSERV
	Combination
	Max
	
	
	0.0303
	0.7233
	32.9993
	6.4396
	0.1932
	0.0619

	Base
	22
	38
	ENVSERV
	Combination
	Min
	
	
	-0.7171
	-1.5926
	19.4814
	-2.8294
	-1.4685
	-0.0705

	Base
	25
	40
	Dead
	LinStatic
	
	
	
	0.4952
	-0.7057
	33.6922
	2.6946
	0.8094
	-0.099

	Base
	25
	40
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	25
	40
	FHEx
	LinStatic
	
	
	
	-1.8813
	0.4236
	-0.5264
	-1.6904
	-4.9334
	-0.0895

	Base
	25
	40
	FHEy
	LinStatic
	
	
	
	1.9467
	-10.8363
	0.6549
	43.2704
	5.0125
	-0.0203

	Base
	25
	40
	Sx
	LinRespSpec
	Max
	
	
	1.754
	0.8596
	0.4078
	3.4318
	4.6416
	0.389

	Base
	25
	40
	Sy
	LinRespSpec
	Max
	
	
	2.1473
	10.8771
	0.734
	43.4333
	5.5292
	0.1921

	Base
	25
	40
	Comb1
	Combination
	
	
	
	0.6933
	-0.988
	47.169
	3.7724
	1.1332
	-0.1386

	Base
	25
	40
	Comb2
	Combination
	
	
	
	0.5942
	-0.8468
	40.4306
	3.2335
	0.9713
	-0.1188

	Base
	25
	40
	Comb3
	Combination
	
	
	
	0.5942
	-0.8468
	40.4306
	3.2335
	0.9713
	-0.1188

	Base
	25
	40
	Comb4
	Combination
	Max
	
	
	0.8448
	-0.724
	40.4889
	3.7238
	1.6344
	-0.0632

	Base
	25
	40
	Comb4
	Combination
	Min
	
	
	0.3437
	-0.9696
	40.3723
	2.7433
	0.3082
	-0.1743

	Base
	25
	40
	Comb5
	Combination
	Max
	
	
	0.9011
	0.7075
	40.5355
	9.4401
	1.7614
	-0.0913

	Base
	25
	40
	Comb5
	Combination
	Min
	
	
	0.2874
	-2.4012
	40.3257
	-2.9731
	0.1812
	-0.1462

	Base
	25
	40
	Comb6
	Combination
	
	
	
	0.4457
	-0.6351
	30.323
	2.4251
	0.7285
	-0.0891

	Base
	25
	40
	Comb7
	Combination
	Max
	
	
	0.6962
	-0.5123
	30.3812
	2.9154
	1.3916
	-0.0335

	Base
	25
	40
	Comb7
	Combination
	Min
	
	
	0.1951
	-0.7579
	30.2647
	1.9349
	0.0654
	-0.1447

	Base
	25
	40
	Comb8
	Combination
	Max
	
	
	0.7525
	0.9192
	30.4278
	8.6318
	1.5186
	-0.0616

	Base
	25
	40
	Comb8
	Combination
	Min
	
	
	0.1388
	-2.1895
	30.2181
	-3.7815
	-0.0616
	-0.1165

	Base
	25
	40
	ENVDIS
	Combination
	Max
	
	
	0.9011
	0.9192
	47.169
	9.4401
	1.7614
	-0.0335

	Base
	25
	40
	ENVDIS
	Combination
	Min
	
	
	0.1388
	-2.4012
	30.2181
	-3.7815
	-0.0616
	-0.1743

	Base
	25
	40
	Serv1
	Combination
	
	
	
	0.4952
	-0.7057
	33.6922
	2.6946
	0.8094
	-0.099

	Base
	25
	40
	Serv2
	Combination
	
	
	
	0.4952
	-0.7057
	33.6922
	2.6946
	0.8094
	-0.099

	Base
	25
	40
	Serv3
	Combination
	
	
	
	0.4952
	-0.7057
	33.6922
	2.6946
	0.8094
	-0.099

	Base
	25
	40
	Serv4
	Combination
	Max
	
	
	0.6706
	-0.6197
	33.7329
	3.0378
	1.2736
	-0.0601

	Base
	25
	40
	Serv4
	Combination
	Min
	
	
	0.3198
	-0.7917
	33.6514
	2.3514
	0.3453
	-0.1379

	Base
	25
	40
	Serv5
	Combination
	Max
	
	
	0.7099
	0.382
	33.7656
	7.0379
	1.3623
	-0.0798

	Base
	25
	40
	Serv5
	Combination
	Min
	
	
	0.2805
	-1.7934
	33.6188
	-1.6487
	0.2565
	-0.1182

	Base
	25
	40
	Serv6
	Combination
	Max
	
	
	0.6267
	-0.6412
	33.7227
	2.952
	1.1575
	-0.0698

	Base
	25
	40
	Serv6
	Combination
	Min
	
	
	0.3636
	-0.7702
	33.6616
	2.4372
	0.4613
	-0.1282

	Base
	25
	40
	Serv7
	Combination
	Max
	
	
	0.6562
	0.1101
	33.7472
	5.9521
	1.2241
	-0.0846

	Base
	25
	40
	Serv7
	Combination
	Min
	
	
	0.3341
	-1.5215
	33.6371
	-0.5629
	0.3947
	-0.1134

	Base
	25
	40
	Serv8
	Combination
	
	
	
	0.2971
	-0.4234
	20.2153
	1.6168
	0.4857
	-0.0594

	Base
	25
	40
	Serv9
	Combination
	Max
	
	
	0.4725
	-0.3374
	20.2561
	1.9599
	0.9498
	-0.0205

	Base
	25
	40
	Serv9
	Combination
	Min
	
	
	0.1217
	-0.5094
	20.1745
	1.2736
	0.0215
	-0.0983

	Base
	25
	40
	Serv10
	Combination
	Max
	
	
	0.5118
	0.6643
	20.2887
	5.9601
	1.0386
	-0.0402

	Base
	25
	40
	Serv10
	Combination
	Min
	
	
	0.0824
	-1.5111
	20.1419
	-2.7266
	-0.0673
	-0.0786

	Base
	25
	40
	ENVSERV
	Combination
	Max
	
	
	0.7099
	0.6643
	33.7656
	7.0379
	1.3623
	-0.0205

	Base
	25
	40
	ENVSERV
	Combination
	Min
	
	
	0.0824
	-1.7934
	20.1419
	-2.7266
	-0.0673
	-0.1379

	Base
	27
	42
	Dead
	LinStatic
	
	
	
	0.3026
	-0.1174
	15.4923
	0.4695
	0.3614
	-0.009

	Base
	27
	42
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	27
	42
	FHEx
	LinStatic
	
	
	
	-0.5677
	-0.042
	0.584
	0.1679
	-1.2095
	0.0652

	Base
	27
	42
	FHEy
	LinStatic
	
	
	
	-0.4538
	-2.1594
	0.5955
	8.6376
	-0.972
	-0.0889

	Base
	27
	42
	Sx
	LinRespSpec
	Max
	
	
	0.5865
	0.1292
	0.5807
	0.5169
	1.2472
	0.0917

	Base
	27
	42
	Sy
	LinRespSpec
	Max
	
	
	0.5393
	2.1311
	0.6988
	8.5243
	1.1542
	0.1073

	Base
	27
	42
	Comb1
	Combination
	
	
	
	0.4236
	-0.1643
	21.6892
	0.6572
	0.5059
	-0.0126

	Base
	27
	42
	Comb2
	Combination
	
	
	
	0.3631
	-0.1408
	18.5907
	0.5634
	0.4337
	-0.0108

	Base
	27
	42
	Comb3
	Combination
	
	
	
	0.3631
	-0.1408
	18.5907
	0.5634
	0.4337
	-0.0108

	Base
	27
	42
	Comb4
	Combination
	Max
	
	
	0.4469
	-0.1224
	18.6737
	0.6372
	0.6118
	0.0023

	Base
	27
	42
	Comb4
	Combination
	Min
	
	
	0.2793
	-0.1593
	18.5077
	0.4895
	0.2555
	-0.0239

	Base
	27
	42
	Comb5
	Combination
	Max
	
	
	0.4402
	0.1637
	18.6906
	1.7815
	0.5986
	0.0045

	Base
	27
	42
	Comb5
	Combination
	Min
	
	
	0.286
	-0.4454
	18.4908
	-0.6548
	0.2687
	-0.0261

	Base
	27
	42
	Comb6
	Combination
	
	
	
	0.2723
	-0.1056
	13.943
	0.4225
	0.3253
	-0.0081

	Base
	27
	42
	Comb7
	Combination
	Max
	
	
	0.3561
	-0.0872
	14.026
	0.4964
	0.5034
	0.005

	Base
	27
	42
	Comb7
	Combination
	Min
	
	
	0.1885
	-0.1241
	13.8601
	0.3487
	0.1471
	-0.0212

	Base
	27
	42
	Comb8
	Combination
	Max
	
	
	0.3494
	0.1989
	14.0429
	1.6406
	0.4902
	0.0072

	Base
	27
	42
	Comb8
	Combination
	Min
	
	
	0.1952
	-0.4101
	13.8432
	-0.7956
	0.1603
	-0.0234

	Base
	27
	42
	ENVDIS
	Combination
	Max
	
	
	0.4469
	0.1989
	21.6892
	1.7815
	0.6118
	0.0072

	Base
	27
	42
	ENVDIS
	Combination
	Min
	
	
	0.1885
	-0.4454
	13.8432
	-0.7956
	0.1471
	-0.0261

	Base
	27
	42
	Serv1
	Combination
	
	
	
	0.3026
	-0.1174
	15.4923
	0.4695
	0.3614
	-0.009

	Base
	27
	42
	Serv2
	Combination
	
	
	
	0.3026
	-0.1174
	15.4923
	0.4695
	0.3614
	-0.009

	Base
	27
	42
	Serv3
	Combination
	
	
	
	0.3026
	-0.1174
	15.4923
	0.4695
	0.3614
	-0.009

	Base
	27
	42
	Serv4
	Combination
	Max
	
	
	0.3612
	-0.1044
	15.5503
	0.5212
	0.4861
	0.0002

	Base
	27
	42
	Serv4
	Combination
	Min
	
	
	0.2439
	-0.1303
	15.4342
	0.4178
	0.2367
	-0.0182

	Base
	27
	42
	Serv5
	Combination
	Max
	
	
	0.3565
	0.0958
	15.5621
	1.3219
	0.4768
	0.0017

	Base
	27
	42
	Serv5
	Combination
	Min
	
	
	0.2486
	-0.3305
	15.4224
	-0.383
	0.246
	-0.0197

	Base
	27
	42
	Serv6
	Combination
	Max
	
	
	0.3466
	-0.1077
	15.5358
	0.5082
	0.4549
	-0.0021

	Base
	27
	42
	Serv6
	Combination
	Min
	
	
	0.2586
	-0.127
	15.4487
	0.4307
	0.2679
	-0.0159

	Base
	27
	42
	Serv7
	Combination
	Max
	
	
	0.343
	0.0425
	15.5447
	1.1088
	0.448
	-0.0009

	Base
	27
	42
	Serv7
	Combination
	Min
	
	
	0.2621
	-0.2772
	15.4398
	-0.1699
	0.2748
	-0.017

	Base
	27
	42
	Serv8
	Combination
	
	
	
	0.1815
	-0.0704
	9.2954
	0.2817
	0.2168
	-0.0054

	Base
	27
	42
	Serv9
	Combination
	Max
	
	
	0.2402
	-0.0575
	9.3534
	0.3334
	0.3416
	0.0038

	Base
	27
	42
	Serv9
	Combination
	Min
	
	
	0.1229
	-0.0833
	9.2373
	0.23
	0.0921
	-0.0146

	Base
	27
	42
	Serv10
	Combination
	Max
	
	
	0.2355
	0.1427
	9.3652
	1.1341
	0.3323
	0.0053

	Base
	27
	42
	Serv10
	Combination
	Min
	
	
	0.1276
	-0.2835
	9.2255
	-0.5707
	0.1014
	-0.0161

	Base
	27
	42
	ENVSERV
	Combination
	Max
	
	
	0.3612
	0.1427
	15.5621
	1.3219
	0.4861
	0.0053

	Base
	27
	42
	ENVSERV
	Combination
	Min
	
	
	0.1229
	-0.3305
	9.2255
	-0.5707
	0.0921
	-0.0197

	Base
	29
	44
	Dead
	LinStatic
	
	
	
	-0.0032
	-0.1373
	16.7213
	0.549
	-0.0179
	-0.0098

	Base
	29
	44
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	29
	44
	FHEx
	LinStatic
	
	
	
	-0.3746
	0.0067
	0.0314
	-0.0269
	-0.8807
	-0.0174

	Base
	29
	44
	FHEy
	LinStatic
	
	
	
	-0.0303
	-2.2782
	0.029
	9.1128
	-0.0606
	-0.0345

	Base
	29
	44
	Sx
	LinRespSpec
	Max
	
	
	0.4584
	0.0293
	0.0299
	0.1171
	1.0807
	0.0653

	Base
	29
	44
	Sy
	LinRespSpec
	Max
	
	
	0.0833
	2.2918
	0.0337
	9.1671
	0.1886
	0.0837

	Base
	29
	44
	Comb1
	Combination
	
	
	
	-0.0045
	-0.1922
	23.4098
	0.7686
	-0.025
	-0.0137

	Base
	29
	44
	Comb2
	Combination
	
	
	
	-0.0039
	-0.1647
	20.0655
	0.6588
	-0.0214
	-0.0118

	Base
	29
	44
	Comb3
	Combination
	
	
	
	-0.0039
	-0.1647
	20.0655
	0.6588
	-0.0214
	-0.0118

	Base
	29
	44
	Comb4
	Combination
	Max
	
	
	0.0616
	-0.1605
	20.0698
	0.6755
	0.1329
	-0.0024

	Base
	29
	44
	Comb4
	Combination
	Min
	
	
	-0.0694
	-0.1689
	20.0613
	0.6421
	-0.1758
	-0.0211

	Base
	29
	44
	Comb5
	Combination
	Max
	
	
	0.008
	0.1628
	20.0704
	1.9688
	0.0055
	0.0002

	Base
	29
	44
	Comb5
	Combination
	Min
	
	
	-0.0158
	-0.4922
	20.0607
	-0.6512
	-0.0484
	-0.0237

	Base
	29
	44
	Comb6
	Combination
	
	
	
	-0.0029
	-0.1235
	15.0492
	0.4941
	-0.0161
	-0.0088

	Base
	29
	44
	Comb7
	Combination
	Max
	
	
	0.0626
	-0.1193
	15.0534
	0.5108
	0.1383
	0.0005

	Base
	29
	44
	Comb7
	Combination
	Min
	
	
	-0.0684
	-0.1277
	15.0449
	0.4774
	-0.1705
	-0.0181

	Base
	29
	44
	Comb8
	Combination
	Max
	
	
	0.009
	0.204
	15.054
	1.8041
	0.0109
	0.0031

	Base
	29
	44
	Comb8
	Combination
	Min
	
	
	-0.0148
	-0.451
	15.0443
	-0.8159
	-0.043
	-0.0208

	Base
	29
	44
	ENVDIS
	Combination
	Max
	
	
	0.0626
	0.204
	23.4098
	1.9688
	0.1383
	0.0031

	Base
	29
	44
	ENVDIS
	Combination
	Min
	
	
	-0.0694
	-0.4922
	15.0443
	-0.8159
	-0.1758
	-0.0237

	Base
	29
	44
	Serv1
	Combination
	
	
	
	-0.0032
	-0.1373
	16.7213
	0.549
	-0.0179
	-0.0098

	Base
	29
	44
	Serv2
	Combination
	
	
	
	-0.0032
	-0.1373
	16.7213
	0.549
	-0.0179
	-0.0098

	Base
	29
	44
	Serv3
	Combination
	
	
	
	-0.0032
	-0.1373
	16.7213
	0.549
	-0.0179
	-0.0098

	Base
	29
	44
	Serv4
	Combination
	Max
	
	
	0.0426
	-0.1343
	16.7243
	0.5607
	0.0902
	-0.0033

	Base
	29
	44
	Serv4
	Combination
	Min
	
	
	-0.0491
	-0.1402
	16.7183
	0.5373
	-0.1259
	-0.0163

	Base
	29
	44
	Serv5
	Combination
	Max
	
	
	0.0051
	0.0919
	16.7247
	1.4657
	0.001
	-0.0014

	Base
	29
	44
	Serv5
	Combination
	Min
	
	
	-0.0116
	-0.3664
	16.7179
	-0.3677
	-0.0367
	-0.0182

	Base
	29
	44
	Serv6
	Combination
	Max
	
	
	0.0312
	-0.1351
	16.7235
	0.5578
	0.0632
	-0.0049

	Base
	29
	44
	Serv6
	Combination
	Min
	
	
	-0.0376
	-0.1394
	16.719
	0.5402
	-0.0989
	-0.0147

	Base
	29
	44
	Serv7
	Combination
	Max
	
	
	0.003
	0.0346
	16.7238
	1.2365
	-0.0037
	-0.0035

	Base
	29
	44
	Serv7
	Combination
	Min
	
	
	-0.0095
	-0.3091
	16.7188
	-0.1385
	-0.032
	-0.0161

	Base
	29
	44
	Serv8
	Combination
	
	
	
	-0.0019
	-0.0824
	10.0328
	0.3294
	-0.0107
	-0.0059

	Base
	29
	44
	Serv9
	Combination
	Max
	
	
	0.0439
	-0.0794
	10.0358
	0.3411
	0.0974
	0.0006

	Base
	29
	44
	Serv9
	Combination
	Min
	
	
	-0.0478
	-0.0853
	10.0298
	0.3177
	-0.1188
	-0.0124

	Base
	29
	44
	Serv10
	Combination
	Max
	
	
	0.0064
	0.1468
	10.0361
	1.2461
	0.0081
	0.0025

	Base
	29
	44
	Serv10
	Combination
	Min
	
	
	-0.0103
	-0.3115
	10.0294
	-0.5873
	-0.0296
	-0.0143

	Base
	29
	44
	ENVSERV
	Combination
	Max
	
	
	0.0439
	0.1468
	16.7247
	1.4657
	0.0974
	0.0025

	Base
	29
	44
	ENVSERV
	Combination
	Min
	
	
	-0.0491
	-0.3664
	10.0294
	-0.5873
	-0.1259
	-0.0182

	Base
	31
	46
	Dead
	LinStatic
	
	
	
	-0.1973
	-0.0017
	4.9627
	0.0074
	-0.2459
	5.691E-06

	Base
	31
	46
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	31
	46
	FHEx
	LinStatic
	
	
	
	-0.2941
	0.0009
	-0.4941
	-0.0038
	-0.5856
	2.009E-05

	Base
	31
	46
	FHEy
	LinStatic
	
	
	
	0.2329
	-0.0314
	0.5297
	0.1256
	0.4658
	3.463E-05

	Base
	31
	46
	Sx
	LinRespSpec
	Max
	
	
	0.3183
	0.0018
	0.4731
	0.0071
	0.6364
	3.986E-05

	Base
	31
	46
	Sy
	LinRespSpec
	Max
	
	
	0.2537
	0.0316
	0.5867
	0.1263
	0.5073
	4.597E-05

	Base
	31
	46
	Comb1
	Combination
	
	
	
	-0.2762
	-0.0024
	6.9478
	0.0103
	-0.3443
	7.968E-06

	Base
	31
	46
	Comb2
	Combination
	
	
	
	-0.2367
	-0.0021
	5.9552
	0.0089
	-0.2951
	6.83E-06

	Base
	31
	46
	Comb3
	Combination
	
	
	
	-0.2367
	-0.0021
	5.9552
	0.0089
	-0.2951
	6.83E-06

	Base
	31
	46
	Comb4
	Combination
	Max
	
	
	-0.1913
	-0.0018
	6.0228
	0.0099
	-0.2042
	1.252E-05

	Base
	31
	46
	Comb4
	Combination
	Min
	
	
	-0.2822
	-0.0023
	5.8877
	0.0078
	-0.386
	1.136E-06

	Base
	31
	46
	Comb5
	Combination
	Max
	
	
	-0.2005
	0.0024
	6.0391
	0.0269
	-0.2226
	1.34E-05

	Base
	31
	46
	Comb5
	Combination
	Min
	
	
	-0.273
	-0.0066
	5.8714
	-0.0092
	-0.3676
	0

	Base
	31
	46
	Comb6
	Combination
	
	
	
	-0.1775
	-0.0016
	4.4664
	0.0066
	-0.2213
	5.122E-06

	Base
	31
	46
	Comb7
	Combination
	Max
	
	
	-0.1321
	-0.0013
	4.534
	0.0077
	-0.1304
	1.082E-05

	Base
	31
	46
	Comb7
	Combination
	Min
	
	
	-0.223
	-0.0018
	4.3988
	0.0056
	-0.3122
	-5.715E-07

	Base
	31
	46
	Comb8
	Combination
	Max
	
	
	-0.1413
	0.0029
	4.5503
	0.0247
	-0.1488
	1.169E-05

	Base
	31
	46
	Comb8
	Combination
	Min
	
	
	-0.2138
	-0.0061
	4.3826
	-0.0114
	-0.2938
	-1.446E-06

	Base
	31
	46
	ENVDIS
	Combination
	Max
	
	
	-0.1321
	0.0029
	6.9478
	0.0269
	-0.1304
	1.34E-05

	Base
	31
	46
	ENVDIS
	Combination
	Min
	
	
	-0.2822
	-0.0066
	4.3826
	-0.0114
	-0.386
	-1.446E-06

	Base
	31
	46
	Serv1
	Combination
	
	
	
	-0.1973
	-0.0017
	4.9627
	0.0074
	-0.2459
	5.691E-06

	Base
	31
	46
	Serv2
	Combination
	
	
	
	-0.1973
	-0.0017
	4.9627
	0.0074
	-0.2459
	5.691E-06

	Base
	31
	46
	Serv3
	Combination
	
	
	
	-0.1973
	-0.0017
	4.9627
	0.0074
	-0.2459
	5.691E-06

	Base
	31
	46
	Serv4
	Combination
	Max
	
	
	-0.1654
	-0.0016
	5.01
	0.0081
	-0.1823
	9.677E-06

	Base
	31
	46
	Serv4
	Combination
	Min
	
	
	-0.2291
	-0.0019
	4.9154
	0.0067
	-0.3096
	1.706E-06

	Base
	31
	46
	Serv5
	Combination
	Max
	
	
	-0.1719
	0.0014
	5.0214
	0.02
	-0.1952
	1.029E-05

	Base
	31
	46
	Serv5
	Combination
	Min
	
	
	-0.2226
	-0.0049
	4.904
	-0.0052
	-0.2967
	1.095E-06

	Base
	31
	46
	Serv6
	Combination
	Max
	
	
	-0.1734
	-0.0016
	4.9982
	0.0079
	-0.1982
	8.68E-06

	Base
	31
	46
	Serv6
	Combination
	Min
	
	
	-0.2212
	-0.0019
	4.9272
	0.0068
	-0.2937
	2.702E-06

	Base
	31
	46
	Serv7
	Combination
	Max
	
	
	-0.1782
	0.0006
	5.0067
	0.0169
	-0.2079
	9.139E-06

	Base
	31
	46
	Serv7
	Combination
	Min
	
	
	-0.2163
	-0.0041
	4.9187
	-0.0021
	-0.284
	2.244E-06

	Base
	31
	46
	Serv8
	Combination
	
	
	
	-0.1184
	-0.001
	2.9776
	0.0044
	-0.1476
	3.415E-06

	Base
	31
	46
	Serv9
	Combination
	Max
	
	
	-0.0865
	-0.0009
	3.0249
	0.0051
	-0.0839
	7.4E-06

	Base
	31
	46
	Serv9
	Combination
	Min
	
	
	-0.1502
	-0.0012
	2.9303
	0.0037
	-0.2112
	-5.708E-07

	Base
	31
	46
	Serv10
	Combination
	Max
	
	
	-0.093
	0.0021
	3.0363
	0.0171
	-0.0968
	8.011E-06

	Base
	31
	46
	Serv10
	Combination
	Min
	
	
	-0.1437
	-0.0042
	2.919
	-0.0082
	-0.1983
	-1.182E-06

	Base
	31
	46
	ENVSERV
	Combination
	Max
	
	
	-0.0865
	0.0021
	5.0214
	0.02
	-0.0839
	1.029E-05

	Base
	31
	46
	ENVSERV
	Combination
	Min
	
	
	-0.2291
	-0.0049
	2.919
	-0.0082
	-0.3096
	-1.182E-06

	Base
	33
	50
	Dead
	LinStatic
	
	
	
	-0.0459
	-0.4241
	18.0362
	1.1861
	-0.0492
	-0.0222

	Base
	33
	50
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	33
	50
	FHEx
	LinStatic
	
	
	
	-0.2788
	-0.5599
	-0.7347
	1.8402
	-0.6987
	-0.0348

	Base
	33
	50
	FHEy
	LinStatic
	
	
	
	0.0633
	-6.3856
	-5.5368
	20.117
	0.2489
	-0.1708

	Base
	33
	50
	Sx
	LinRespSpec
	Max
	
	
	0.0922
	0.7694
	1.6358
	2.5186
	0.2287
	0.0834

	Base
	33
	50
	Sy
	LinRespSpec
	Max
	
	
	0.08
	6.3496
	5.6834
	20.0111
	0.2899
	0.2486

	Base
	33
	50
	Comb1
	Combination
	
	
	
	-0.0642
	-0.5938
	25.2507
	1.6605
	-0.0689
	-0.0311

	Base
	33
	50
	Comb2
	Combination
	
	
	
	-0.055
	-0.509
	21.6435
	1.4233
	-0.0591
	-0.0267

	Base
	33
	50
	Comb3
	Combination
	
	
	
	-0.055
	-0.509
	21.6435
	1.4233
	-0.0591
	-0.0267

	Base
	33
	50
	Comb4
	Combination
	Max
	
	
	-0.0418
	-0.399
	21.8771
	1.7831
	-0.0264
	-0.0148

	Base
	33
	50
	Comb4
	Combination
	Min
	
	
	-0.0682
	-0.6189
	21.4098
	1.0635
	-0.0917
	-0.0386

	Base
	33
	50
	Comb5
	Combination
	Max
	
	
	-0.0436
	0.3984
	22.4556
	4.2829
	-0.0176
	0.0088

	Base
	33
	50
	Comb5
	Combination
	Min
	
	
	-0.0665
	-1.4163
	20.8313
	-1.4363
	-0.1005
	-0.0622

	Base
	33
	50
	Comb6
	Combination
	
	
	
	-0.0413
	-0.3817
	16.2326
	1.0675
	-0.0443
	-0.02

	Base
	33
	50
	Comb7
	Combination
	Max
	
	
	-0.0281
	-0.2718
	16.4663
	1.4273
	-0.0116
	-0.0081

	Base
	33
	50
	Comb7
	Combination
	Min
	
	
	-0.0544
	-0.4916
	15.9989
	0.7077
	-0.077
	-0.0319

	Base
	33
	50
	Comb8
	Combination
	Max
	
	
	-0.0298
	0.5256
	17.0448
	3.9271
	-0.0029
	0.0155

	Base
	33
	50
	Comb8
	Combination
	Min
	
	
	-0.0527
	-1.2891
	15.4204
	-1.7921
	-0.0857
	-0.0555

	Base
	33
	50
	ENVDIS
	Combination
	Max
	
	
	-0.0281
	0.5256
	25.2507
	4.2829
	-0.0029
	0.0155

	Base
	33
	50
	ENVDIS
	Combination
	Min
	
	
	-0.0682
	-1.4163
	15.4204
	-1.7921
	-0.1005
	-0.0622

	Base
	33
	50
	Serv1
	Combination
	
	
	
	-0.0459
	-0.4241
	18.0362
	1.1861
	-0.0492
	-0.0222

	Base
	33
	50
	Serv2
	Combination
	
	
	
	-0.0459
	-0.4241
	18.0362
	1.1861
	-0.0492
	-0.0222

	Base
	33
	50
	Serv3
	Combination
	
	
	
	-0.0459
	-0.4241
	18.0362
	1.1861
	-0.0492
	-0.0222

	Base
	33
	50
	Serv4
	Combination
	Max
	
	
	-0.0366
	-0.3472
	18.1998
	1.4379
	-0.0264
	-0.0139

	Base
	33
	50
	Serv4
	Combination
	Min
	
	
	-0.0551
	-0.5011
	17.8726
	0.9342
	-0.0721
	-0.0306

	Base
	33
	50
	Serv5
	Combination
	Max
	
	
	-0.0378
	0.2108
	18.6046
	3.1872
	-0.0202
	0.0026

	Base
	33
	50
	Serv5
	Combination
	Min
	
	
	-0.0539
	-1.0591
	17.4679
	-0.815
	-0.0782
	-0.0471

	Base
	33
	50
	Serv6
	Combination
	Max
	
	
	-0.0389
	-0.3664
	18.1589
	1.375
	-0.0321
	-0.016

	Base
	33
	50
	Serv6
	Combination
	Min
	
	
	-0.0528
	-0.4818
	17.9135
	0.9972
	-0.0664
	-0.0285

	Base
	33
	50
	Serv7
	Combination
	Max
	
	
	-0.0398
	0.0521
	18.4625
	2.6869
	-0.0275
	-0.0036

	Base
	33
	50
	Serv7
	Combination
	Min
	
	
	-0.0519
	-0.9003
	17.61
	-0.3147
	-0.071
	-0.0409

	Base
	33
	50
	Serv8
	Combination
	
	
	
	-0.0275
	-0.2545
	10.8217
	0.7117
	-0.0295
	-0.0133

	Base
	33
	50
	Serv9
	Combination
	Max
	
	
	-0.0183
	-0.1775
	10.9853
	0.9635
	-0.0067
	-0.005

	Base
	33
	50
	Serv9
	Combination
	Min
	
	
	-0.0367
	-0.3314
	10.6582
	0.4598
	-0.0524
	-0.0217

	Base
	33
	50
	Serv10
	Combination
	Max
	
	
	-0.0195
	0.3805
	11.3901
	2.7128
	-0.0005
	0.0115

	Base
	33
	50
	Serv10
	Combination
	Min
	
	
	-0.0355
	-0.8894
	10.2534
	-1.2895
	-0.0585
	-0.0382

	Base
	33
	50
	ENVSERV
	Combination
	Max
	
	
	-0.0183
	0.3805
	18.6046
	3.1872
	-0.0005
	0.0115

	Base
	33
	50
	ENVSERV
	Combination
	Min
	
	
	-0.0551
	-1.0591
	10.2534
	-1.2895
	-0.0782
	-0.0471

	Base
	36
	52
	Dead
	LinStatic
	
	
	
	0.0312
	-0.306
	16.9579
	1.2054
	0.0487
	0.0009

	Base
	36
	52
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	36
	52
	FHEx
	LinStatic
	
	
	
	-0.4424
	-0.0187
	-0.0015
	0.0749
	-1.1074
	0.2596

	Base
	36
	52
	FHEy
	LinStatic
	
	
	
	-0.0104
	-4.5645
	-0.0566
	18.255
	-0.0105
	0.1885

	Base
	36
	52
	Sx
	LinRespSpec
	Max
	
	
	0.1749
	0.088
	0.0025
	0.352
	0.4443
	0.3475

	Base
	36
	52
	Sy
	LinRespSpec
	Max
	
	
	0.0316
	4.6345
	0.0601
	18.535
	0.0825
	0.3109

	Base
	36
	52
	Comb1
	Combination
	
	
	
	0.0436
	-0.4284
	23.741
	1.6876
	0.0682
	0.0013

	Base
	36
	52
	Comb2
	Combination
	
	
	
	0.0374
	-0.3672
	20.3494
	1.4465
	0.0585
	0.0011

	Base
	36
	52
	Comb3
	Combination
	
	
	
	0.0374
	-0.3672
	20.3494
	1.4465
	0.0585
	0.0011

	Base
	36
	52
	Comb4
	Combination
	Max
	
	
	0.0624
	-0.3546
	20.3498
	1.4968
	0.122
	0.0507

	Base
	36
	52
	Comb4
	Combination
	Min
	
	
	0.0124
	-0.3797
	20.3491
	1.3962
	-0.005
	-0.0486

	Base
	36
	52
	Comb5
	Combination
	Max
	
	
	0.0419
	0.2951
	20.358
	4.0951
	0.0703
	0.0455

	Base
	36
	52
	Comb5
	Combination
	Min
	
	
	0.0329
	-1.0294
	20.3408
	-1.2022
	0.0467
	-0.0433

	Base
	36
	52
	Comb6
	Combination
	
	
	
	0.0281
	-0.2754
	15.2621
	1.0849
	0.0439
	0.0008

	Base
	36
	52
	Comb7
	Combination
	Max
	
	
	0.053
	-0.2628
	15.2624
	1.1351
	0.1073
	0.0505

	Base
	36
	52
	Comb7
	Combination
	Min
	
	
	0.0031
	-0.288
	15.2617
	1.0346
	-0.0196
	-0.0488

	Base
	36
	52
	Comb8
	Combination
	Max
	
	
	0.0326
	0.3869
	15.2707
	3.7335
	0.0557
	0.0452

	Base
	36
	52
	Comb8
	Combination
	Min
	
	
	0.0235
	-0.9377
	15.2535
	-1.5638
	0.0321
	-0.0436

	Base
	36
	52
	ENVDIS
	Combination
	Max
	
	
	0.0624
	0.3869
	23.741
	4.0951
	0.122
	0.0507

	Base
	36
	52
	ENVDIS
	Combination
	Min
	
	
	0.0031
	-1.0294
	15.2535
	-1.5638
	-0.0196
	-0.0488

	Base
	36
	52
	Serv1
	Combination
	
	
	
	0.0312
	-0.306
	16.9579
	1.2054
	0.0487
	0.0009

	Base
	36
	52
	Serv2
	Combination
	
	
	
	0.0312
	-0.306
	16.9579
	1.2054
	0.0487
	0.0009

	Base
	36
	52
	Serv3
	Combination
	
	
	
	0.0312
	-0.306
	16.9579
	1.2054
	0.0487
	0.0009

	Base
	36
	52
	Serv4
	Combination
	Max
	
	
	0.0487
	-0.2972
	16.9581
	1.2406
	0.0932
	0.0357

	Base
	36
	52
	Serv4
	Combination
	Min
	
	
	0.0137
	-0.3148
	16.9576
	1.1702
	0.0043
	-0.0338

	Base
	36
	52
	Serv5
	Combination
	Max
	
	
	0.0343
	0.1575
	16.9639
	3.0589
	0.057
	0.032

	Base
	36
	52
	Serv5
	Combination
	Min
	
	
	0.028
	-0.7694
	16.9519
	-0.6481
	0.0405
	-0.0302

	Base
	36
	52
	Serv6
	Combination
	Max
	
	
	0.0443
	-0.2994
	16.9581
	1.2318
	0.0821
	0.027

	Base
	36
	52
	Serv6
	Combination
	Min
	
	
	0.0181
	-0.3126
	16.9577
	1.179
	0.0154
	-0.0252

	Base
	36
	52
	Serv7
	Combination
	Max
	
	
	0.0335
	0.0416
	16.9624
	2.5955
	0.0549
	0.0242

	Base
	36
	52
	Serv7
	Combination
	Min
	
	
	0.0288
	-0.6536
	16.9534
	-0.1847
	0.0426
	-0.0224

	Base
	36
	52
	Serv8
	Combination
	
	
	
	0.0187
	-0.1836
	10.1747
	0.7232
	0.0292
	0.0005

	Base
	36
	52
	Serv9
	Combination
	Max
	
	
	0.0362
	-0.1748
	10.175
	0.7584
	0.0737
	0.0353

	Base
	36
	52
	Serv9
	Combination
	Min
	
	
	0.0012
	-0.1924
	10.1745
	0.688
	-0.0152
	-0.0342

	Base
	36
	52
	Serv10
	Combination
	Max
	
	
	0.0219
	0.2799
	10.1807
	2.5767
	0.0375
	0.0316

	Base
	36
	52
	Serv10
	Combination
	Min
	
	
	0.0155
	-0.647
	10.1687
	-1.1303
	0.021
	-0.0305

	Base
	36
	52
	ENVSERV
	Combination
	Max
	
	
	0.0487
	0.2799
	16.9639
	3.0589
	0.0932
	0.0357

	Base
	36
	52
	ENVSERV
	Combination
	Min
	
	
	0.0012
	-0.7694
	10.1687
	-1.1303
	-0.0152
	-0.0342

	Base
	37
	54
	Dead
	LinStatic
	
	
	
	0.244
	-0.1148
	18.0462
	0.9516
	0.31
	0.0087

	Base
	37
	54
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	37
	54
	FHEx
	LinStatic
	
	
	
	-0.2657
	0.5091
	0.6824
	-1.7073
	-0.6718
	0.0281

	Base
	37
	54
	FHEy
	LinStatic
	
	
	
	-0.1718
	-6.3229
	-1.1577
	20.172
	-0.4344
	-0.2663

	Base
	37
	54
	Sx
	LinRespSpec
	Max
	
	
	0.0772
	0.6348
	0.9019
	2.1281
	0.1953
	0.1589

	Base
	37
	54
	Sy
	LinRespSpec
	Max
	
	
	0.1858
	6.4199
	1.3038
	20.4961
	0.4703
	0.3183

	Base
	37
	54
	Comb1
	Combination
	
	
	
	0.3416
	-0.1607
	25.2646
	1.3323
	0.434
	0.0122

	Base
	37
	54
	Comb2
	Combination
	
	
	
	0.2928
	-0.1377
	21.6554
	1.1419
	0.372
	0.0105

	Base
	37
	54
	Comb3
	Combination
	
	
	
	0.2928
	-0.1377
	21.6554
	1.1419
	0.372
	0.0105

	Base
	37
	54
	Comb4
	Combination
	Max
	
	
	0.3039
	-0.047
	21.7843
	1.446
	0.3999
	0.0332

	Base
	37
	54
	Comb4
	Combination
	Min
	
	
	0.2818
	-0.2284
	21.5266
	0.8379
	0.3441
	-0.0122

	Base
	37
	54
	Comb5
	Combination
	Max
	
	
	0.3194
	0.7797
	21.8417
	4.0708
	0.4392
	0.056

	Base
	37
	54
	Comb5
	Combination
	Min
	
	
	0.2663
	-1.0551
	21.4691
	-1.787
	0.3048
	-0.035

	Base
	37
	54
	Comb6
	Combination
	
	
	
	0.2196
	-0.1033
	16.2416
	0.8565
	0.279
	0.0079

	Base
	37
	54
	Comb7
	Combination
	Max
	
	
	0.2307
	-0.0126
	16.3704
	1.1605
	0.3069
	0.0306

	Base
	37
	54
	Comb7
	Combination
	Min
	
	
	0.2086
	-0.194
	16.1127
	0.5524
	0.2511
	-0.0148

	Base
	37
	54
	Comb8
	Combination
	Max
	
	
	0.2462
	0.8141
	16.4279
	3.7854
	0.3462
	0.0534

	Base
	37
	54
	Comb8
	Combination
	Min
	
	
	0.1931
	-1.0207
	16.0552
	-2.0724
	0.2118
	-0.0376

	Base
	37
	54
	ENVDIS
	Combination
	Max
	
	
	0.3416
	0.8141
	25.2646
	4.0708
	0.4392
	0.056

	Base
	37
	54
	ENVDIS
	Combination
	Min
	
	
	0.1931
	-1.0551
	16.0552
	-2.0724
	0.2118
	-0.0376

	Base
	37
	54
	Serv1
	Combination
	
	
	
	0.244
	-0.1148
	18.0462
	0.9516
	0.31
	0.0087

	Base
	37
	54
	Serv2
	Combination
	
	
	
	0.244
	-0.1148
	18.0462
	0.9516
	0.31
	0.0087

	Base
	37
	54
	Serv3
	Combination
	
	
	
	0.244
	-0.1148
	18.0462
	0.9516
	0.31
	0.0087

	Base
	37
	54
	Serv4
	Combination
	Max
	
	
	0.2517
	-0.0513
	18.1364
	1.1644
	0.3295
	0.0246

	Base
	37
	54
	Serv4
	Combination
	Min
	
	
	0.2363
	-0.1782
	17.956
	0.7388
	0.2904
	-0.0071

	Base
	37
	54
	Serv5
	Combination
	Max
	
	
	0.2626
	0.5272
	18.1766
	3.0012
	0.357
	0.0406

	Base
	37
	54
	Serv5
	Combination
	Min
	
	
	0.2254
	-0.7568
	17.9158
	-1.098
	0.2629
	-0.0231

	Base
	37
	54
	Serv6
	Combination
	Max
	
	
	0.2498
	-0.0672
	18.1138
	1.1112
	0.3246
	0.0207

	Base
	37
	54
	Serv6
	Combination
	Min
	
	
	0.2382
	-0.1624
	17.9785
	0.792
	0.2953
	-0.0032

	Base
	37
	54
	Serv7
	Combination
	Max
	
	
	0.258
	0.3667
	18.144
	2.4888
	0.3452
	0.0326

	Base
	37
	54
	Serv7
	Combination
	Min
	
	
	0.2301
	-0.5963
	17.9484
	-0.5856
	0.2747
	-0.0151

	Base
	37
	54
	Serv8
	Combination
	
	
	
	0.1464
	-0.0689
	10.8277
	0.571
	0.186
	0.0052

	Base
	37
	54
	Serv9
	Combination
	Max
	
	
	0.1541
	-0.0054
	10.9179
	0.7838
	0.2055
	0.0211

	Base
	37
	54
	Serv9
	Combination
	Min
	
	
	0.1387
	-0.1323
	10.7375
	0.3582
	0.1665
	-0.0106

	Base
	37
	54
	Serv10
	Combination
	Max
	
	
	0.165
	0.5731
	10.9581
	2.6206
	0.233
	0.0371

	Base
	37
	54
	Serv10
	Combination
	Min
	
	
	0.1278
	-0.7109
	10.6973
	-1.4786
	0.139
	-0.0266

	Base
	37
	54
	ENVSERV
	Combination
	Max
	
	
	0.2626
	0.5731
	18.1766
	3.0012
	0.357
	0.0406

	Base
	37
	54
	ENVSERV
	Combination
	Min
	
	
	0.1278
	-0.7568
	10.6973
	-1.4786
	0.139
	-0.0266

	Base
	38
	79
	Dead
	LinStatic
	
	
	
	2.223
	-3.6789
	20.9293
	0.4351
	3.1751
	-0.1456

	Base
	38
	79
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	38
	79
	FHEx
	LinStatic
	
	
	
	-5.4533
	3.1932
	-7.0243
	0.415
	1.2016
	-0.0345

	Base
	38
	79
	FHEy
	LinStatic
	
	
	
	6.4878
	-25.4719
	218.6784
	5.9035
	-1.5531
	-0.3169

	Base
	38
	79
	Sx
	LinRespSpec
	Max
	
	
	0.6784
	5.872
	25.6347
	0.6917
	0.4799
	0.0952

	Base
	38
	79
	Sy
	LinRespSpec
	Max
	
	
	6.2046
	25.6457
	215.1294
	5.7772
	1.3691
	0.3069

	Base
	38
	79
	Comb1
	Combination
	
	
	
	3.1121
	-5.1505
	29.301
	0.6091
	4.4451
	-0.2038

	Base
	38
	79
	Comb2
	Combination
	
	
	
	2.6675
	-4.4147
	25.1151
	0.5221
	3.8101
	-0.1747

	Base
	38
	79
	Comb3
	Combination
	
	
	
	2.6675
	-4.4147
	25.1151
	0.5221
	3.8101
	-0.1747

	Base
	38
	79
	Comb4
	Combination
	Max
	
	
	2.7645
	-3.5758
	28.7772
	0.6209
	3.8786
	-0.1611

	Base
	38
	79
	Comb4
	Combination
	Min
	
	
	2.5706
	-5.2535
	21.453
	0.4233
	3.7415
	-0.1883

	Base
	38
	79
	Comb5
	Combination
	Max
	
	
	3.5542
	-0.7499
	55.8571
	1.3476
	4.0057
	-0.1308

	Base
	38
	79
	Comb5
	Combination
	Min
	
	
	1.7809
	-8.0794
	-5.6269
	-0.3035
	3.6144
	-0.2186

	Base
	38
	79
	Comb6
	Combination
	
	
	
	2.0007
	-3.311
	18.8363
	0.3916
	2.8576
	-0.131

	Base
	38
	79
	Comb7
	Combination
	Max
	
	
	2.0976
	-2.4721
	22.4984
	0.4904
	2.9261
	-0.1174

	Base
	38
	79
	Comb7
	Combination
	Min
	
	
	1.9037
	-4.1499
	15.1743
	0.2927
	2.789
	-0.1446

	Base
	38
	79
	Comb8
	Combination
	Max
	
	
	2.8873
	0.3538
	49.5783
	1.2171
	3.0532
	-0.0872

	Base
	38
	79
	Comb8
	Combination
	Min
	
	
	1.114
	-6.9758
	-11.9056
	-0.434
	2.6619
	-0.1749

	Base
	38
	79
	ENVDIS
	Combination
	Max
	
	
	3.5542
	0.3538
	55.8571
	1.3476
	4.4451
	-0.0872

	Base
	38
	79
	ENVDIS
	Combination
	Min
	
	
	1.114
	-8.0794
	-11.9056
	-0.434
	2.6619
	-0.2186

	Base
	38
	79
	Serv1
	Combination
	
	
	
	2.223
	-3.6789
	20.9293
	0.4351
	3.1751
	-0.1456

	Base
	38
	79
	Serv2
	Combination
	
	
	
	2.223
	-3.6789
	20.9293
	0.4351
	3.1751
	-0.1456

	Base
	38
	79
	Serv3
	Combination
	
	
	
	2.223
	-3.6789
	20.9293
	0.4351
	3.1751
	-0.1456

	Base
	38
	79
	Serv4
	Combination
	Max
	
	
	2.2908
	-3.0917
	23.4927
	0.5042
	3.2231
	-0.1361

	Base
	38
	79
	Serv4
	Combination
	Min
	
	
	2.1551
	-4.2661
	18.3658
	0.3659
	3.1271
	-0.1551

	Base
	38
	79
	Serv5
	Combination
	Max
	
	
	2.8434
	-1.1143
	42.4422
	1.0128
	3.312
	-0.1149

	Base
	38
	79
	Serv5
	Combination
	Min
	
	
	1.6025
	-6.2435
	-0.5837
	-0.1427
	3.0382
	-0.1763

	Base
	38
	79
	Serv6
	Combination
	Max
	
	
	2.2738
	-3.2385
	22.8519
	0.4869
	3.2111
	-0.1384

	Base
	38
	79
	Serv6
	Combination
	Min
	
	
	2.1721
	-4.1193
	19.0067
	0.3832
	3.1391
	-0.1527

	Base
	38
	79
	Serv7
	Combination
	Max
	
	
	2.6883
	-1.7555
	37.064
	0.8684
	3.2778
	-0.1226

	Base
	38
	79
	Serv7
	Combination
	Min
	
	
	1.7576
	-5.6023
	4.7946
	0.0018
	3.0724
	-0.1686

	Base
	38
	79
	Serv8
	Combination
	
	
	
	1.3338
	-2.2073
	12.5576
	0.261
	1.905
	-0.0873

	Base
	38
	79
	Serv9
	Combination
	Max
	
	
	1.4016
	-1.6201
	15.121
	0.3302
	1.953
	-0.0778

	Base
	38
	79
	Serv9
	Combination
	Min
	
	
	1.2659
	-2.7945
	9.9941
	0.1919
	1.8571
	-0.0969

	Base
	38
	79
	Serv10
	Combination
	Max
	
	
	1.9542
	0.3572
	34.0705
	0.8388
	2.042
	-0.0567

	Base
	38
	79
	Serv10
	Combination
	Min
	
	
	0.7133
	-4.7719
	-8.9554
	-0.3167
	1.7681
	-0.118

	Base
	38
	79
	ENVSERV
	Combination
	Max
	
	
	2.8434
	0.3572
	42.4422
	1.0128
	3.312
	-0.0567

	Base
	38
	79
	ENVSERV
	Combination
	Min
	
	
	0.7133
	-6.2435
	-8.9554
	-0.3167
	1.7681
	-0.1763

	Base
	39
	82
	Dead
	LinStatic
	
	
	
	1.884
	-1.9313
	58.5386
	5.2898
	0.545
	-0.162

	Base
	39
	82
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	39
	82
	FHEx
	LinStatic
	
	
	
	-73.6145
	-2.1083
	-18.339
	3.2172
	-21.6249
	-3.0295

	Base
	39
	82
	FHEy
	LinStatic
	
	
	
	29.9583
	-12.2757
	-244.261
	33.7856
	6.9311
	0.4096

	Base
	39
	82
	Sx
	LinRespSpec
	Max
	
	
	26.6654
	2.4186
	29.2088
	4.3867
	6.8022
	4.1532

	Base
	39
	82
	Sy
	LinRespSpec
	Max
	
	
	30.5364
	12.3197
	242.9094
	33.6616
	7.5346
	3.1336

	Base
	39
	82
	Comb1
	Combination
	
	
	
	2.6376
	-2.7038
	81.954
	7.4057
	0.7629
	-0.2268

	Base
	39
	82
	Comb2
	Combination
	
	
	
	2.2608
	-2.3176
	70.2463
	6.3478
	0.654
	-0.1944

	Base
	39
	82
	Comb3
	Combination
	
	
	
	2.2608
	-2.3176
	70.2463
	6.3478
	0.654
	-0.1944

	Base
	39
	82
	Comb4
	Combination
	Max
	
	
	6.0701
	-1.972
	74.419
	6.9744
	1.6257
	0.3989

	Base
	39
	82
	Comb4
	Combination
	Min
	
	
	-1.5485
	-2.6631
	66.0736
	5.7211
	-0.3178
	-0.7877

	Base
	39
	82
	Comb5
	Combination
	Max
	
	
	6.6245
	-0.5571
	104.9581
	11.158
	1.7306
	0.2534

	Base
	39
	82
	Comb5
	Combination
	Min
	
	
	-2.1028
	-4.078
	35.5346
	1.5375
	-0.4227
	-0.6422

	Base
	39
	82
	Comb6
	Combination
	
	
	
	1.6956
	-1.7382
	52.6847
	4.7608
	0.4905
	-0.1458

	Base
	39
	82
	Comb7
	Combination
	Max
	
	
	5.5049
	-1.3926
	56.8574
	5.3875
	1.4622
	0.4475

	Base
	39
	82
	Comb7
	Combination
	Min
	
	
	-2.1137
	-2.0837
	48.5121
	4.1342
	-0.4813
	-0.7391

	Base
	39
	82
	Comb8
	Combination
	Max
	
	
	6.0593
	0.0223
	87.3965
	9.5711
	1.5672
	0.302

	Base
	39
	82
	Comb8
	Combination
	Min
	
	
	-2.668
	-3.4986
	17.973
	-0.0494
	-0.5862
	-0.5936

	Base
	39
	82
	ENVDIS
	Combination
	Max
	
	
	6.6245
	0.0223
	104.9581
	11.158
	1.7306
	0.4475

	Base
	39
	82
	ENVDIS
	Combination
	Min
	
	
	-2.668
	-4.078
	17.973
	-0.0494
	-0.5862
	-0.7877

	Base
	39
	82
	Serv1
	Combination
	
	
	
	1.884
	-1.9313
	58.5386
	5.2898
	0.545
	-0.162

	Base
	39
	82
	Serv2
	Combination
	
	
	
	1.884
	-1.9313
	58.5386
	5.2898
	0.545
	-0.162

	Base
	39
	82
	Serv3
	Combination
	
	
	
	1.884
	-1.9313
	58.5386
	5.2898
	0.545
	-0.162

	Base
	39
	82
	Serv4
	Combination
	Max
	
	
	4.5505
	-1.6894
	61.4595
	5.7285
	1.2252
	0.2533

	Base
	39
	82
	Serv4
	Combination
	Min
	
	
	-0.7825
	-2.1732
	55.6177
	4.8511
	-0.1353
	-0.5773

	Base
	39
	82
	Serv5
	Combination
	Max
	
	
	4.9376
	-0.6993
	82.8295
	8.656
	1.2984
	0.1514

	Base
	39
	82
	Serv5
	Combination
	Min
	
	
	-1.1696
	-3.1633
	34.2477
	1.9236
	-0.2085
	-0.4753

	Base
	39
	82
	Serv6
	Combination
	Max
	
	
	3.8839
	-1.7499
	60.7293
	5.6188
	1.0551
	0.1495

	Base
	39
	82
	Serv6
	Combination
	Min
	
	
	-0.1159
	-2.1127
	56.3479
	4.9608
	0.0348
	-0.4735

	Base
	39
	82
	Serv7
	Combination
	Max
	
	
	4.1742
	-1.0073
	76.7568
	7.8144
	1.1101
	0.073

	Base
	39
	82
	Serv7
	Combination
	Min
	
	
	-0.4062
	-2.8553
	40.3204
	2.7652
	-0.0201
	-0.397

	Base
	39
	82
	Serv8
	Combination
	
	
	
	1.1304
	-1.1588
	35.1232
	3.1739
	0.327
	-0.0972

	Base
	39
	82
	Serv9
	Combination
	Max
	
	
	3.7969
	-0.9169
	38.044
	3.6125
	1.0072
	0.3181

	Base
	39
	82
	Serv9
	Combination
	Min
	
	
	-1.5361
	-1.4006
	32.2023
	2.7352
	-0.3532
	-0.5125

	Base
	39
	82
	Serv10
	Combination
	Max
	
	
	4.184
	0.0732
	59.4141
	6.54
	1.0804
	0.2162

	Base
	39
	82
	Serv10
	Combination
	Min
	
	
	-1.9232
	-2.3907
	10.8322
	-0.1923
	-0.4265
	-0.4106

	Base
	39
	82
	ENVSERV
	Combination
	Max
	
	
	4.9376
	0.0732
	82.8295
	8.656
	1.2984
	0.3181

	Base
	39
	82
	ENVSERV
	Combination
	Min
	
	
	-1.9232
	-3.1633
	10.8322
	-0.1923
	-0.4265
	-0.5773

	Base
	40
	86
	Dead
	LinStatic
	
	
	
	5.7298
	-0.1402
	80.6734
	0.4896
	1.9084
	0.3318

	Base
	40
	86
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	40
	86
	FHEx
	LinStatic
	
	
	
	-69.4684
	-2.1063
	13.3196
	2.6607
	-20.6337
	1.7698

	Base
	40
	86
	FHEy
	LinStatic
	
	
	
	66.8739
	-11.9419
	203.9342
	27.5749
	16.0354
	4.0597

	Base
	40
	86
	Sx
	LinRespSpec
	Max
	
	
	27.7247
	2.5483
	18.2789
	3.6656
	7.0033
	2.228

	Base
	40
	86
	Sy
	LinRespSpec
	Max
	
	
	74.8808
	12.1922
	201.4427
	27.4763
	17.9197
	5.3177

	Base
	40
	86
	Comb1
	Combination
	
	
	
	8.0217
	-0.1963
	112.9428
	0.6854
	2.6718
	0.4645

	Base
	40
	86
	Comb2
	Combination
	
	
	
	6.8757
	-0.1683
	96.8081
	0.5875
	2.2901
	0.3981

	Base
	40
	86
	Comb3
	Combination
	
	
	
	6.8757
	-0.1683
	96.8081
	0.5875
	2.2901
	0.3981

	Base
	40
	86
	Comb4
	Combination
	Max
	
	
	10.8364
	0.1957
	99.4194
	1.1111
	3.2905
	0.7164

	Base
	40
	86
	Comb4
	Combination
	Min
	
	
	2.9151
	-0.5323
	94.1968
	0.0638
	1.2896
	0.0799

	Base
	40
	86
	Comb5
	Combination
	Max
	
	
	17.5762
	1.574
	125.5943
	4.5138
	4.8508
	1.158

	Base
	40
	86
	Comb5
	Combination
	Min
	
	
	-3.8247
	-1.9106
	68.0219
	-3.3389
	-0.2706
	-0.3618

	Base
	40
	86
	Comb6
	Combination
	
	
	
	5.1568
	-0.1262
	72.6061
	0.4406
	1.7176
	0.2986

	Base
	40
	86
	Comb7
	Combination
	Max
	
	
	9.1175
	0.2378
	75.2173
	0.9643
	2.718
	0.6169

	Base
	40
	86
	Comb7
	Combination
	Min
	
	
	1.1961
	-0.4903
	69.9948
	-0.083
	0.7171
	-0.0197

	Base
	40
	86
	Comb8
	Combination
	Max
	
	
	15.8573
	1.616
	101.3922
	4.367
	4.2783
	1.0585

	Base
	40
	86
	Comb8
	Combination
	Min
	
	
	-5.5437
	-1.8685
	43.8199
	-3.4858
	-0.8432
	-0.4613

	Base
	40
	86
	ENVDIS
	Combination
	Max
	
	
	17.5762
	1.616
	125.5943
	4.5138
	4.8508
	1.158

	Base
	40
	86
	ENVDIS
	Combination
	Min
	
	
	-5.5437
	-1.9106
	43.8199
	-3.4858
	-0.8432
	-0.4613

	Base
	40
	86
	Serv1
	Combination
	
	
	
	5.7298
	-0.1402
	80.6734
	0.4896
	1.9084
	0.3318

	Base
	40
	86
	Serv2
	Combination
	
	
	
	5.7298
	-0.1402
	80.6734
	0.4896
	1.9084
	0.3318

	Base
	40
	86
	Serv3
	Combination
	
	
	
	5.7298
	-0.1402
	80.6734
	0.4896
	1.9084
	0.3318

	Base
	40
	86
	Serv4
	Combination
	Max
	
	
	8.5022
	0.1146
	82.5013
	0.8561
	2.6087
	0.5546

	Base
	40
	86
	Serv4
	Combination
	Min
	
	
	2.9573
	-0.3951
	78.8455
	0.123
	1.2081
	0.109

	Base
	40
	86
	Serv5
	Combination
	Max
	
	
	13.2178
	1.079
	100.8177
	3.2372
	3.7004
	0.8635

	Base
	40
	86
	Serv5
	Combination
	Min
	
	
	-1.7583
	-1.3595
	60.5291
	-2.2581
	0.1164
	-0.2

	Base
	40
	86
	Serv6
	Combination
	Max
	
	
	7.8091
	0.0509
	82.0443
	0.7645
	2.4336
	0.4989

	Base
	40
	86
	Serv6
	Combination
	Min
	
	
	3.6504
	-0.3314
	79.3025
	0.2146
	1.3831
	0.1647

	Base
	40
	86
	Serv7
	Combination
	Max
	
	
	11.3458
	0.7742
	95.7816
	2.5503
	3.2524
	0.7306

	Base
	40
	86
	Serv7
	Combination
	Min
	
	
	0.1137
	-1.0547
	65.5652
	-1.5712
	0.5644
	-0.067

	Base
	40
	86
	Serv8
	Combination
	
	
	
	3.4379
	-0.0841
	48.404
	0.2937
	1.145
	0.1991

	Base
	40
	86
	Serv9
	Combination
	Max
	
	
	6.2103
	0.1707
	50.2319
	0.6603
	1.8454
	0.4219

	Base
	40
	86
	Serv9
	Combination
	Min
	
	
	0.6654
	-0.339
	46.5762
	-0.0728
	0.4447
	-0.0237

	Base
	40
	86
	Serv10
	Combination
	Max
	
	
	10.9259
	1.1351
	68.5483
	3.0414
	2.937
	0.7308

	Base
	40
	86
	Serv10
	Combination
	Min
	
	
	-4.0502
	-1.3034
	28.2598
	-2.4539
	-0.6469
	-0.3327

	Base
	40
	86
	ENVSERV
	Combination
	Max
	
	
	13.2178
	1.1351
	100.8177
	3.2372
	3.7004
	0.8635

	Base
	40
	86
	ENVSERV
	Combination
	Min
	
	
	-4.0502
	-1.3595
	28.2598
	-2.4539
	-0.6469
	-0.3327

	Base
	41
	90
	Dead
	LinStatic
	
	
	
	-1.9589
	2.9233
	93.4916
	-7.7366
	-0.3817
	0.2523

	Base
	41
	90
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	41
	90
	FHEx
	LinStatic
	
	
	
	-72.6974
	2.1874
	-12.9935
	-2.8344
	-20.4705
	-0.0814

	Base
	41
	90
	FHEy
	LinStatic
	
	
	
	-40.6283
	-3.3956
	240.2256
	32.6421
	-14.3114
	0.5792

	Base
	41
	90
	Sx
	LinRespSpec
	Max
	
	
	24.2715
	4.0369
	18.4716
	3.6413
	6.0456
	2.5052

	Base
	41
	90
	Sy
	LinRespSpec
	Max
	
	
	43.1752
	2.8638
	244.1511
	33.3868
	15.0944
	1.5002

	Base
	41
	90
	Comb1
	Combination
	
	
	
	-2.7424
	4.0926
	130.8882
	-10.8312
	-0.5344
	0.3532

	Base
	41
	90
	Comb2
	Combination
	
	
	
	-2.3507
	3.508
	112.1899
	-9.2839
	-0.4581
	0.3027

	Base
	41
	90
	Comb3
	Combination
	
	
	
	-2.3507
	3.508
	112.1899
	-9.2839
	-0.4581
	0.3027

	Base
	41
	90
	Comb4
	Combination
	Max
	
	
	1.1167
	4.0847
	114.8287
	-8.7637
	0.4056
	0.6606

	Base
	41
	90
	Comb4
	Combination
	Min
	
	
	-5.818
	2.9313
	109.5511
	-9.8041
	-1.3218
	-0.0552

	Base
	41
	90
	Comb5
	Combination
	Max
	
	
	3.8191
	3.9172
	147.0791
	-4.5129
	1.6989
	0.5171

	Base
	41
	90
	Comb5
	Combination
	Min
	
	
	-8.5204
	3.0987
	77.3007
	-14.0549
	-2.6151
	0.0883

	Base
	41
	90
	Comb6
	Combination
	
	
	
	-1.763
	2.631
	84.1424
	-6.9629
	-0.3436
	0.227

	Base
	41
	90
	Comb7
	Combination
	Max
	
	
	1.7044
	3.2077
	86.7812
	-6.4428
	0.5201
	0.5849

	Base
	41
	90
	Comb7
	Combination
	Min
	
	
	-5.2304
	2.0543
	81.5036
	-7.4831
	-1.2072
	-0.1309

	Base
	41
	90
	Comb8
	Combination
	Max
	
	
	4.4067
	3.0402
	119.0316
	-2.192
	1.8134
	0.4414

	Base
	41
	90
	Comb8
	Combination
	Min
	
	
	-7.9327
	2.2217
	49.2532
	-11.7339
	-2.5006
	0.0126

	Base
	41
	90
	ENVDIS
	Combination
	Max
	
	
	4.4067
	4.0926
	147.0791
	-2.192
	1.8134
	0.6606

	Base
	41
	90
	ENVDIS
	Combination
	Min
	
	
	-8.5204
	2.0543
	49.2532
	-14.0549
	-2.6151
	-0.1309

	Base
	41
	90
	Serv1
	Combination
	
	
	
	-1.9589
	2.9233
	93.4916
	-7.7366
	-0.3817
	0.2523

	Base
	41
	90
	Serv2
	Combination
	
	
	
	-1.9589
	2.9233
	93.4916
	-7.7366
	-0.3817
	0.2523

	Base
	41
	90
	Serv3
	Combination
	
	
	
	-1.9589
	2.9233
	93.4916
	-7.7366
	-0.3817
	0.2523

	Base
	41
	90
	Serv4
	Combination
	Max
	
	
	0.4683
	3.327
	95.3387
	-7.3725
	0.2228
	0.5028

	Base
	41
	90
	Serv4
	Combination
	Min
	
	
	-4.386
	2.5196
	91.6444
	-8.1007
	-0.9863
	0.0017

	Base
	41
	90
	Serv5
	Combination
	Max
	
	
	2.3586
	3.2097
	117.9067
	-4.3979
	1.1277
	0.4023

	Base
	41
	90
	Serv5
	Combination
	Min
	
	
	-6.2764
	2.6369
	69.0764
	-11.0753
	-1.8912
	0.1022

	Base
	41
	90
	Serv6
	Combination
	Max
	
	
	-0.1385
	3.2261
	94.8769
	-7.4635
	0.0717
	0.4401

	Base
	41
	90
	Serv6
	Combination
	Min
	
	
	-3.7793
	2.6206
	92.1062
	-8.0097
	-0.8352
	0.0644

	Base
	41
	90
	Serv7
	Combination
	Max
	
	
	1.2792
	3.1381
	111.8029
	-5.2326
	0.7503
	0.3648

	Base
	41
	90
	Serv7
	Combination
	Min
	
	
	-5.197
	2.7085
	75.1802
	-10.2406
	-1.5138
	0.1397

	Base
	41
	90
	Serv8
	Combination
	
	
	
	-1.1753
	1.754
	56.0949
	-4.642
	-0.229
	0.1514

	Base
	41
	90
	Serv9
	Combination
	Max
	
	
	1.2518
	2.1577
	57.9421
	-4.2778
	0.3755
	0.4019

	Base
	41
	90
	Serv9
	Combination
	Min
	
	
	-3.6025
	1.3503
	54.2478
	-5.0061
	-0.8336
	-0.0992

	Base
	41
	90
	Serv10
	Combination
	Max
	
	
	3.1422
	2.0404
	80.51
	-1.3033
	1.2804
	0.3014

	Base
	41
	90
	Serv10
	Combination
	Min
	
	
	-5.4929
	1.4676
	31.6798
	-7.9806
	-1.7385
	0.0013

	Base
	41
	90
	ENVSERV
	Combination
	Max
	
	
	3.1422
	3.327
	117.9067
	-1.3033
	1.2804
	0.5028

	Base
	41
	90
	ENVSERV
	Combination
	Min
	
	
	-6.2764
	1.3503
	31.6798
	-11.0753
	-1.8912
	-0.0992

	Base
	44
	94
	Dead
	LinStatic
	
	
	
	0.4614
	-1.5377
	52.1579
	3.5714
	-0.6331
	0.345

	Base
	44
	94
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	44
	94
	FHEx
	LinStatic
	
	
	
	-66.2179
	1.1172
	18.9549
	-2.9904
	-20.7004
	-0.5053

	Base
	44
	94
	FHEy
	LinStatic
	
	
	
	-23.5684
	-9.1213
	-254.2108
	32.1149
	-11.8836
	5.982

	Base
	44
	94
	Sx
	LinRespSpec
	Max
	
	
	21.1332
	2.5257
	25.4457
	3.5835
	6.5719
	3.6311

	Base
	44
	94
	Sy
	LinRespSpec
	Max
	
	
	24.5376
	8.6994
	259.0094
	32.6172
	13.3567
	7.1899

	Base
	44
	94
	Comb1
	Combination
	
	
	
	0.646
	-2.1528
	73.0211
	4.9999
	-0.8863
	0.483

	Base
	44
	94
	Comb2
	Combination
	
	
	
	0.5537
	-1.8453
	62.5895
	4.2857
	-0.7597
	0.414

	Base
	44
	94
	Comb3
	Combination
	
	
	
	0.5537
	-1.8453
	62.5895
	4.2857
	-0.7597
	0.414

	Base
	44
	94
	Comb4
	Combination
	Max
	
	
	3.5727
	-1.4845
	66.2246
	4.7976
	0.1791
	0.9327

	Base
	44
	94
	Comb4
	Combination
	Min
	
	
	-2.4653
	-2.2061
	58.9544
	3.7737
	-1.6985
	-0.1048

	Base
	44
	94
	Comb5
	Combination
	Max
	
	
	4.0601
	-0.6021
	99.602
	8.9466
	1.149
	1.4414

	Base
	44
	94
	Comb5
	Combination
	Min
	
	
	-2.9527
	-3.0884
	25.5771
	-0.3753
	-2.6684
	-0.6135

	Base
	44
	94
	Comb6
	Combination
	
	
	
	0.4153
	-1.384
	46.9421
	3.2142
	-0.5698
	0.3105

	Base
	44
	94
	Comb7
	Combination
	Max
	
	
	3.4343
	-1.0231
	50.5772
	3.7262
	0.3691
	0.8292

	Base
	44
	94
	Comb7
	Combination
	Min
	
	
	-2.6038
	-1.7448
	43.307
	2.7023
	-1.5086
	-0.2083

	Base
	44
	94
	Comb8
	Combination
	Max
	
	
	3.9217
	-0.1408
	83.9546
	7.8752
	1.3389
	1.3379

	Base
	44
	94
	Comb8
	Combination
	Min
	
	
	-3.0912
	-2.6271
	9.9297
	-1.4468
	-2.4785
	-0.717

	Base
	44
	94
	ENVDIS
	Combination
	Max
	
	
	4.0601
	-0.1408
	99.602
	8.9466
	1.3389
	1.4414

	Base
	44
	94
	ENVDIS
	Combination
	Min
	
	
	-3.0912
	-3.0884
	9.9297
	-1.4468
	-2.6684
	-0.717

	Base
	44
	94
	Serv1
	Combination
	
	
	
	0.4614
	-1.5377
	52.1579
	3.5714
	-0.6331
	0.345

	Base
	44
	94
	Serv2
	Combination
	
	
	
	0.4614
	-1.5377
	52.1579
	3.5714
	-0.6331
	0.345

	Base
	44
	94
	Serv3
	Combination
	
	
	
	0.4614
	-1.5377
	52.1579
	3.5714
	-0.6331
	0.345

	Base
	44
	94
	Serv4
	Combination
	Max
	
	
	2.5747
	-1.2852
	54.7025
	3.9297
	0.0241
	0.7081

	Base
	44
	94
	Serv4
	Combination
	Min
	
	
	-1.6519
	-1.7903
	49.6134
	3.213
	-1.2903
	-0.0181

	Base
	44
	94
	Serv5
	Combination
	Max
	
	
	2.9152
	-0.6678
	78.0589
	6.8331
	0.7026
	1.064

	Base
	44
	94
	Serv5
	Combination
	Min
	
	
	-1.9923
	-2.4077
	26.257
	0.3097
	-1.9688
	-0.374

	Base
	44
	94
	Serv6
	Combination
	Max
	
	
	2.0464
	-1.3483
	54.0664
	3.8401
	-0.1402
	0.6173

	Base
	44
	94
	Serv6
	Combination
	Min
	
	
	-1.1236
	-1.7272
	50.2495
	3.3026
	-1.126
	0.0726

	Base
	44
	94
	Serv7
	Combination
	Max
	
	
	2.3017
	-0.8853
	71.5836
	6.0177
	0.3687
	0.8842

	Base
	44
	94
	Serv7
	Combination
	Min
	
	
	-1.3789
	-2.1902
	32.7322
	1.1251
	-1.6348
	-0.1943

	Base
	44
	94
	Serv8
	Combination
	
	
	
	0.2768
	-0.9226
	31.2948
	2.1428
	-0.3798
	0.207

	Base
	44
	94
	Serv9
	Combination
	Max
	
	
	2.3902
	-0.6701
	33.8393
	2.5012
	0.2773
	0.5701

	Base
	44
	94
	Serv9
	Combination
	Min
	
	
	-1.8365
	-1.1752
	28.7502
	1.7845
	-1.037
	-0.1561

	Base
	44
	94
	Serv10
	Combination
	Max
	
	
	2.7306
	-0.0527
	57.1957
	5.4045
	0.9558
	0.926

	Base
	44
	94
	Serv10
	Combination
	Min
	
	
	-2.1769
	-1.7926
	5.3938
	-1.1189
	-1.7155
	-0.512

	Base
	44
	94
	ENVSERV
	Combination
	Max
	
	
	2.9152
	-0.0527
	78.0589
	6.8331
	0.9558
	1.064

	Base
	44
	94
	ENVSERV
	Combination
	Min
	
	
	-2.1769
	-2.4077
	5.3938
	-1.1189
	-1.9688
	-0.512

	Base
	45
	108
	Dead
	LinStatic
	
	
	
	2.1368
	-0.0197
	7.7013
	0.0105
	0.1067
	-0.0196

	Base
	45
	108
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	45
	108
	FHEx
	LinStatic
	
	
	
	-5.1379
	0.0441
	-18.3304
	0.0197
	-1.4231
	0.0657

	Base
	45
	108
	FHEy
	LinStatic
	
	
	
	1.4406
	-1.9867
	9.9122
	0.5252
	1.493
	-1.0892

	Base
	45
	108
	Sx
	LinRespSpec
	Max
	
	
	3.8661
	0.4173
	14.9692
	0.0802
	1.1492
	0.2549

	Base
	45
	108
	Sy
	LinRespSpec
	Max
	
	
	4.3286
	1.1658
	17.6828
	0.3186
	1.8426
	0.6493

	Base
	45
	108
	Comb1
	Combination
	
	
	
	2.9915
	-0.0276
	10.7819
	0.0148
	0.1494
	-0.0274

	Base
	45
	108
	Comb2
	Combination
	
	
	
	2.5641
	-0.0236
	9.2416
	0.0127
	0.128
	-0.0235

	Base
	45
	108
	Comb3
	Combination
	
	
	
	2.5641
	-0.0236
	9.2416
	0.0127
	0.128
	-0.0235

	Base
	45
	108
	Comb4
	Combination
	Max
	
	
	3.1164
	0.036
	11.3801
	0.0241
	0.2922
	0.0129

	Base
	45
	108
	Comb4
	Combination
	Min
	
	
	2.0118
	-0.0832
	7.1031
	0.0012
	-0.0361
	-0.0599

	Base
	45
	108
	Comb5
	Combination
	Max
	
	
	3.1827
	0.143
	11.7685
	0.0582
	0.3913
	0.0693

	Base
	45
	108
	Comb5
	Combination
	Min
	
	
	1.9455
	-0.1902
	6.7147
	-0.0329
	-0.1353
	-0.1163

	Base
	45
	108
	Comb6
	Combination
	
	
	
	1.9231
	-0.0177
	6.9312
	0.0095
	0.096
	-0.0176

	Base
	45
	108
	Comb7
	Combination
	Max
	
	
	2.4754
	0.0419
	9.0697
	0.0209
	0.2602
	0.0188

	Base
	45
	108
	Comb7
	Combination
	Min
	
	
	1.3708
	-0.0773
	4.7927
	-0.002
	-0.0682
	-0.054

	Base
	45
	108
	Comb8
	Combination
	Max
	
	
	2.5416
	0.1489
	9.4581
	0.055
	0.3593
	0.0752

	Base
	45
	108
	Comb8
	Combination
	Min
	
	
	1.3045
	-0.1843
	4.4043
	-0.036
	-0.1673
	-0.1104

	Base
	45
	108
	ENVDIS
	Combination
	Max
	
	
	3.1827
	0.1489
	11.7685
	0.0582
	0.3913
	0.0752

	Base
	45
	108
	ENVDIS
	Combination
	Min
	
	
	1.3045
	-0.1902
	4.4043
	-0.036
	-0.1673
	-0.1163

	Base
	45
	108
	Serv1
	Combination
	
	
	
	2.1368
	-0.0197
	7.7013
	0.0105
	0.1067
	-0.0196

	Base
	45
	108
	Serv2
	Combination
	
	
	
	2.1368
	-0.0197
	7.7013
	0.0105
	0.1067
	-0.0196

	Base
	45
	108
	Serv3
	Combination
	
	
	
	2.1368
	-0.0197
	7.7013
	0.0105
	0.1067
	-0.0196

	Base
	45
	108
	Serv4
	Combination
	Max
	
	
	2.5234
	0.022
	9.1983
	0.0186
	0.2216
	0.0059

	Base
	45
	108
	Serv4
	Combination
	Min
	
	
	1.7501
	-0.0614
	6.2044
	0.0025
	-0.0082
	-0.0451

	Base
	45
	108
	Serv5
	Combination
	Max
	
	
	2.5696
	0.0969
	9.4696
	0.0424
	0.2909
	0.0453

	Base
	45
	108
	Serv5
	Combination
	Min
	
	
	1.7039
	-0.1363
	5.9331
	-0.0213
	-0.0776
	-0.0845

	Base
	45
	108
	Serv6
	Combination
	Max
	
	
	2.4267
	0.0116
	8.824
	0.0166
	0.1929
	-0.0005

	Base
	45
	108
	Serv6
	Combination
	Min
	
	
	1.8468
	-0.051
	6.5786
	0.0045
	0.0205
	-0.0387

	Base
	45
	108
	Serv7
	Combination
	Max
	
	
	2.4614
	0.0677
	9.0276
	0.0344
	0.2449
	0.0291

	Base
	45
	108
	Serv7
	Combination
	Min
	
	
	1.8121
	-0.1071
	6.3751
	-0.0134
	-0.0315
	-0.0683

	Base
	45
	108
	Serv8
	Combination
	
	
	
	1.2821
	-0.0118
	4.6208
	0.0063
	0.064
	-0.0118

	Base
	45
	108
	Serv9
	Combination
	Max
	
	
	1.6687
	0.0299
	6.1177
	0.0143
	0.1789
	0.0137

	Base
	45
	108
	Serv9
	Combination
	Min
	
	
	0.8954
	-0.0535
	3.1239
	-0.0017
	-0.0509
	-0.0372

	Base
	45
	108
	Serv10
	Combination
	Max
	
	
	1.7149
	0.1048
	6.3891
	0.0382
	0.2483
	0.0532

	Base
	45
	108
	Serv10
	Combination
	Min
	
	
	0.8492
	-0.1284
	2.8525
	-0.0255
	-0.1203
	-0.0767

	Base
	45
	108
	ENVSERV
	Combination
	Max
	
	
	2.5696
	0.1048
	9.4696
	0.0424
	0.2909
	0.0532

	Base
	45
	108
	ENVSERV
	Combination
	Min
	
	
	0.8492
	-0.1363
	2.8525
	-0.0255
	-0.1203
	-0.0845

	Base
	49
	110
	Dead
	LinStatic
	
	
	
	0.0138
	-1.4094
	6.5124
	0.0559
	0.0114
	0.0034

	Base
	49
	110
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	49
	110
	FHEx
	LinStatic
	
	
	
	-1.0961
	-3.3175
	7.419
	0.2547
	-0.2398
	-0.723

	Base
	49
	110
	FHEy
	LinStatic
	
	
	
	0.6479
	-4.5605
	24.4796
	2.1186
	0.0416
	0.4276

	Base
	49
	110
	Sx
	LinRespSpec
	Max
	
	
	1.881
	2.6244
	7.3382
	0.356
	0.3424
	1.2322

	Base
	49
	110
	Sy
	LinRespSpec
	Max
	
	
	0.5256
	2.4585
	14.045
	1.3648
	0.1354
	0.3236

	Base
	49
	110
	Comb1
	Combination
	
	
	
	0.0194
	-1.9731
	9.1173
	0.0783
	0.016
	0.0047

	Base
	49
	110
	Comb2
	Combination
	
	
	
	0.0166
	-1.6912
	7.8149
	0.0671
	0.0137
	0.0041

	Base
	49
	110
	Comb3
	Combination
	
	
	
	0.0166
	-1.6912
	7.8149
	0.0671
	0.0137
	0.0041

	Base
	49
	110
	Comb4
	Combination
	Max
	
	
	0.2853
	-1.3163
	8.8632
	0.118
	0.0626
	0.1801

	Base
	49
	110
	Comb4
	Combination
	Min
	
	
	-0.2521
	-2.0661
	6.7665
	0.0163
	-0.0352
	-0.172

	Base
	49
	110
	Comb5
	Combination
	Max
	
	
	0.0917
	-1.3399
	9.8219
	0.2622
	0.033
	0.0503

	Base
	49
	110
	Comb5
	Combination
	Min
	
	
	-0.0585
	-2.0426
	5.8078
	-0.1279
	-0.0057
	-0.0422

	Base
	49
	110
	Comb6
	Combination
	
	
	
	0.0125
	-1.2684
	5.8611
	0.0503
	0.0103
	0.003

	Base
	49
	110
	Comb7
	Combination
	Max
	
	
	0.2812
	-0.8935
	6.9095
	0.1012
	0.0592
	0.1791

	Base
	49
	110
	Comb7
	Combination
	Min
	
	
	-0.2563
	-1.6433
	4.8128
	-0.0005
	-0.0386
	-0.173

	Base
	49
	110
	Comb8
	Combination
	Max
	
	
	0.0876
	-0.9171
	7.8682
	0.2454
	0.0296
	0.0493

	Base
	49
	110
	Comb8
	Combination
	Min
	
	
	-0.0627
	-1.6197
	3.8541
	-0.1447
	-0.0091
	-0.0432

	Base
	49
	110
	ENVDIS
	Combination
	Max
	
	
	0.2853
	-0.8935
	9.8219
	0.2622
	0.0626
	0.1801

	Base
	49
	110
	ENVDIS
	Combination
	Min
	
	
	-0.2563
	-2.0661
	3.8541
	-0.1447
	-0.0386
	-0.173

	Base
	49
	110
	Serv1
	Combination
	
	
	
	0.0138
	-1.4094
	6.5124
	0.0559
	0.0114
	0.0034

	Base
	49
	110
	Serv2
	Combination
	
	
	
	0.0138
	-1.4094
	6.5124
	0.0559
	0.0114
	0.0034

	Base
	49
	110
	Serv3
	Combination
	
	
	
	0.0138
	-1.4094
	6.5124
	0.0559
	0.0114
	0.0034

	Base
	49
	110
	Serv4
	Combination
	Max
	
	
	0.2019
	-1.1469
	7.2462
	0.0915
	0.0456
	0.1266

	Base
	49
	110
	Serv4
	Combination
	Min
	
	
	-0.1743
	-1.6718
	5.7786
	0.0203
	-0.0228
	-0.1198

	Base
	49
	110
	Serv5
	Combination
	Max
	
	
	0.0664
	-1.1635
	7.9169
	0.1924
	0.0249
	0.0357

	Base
	49
	110
	Serv5
	Combination
	Min
	
	
	-0.0387
	-1.6552
	5.1079
	-0.0805
	-0.0021
	-0.029

	Base
	49
	110
	Serv6
	Combination
	Max
	
	
	0.1549
	-1.2125
	7.0628
	0.0826
	0.0371
	0.0958

	Base
	49
	110
	Serv6
	Combination
	Min
	
	
	-0.1272
	-1.6062
	5.962
	0.0292
	-0.0143
	-0.089

	Base
	49
	110
	Serv7
	Combination
	Max
	
	
	0.0533
	-1.225
	7.5658
	0.1583
	0.0216
	0.0277

	Base
	49
	110
	Serv7
	Combination
	Min
	
	
	-0.0256
	-1.5938
	5.459
	-0.0464
	0.0013
	-0.0209

	Base
	49
	110
	Serv8
	Combination
	
	
	
	0.0083
	-0.8456
	3.9074
	0.0336
	0.0068
	0.002

	Base
	49
	110
	Serv9
	Combination
	Max
	
	
	0.1964
	-0.5832
	4.6413
	0.0692
	0.0411
	0.1253

	Base
	49
	110
	Serv9
	Combination
	Min
	
	
	-0.1798
	-1.1081
	3.1736
	-0.002
	-0.0274
	-0.1212

	Base
	49
	110
	Serv10
	Combination
	Max
	
	
	0.0609
	-0.5998
	5.3119
	0.17
	0.0204
	0.0344

	Base
	49
	110
	Serv10
	Combination
	Min
	
	
	-0.0443
	-1.0915
	2.5029
	-0.1029
	-0.0067
	-0.0303

	Base
	49
	110
	ENVSERV
	Combination
	Max
	
	
	0.2019
	-0.5832
	7.9169
	0.1924
	0.0456
	0.1266

	Base
	49
	110
	ENVSERV
	Combination
	Min
	
	
	-0.1798
	-1.6718
	2.5029
	-0.1029
	-0.0274
	-0.1212

	Base
	52
	117
	Dead
	LinStatic
	
	
	
	0.0006
	1.2174
	5.1902
	0.1106
	0.0004
	-0.0051

	Base
	52
	117
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	52
	117
	FHEx
	LinStatic
	
	
	
	0.5017
	2.8648
	7.0055
	-0.2858
	-0.0915
	-0.1057

	Base
	52
	117
	FHEy
	LinStatic
	
	
	
	0.3001
	-8.2875
	-31.2016
	2.7742
	-0.0554
	-0.1581

	Base
	52
	117
	Sx
	LinRespSpec
	Max
	
	
	1.4057
	1.8323
	4.9075
	0.3243
	0.1819
	0.3949

	Base
	52
	117
	Sy
	LinRespSpec
	Max
	
	
	0.4575
	3.9608
	18.2704
	1.7768
	0.0778
	0.1513

	Base
	52
	117
	Comb1
	Combination
	
	
	
	0.0009
	1.7044
	7.2663
	0.1549
	0.0006
	-0.0072

	Base
	52
	117
	Comb2
	Combination
	
	
	
	0.0007
	1.4609
	6.2282
	0.1327
	0.0005
	-0.0061

	Base
	52
	117
	Comb3
	Combination
	
	
	
	0.0007
	1.4609
	6.2282
	0.1327
	0.0005
	-0.0061

	Base
	52
	117
	Comb4
	Combination
	Max
	
	
	0.2016
	1.7227
	6.9293
	0.1791
	0.0265
	0.0503

	Base
	52
	117
	Comb4
	Combination
	Min
	
	
	-0.2001
	1.1992
	5.5272
	0.0864
	-0.0255
	-0.0626

	Base
	52
	117
	Comb5
	Combination
	Max
	
	
	0.0661
	2.0269
	8.8391
	0.3866
	0.0116
	0.0155

	Base
	52
	117
	Comb5
	Combination
	Min
	
	
	-0.0646
	0.8949
	3.6174
	-0.1212
	-0.0106
	-0.0278

	Base
	52
	117
	Comb6
	Combination
	
	
	
	0.0006
	1.0957
	4.6712
	0.0996
	0.0004
	-0.0046

	Base
	52
	117
	Comb7
	Combination
	Max
	
	
	0.2014
	1.3575
	5.3722
	0.1459
	0.0264
	0.0518

	Base
	52
	117
	Comb7
	Combination
	Min
	
	
	-0.2003
	0.8339
	3.9701
	0.0532
	-0.0256
	-0.061

	Base
	52
	117
	Comb8
	Combination
	Max
	
	
	0.0659
	1.6617
	7.282
	0.3535
	0.0115
	0.017

	Base
	52
	117
	Comb8
	Combination
	Min
	
	
	-0.0648
	0.5297
	2.0603
	-0.1543
	-0.0107
	-0.0262

	Base
	52
	117
	ENVDIS
	Combination
	Max
	
	
	0.2016
	2.0269
	8.8391
	0.3866
	0.0265
	0.0518

	Base
	52
	117
	ENVDIS
	Combination
	Min
	
	
	-0.2003
	0.5297
	2.0603
	-0.1543
	-0.0256
	-0.0626

	Base
	52
	117
	Serv1
	Combination
	
	
	
	0.0006
	1.2174
	5.1902
	0.1106
	0.0004
	-0.0051

	Base
	52
	117
	Serv2
	Combination
	
	
	
	0.0006
	1.2174
	5.1902
	0.1106
	0.0004
	-0.0051

	Base
	52
	117
	Serv3
	Combination
	
	
	
	0.0006
	1.2174
	5.1902
	0.1106
	0.0004
	-0.0051

	Base
	52
	117
	Serv4
	Combination
	Max
	
	
	0.1412
	1.4007
	5.6809
	0.143
	0.0186
	0.0344

	Base
	52
	117
	Serv4
	Combination
	Min
	
	
	-0.14
	1.0342
	4.6994
	0.0782
	-0.0177
	-0.0446

	Base
	52
	117
	Serv5
	Combination
	Max
	
	
	0.0464
	1.6135
	7.0172
	0.2883
	0.0082
	0.01

	Base
	52
	117
	Serv5
	Combination
	Min
	
	
	-0.0451
	0.8214
	3.3632
	-0.0671
	-0.0073
	-0.0202

	Base
	52
	117
	Serv6
	Combination
	Max
	
	
	0.106
	1.3549
	5.5583
	0.1349
	0.0141
	0.0245

	Base
	52
	117
	Serv6
	Combination
	Min
	
	
	-0.1048
	1.08
	4.8221
	0.0863
	-0.0132
	-0.0347

	Base
	52
	117
	Serv7
	Combination
	Max
	
	
	0.0349
	1.5145
	6.5605
	0.2439
	0.0063
	0.0062

	Base
	52
	117
	Serv7
	Combination
	Min
	
	
	-0.0337
	0.9204
	3.8199
	-0.0226
	-0.0054
	-0.0165

	Base
	52
	117
	Serv8
	Combination
	
	
	
	0.0004
	0.7305
	3.1141
	0.0664
	0.0003
	-0.0031

	Base
	52
	117
	Serv9
	Combination
	Max
	
	
	0.1409
	0.9137
	3.6049
	0.0988
	0.0185
	0.0364

	Base
	52
	117
	Serv9
	Combination
	Min
	
	
	-0.1402
	0.5472
	2.6234
	0.0339
	-0.0179
	-0.0426

	Base
	52
	117
	Serv10
	Combination
	Max
	
	
	0.0461
	1.1265
	4.9412
	0.244
	0.008
	0.0121

	Base
	52
	117
	Serv10
	Combination
	Min
	
	
	-0.0454
	0.3344
	1.2871
	-0.1113
	-0.0075
	-0.0182

	Base
	52
	117
	ENVSERV
	Combination
	Max
	
	
	0.1412
	1.6135
	7.0172
	0.2883
	0.0186
	0.0364

	Base
	52
	117
	ENVSERV
	Combination
	Min
	
	
	-0.1402
	0.3344
	1.2871
	-0.1113
	-0.0179
	-0.0446

	Base
	53
	119
	Dead
	LinStatic
	
	
	
	1.4998
	0.0049
	6.5683
	0.0025
	0.0008
	-0.0048

	Base
	53
	119
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	53
	119
	FHEx
	LinStatic
	
	
	
	-5.6444
	0.0334
	-15.7337
	-0.0038
	-1.148
	0.0013

	Base
	53
	119
	FHEy
	LinStatic
	
	
	
	-0.0272
	0.7475
	-3.1401
	0.1531
	-0.8579
	0.0403

	Base
	53
	119
	Sx
	LinRespSpec
	Max
	
	
	3.1372
	0.498
	11.8324
	0.0555
	0.8958
	0.1776

	Base
	53
	119
	Sy
	LinRespSpec
	Max
	
	
	3.3674
	1.4621
	11.0589
	0.1551
	1.2197
	0.3998

	Base
	53
	119
	Comb1
	Combination
	
	
	
	2.0997
	0.0068
	9.1956
	0.0035
	0.0011
	-0.0068

	Base
	53
	119
	Comb2
	Combination
	
	
	
	1.7998
	0.0059
	7.8819
	0.003
	0.001
	-0.0058

	Base
	53
	119
	Comb3
	Combination
	
	
	
	1.7998
	0.0059
	7.8819
	0.003
	0.001
	-0.0058

	Base
	53
	119
	Comb4
	Combination
	Max
	
	
	2.2479
	0.077
	9.5723
	0.0109
	0.129
	0.0196

	Base
	53
	119
	Comb4
	Combination
	Min
	
	
	1.3516
	-0.0653
	6.1916
	-0.005
	-0.127
	-0.0312

	Base
	53
	119
	Comb5
	Combination
	Max
	
	
	2.281
	0.2148
	9.4622
	0.0251
	0.1753
	0.0513

	Base
	53
	119
	Comb5
	Combination
	Min
	
	
	1.3186
	-0.2031
	6.3016
	-0.0192
	-0.1733
	-0.0629

	Base
	53
	119
	Comb6
	Combination
	
	
	
	1.3498
	0.0044
	5.9114
	0.0022
	0.0007
	-0.0043

	Base
	53
	119
	Comb7
	Combination
	Max
	
	
	1.798
	0.0755
	7.6018
	0.0102
	0.1287
	0.021

	Base
	53
	119
	Comb7
	Combination
	Min
	
	
	0.9016
	-0.0667
	4.2211
	-0.0057
	-0.1272
	-0.0297

	Base
	53
	119
	Comb8
	Combination
	Max
	
	
	1.831
	0.2133
	7.4918
	0.0244
	0.175
	0.0528

	Base
	53
	119
	Comb8
	Combination
	Min
	
	
	0.8686
	-0.2045
	4.3311
	-0.0199
	-0.1736
	-0.0615

	Base
	53
	119
	ENVDIS
	Combination
	Max
	
	
	2.281
	0.2148
	9.5723
	0.0251
	0.1753
	0.0528

	Base
	53
	119
	ENVDIS
	Combination
	Min
	
	
	0.8686
	-0.2045
	4.2211
	-0.0199
	-0.1736
	-0.0629

	Base
	53
	119
	Serv1
	Combination
	
	
	
	1.4998
	0.0049
	6.5683
	0.0025
	0.0008
	-0.0048

	Base
	53
	119
	Serv2
	Combination
	
	
	
	1.4998
	0.0049
	6.5683
	0.0025
	0.0008
	-0.0048

	Base
	53
	119
	Serv3
	Combination
	
	
	
	1.4998
	0.0049
	6.5683
	0.0025
	0.0008
	-0.0048

	Base
	53
	119
	Serv4
	Combination
	Max
	
	
	1.8135
	0.0547
	7.7515
	0.008
	0.0904
	0.0129

	Base
	53
	119
	Serv4
	Combination
	Min
	
	
	1.1861
	-0.0449
	5.385
	-0.0031
	-0.0888
	-0.0226

	Base
	53
	119
	Serv5
	Combination
	Max
	
	
	1.8365
	0.1511
	7.6742
	0.018
	0.1228
	0.0352

	Base
	53
	119
	Serv5
	Combination
	Min
	
	
	1.1631
	-0.1413
	5.4624
	-0.013
	-0.1212
	-0.0448

	Base
	53
	119
	Serv6
	Combination
	Max
	
	
	1.7351
	0.0422
	7.4557
	0.0066
	0.068
	0.0085

	Base
	53
	119
	Serv6
	Combination
	Min
	
	
	1.2645
	-0.0325
	5.6808
	-0.0017
	-0.0664
	-0.0181

	Base
	53
	119
	Serv7
	Combination
	Max
	
	
	1.7523
	0.1145
	7.3977
	0.0141
	0.0923
	0.0252

	Base
	53
	119
	Serv7
	Combination
	Min
	
	
	1.2472
	-0.1048
	5.7388
	-0.0092
	-0.0907
	-0.0348

	Base
	53
	119
	Serv8
	Combination
	
	
	
	0.8999
	0.0029
	3.941
	0.0015
	0.0005
	-0.0029

	Base
	53
	119
	Serv9
	Combination
	Max
	
	
	1.2136
	0.0527
	5.1242
	0.007
	0.0901
	0.0149

	Base
	53
	119
	Serv9
	Combination
	Min
	
	
	0.5862
	-0.0469
	2.7577
	-0.0041
	-0.0891
	-0.0207

	Base
	53
	119
	Serv10
	Combination
	Max
	
	
	1.2366
	0.1491
	5.0469
	0.017
	0.1225
	0.0371

	Base
	53
	119
	Serv10
	Combination
	Min
	
	
	0.5631
	-0.1433
	2.8351
	-0.014
	-0.1215
	-0.0429

	Base
	53
	119
	ENVSERV
	Combination
	Max
	
	
	1.8365
	0.1511
	7.7515
	0.018
	0.1228
	0.0371

	Base
	53
	119
	ENVSERV
	Combination
	Min
	
	
	0.5631
	-0.1433
	2.7577
	-0.014
	-0.1215
	-0.0448

	Base
	55
	124
	Dead
	LinStatic
	
	
	
	1.206
	0.0044
	6.0828
	0.0034
	0.0236
	-0.0012

	Base
	55
	124
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	55
	124
	FHEx
	LinStatic
	
	
	
	-1.3134
	0.0181
	-6.2893
	-0.0054
	-0.4786
	0.0049

	Base
	55
	124
	FHEy
	LinStatic
	
	
	
	0.9536
	0.6869
	9.5809
	0.1319
	0.7209
	-0.1092

	Base
	55
	124
	Sx
	LinRespSpec
	Max
	
	
	1.0892
	0.1046
	5.6521
	0.0206
	0.4294
	0.0562

	Base
	55
	124
	Sy
	LinRespSpec
	Max
	
	
	1.0391
	0.571
	9.2503
	0.0872
	0.697
	0.1746

	Base
	55
	124
	Comb1
	Combination
	
	
	
	1.6884
	0.0062
	8.516
	0.0048
	0.0331
	-0.0017

	Base
	55
	124
	Comb2
	Combination
	
	
	
	1.4472
	0.0053
	7.2994
	0.0041
	0.0284
	-0.0014

	Base
	55
	124
	Comb3
	Combination
	
	
	
	1.4472
	0.0053
	7.2994
	0.0041
	0.0284
	-0.0014

	Base
	55
	124
	Comb4
	Combination
	Max
	
	
	1.6028
	0.0203
	8.1068
	0.0071
	0.0897
	0.0066

	Base
	55
	124
	Comb4
	Combination
	Min
	
	
	1.2916
	-0.0096
	6.492
	0.0012
	-0.033
	-0.0094

	Base
	55
	124
	Comb5
	Combination
	Max
	
	
	1.5956
	0.0869
	8.6213
	0.0166
	0.128
	0.0235

	Base
	55
	124
	Comb5
	Combination
	Min
	
	
	1.2987
	-0.0763
	5.9775
	-0.0083
	-0.0712
	-0.0264

	Base
	55
	124
	Comb6
	Combination
	
	
	
	1.0854
	0.004
	5.4746
	0.0031
	0.0213
	-0.0011

	Base
	55
	124
	Comb7
	Combination
	Max
	
	
	1.241
	0.0189
	6.282
	0.006
	0.0826
	0.007

	Base
	55
	124
	Comb7
	Combination
	Min
	
	
	0.9298
	-0.0109
	4.6671
	0.0002
	-0.0401
	-0.0091

	Base
	55
	124
	Comb8
	Combination
	Max
	
	
	1.2338
	0.0856
	6.7964
	0.0156
	0.1209
	0.0239

	Base
	55
	124
	Comb8
	Combination
	Min
	
	
	0.9369
	-0.0776
	4.1527
	-0.0094
	-0.0783
	-0.026

	Base
	55
	124
	ENVDIS
	Combination
	Max
	
	
	1.6884
	0.0869
	8.6213
	0.0166
	0.128
	0.0239

	Base
	55
	124
	ENVDIS
	Combination
	Min
	
	
	0.9298
	-0.0776
	4.1527
	-0.0094
	-0.0783
	-0.0264

	Base
	55
	124
	Serv1
	Combination
	
	
	
	1.206
	0.0044
	6.0828
	0.0034
	0.0236
	-0.0012

	Base
	55
	124
	Serv2
	Combination
	
	
	
	1.206
	0.0044
	6.0828
	0.0034
	0.0236
	-0.0012

	Base
	55
	124
	Serv3
	Combination
	
	
	
	1.206
	0.0044
	6.0828
	0.0034
	0.0236
	-0.0012

	Base
	55
	124
	Serv4
	Combination
	Max
	
	
	1.3149
	0.0149
	6.648
	0.0055
	0.0666
	0.0044

	Base
	55
	124
	Serv4
	Combination
	Min
	
	
	1.097
	-0.006
	5.5176
	0.0014
	-0.0193
	-0.0068

	Base
	55
	124
	Serv5
	Combination
	Max
	
	
	1.3099
	0.0616
	7.0079
	0.0122
	0.0933
	0.0163

	Base
	55
	124
	Serv5
	Combination
	Min
	
	
	1.1021
	-0.0527
	5.1578
	-0.0053
	-0.0461
	-0.0186

	Base
	55
	124
	Serv6
	Combination
	Max
	
	
	1.2877
	0.0123
	6.5067
	0.005
	0.0558
	0.003

	Base
	55
	124
	Serv6
	Combination
	Min
	
	
	1.1243
	-0.0034
	5.6589
	0.0019
	-0.0086
	-0.0054

	Base
	55
	124
	Serv7
	Combination
	Max
	
	
	1.2839
	0.0473
	6.7766
	0.01
	0.0759
	0.0119

	Base
	55
	124
	Serv7
	Combination
	Min
	
	
	1.128
	-0.0384
	5.3891
	-0.0031
	-0.0286
	-0.0143

	Base
	55
	124
	Serv8
	Combination
	
	
	
	0.7236
	0.0027
	3.6497
	0.0021
	0.0142
	-0.0007

	Base
	55
	124
	Serv9
	Combination
	Max
	
	
	0.8325
	0.0131
	4.2149
	0.0041
	0.0571
	0.0049

	Base
	55
	124
	Serv9
	Combination
	Min
	
	
	0.6147
	-0.0078
	3.0845
	9.541E-06
	-0.0287
	-0.0063

	Base
	55
	124
	Serv10
	Combination
	Max
	
	
	0.8275
	0.0598
	4.5747
	0.0108
	0.0839
	0.0168

	Base
	55
	124
	Serv10
	Combination
	Min
	
	
	0.6197
	-0.0544
	2.7247
	-0.0067
	-0.0555
	-0.0182

	Base
	55
	124
	ENVSERV
	Combination
	Max
	
	
	1.3149
	0.0616
	7.0079
	0.0122
	0.0933
	0.0168

	Base
	55
	124
	ENVSERV
	Combination
	Min
	
	
	0.6147
	-0.0544
	2.7247
	-0.0067
	-0.0555
	-0.0186

	Base
	56
	125
	Dead
	LinStatic
	
	
	
	-1.0829
	-0.0064
	5.2275
	0.0043
	0.041
	0.0027

	Base
	56
	125
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	56
	125
	FHEx
	LinStatic
	
	
	
	-0.4967
	-0.0161
	6.2893
	-0.0028
	-0.4722
	-0.0001

	Base
	56
	125
	FHEy
	LinStatic
	
	
	
	1.8037
	-0.8041
	-9.5809
	0.3367
	0.7275
	-0.065

	Base
	56
	125
	Sx
	LinRespSpec
	Max
	
	
	0.5544
	0.1143
	5.6521
	0.0418
	0.4252
	0.0383

	Base
	56
	125
	Sy
	LinRespSpec
	Max
	
	
	1.6264
	0.6483
	9.2503
	0.2601
	0.7015
	0.1378

	Base
	56
	125
	Comb1
	Combination
	
	
	
	-1.516
	-0.0089
	7.3184
	0.006
	0.0574
	0.0038

	Base
	56
	125
	Comb2
	Combination
	
	
	
	-1.2995
	-0.0076
	6.2729
	0.0051
	0.0492
	0.0033

	Base
	56
	125
	Comb3
	Combination
	
	
	
	-1.2995
	-0.0076
	6.2729
	0.0051
	0.0492
	0.0033

	Base
	56
	125
	Comb4
	Combination
	Max
	
	
	-1.2202
	0.0087
	7.0804
	0.0111
	0.11
	0.0088

	Base
	56
	125
	Comb4
	Combination
	Min
	
	
	-1.3787
	-0.024
	5.4655
	-0.0009
	-0.0115
	-0.0022

	Base
	56
	125
	Comb5
	Combination
	Max
	
	
	-1.067
	0.085
	7.5948
	0.0423
	0.1495
	0.023

	Base
	56
	125
	Comb5
	Combination
	Min
	
	
	-1.5319
	-0.1003
	4.9511
	-0.0321
	-0.051
	-0.0164

	Base
	56
	125
	Comb6
	Combination
	
	
	
	-0.9746
	-0.0057
	4.7047
	0.0038
	0.0369
	0.0025

	Base
	56
	125
	Comb7
	Combination
	Max
	
	
	-0.8954
	0.0106
	5.5122
	0.0098
	0.0977
	0.0079

	Base
	56
	125
	Comb7
	Combination
	Min
	
	
	-1.0538
	-0.0221
	3.8973
	-0.0021
	-0.0238
	-0.003

	Base
	56
	125
	Comb8
	Combination
	Max
	
	
	-0.7422
	0.0869
	6.0266
	0.041
	0.1372
	0.0222

	Base
	56
	125
	Comb8
	Combination
	Min
	
	
	-1.207
	-0.0984
	3.3828
	-0.0333
	-0.0633
	-0.0172

	Base
	56
	125
	ENVDIS
	Combination
	Max
	
	
	-0.7422
	0.0869
	7.5948
	0.0423
	0.1495
	0.023

	Base
	56
	125
	ENVDIS
	Combination
	Min
	
	
	-1.5319
	-0.1003
	3.3828
	-0.0333
	-0.0633
	-0.0172

	Base
	56
	125
	Serv1
	Combination
	
	
	
	-1.0829
	-0.0064
	5.2275
	0.0043
	0.041
	0.0027

	Base
	56
	125
	Serv2
	Combination
	
	
	
	-1.0829
	-0.0064
	5.2275
	0.0043
	0.041
	0.0027

	Base
	56
	125
	Serv3
	Combination
	
	
	
	-1.0829
	-0.0064
	5.2275
	0.0043
	0.041
	0.0027

	Base
	56
	125
	Serv4
	Combination
	Max
	
	
	-1.0274
	0.0051
	5.7927
	0.0084
	0.0835
	0.0066

	Base
	56
	125
	Serv4
	Combination
	Min
	
	
	-1.1383
	-0.0178
	4.6623
	0.0001
	-0.0015
	-0.0011

	Base
	56
	125
	Serv5
	Combination
	Max
	
	
	-0.9202
	0.0585
	6.1525
	0.0303
	0.1112
	0.0165

	Base
	56
	125
	Serv5
	Combination
	Min
	
	
	-1.2455
	-0.0712
	4.3024
	-0.0218
	-0.0291
	-0.011

	Base
	56
	125
	Serv6
	Combination
	Max
	
	
	-1.0413
	0.0022
	5.6514
	0.0074
	0.0729
	0.0056

	Base
	56
	125
	Serv6
	Combination
	Min
	
	
	-1.1245
	-0.0149
	4.8036
	0.0011
	0.0091
	-0.0001

	Base
	56
	125
	Serv7
	Combination
	Max
	
	
	-0.9609
	0.0422
	5.9212
	0.0238
	0.0936
	0.0131

	Base
	56
	125
	Serv7
	Combination
	Min
	
	
	-1.2049
	-0.055
	4.5337
	-0.0153
	-0.0116
	-0.0076

	Base
	56
	125
	Serv8
	Combination
	
	
	
	-0.6497
	-0.0038
	3.1365
	0.0026
	0.0246
	0.0016

	Base
	56
	125
	Serv9
	Combination
	Max
	
	
	-0.5943
	0.0076
	3.7017
	0.0067
	0.0671
	0.0055

	Base
	56
	125
	Serv9
	Combination
	Min
	
	
	-0.7052
	-0.0153
	2.5713
	-0.0016
	-0.0179
	-0.0022

	Base
	56
	125
	Serv10
	Combination
	Max
	
	
	-0.4871
	0.061
	4.0615
	0.0286
	0.0948
	0.0154

	Base
	56
	125
	Serv10
	Combination
	Min
	
	
	-0.8124
	-0.0687
	2.2114
	-0.0235
	-0.0455
	-0.0121

	Base
	56
	125
	ENVSERV
	Combination
	Max
	
	
	-0.4871
	0.061
	6.1525
	0.0303
	0.1112
	0.0165

	Base
	56
	125
	ENVSERV
	Combination
	Min
	
	
	-1.2455
	-0.0712
	2.2114
	-0.0235
	-0.0455
	-0.0121

	Base
	57
	129
	Dead
	LinStatic
	
	
	
	-0.0038
	1.447
	5.8605
	0.0782
	0.0067
	-0.0007

	Base
	57
	129
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	57
	129
	FHEx
	LinStatic
	
	
	
	0.4905
	0.6675
	1.0603
	-0.148
	-0.106
	-0.0709

	Base
	57
	129
	FHEy
	LinStatic
	
	
	
	-0.108
	-3.5855
	-21.3762
	2.1629
	0.0621
	0.0064

	Base
	57
	129
	Sx
	LinRespSpec
	Max
	
	
	1.1337
	1.522
	4.142
	0.4452
	0.1569
	0.2432

	Base
	57
	129
	Sy
	LinRespSpec
	Max
	
	
	0.228
	1.8214
	14.8136
	1.5064
	0.0723
	0.0514

	Base
	57
	129
	Comb1
	Combination
	
	
	
	-0.0053
	2.0259
	8.2047
	0.1095
	0.0094
	-0.001

	Base
	57
	129
	Comb2
	Combination
	
	
	
	-0.0046
	1.7365
	7.0326
	0.0939
	0.008
	-0.0008

	Base
	57
	129
	Comb3
	Combination
	
	
	
	-0.0046
	1.7365
	7.0326
	0.0939
	0.008
	-0.0008

	Base
	57
	129
	Comb4
	Combination
	Max
	
	
	0.1574
	1.9539
	7.6243
	0.1575
	0.0304
	0.0339

	Base
	57
	129
	Comb4
	Combination
	Min
	
	
	-0.1665
	1.519
	6.4409
	0.0303
	-0.0144
	-0.0356

	Base
	57
	129
	Comb5
	Combination
	Max
	
	
	0.028
	1.9967
	9.1495
	0.3091
	0.0184
	0.0065

	Base
	57
	129
	Comb5
	Combination
	Min
	
	
	-0.0372
	1.4762
	4.9157
	-0.1214
	-0.0023
	-0.0082

	Base
	57
	129
	Comb6
	Combination
	
	
	
	-0.0034
	1.3023
	5.2744
	0.0704
	0.006
	-0.0006

	Base
	57
	129
	Comb7
	Combination
	Max
	
	
	0.1585
	1.5198
	5.8662
	0.134
	0.0284
	0.0341

	Base
	57
	129
	Comb7
	Combination
	Min
	
	
	-0.1654
	1.0849
	4.6827
	0.0068
	-0.0164
	-0.0354

	Base
	57
	129
	Comb8
	Combination
	Max
	
	
	0.0291
	1.5626
	7.3913
	0.2856
	0.0164
	0.0067

	Base
	57
	129
	Comb8
	Combination
	Min
	
	
	-0.036
	1.0421
	3.1576
	-0.1449
	-0.0043
	-0.008

	Base
	57
	129
	ENVDIS
	Combination
	Max
	
	
	0.1585
	2.0259
	9.1495
	0.3091
	0.0304
	0.0341

	Base
	57
	129
	ENVDIS
	Combination
	Min
	
	
	-0.1665
	1.0421
	3.1576
	-0.1449
	-0.0164
	-0.0356

	Base
	57
	129
	Serv1
	Combination
	
	
	
	-0.0038
	1.447
	5.8605
	0.0782
	0.0067
	-0.0007

	Base
	57
	129
	Serv2
	Combination
	
	
	
	-0.0038
	1.447
	5.8605
	0.0782
	0.0067
	-0.0007

	Base
	57
	129
	Serv3
	Combination
	
	
	
	-0.0038
	1.447
	5.8605
	0.0782
	0.0067
	-0.0007

	Base
	57
	129
	Serv4
	Combination
	Max
	
	
	0.1096
	1.5992
	6.2747
	0.1227
	0.0224
	0.0236

	Base
	57
	129
	Serv4
	Combination
	Min
	
	
	-0.1172
	1.2948
	5.4463
	0.0337
	-0.009
	-0.025

	Base
	57
	129
	Serv5
	Combination
	Max
	
	
	0.019
	1.6292
	7.3419
	0.2288
	0.0139
	0.0044

	Base
	57
	129
	Serv5
	Combination
	Min
	
	
	-0.0266
	1.2649
	4.3791
	-0.0724
	-0.0005
	-0.0058

	Base
	57
	129
	Serv6
	Combination
	Max
	
	
	0.0812
	1.5612
	6.1711
	0.1116
	0.0185
	0.0175

	Base
	57
	129
	Serv6
	Combination
	Min
	
	
	-0.0888
	1.3329
	5.5499
	0.0448
	-0.0051
	-0.0189

	Base
	57
	129
	Serv7
	Combination
	Max
	
	
	0.0133
	1.5836
	6.9715
	0.1912
	0.0121
	0.0032

	Base
	57
	129
	Serv7
	Combination
	Min
	
	
	-0.0209
	1.3104
	4.7495
	-0.0348
	0.0013
	-0.0045

	Base
	57
	129
	Serv8
	Combination
	
	
	
	-0.0023
	0.8682
	3.5163
	0.0469
	0.004
	-0.0004

	Base
	57
	129
	Serv9
	Combination
	Max
	
	
	0.1111
	1.0204
	3.9305
	0.0914
	0.0197
	0.0239

	Base
	57
	129
	Serv9
	Combination
	Min
	
	
	-0.1157
	0.716
	3.1021
	0.0024
	-0.0117
	-0.0247

	Base
	57
	129
	Serv10
	Combination
	Max
	
	
	0.0205
	1.0504
	4.9977
	0.1976
	0.0112
	0.0047

	Base
	57
	129
	Serv10
	Combination
	Min
	
	
	-0.0251
	0.6861
	2.0349
	-0.1037
	-0.0032
	-0.0056

	Base
	57
	129
	ENVSERV
	Combination
	Max
	
	
	0.1111
	1.6292
	7.3419
	0.2288
	0.0224
	0.0239

	Base
	57
	129
	ENVSERV
	Combination
	Min
	
	
	-0.1172
	0.6861
	2.0349
	-0.1037
	-0.0117
	-0.025

	Base
	58
	132
	Dead
	LinStatic
	
	
	
	-0.0007
	-1.5611
	6.6554
	0.0464
	-0.0033
	-0.0044

	Base
	58
	132
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	58
	132
	FHEx
	LinStatic
	
	
	
	0.4775
	3.9653
	-8.4726
	-0.2951
	-0.0843
	0.0335

	Base
	58
	132
	FHEy
	LinStatic
	
	
	
	0.7974
	-5.163
	23.2153
	2.0666
	-0.0505
	0.1499

	Base
	58
	132
	Sx
	LinRespSpec
	Max
	
	
	1.4758
	3.2394
	8.6387
	0.4178
	0.1291
	0.2348

	Base
	58
	132
	Sy
	LinRespSpec
	Max
	
	
	0.6899
	3.712
	12.103
	1.2356
	0.0718
	0.1664

	Base
	58
	132
	Comb1
	Combination
	
	
	
	-0.001
	-2.1855
	9.3175
	0.065
	-0.0046
	-0.0062

	Base
	58
	132
	Comb2
	Combination
	
	
	
	-0.0008
	-1.8733
	7.9864
	0.0557
	-0.0039
	-0.0053

	Base
	58
	132
	Comb3
	Combination
	
	
	
	-0.0008
	-1.8733
	7.9864
	0.0557
	-0.0039
	-0.0053

	Base
	58
	132
	Comb4
	Combination
	Max
	
	
	0.21
	-1.4105
	9.2205
	0.1154
	0.0145
	0.0282

	Base
	58
	132
	Comb4
	Combination
	Min
	
	
	-0.2116
	-2.3361
	6.7523
	-0.004
	-0.0224
	-0.0389

	Base
	58
	132
	Comb5
	Combination
	Max
	
	
	0.0978
	-1.3429
	9.716
	0.2323
	0.0063
	0.0184

	Base
	58
	132
	Comb5
	Combination
	Min
	
	
	-0.0994
	-2.4038
	6.2569
	-0.1209
	-0.0142
	-0.0291

	Base
	58
	132
	Comb6
	Combination
	
	
	
	-0.0006
	-1.405
	5.9898
	0.0418
	-0.003
	-0.004

	Base
	58
	132
	Comb7
	Combination
	Max
	
	
	0.2102
	-0.9422
	7.2239
	0.1015
	0.0155
	0.0295

	Base
	58
	132
	Comb7
	Combination
	Min
	
	
	-0.2114
	-1.8678
	4.7557
	-0.0179
	-0.0214
	-0.0375

	Base
	58
	132
	Comb8
	Combination
	Max
	
	
	0.098
	-0.8745
	7.7193
	0.2183
	0.0073
	0.0198

	Base
	58
	132
	Comb8
	Combination
	Min
	
	
	-0.0992
	-1.9354
	4.2603
	-0.1348
	-0.0132
	-0.0278

	Base
	58
	132
	ENVDIS
	Combination
	Max
	
	
	0.2102
	-0.8745
	9.716
	0.2323
	0.0155
	0.0295

	Base
	58
	132
	ENVDIS
	Combination
	Min
	
	
	-0.2116
	-2.4038
	4.2603
	-0.1348
	-0.0224
	-0.0389

	Base
	58
	132
	Serv1
	Combination
	
	
	
	-0.0007
	-1.5611
	6.6554
	0.0464
	-0.0033
	-0.0044

	Base
	58
	132
	Serv2
	Combination
	
	
	
	-0.0007
	-1.5611
	6.6554
	0.0464
	-0.0033
	-0.0044

	Base
	58
	132
	Serv3
	Combination
	
	
	
	-0.0007
	-1.5611
	6.6554
	0.0464
	-0.0033
	-0.0044

	Base
	58
	132
	Serv4
	Combination
	Max
	
	
	0.1469
	-1.2372
	7.5192
	0.0882
	0.0096
	0.019

	Base
	58
	132
	Serv4
	Combination
	Min
	
	
	-0.1483
	-1.885
	5.7915
	0.0046
	-0.0162
	-0.0279

	Base
	58
	132
	Serv5
	Combination
	Max
	
	
	0.0683
	-1.1899
	7.8657
	0.17
	0.0039
	0.0122

	Base
	58
	132
	Serv5
	Combination
	Min
	
	
	-0.0697
	-1.9323
	5.4451
	-0.0771
	-0.0105
	-0.0211

	Base
	58
	132
	Serv6
	Combination
	Max
	
	
	0.11
	-1.3181
	7.3033
	0.0778
	0.0064
	0.0132

	Base
	58
	132
	Serv6
	Combination
	Min
	
	
	-0.1114
	-1.8041
	6.0075
	0.0151
	-0.013
	-0.0221

	Base
	58
	132
	Serv7
	Combination
	Max
	
	
	0.0511
	-1.2827
	7.5631
	0.1391
	0.0021
	0.008

	Base
	58
	132
	Serv7
	Combination
	Min
	
	
	-0.0524
	-1.8395
	5.7476
	-0.0462
	-0.0087
	-0.0169

	Base
	58
	132
	Serv8
	Combination
	
	
	
	-0.0004
	-0.9367
	3.9932
	0.0279
	-0.002
	-0.0027

	Base
	58
	132
	Serv9
	Combination
	Max
	
	
	0.1472
	-0.6127
	4.8571
	0.0696
	0.0109
	0.0208

	Base
	58
	132
	Serv9
	Combination
	Min
	
	
	-0.148
	-1.2606
	3.1293
	-0.0139
	-0.0149
	-0.0262

	Base
	58
	132
	Serv10
	Combination
	Max
	
	
	0.0686
	-0.5655
	5.2035
	0.1514
	0.0052
	0.014

	Base
	58
	132
	Serv10
	Combination
	Min
	
	
	-0.0694
	-1.3079
	2.7829
	-0.0957
	-0.0092
	-0.0193

	Base
	58
	132
	ENVSERV
	Combination
	Max
	
	
	0.1472
	-0.5655
	7.8657
	0.17
	0.0109
	0.0208

	Base
	58
	132
	ENVSERV
	Combination
	Min
	
	
	-0.1483
	-1.9323
	2.7829
	-0.0957
	-0.0162
	-0.0279

	Base
	59
	134
	Dead
	LinStatic
	
	
	
	-1.8731
	-0.0061
	7.3982
	0.0032
	-0.0641
	0.0017

	Base
	59
	134
	Live
	LinStatic
	
	
	
	0
	0
	0
	0
	0
	0

	Base
	59
	134
	FHEx
	LinStatic
	
	
	
	-5.8651
	0.0195
	21.2115
	0.0036
	-1.8934
	0.0062

	Base
	59
	134
	FHEy
	LinStatic
	
	
	
	-1.9388
	1.2946
	13.3845
	0.1718
	-2.1259
	-0.7524

	Base
	59
	134
	Sx
	LinRespSpec
	Max
	
	
	5.9378
	1.0328
	20.3592
	0.0515
	1.8499
	0.6009

	Base
	59
	134
	Sy
	LinRespSpec
	Max
	
	
	3.6565
	1.6933
	21.6822
	0.1312
	2.4825
	1.0609

	Base
	59
	134
	Comb1
	Combination
	
	
	
	-2.6223
	-0.0085
	10.3575
	0.0045
	-0.0897
	0.0024

	Base
	59
	134
	Comb2
	Combination
	
	
	
	-2.2477
	-0.0073
	8.8779
	0.0038
	-0.0769
	0.0021

	Base
	59
	134
	Comb3
	Combination
	
	
	
	-2.2477
	-0.0073
	8.8779
	0.0038
	-0.0769
	0.0021

	Base
	59
	134
	Comb4
	Combination
	Max
	
	
	-1.3994
	0.1402
	11.7863
	0.0112
	0.1874
	0.0879

	Base
	59
	134
	Comb4
	Combination
	Min
	
	
	-3.0959
	-0.1549
	5.9694
	-0.0035
	-0.3412
	-0.0838

	Base
	59
	134
	Comb5
	Combination
	Max
	
	
	-1.7252
	0.2346
	11.9763
	0.0226
	0.2779
	0.1537

	Base
	59
	134
	Comb5
	Combination
	Min
	
	
	-2.7702
	-0.2493
	5.7795
	-0.0149
	-0.4316
	-0.1495

	Base
	59
	134
	Comb6
	Combination
	
	
	
	-1.6858
	-0.0055
	6.6584
	0.0029
	-0.0577
	0.0016

	Base
	59
	134
	Comb7
	Combination
	Max
	
	
	-0.8375
	0.1421
	9.5669
	0.0102
	0.2066
	0.0874

	Base
	59
	134
	Comb7
	Combination
	Min
	
	
	-2.534
	-0.153
	3.7499
	-0.0045
	-0.3219
	-0.0843

	Base
	59
	134
	Comb8
	Combination
	Max
	
	
	-1.1633
	0.2365
	9.7568
	0.0216
	0.2971
	0.1532

	Base
	59
	134
	Comb8
	Combination
	Min
	
	
	-2.2083
	-0.2475
	3.56
	-0.0159
	-0.4124
	-0.15

	Base
	59
	134
	ENVDIS
	Combination
	Max
	
	
	-0.8375
	0.2365
	11.9763
	0.0226
	0.2971
	0.1537

	Base
	59
	134
	ENVDIS
	Combination
	Min
	
	
	-3.0959
	-0.2493
	3.56
	-0.0159
	-0.4316
	-0.15

	Base
	59
	134
	Serv1
	Combination
	
	
	
	-1.8731
	-0.0061
	7.3982
	0.0032
	-0.0641
	0.0017

	Base
	59
	134
	Serv2
	Combination
	
	
	
	-1.8731
	-0.0061
	7.3982
	0.0032
	-0.0641
	0.0017

	Base
	59
	134
	Serv3
	Combination
	
	
	
	-1.8731
	-0.0061
	7.3982
	0.0032
	-0.0641
	0.0017

	Base
	59
	134
	Serv4
	Combination
	Max
	
	
	-1.2793
	0.0972
	9.4342
	0.0083
	0.1209
	0.0618

	Base
	59
	134
	Serv4
	Combination
	Min
	
	
	-2.4669
	-0.1094
	5.3623
	-0.002
	-0.2491
	-0.0584

	Base
	59
	134
	Serv5
	Combination
	Max
	
	
	-1.5074
	0.1632
	9.5665
	0.0163
	0.1842
	0.1078

	Base
	59
	134
	Serv5
	Combination
	Min
	
	
	-2.2387
	-0.1754
	5.23
	-0.0099
	-0.3123
	-0.1044

	Base
	59
	134
	Serv6
	Combination
	Max
	
	
	-1.4277
	0.0714
	8.9252
	0.007
	0.0747
	0.0468

	Base
	59
	134
	Serv6
	Combination
	Min
	
	
	-2.3184
	-0.0836
	5.8713
	-0.0007
	-0.2028
	-0.0433

	Base
	59
	134
	Serv7
	Combination
	Max
	
	
	-1.5988
	0.1209
	9.0244
	0.013
	0.1221
	0.0813

	Base
	59
	134
	Serv7
	Combination
	Min
	
	
	-2.1473
	-0.1331
	5.7721
	-0.0067
	-0.2503
	-0.0778

	Base
	59
	134
	Serv8
	Combination
	
	
	
	-1.1238
	-0.0037
	4.4389
	0.0019
	-0.0384
	0.001

	Base
	59
	134
	Serv9
	Combination
	Max
	
	
	-0.5301
	0.0996
	6.4749
	0.0071
	0.1465
	0.0611

	Base
	59
	134
	Serv9
	Combination
	Min
	
	
	-1.7176
	-0.1069
	2.403
	-0.0032
	-0.2234
	-0.059

	Base
	59
	134
	Serv10
	Combination
	Max
	
	
	-0.7582
	0.1657
	6.6072
	0.015
	0.2098
	0.1071

	Base
	59
	134
	Serv10
	Combination
	Min
	
	
	-1.4895
	-0.173
	2.2707
	-0.0112
	-0.2867
	-0.105

	Base
	59
	134
	ENVSERV
	Combination
	Max
	
	
	-0.5301
	0.1657
	9.5665
	0.0163
	0.2098
	0.1078

	Base
	59
	134
	ENVSERV
	Combination
	Min
	
	
	-2.4669
	-0.1754
	2.2707
	-0.0112
	-0.3123
	-0.105



5.4 Modal Results
Table 5.5 - Modal Periods And Frequencies
	Case
	Mode
	Period
sec
	Frequency
cyc/sec
	CircFreq
rad/sec
	Eigenvalue
rad2/sec2

	Modal
	1
	0.175
	5.721
	35.9451
	1292.0508

	Modal
	2
	0.082
	12.195
	76.6221
	5870.9408

	Modal
	3
	0.079
	12.681
	79.6755
	6348.1883

	Modal
	4
	0.052
	19.168
	120.4372
	14505.1169

	Modal
	5
	0.047
	21.193
	133.1618
	17732.0692

	Modal
	6
	0.041
	24.685
	155.1
	24056.0099

	Modal
	7
	0.033
	30.434
	191.2255
	36567.1865

	Modal
	8
	0.028
	35.217
	221.2742
	48962.2817

	Modal
	9
	0.027
	37.285
	234.2673
	54881.1798

	Modal
	10
	0.027
	37.626
	236.4109
	55890.1249

	Modal
	11
	0.026
	38.405
	241.3074
	58229.2447

	Modal
	12
	0.025
	39.273
	246.7614
	60891.1794

	Modal
	13
	0.025
	39.998
	251.3145
	63158.9991

	Modal
	14
	0.024
	40.893
	256.9367
	66016.4862

	Modal
	15
	0.024
	41.909
	263.3203
	69337.5866



Table 5.6 - Modal Participating Mass Ratios (Part 1 of 2)
	Case
	Mode
	Period
sec
	UX
	UY
	UZ
	SumUX
	SumUY
	SumUZ
	RX
	RY
	RZ
	SumRX

	Modal
	1
	0.175
	0
	0.0002
	0
	0
	0.0002
	0
	0.0002
	0
	0
	0.0002

	Modal
	2
	0.082
	0.0003
	0.7071
	0
	0.0003
	0.7073
	0
	0.7071
	0.0003
	0.0038
	0.7073

	Modal
	3
	0.079
	0.0437
	0.0073
	0
	0.0439
	0.7145
	0
	0.0073
	0.0437
	0.2205
	0.7145

	Modal
	4
	0.052
	0.0001
	0.0032
	0
	0.0441
	0.7177
	0
	0.0032
	0.0001
	0.0106
	0.7177

	Modal
	5
	0.047
	0.0027
	0.0005
	0
	0.0468
	0.7182
	0
	0.0005
	0.0027
	0.0264
	0.7182

	Modal
	6
	0.041
	0.0002
	0.0009
	0
	0.047
	0.7191
	0
	0.0009
	0.0002
	0.0096
	0.7191

	Modal
	7
	0.033
	0.0389
	0.0045
	0
	0.0859
	0.7237
	0
	0.0045
	0.0389
	0.2345
	0.7237

	Modal
	8
	0.028
	0.0031
	0.1052
	0
	0.089
	0.8289
	0
	0.1052
	0.0031
	0.0219
	0.8289

	Modal
	9
	0.027
	0.0226
	0.0101
	0
	0.1116
	0.839
	0
	0.0101
	0.0226
	0.0044
	0.839

	Modal
	10
	0.027
	0.0708
	0.0051
	0
	0.1824
	0.8442
	0
	0.0051
	0.0708
	0.0001
	0.8442

	Modal
	11
	0.026
	0.153
	0.0084
	0
	0.3353
	0.8526
	0
	0.0084
	0.153
	0.0042
	0.8526

	Modal
	12
	0.025
	0.2412
	0.0274
	0
	0.5765
	0.88
	0
	0.0274
	0.2412
	0.0037
	0.88

	Modal
	13
	0.025
	0.0381
	0.0008
	0
	0.6146
	0.8808
	0
	0.0008
	0.0381
	0.1592
	0.8808

	Modal
	14
	0.024
	0.003
	0.0015
	0
	0.6176
	0.8823
	0
	0.0015
	0.003
	0.0175
	0.8823

	Modal
	15
	0.024
	0.0051
	0.0173
	0
	0.6228
	0.8996
	0
	0.0173
	0.0051
	0.0054
	0.8996



Table 5.6 - Modal Participating Mass Ratios (Part 2 of 2)
	SumRY
	SumRZ

	0
	0

	0.0003
	0.0038

	0.0439
	0.2243

	0.0441
	0.2349

	0.0468
	0.2613

	0.047
	0.2709

	0.0859
	0.5053

	0.089
	0.5273

	0.1116
	0.5317

	0.1824
	0.5317

	0.3353
	0.5359

	0.5765
	0.5396

	0.6146
	0.6988

	0.6176
	0.7163

	0.6228
	0.7217



Table 5.7 - Modal Load Participation Ratios
	Case
	ItemType
	Item
	Static
%
	Dynamic
%

	Modal
	Acceleration
	UX
	90.38
	62.28

	Modal
	Acceleration
	UY
	99.26
	89.96

	Modal
	Acceleration
	UZ
	0
	0



Table 5.8 - Modal Direction Factors
	Case
	Mode
	Period
sec
	UX
	UY
	UZ
	RZ

	Modal
	1
	0.175
	0
	0.999
	0
	0.001

	Modal
	2
	0.082
	0
	0.991
	0
	0.009

	Modal
	3
	0.079
	0.71
	0.118
	0
	0.172

	Modal
	4
	0.052
	0
	0
	0
	1

	Modal
	5
	0.047
	0.021
	0.004
	0
	0.975

	Modal
	6
	0.041
	0.005
	0.022
	0
	0.973

	Modal
	7
	0.033
	0.01
	0.001
	0
	0.989

	Modal
	8
	0.028
	0
	0.015
	0
	0.985

	Modal
	9
	0.027
	0.009
	0.004
	0
	0.987

	Modal
	10
	0.027
	0.04
	0.003
	0
	0.957

	Modal
	11
	0.026
	0.043
	0.002
	0
	0.954

	Modal
	12
	0.025
	0.031
	0.004
	0
	0.966

	Modal
	13
	0.025
	0.001
	0
	0
	0.999

	Modal
	14
	0.024
	0.002
	0.001
	0
	0.996

	Modal
	15
	0.024
	0.037
	0.123
	0
	0.841
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